SECTION 08 53 13

VINYL WINDOWS

Display hidden notes to specifier. (Don't know how? Click Here) 
 Copyright 2006 -  2024 ARCAT, Inc. - All rights reserved

PART 1    GENERAL
1.1	SECTION INCLUDES
A.	Vinyl windows for new construction.
B.	Vinyl commercial windows.
C.	Sliding patio doors.
D.	Vinyl replacement windows.
1.2	RELATED SECTIONS
A.	Section 03 30 00 - Cast-in-Place Concrete.
B.	Section 04 27 23 - Cavity Wall Unit Masonry.
C.	Section 06 10 00 - Rough Carpentry.
D.	Section 06 20 00 - Finish Carpentry.
E.	Section 07 46 16 - Aluminum Siding.
1.3	REFERENCES
A.	American Architectural Manufacturers Association (AAMA): 
1.	AAMA/WDMA/CSA 101/I.S.2/A440-05, A440-08, A440-11 and A440-17 - NAFS - North American Fenestration Standard Specification for windows, doors, and skylights.
2.	AAMA 701/702 - Combined Voluntary Specifications for Pile Weather strip and Replaceable Fenestration Weather seals.
3.	AAMA 902 - Voluntary Specification for Sash Balances.
B.	ASTM International (ASTM):
1.	ASTM E 283 - Standard Test Method for Determining the Rate of Air Leakage Through Exterior Windows, Curtain Walls and Doors Under Specified Pressure Differences Across the Specimen.
2.	ASTM E 330 - Standard Test Method for Structural Performance of Exterior Windows, Curtain Walls and Doors by Uniform Static Air Pressure Difference.
3.	ASTM E 547 - Standard Test Method for Water Penetration of Exterior Windows, Skylights, Doors and Curtain Walls by Cyclic Static Air Pressure Difference.
4.	ASTM E2190 - Standard Specification for the Classification of the Durability of Sealed Insulating Glass Units.
5.	ASTM F588 - Standard Test Methods for Measuring the Forced Entry Resistance of Window Assemblies, Excluding Glazing Impact.
C.	NFRC 100/200/500 - Procedures for Determining Fenestration Product U-Factors, Solar Heat Gain Coefficient (SHGc), and Visible Transmittance at Normal Incidence (VT).
1.4	SUBMITTALS
A.	Submit under provisions of Section 01 30 00 - Administrative Requirements.
B.	Product Data: Submit the following documents for each type of window.
1.	Manufacturer's technical data, product descriptions and installation guides.
2.	Elevation for each style window specified indicating its size, glazing type, muntin type and design.
3.	Manufacturer's head, jamb and sill details for each window type specified.
C.	Verification Samples: Operating units of each style window specified.
1.	Verification samples may be operating scaled-down mock-ups of actual-size units.
2.	Operating hardware such as balances, sash locks and weather-stripping.
3.	Verification samples will be returned to manufacturer's representative at project closeout.
D.	Test Reports: Certified independent testing agency reports indicating window units meet or exceed specified performance requirements.
1.5	QUALITY ASSURANCE
A.	Manufacturer Qualifications: Minimum ten years producing vinyl (PVC) windows.
B.	Installer Qualifications: Minimum 2 years of experience on projects of similar size and acceptable to window manufacturer.
C.	Source Limitations: Obtain window units from one manufacturer through a single source.
D.	Testing: Provide window units independently tested and found to be in compliance with AAMA/WDMA/CSA 101/I.S.2/A440-05, A440-08, A440-11 or A440-17 performance standards.
E.	Code Compliance: Provide windows that are labeled in compliance with the jurisdiction having authority in the location of the project.
F.	Mock-Up: Provide a mock-up for evaluation of surface preparation techniques and application workmanship.
1.	Finish areas designated by Architect.
2.	Do not proceed with remaining work until workmanship and color are approved by Architect.
3.	Rebuild mock-up area as required to produce acceptable work.
1.6	DELIVERY, STORAGE, AND HANDLING
A.	Deliver windows to project site in undamaged condition; handle windows to prevent damage to components and to finishes.
B.	Store products in manufacturer's unopened packaging, out of direct sunlight or high temperature locations, until ready for installation.
1.7	PROJECT CONDITIONS
A.	Maintain environmental conditions (temperature, humidity and ventilation) within limits recommended by manufacturer for optimum results. Do not install products under environmental conditions outside manufacturer's recommended limits.
1.8	WARRANTY
A.	Manufacturer's standard warranty against defects in workmanship and materials.
1.	Limited Lifetime Limited Transferable warranty on extruded solid vinyl member and component parts. Insulated glass is warranted against material obstruction of transparency resulting from film formation or dust collection on the interior glass surfaces for a period of twenty (20) years. Consult warranty for complete details.
2.	Limited 10 Year warranty period for commercial project work such as apartments, housing authorities and other buildings not used by individual homeowners, covering all vinyl, glass and component parts. Consult warranty for complete details.
PART 2    PRODUCTS
2.1	MANUFACTURERS
A.	Acceptable Manufacturer: Harvey Building Products , which is located at:<BR />1400 Main St.<BR />Waltham, MA 02451-1689<BR />Toll Free Tel: 800-822-0437<BR />Email: request info (architects@harveybp.com);Web: https://www.harveywindows.com 
B.	Substitutions: Not permitted.
C.	Requests for substitutions will be considered in accordance with provisions of Section 01 60 00 - Product Requirements. Substitutions must be submitted to Architect two weeks prior to bid opening.
2.2	NEW CONSTRUCTION TRIBUTE DOUBLE HUNG WINDOWS
A.	Construction:
1.	Frame: 0.065 inch (1.65 mm) thick polyvinyl chloride (PVC). Miter cut and fusion welded corners. Operable sash: 0.070 inch (1.8 mm) thick. Fusion welded corners.
2.	Siding Attachment: With or without extension jamb receiver pocket.
a.	Integral 13/16 inch (21 mm) "J" fin pocket.
b.	Integral L-fin. Only available with receiver pocket.
c.	L-fin (Integral J w/ L-adapter).
3.	Color: White Vinyl.
4.	Color: White Vinyl with Dark Bronze Exterior Finish - Painted.
5.	Color: White Vinyl with Black Exterior Finish - Painted.
6.	Color: Custom Exterior Finish - Painted. As determined by the Architect.
7.	Glazing: Insulating glass units secured to sash frame using a silicone sealant and rigid PVC glazing bead. Complies with ASTM E2190.
8.	Sash Balances: Factory calibrated block and tackle, complying with AAMA-902. Balance cords shall be anchored to locking terminal housings that lock in place when the sash is tilted in. The locking terminal and pivot bar system shall provide accurate alignment of the sash and the frame during operation.
9.	Two low-profile sash locks operate tilt release latches allowing sash to tilt in. 
10.	Weather Stripping: In compliance with AAMA 701.2.
11.	Screens: Extruded aluminum full screen with 16 x 16 VIEWS (Virtually Invisible Enhanced Window Screen) mesh.
12.	Screens:  Extruded aluminum locking half screen with 16 x 16 VIEWS (Virtually Invisible Enhanced Window Screen) mesh. 
13.	Screens: Premium FlexScreen (Standard on Exterior Painted) 
14.	Grids: 5/8 inch (16 mm) Colonial contour grids between glass (GBG) dividers.
15.	Grids: 1 inch (25 mm) Colonial contour grids between glass (GBG) dividers. 
16.	Grids: 5/8 inch (16 mm) SDL (Simulated Divided Lites).
17.	Grids: 1 inch (25 mm) SDL (Simulated Divided Lites).
B.	Performance:
1.	Structural Rating: H-LC35 (DP 35) - Test Size: 48 inches x 84 inches (1219 mm x 2134 mm) in accordance with AAMA/WDMA/CSA 101/I.S.2 /A440-17.
2.	Structural Rating: H-LC 50 (DP 50) - Test Size: 42 inches x 77 inches (1067 mm x 1956 mm) in accordance with AAMA/WDMA/CSA 101/I.S.2 /A440-17.
3.	Forced Entry: Type B, Grade 10 in accordance with ASTM F 588.
4.	Glazing Type: Thermal transmittance in accordance with NFRC 100/200/500.
a.	ThermaLock RS No Grids: U-Factor 0.25/ R-Value 4.0/ SHGc 0.29/ VT 0.52.
b.	ThermaLock RS With Grids: U-Factor 0.25/ R-Value 4.0/ SHGc 0.26/ VT 0.46.
c.	ThermaLock 3X No Grids: FOAM U-Factor 0.21/ R-Value 4.76/ SHGc 0.24/ VT 0.44.
d.	ThermaLock 3x With Grids: FOAM U-Factor 0.22/ R-Value 4.54/ SHGc 0.21/ VT 0.39.
e.	SunGain No Grids: U-Factor 0.30/ R-Value 3.33/ SHGc 0.48/ VT 0.58.
f.	SunGain With Grids: U-Factor 0.30/ R-Value 3.33/ SHGc 0.43/ VT 0.51.
g.	ThermaGuard No Grids: U-Factor 0.29/ R-Value 3.44/ SHGc 0.30/ VT 0.53.
h.	ThermaGuard With Grids: U-Factor 0.29/ R-Value 3.44/ SHGc 0.27/ VT 0.47.
2.3	NEW CONSTRUCTION SLIMLINE SINGLE HUNG WINDOWS
A.	Construction:
1.	Frame: 0.065 inch (1.7 mm) thick polyvinyl chloride (PVC). Miter cut and fusion welded corners. Sash: 0.065 inch (1.7 mm) thick. Fusion welded corners.
2.	Siding Attachment: With or without extension jamb receiver pocket.
a.	Integral 13/16 inch (21 mm) "J" fin pocket. 
b.	Integral L-fin (Only available with receiver pocket).
c.	L-fin (Integral J w/ L-adapter).
3.	Color: White Vinyl.
4.	Glazing: Insulating glass units secured to sash frame using a silicone sealant and dual durometer glazing bead. Complies with ASTM E 2190.
5.	Sash Balances: Factory calibrated block and tackle, complying with AAMA-902. Balance cords shall be anchored to glass filled nylon terminal housings that lock in place once the sash is tilted in. The locking terminal and pivot bar system shall be designed to positively interlock, to provide accurate alignment of the sash and the frame during installation and operation.
6.	Sash Locks: Knife type locks anchored with screws. Double locks when openings are 30 1/2 inches (774 mm) wide and greater.
7.	Weather Stripping: In compliance with AAMA 701.2.
8.	Screens:  FlexScreen half screen.  18 x 16 charcoal finish fiberglass mesh. 
9.	Screens: Extruded aluminum half screen. 18 x 16 charcoal finish fiberglass mesh.
10.	Screens:  Rolled Form aluminum half screen. 18 x 16 charcoal finish fiberglass mesh. 
11.	Grids: 5/8 inch (16 mm) Colonial contour grids between glass (GBG) dividers.
B.	Performance:
1.	Structural Rating: H-LC30 (DP30) - Test Size: 46 inches x 77 inches (1168 mm x 1956 mm) in accordance with AAMA/WDMA/CSA 101/I.S.2/A440-17.
2.	Structural Rating: H-LC50 (DP50) - Test Size: 40 inches x 63 inches (1016 mm x 1600 mm) in accordance with AAMA/WDMA/CSA 101/I.S.2/A440-17.
3.	Forced Entry: Type B, Grade 10 in accordance with ASTM F 588.
4.	Sound Transmission Class (STC): 26.
5.	Sound Transmission Class (STC): 34. 
6.	Glazing Type: Thermal transmittance in accordance with NFRC 100/200/500.
a.	Clear No Grids: U-Factor 0.46/ R-Value 2.17/ SHGc 0.61/ VT 0.64.
b.	Clear With Grids: U-Factor 0.46/ R-Value 2.17/ SHGc 0.54/ VT 0.57.
c.	Low-E No Grids: U-Factor 0.32/ R-Value 3.12/ SHGc 0.32/ VT 0.57.
d.	Low-E With Grids: U-Factor 0.32/ R-Value 3.12/ SHGc 0.29/ VT 0.50.
e.	ThermaGuard No Grids: U-Factor 0.29/ R-Value 3.44/ SHGc 0.31/ VT 0.57. 
f.	ThermaGuard With Grids: U-Factor 0.29/ R-Value 3.44/ SHGc 0.28/ VT 0.50.
g.	ThermaLock RS No Grids: U-Factor 0.25/ R-Value 4.00/ SHGc 0.31/ VT 0.56.
h.	ThermaLock RS With Grids: U-Factor 0.25/ R-Value 4.00/ SHGc 0.28/ VT 0.50.
i.	SunGain No Grids: U-Factor 0.30/ R-Value 3.33/ SHGc 0.51/ VT 0.62.
j.	SunGain With Grids: U-Factor 0.30/ R-Value 3.33/ SHGc 0.46/ VT 0.55.
k.	SunShield No Grids: U-Factor 0.28/ R-Value 3.57/ SHGc 0.22/ VT 0.51.
l.	SunShield With Grids: U-Factor 0.28/ R-Value 3.57/ SHGc 0.20/ VT 0.45.
2.4	NEW CONSTRUCTION SLIMLINE DOUBLE HUNG WINDOWS 
A.	Construction: 
1.	Frame and Sash: 0.065 inch (1.7 mm) thick polyvinyl chloride (PVC) with miter cut and fusion welded corners.
2.	Siding Attachment: With or without extension jamb receiver pocket.
a.	Integral 13/16 inch (21 mm) "J" fin pocket. 
b.	Integral L-fin. Only available with receiver pocket.
c.	L-fin (Integral J with L-adapter).
3.	Color: White Vinyl.
4.	Glazing: Insulating glass units secured to sash frame using a silicone sealant and dual durometer glazing bead. Complies with ASTM E 2190. 
5.	Sash Balances: Factory calibrated block and tackle, complying with AAMA-902. Balance cords shall be anchored to glass filled nylon terminal housings that lock in place once the sash is tilted in. The locking terminal and pivot bar system shall be designed to positively interlock, to provide accurate alignment of the sash and the frame during installation and operation. 
6.	Sash Locks: Knife type locks anchored with screws. Double locks when openings are 30 1/2 inches (774 mm) wide and greater.
7.	Weather Stripping: In compliance with AAMA 701.2. 
8.	Screens:  FlexScreen half screen.  18 x 16 charcoal finish fiberglass mesh. 
9.	Screens: Extruded aluminum half screen. 18 x 16 charcoal finish fiberglass mesh.
10.	Screens: Rolled Form aluminum half screen. 18 x 16 charcoal finish fiberglass mesh. 
11.	Screens:  FlexScreen full screen.  18 x 16 charcoal finish fiberglass mesh. 
12.	Screens:  Extruded aluminum full screen. 18 x 16 charcoal finish fiberglass mesh. 
13.	Screens:  Rolled Form aluminum full screen. 18 x 16 charcoal finish fiberglass mesh. 
14.	Grids: 5/8 inch (16 mm) Colonial contour grids between glass (GBG) dividers. 
B.	Performance:
1.	Structural Rating: H-LC30 (DP30) - Test Size: 46 inches x 77 inches (1168 mm x 1956 mm) in accordance with AAMA/WDMA/CSA 101/I.S.2/A440-17 
2.	Structural Rating: H-LC50 (DP50) - Test Size: 40 inches x 63 inches (1016 mm x 1600 mm) in accordance with AAMA/WDMA/CSA 101/I.S.2/A440-17. 
3.	Forced Entry: Type B, Grade 10 in accordance with ASTM F 588. 
4.	Sound Transmission Class (STC): 26. 
5.	Sound Transmission Class (STC): 34. 
6.	Glazing Type: Thermal transmittance in accordance with NFRC 100/200/500.
a.	Clear No Grids: U-Factor 0.46/ R-Value 2.17/ SHGc 0.61/ VT 0.64.
b.	Clear With Grids: U-Factor 0.46/ R-Value 2.17/ SHGc 0.54/ VT 0.57.
c.	Low-E No Grids: U-Factor 0.32/ R-Value 3.12/ SHGc 0.32/ VT 0.57.
d.	Low-E With Grids: U-Factor 0.32/ R-Value 3.12/ SHGc 0.29/ VT 0.50.
e.	ThermaGuard No Grids: U-Factor 0.29/ R-Value 3.44/ SHGc 0.31/ VT 0.57.
f.	ThermaGuard With Grids: U-Factor 0.29/ R-Value 3.44/ SHGc 0.28/ VT 0.50.
g.	ThermaLock RS No Grids: U-Factor 0.25/ R-Value 4.00/ SHGc 0.31/ VT 0.55.
h.	ThermaLock RS With Grids: U-Factor 0.25/ R-Value 4.00/ SHGc 0.28/ VT 0.49.
i.	SunGain No Grids: U-Factor 0.30/ R-Value 3.33/ SHGc 0.51/ VT 0.62.
j.	SunGain With Grids: U-Factor 0.30/ R-Value 3.33/ SHGc 0.46/ VT 0.55.
2.5	NEW CONSTRUCTION V100 SINGLE HUNG WINDOWS
A.	Construction:
1.	Frame: 0.065 inch (1.7 mm) thick polyvinyl chloride (PVC). Miter cut and fusion welded corners. Sash: 0.065 inch (1.7 mm) thick. Fusion welded corners.
2.	Siding Attachment: With or without extension jamb receiver pocket.
a.	Integral 13/16 inch (21 mm) "J" fin pocket. 
b.	Integral L-fin (Only available with receiver pocket).
c.	L-fin (Integral J w/ L-adapter).
3.	Color: White Vinyl.
4.	Glazing: Insulating glass units secured to sash frame using a silicone sealant and dual durometer glazing bead. Complies with ASTM E 2190.
5.	Sash Balances: Factory calibrated block and tackle, complying with AAMA-902. Balance cords shall be anchored to glass filled nylon terminal housings that lock in place once the sash is tilted in. The locking terminal and pivot bar system shall be designed to positively interlock, to provide accurate alignment of the sash and the frame during installation and operation.
6.	Sash Locks: Knife type locks anchored with screws. Double locks when openings are 30 1/2 inches (774 mm) wide and greater.
7.	Weather Stripping: In compliance with AAMA 701.2.
8.	Screens: Rolled Form aluminum half screen. 18 x 16 charcoal finish fiberglass mesh.
9.	Screens:  FlexScreen half screen.  18 x 16 charcoal finish fiberglass mesh. 
10.	Grids: 5/8 inch (16 mm) Colonial contour grids between glass (GBG) dividers.
B.	Performance:
1.	Structural Rating: H-LC30 (DP30) - Test Size: 46 inches x 77 inches (1168 mm x 1956 mm) in accordance with AAMA/WDMA/CSA 101/I.S.2/A440-17.
2.	Structural Rating: H-LC50 (DP50) - Test Size: 40 inches x 63 inches (1016 mm x 1600 mm) in accordance with AAMA/WDMA/CSA 101/I.S.2/A440-17.
3.	Forced Entry: Type B, Grade 10 in accordance with ASTM F 588.
4.	Sound Transmission Class (STC): 26.
5.	Glazing Type: Thermal transmittance in accordance with NFRC 100/200/500.
a.	Clear No Grids: U-Factor 0.46/ R-Value 2.17/ SHGc 0.61/ VT 0.64.
b.	Clear With Grids: U-Factor 0.46/ R-Value 2.17/ SHGc 0.54/ VT 0.57.
c.	Low-E No Grids: U-Factor 0.32/ R-Value 3.12/ SHGc 0.32/ VT 0.57.
d.	Low-E With Grids: U-Factor 0.32/ R-Value 3.12/ SHGc 0.29/ VT 0.50.
e.	ThermaGuard No Grids: U-Factor 0.29/ R-Value 3.44/ SHGc 0.31/ VT 0.57.
f.	ThermaGuard With Grids: U-Factor 0.29/ R-Value 3.44/ SHGc 0.28/ VT 0.50.
g.	ThermaLock RS No Grids: U-Factor 0.25/ R-Value 4.00/ SHGc 0.31/ VT 0.55.
h.	ThermaLock RS With Grids: U-Factor 0.25/ R-Value 4.00/ SHGc 0.28/ VT 0.49.
i.	SunGain No Grids: U-Factor 0.30/ R-Value 3.33/ SHGc 0.51/ VT 0.62.
j.	SunGain With Grids: U-Factor 0.30/ R-Value 3.33/ SHGc 0.46/ VT 0.55.
k.	SunShield No Grids: U-Factor 0.28/ R-Value 3.57/ SHGc 0.22/ VT 0.59.
l.	SunShield With Grids: U-Factor 0.28/ R-Value 3.57/ SHGc 0.20/ VT 0.45.
2.6	NEW CONSTRUCTION CLASSIC DOUBLE HUNG WINDOWS
A.	Construction:
1.	Frame: 0.065 inch (1.7 mm) thick polyvinyl chloride (PVC) with miter cut and fusion welded corners.  Sash:   0.060 inch (1.5 mm) thick polyvinyl chloride (PVC) with miter cut and fusion welded corners.
2.	Siding Attachment: With or without extension jamb receiver pocket.
a.	Integral 13/16 inch (21 mm) "J" fin pocket.
b.	Integral L-fin. Only available with receiver pocket.
c.	L-fin (Integral J w/ L-adapter).
3.	Color: White Vinyl.
4.	Color: Almond Vinyl.
5.	Color: White Vinyl with Dark Bronze Exterior Finish - Painted.
6.	Color: White Vinyl with Black Exterior Finish - Painted.
7.	Color: Custom Exterior Finish - Painted. As determined by the Architect.
8.	Glazing: Insulating glass units secured to sash frame using a silicone sealant and exterior glazing bead. Complies with ASTM E2190.
9.	Sash Balances: Factory calibrated block and tackle, complying with AAMA-902. Balance cords shall be anchored to locking terminal housings when the sash is tilted in. The locking terminal and pivot bar system shall provide accurate alignment of the sash and the frame during operation.
10.	Sash Locks: Cam type lock anchored with screws. Double locks when openings are 30 1/2 inches (774 mm) wide and greater.
11.	Weather Stripping: In compliance with AAMA 701.2.
12.	Screens: Extruded aluminum full screen. 18 x 16 charcoal finish fiberglass mesh.
13.	Screens: Extruded aluminum locking half screen. 18 x 16 charcoal finish fiberglass mesh.
14.	Screens:  FlexScreen full screen (Standard on Exterior Painted). 
15.	Screens: FlexScreen half screen (Standard on Exterior Painted)
16.	Grids: 5/8 inch (16 mm) Colonial contour grids between glass (GBG) dividers.
17.	Grids: 1 inch (25 mm) Colonial contour grids between glass (GBG) dividers. 
18.	Grids: 5/8 inch (16 mm) SDL (Simulated Divided Lites).
19.	Grids: 1 inch (25 mm) SDL (Simulated Divided Lites).
B.	Performance:
1.	Structural rating H-LC40 (DP40) - Test Size: 48 inches x 84 inches (1219 mm x 2134 mm) in accordance with AAMA/WDMA/CSA 101/I.S.2/A440-17.
2.	Structural rating H-LC50 (DP50) - Test Size: 42 inches x 77 inches (1067 mm x 1956 mm) in accordance with AAMA/WDMA/CSA 101/I.S.2/A440-17.
3.	Forced Entry: Type B, Grade 10 in accordance with ASTM F 588.
4.	Sound Transmission Class (STC): 27.
5.	Sound Transmission Class (STC): 34. 
6.	Thermal Transmittance: The following values are in accordance with NFRC 100/200/500.
a.	Clear No Grids: U-Factor 0.45/ R-Value 2.17/ SHGc 0.59/ VT 0.62.
b.	Clear With Grids: U-Factor 0.45/ R-Value 2.17/ SHGc 0.53/ VT 0.55.
c.	Low-E No Grids: U-Factor 0.32/ R-Value 3.03/ SHGc 0.31/ VT 0.55.
d.	Low-E With Grids: U-Factor 0.32/ R-Value 3.03/ SHGc 0.28/ VT 0.49.
e.	ThermaGuard No Grids: U-Factor 0.29/ R-Value 3.44/ SHGc 0.31/ VT 0.55.
f.	ThermaGuard With Grids: U-Factor 0.29/ R-Value 3.44/ SHGc 0.28/ VT 0.49.
g.	ThermaLock 3X No Grids: U-Factor 0.21/ R-Value 4.76/ SHGc 0.25/ VT 0.46.
h.	ThermaLock 3X With Grids: U-Factor 0.22/ R-Value 4.54/ SHGc 0.22/ VT 0.41.
i.	ThermaLock RS No Grids: U-Factor 0.25/ R-Value 4.00/ SHGc 0.30/ VT 0.54.
j.	ThermaLock RS With Grids: U-Factor 0.25/ R-Value 4.00/ SHGc 0.27/ VT 0.48.
k.	ThermaLock No Grids:  U-Factor 0.27/ R-Value 3.70/ SHGc 0.29/ VT 0.49. 
l.	ThermaLock With Grids:  U-Factor 0.27/ R-Value 3.70/ SHGc 0.26/ VT 0.44. 
m.	SunGain No Grids: U-Factor 0.30/ R-Value 3.33/ SHGc 0.50/ VT 0.60.
n.	SunGain With Grids: U-Factor 0.30/ R-Value 3.33/ SHGc 0.45/ VT 0.54. 
o.	SunShield No Grids: U-Factor 0.28/ R-Value 3.57/ SHGc 0.21/ VT 0.49.
p.	SunShield With Grids: U-Factor 0.28/ R-Value 3.57/ SHGc 0.19/ VT 0.44.
2.7	NEW CONSTRUCTION CASEMENT WINDOWS
A.	Construction:
1.	Frame and Sash: 0.070 inch (1.8 mm) thick polyvinyl chloride (PVC) with miter cut and fusion welded corners.
2.	Siding Attachment: With or without extension jamb receiver pocket.
a.	Integral 13/16 inch (21 mm) "J" fin pocket.
b.	Integral L-fin. Only available with receiver pocket.
c.	L-fin (Integral J w/ L-adapter).
3.	Color: White Vinyl.
4.	Color: Almond Vinyl.
5.	Color: White Vinyl with Dark Bronze Exterior Finish - Painted.
6.	Color: White Vinyl with Black Exterior Finish - Painted.
7.	Color: Custom Exterior Finish - Painted. As determined by the Architect.
8.	Glazing: Insulating glass units secured to sash frame using a silicone sealant and rigid PVC glazing bead. Complies with ASTM E2190. 
9.	Hinges: Maxim 14 series.
10.	Sash Locks: Sequentially locking multi-point type with single handle actuator.
11.	Operator: Encore series.
12.	Weather stripping: In compliance with AAMA 701.2.
13.	Screens: Extruded aluminum frame. 18 x 16 charcoal finish fiberglass mesh.
14.	Screens: Extruded aluminum frame. 18 x 16 charcoal finish aluminum mesh.
15.	Grids: 5/8 inch (16 mm) Colonial contour grids between glass (GBG) dividers.
16.	Grids: 1 inch (25 mm) Colonial contour grids between glass (GBG) dividers. 
17.	Grids: 5/8 inch (16 mm) SDL (Simulated Divided Lites).
18.	Grids: 1 inch (25 mm) SDL (Simulated Divided Lites).
B.	Performance:
1.	Structural Rating: C-55 (DP 55) Test Size:  36 inches x 80 inches (914 mm x 2032 mm) in accordance with AAMA/WDMA/CSA 101/I.S.2/A440-17.
2.	Forced Entry: Type B, Grade 10 in accordance with ASTM F588.
3.	Sound Transmission Class (STC): 26.
4.	Sound Transmission Class (STC): 29.
5.	Sound Transmission Class (STC): 34. 
6.	Glazing Type: Thermal transmittance in accordance with NFRC 100/200/500.
a.	Clear No Grids: U-Factor 0.43/ R-Value 2.32/ SHGc 0.47/ VT 0.49.
b.	Clear With Grids: U-Factor 0.43/ R-Value 2.32/ SHGc 0.42/ VT 0.44.
c.	Low-E No Grids: U-Factor 0.31/ R-Value 3.22/ SHGc 0.25/ VT 0.44.
d.	Low-E With Grids: U-Factor 0.31/ R-Value 3.22/ SHGc 0.22/ VT 0.39.
e.	ThermaGuard No Grids: U-Factor 0.29/ R-Value 3.44/ SHGc 0.24/ VT 0.44.
f.	ThermaGuard With Grids: U-Factor 0.29 / R-Value 3.44/ SHGc 0.22/ VT 0.39.
g.	ThermaLock No Grids: U-Factor 0.27/ R-Value 3.70/ SHGc 0.23/ VT 0.39. 
h.	ThermaLock With Grids: U-Factor 0.27/ R-Value 3.70/ SHGc 0.21/ VT 0.35.
i.	ThermaLock 3X No Grids: U-Factor 0.22/ R-Value 4.54/ SHGc 0.20/ VT 0.36.
j.	ThermaLock 3X With Grids: U-Factor 0.23/ R-Value 4.54/ SHGc 0.18/ VT 0.32.
k.	SunGain No Grids: U-Factor 0.29/ R-Value 3.44/ SHGc 0.40/ VT 0.48.
l.	SunGain With Grids: U-Factor 0.29/ R-Value 3.44/ SHGc 0.36/ VT 0.43.
m.	SunShield No Grids: U-Factor 0.27/ R-Value 3.70/ SHGc 0.17/ VT 0.39.
n.	SunShield With Grids: U-Factor 0.27/ R-Value 3.70/ SHGc 0.15/ VT 0.35.
2.8	NEW CONSTRUCTION AWNING WINDOWS
A.	Construction:
1.	Frame and Sash: 0.070 inch (1.8 mm) thick polyvinyl chloride (PVC) with miter cut and fusion welded corners.
2.	Siding Attachment: With or without extension jamb receiver pocket.
a.	Integral 13/16 inch (21 mm) "J" fin pocket.
b.	Integral L-fin. Only available with receiver pocket.
c.	L-fin (Integral J w/ L-adapter).
3.	Color: White Vinyl.
4.	Color: Almond Vinyl.
5.	Color: White Vinyl with Dark Bronze Exterior Finish - Painted.
6.	Color: White Vinyl with Black Exterior Finish - Painted.
7.	Color: Custom Exterior Finish - Painted. As determined by the Architect.
8.	Glazing: Insulating glass units secured to sash frame using a silicone sealant and rigid PVC glazing bead. Complies with ASTM E2190.
9.	Hinges: Maxim 13 series.
10.	Sash Locks: Maxim 24 Series single point locks.
11.	Weather stripping: In compliance with AAMA 701.2.
12.	Screens: Extruded aluminum frame. 18 x 16 charcoal finish fiberglass mesh.
13.	Screens: Extruded aluminum frame. 18 x 16 charcoal finish aluminum mesh.
14.	Grids: 5/8 inch (16 mm) Colonial contour grids between glass (GBG) dividers.
15.	Grids: 1 inch (25 mm) Colonial contour grids between glass (GBG) dividers.
16.	Grids: 5/8 inch (16 mm) SDL (Simulated Divided Lites).
17.	Grids: 1 inch (25 mm) SDL (Simulated Divided Lites).
B.	Performance:
1.	Structural Rating: AP-LC40 (DP40) - Test Size: 60 inches x 42 inches (1524 mm x 1067 mm) in accordance with AAMA/WDMA/CSA 101/I.S.2/A440-05.
2.	Structural Rating: AP-C75 (DP 75). Test Size: 48 inches x 32 inches (1219 mm x 813 mm).
3.	Structural Rating: AP-LC55 (DP 55). Test Size: 48 inches x 58 inches (1219 mm x 1473 mm).
4.	Forced Entry: Type B, Grade 10 in accordance with ASTM F588.
5.	Sound Transmission Class (STC): 26.
6.	Sound Transmission Class (STC): 29.
7.	Sound Transmission Class (STC): 34. 
8.	Glazing Type: Thermal transmittance in accordance with NFRC 100/200/500.
a.	Clear No Grids: U-Factor 0.43/ R-Value 2.32/ SHGc 0.47/ VT 0.49.
b.	Clear With Grids: U-Factor 0.43/ R-Value 2.32/ SHGc 0.42/ VT 0.44.
c.	Low-E No Grids: U-Factor 0.31/ R-Value 3.12/ SHGc 0.25/ VT 0.44.
d.	Low-E With Grids: U-Factor 0.31/ R-Value 3.12/ SHGc 0.22/ VT 0.39. 
e.	ThermaGuard No Grids: U-Factor 0.29/ R-Value 3.44/ SHGc 0.24/ VT 0.44.
f.	ThermaGuard With Grids: U-Factor 0.29/ R-Value 3.44/ SHGc 0.22/ VT 0.39.
g.	ThermaLock No Grids: U-Factor 0.27/ R-Value 3.70/ SHGc 0.23/ VT 0.39. 
h.	ThermaLock With Grids: U-Factor 0.27/ R-Value 3.70/ SHGc 0.21/ VT 0.35.
i.	ThermaLock 3X No Grids: U-Factor 0.23/ R Value 4.34/SHGc 0.20/ VT 0.36.
j.	ThermaLock 3X With Grids: U-Factor 0.23/ R Value 4.34/ SHGc 0.18/ VT 0.32.
k.	SunGain No Grids: U-Factor 0.30/ R-Value 3.33/ SHGc 0.40/ VT 0.48.
l.	SunGain With Grids: U-Factor 0.30/ R-Value 3.33/ SHGc 0.36/ VT 0.43.
m.	SunShield No Grids: U-Factor 0.28/ R-Value 3.57/ SHGc 0.17/ VT 0.39.
n.	SunShield With Grids: U-Factor 0.28/ R-Value 3.57/ SHGc 0.15/ VT 0.35.
2.9	NEW CONSTRUCTION HOPPER WINDOWS
A.	Construction:
1.	Frame: 0.065 inch (1.7 mm) thick polyvinyl chloride (PVC), Frame corners miter cut and fusion welded. Sash: 0.065 inch (1.7 mm) thick with mechanically fastened corners.
2.	Siding Attachment: Snap-on applied 3/4 inch (20 mm) "J" fin.
3.	Siding Attachment: Snap-on applied "L" fin.
4.	Color: White Vinyl.
5.	Color: Almond Vinyl.
6.	Color: White Vinyl with Dark Bronze Exterior Finish - Painted.
7.	Color: White Vinyl with Black Exterior Finish - Painted.
8.	Color: Custom Exterior Finish - Painted. As determined by the Architect.
9.	Glazing: Insulating glass units shall be channel glazed and secured to sash frame using a sealant in corners. Complies with ASTM E2190.
10.	Hinges: Stainless Steel Maxim 13 series.
11.	Sash Locks: Knife type. Double locks when openings are 30 3/4 inches (781 mm) and wider.
12.	Weather stripping: In compliance with AAMA 701.2.
13.	Screens: Extruded aluminum frame. 18 x 16 charcoal finish fiberglass mesh.
14.	Screens: Extruded aluminum frame. 18 x 16 charcoal finish aluminum mesh.
15.	Grids: 5/8 inch (16 mm) Colonial contour grids between glass (GBG) dividers. 
16.	Grids: 1 inch (25 mm) Colonial contour grids between glass (GBG) dividers.
B.	Performance:
1.	Structural Rating: AP-R-15(DP15) - Test Size: 48 inches x 32 inches (1219 mm x 813 mm) in accordance with AAMA/WDMA/CSA 101/I.S.2/A440-05.
2.	Forced Entry: Type B, Grade 10 in accordance with ASTM F 588.
3.	Sound Transmission Class (STC): 27.
4.	Sound Transmission Class (STC): 33. 
5.	Glazing Type: Thermal transmittance in accordance with NFRC 100/200/500.
a.	Clear No Grids: U-Factor 0.46/ R-Value 2.17/ SHGc 0.55/ VT 0.57.
b.	Clear With Grids: U-Factor 0.46/ R-Value 2.17/ SHGc 0.50/ VT 0.51.
c.	Low-E No Grids: U-Factor 0.34/ R-Value 2.94/ SHGc 0.29/ VT 0.51.
d.	Low-E With Grids: U-Factor 0.34/ R-Value 2.94/ SHGc 0.26/ VT 0.46.
e.	DSB Low-E/Argon No Grids: U-Factor 0.30/ R-Value 3.33/ SHGc 0.28/ VT 0.50.
f.	DSB Low-E/Argon With Grids: U-Factor 0.30/ R-Value 3.33/ SHGc 0.26/ VT 0.45.
g.	ThermaLock RS No Grids: U-Factor 0.27/ R-Value 3.70/ SHGc 0.28/ VT 0.50. 
h.	ThermaLock RS With Grids: U-Factor 0.27/ R-Value 3.70/ SHGc 0.26/ VT 0.45.
i.	ThermaLock 3X No Grids: U-Factor 0.23/ R-Factor 4.34/ SHGc 0.23/ VT 0.42.
j.	ThermaLock 3X With Grids: U-Factor 0.23/ R-Factor 4.34/ SHGc 0.21/ VT 0.38.
k.	SunGain No Grids: U-Factor 0.30/ R-Value 3.33/ SHGc 0.46/ VT 0.55.
l.	SunGain With Grids: U-Factor 0.30/ R-Value 3.33/ SHGc 0.42/ VT 0.50.
2.10	NEW CONSTRUCTION ROLLING WINDOWS
A.	Construction:
1.	Frame: 0.090 inch (2.3 mm) thick polyvinyl chloride (PVC). Miter cut and fusion welded corners. Sash: 0.080 inch (2 mm) thick. Miter cut and fusion welded corners.
2.	Siding Attachment: With or without extension jamb receiver pocket.
a.	Integral 13/16 inch (20 mm) "J" fin pocket.
b.	Integral L-fin. Only available with receiver pocket. 
c.	L-fin (Integral J with L adapter).
3.	Color: White Vinyl.
4.	Color: Almond Vinyl.
5.	Color: White Vinyl with Dark Bronze Exterior Finish - Painted.
6.	Color: White Vinyl with Black Exterior Finish - Painted.
7.	Color: Custom Exterior Finish - Painted. As determined by the Architect.
8.	Glazing: Insulating glass units secured to sash frame using a silicone sealant and exterior dual durometer glazing bead. Complies with ASTM E2190.
9.	Sash Locks: Cam type.
10.	Weather stripping: In compliance with AAMA 701.2.
11.	Screens: Extruded aluminum frame. 18 x 16 charcoal finish fiberglass mesh.
12.	Screens: Extruded aluminum frame. 18 x 16 charcoal finish aluminum mesh.
13.	Screens: FlexScreen (Standard on Exterior Painted)
14.	Grids: 5/8 inch (16 mm) Colonial contour grids between glass (GBG) dividers.
15.	Grids: 1 inch (25 mm) Colonial contour grids between glass (GBG) dividers. 
16.	Grids: 5/8 inch (16 mm) SDL (Simulated Divided Lites).
17.	Grids: 1 inch (25 mm) SDL (Simulated Divided Lites).
B.	Performance:
1.	Structural Rating: HS-LC35 (DP 35) - Test Size: 72 inches x 62 1/2 inches (1829 mm x 1588 mm) in accordance with AAMA/WDMA/CSA 101/I.S.2/A440-11.
2.	Structural Rating: HS-LC35 (DP 25) - Test Size: 120 inches x 62 1/2 inches (3048 mm x 1588 mm) in accordance with AAMA/WDMA/CSA 101/I.S.2/A440-11.
3.	Forced Entry: Type A, Grade 10 in accordance with ASTM F 588.
4.	Sound Transmission Class (STC): 26 Two Lite.
5.	Sound Transmission Class (STC): 33 Two Lite.
6.	Glazing Type: Thermal transmittance in accordance with NFRC 100/200/500.
a.	Clear No Grids: U-Factor 0.47/ R-Value 2.17/ SHGc 0.60/ VT 0.62.
b.	Clear With Grids: U-Factor 0.47/ R-Value 2.17/ SHGc 0.53/ VT 0.55.
c.	Low-E No Grids: U-Factor 0.33/ R-Value 3.03/ SHGc 0.31/ VT 0.55.
d.	Low-E With Grids: U-Factor 0.33/ R-Value 3.03/ SHGc 0.28/ VT 0.49.
e.	ThermaGuard No Grids: U-Factor 0.30/ R-Value 3.33/ SHGc 0.31/ VT 0.55.
f.	ThermaGuard With Grids: U-Factor 0.30/ R-Value 3.33/ SHGc 0.28/ VT 0.49.
g.	ThermaLock RS No Grids: U-Factor 0.26/ R-Value 3.84/ SHGc 0.30/ VT 0.55.
h.	ThermaLock RS With Grids: U-Factor 0.26/ R-Value 3.84/ SHGc 0.27/ VT 0.49.
i.	ThermaLock 3X No Grids: U-Factor 0.22/ R Value 4.54/ SHGc 0.25/ VT 0.46.
j.	ThermaLock 3X With Grids: U-Factor 0.23/ R Value 4.34/ SHGc 0.22/ VT 0.41.
k.	SunGain No Grids: U-Factor 0.30/ R-Value 3.33/ SHGc 0.50/ VT 0.61.
l.	SunGain With Grids: U-Factor 0.30/ R-Value 3.33/ SHGc 0.45/ VT 0.54.
m.	SunShield No Grids:  U-Factor 0.29/ R-Value 3.44/ SHGc 0.21/ VT 0.49. 
n.	SunShield With Grids:  U-Factor 0.29/ R-Value 3.44/ SHGc 0.19/ VT 0.44. 
2.11	NEW CONSTRUCTION PICTURE WINDOWS
A.	Construction:
1.	Frame: 0.075 inch (1.9 mm) wall thick polyvinyl chloride (PVC). Miter cut and fusion welded corners.
2.	Siding Attachment: With or without extension jamb receiver pocket.
a.	Integral 13/16 inch (21 mm) "J" fin pocket.
b.	Integral L-fin. Only available with receiver pocket.
c.	L-fin (Integral J w/ L-adapter).
3.	Color: White Vinyl.
4.	Color: Almond Vinyl.
5.	Color: White Vinyl with Dark Bronze Exterior Finish - Painted.
6.	Color: White Vinyl with Black Exterior Finish - Painted.
7.	Color: Custom Exterior Finish - Painted. As determined by the Architect.
8.	Glazing: Insulating glass units secured to sash frame using a sealant in the corners and glazing bead. Complies with ASTM E2190. 
9.	Grids: 5/8 inch (16 mm) Colonial contour grids between glass (GBG) dividers.
10.	Grids: 1 inch (25 mm) Colonial contour grids between glass (GBG) dividers. 
11.	Grids: 5/8 inch (16 mm) SDL (Simulated Divided Lites).
12.	Grids: 1 inch (25 mm) SDL (Simulated Divided Lites).
B.	Performance:
1.	Structural Rating: F-C55 (DP55) - Test Size: 72 inches x 72 inches (1829 mm x 1829 mm) in accordance with AAMA/WDMA/CSA 101/I.S.2/A440-11.
2.	Forced Entry: Type D, Grade 10 in accordance with ASTM F 588.
3.	Sound Transmission Class (STC): 29.
4.	Sound Transmission Class (STC): 32.
5.	Glazing Type: Thermal transmittance in accordance with NFRC 100/200/500.
a.	Clear No Grids: U-Factor 0.45/ R-Value 2.22/ SHGc 0.63/ VT 0.66.
b.	Clear With Grids: U-Factor 0.45/ R-Value 2.22/ SHGc 0.56/ VT 0.59.
c.	Low-E No Grids: U-Factor 0.30/ R-Value 3.33/ SHGc 0.33/ VT 0.59.
d.	Low-E With Grids: U-Factor 0.30/ R-Value 3.33/ SHGc 0.30/ VT 0.52.
e.	Low-E/Argon No Grids: U-Factor 0.26/ R-Value 3.84/ SHGc 0.32/ VT 0.59.
f.	Low-E/Argon With Grids: U-Factor 0.26/ R-Value 3.84/ SHGc 0.29/ VT 0.52.
g.	ThermaLock No Grids: U-Factor 0.26/ R-Value 3.84/ SHGc 0.30/VT 0.52.
h.	ThermaLock With Grids: U-Factor 0.26/ R-Value 3.84/ SHGc 0.28/ VT 0.47.
i.	ThermaLock 3X No Grids: U-Factor 0.19/ R Value 5.26/SHGc 0.26/ VT 0.49.
j.	ThermaLock 3X With Grids: U-Factor 0.20/ R Value 5.00/SHGc 0.24/ VT 0.43.
k.	SunGain No Grids: U-Factor 0.27/ R-Value 3.70/ SHGc 0.53/ VT 0.64.
l.	SunGain With Grids: U-Factor 0.27/ R-Value 3.70/ SHGc 0.47/ VT 0.57.
m.	SunShield No Grids: U-Factor 0.25/ R-Value 4.00/ SHGc 0.22/ VT 0.52.
n.	SunShield With Grids: U-Factor 0.25/ R-Value 4.00/ SHGc 0.20/ VT 0.47
2.12	NEW CONSTRUCTION DESIGNER SHAPES WINDOWS
A.	Construction:
1.	Frame: Nominal 0.1 inch (2.5 mm) wall thickness polyvinyl chloride (PVC), Miter cut and fusion welded corners.
2.	Siding Attachment: Integral 13/16 inch (21 mm) "J" fin pocket.
3.	Siding Attachment: L-fin (Integral J w/ L-adapter).
4.	Color: White Vinyl.
5.	Color: Almond Vinyl.
6.	Color: White Vinyl with Dark Bronze Exterior Finish - Painted.
7.	Color: White Vinyl with Black Exterior Finish - Painted.
8.	Color: Custom Exterior Finish - Painted. As determined by the Architect.
9.	Glazing: Insulating glass units secured to sash frame using a silicone sealant and dual durometer glazing bead. Complies with ASTM E2190. 
10.	Grids: Colonial contour grids between glass (GBG) dividers.
B.	Performance:
1.	Structural Rating: F-C50 (DP50) - Test Size:  78 inches x 85 1/4 inches (1981 mm x 2165 mm) in accordance with AAMA/WDMA/CSA 101/I.S.2/A440-17.
2.	Forced Entry: Type D, Grade 10 in accordance with ASTM F588.
3.	Glazing Type: Thermal transmittance in accordance with NFRC 100/200/500.
a.	Clear DSB No Grids: U-Factor 0.46/ R-Value 2.17/ SHGc 0.68/ VT 0.72.
b.	Clear DSB With Grids: U-Factor 0.46/ R-Value 2.17/ SHGc 0.61/ VT 0.64.
c.	Low-E DSB No Grids: U-Factor 0.31/ R-Value 3.22/ SHGc 0.32/ VT 0.61.
d.	Low-E DSB With Grids: U-Factor 0.31/ R-Value 3.22/ SHGc 0.29/ VT 0.55.
e.	Low-E/Argon DSB No Grids: U-Factor 0.27/ R-Value 3.70/ SHGc 0.32/ VT 0.61.
f.	Low-E/Argon DSB With Grids: U-Factor 0.27/ R-Value 3.70/ SHGc 0.29/ VT - 0.55.
g.	ThermaLock DSB No Grids: U-Factor 0.27/ R-Value 3.70/ SHGc 0.30/VT 0.52.
h.	ThermaLock DSB With Grids: U-Factor 0.27/ R-Value 3.70/ SHGc 0.27/ VT 0.47.
i.	SunGain DSB No Grids: U-Factor 0.29/ R-Value 3.44/ SHGc 0.56/ VT 0.69.
j.	SunGain DSB With Grids: U-Factor 0.29/ R-Value 3.44/ SHGc 0.51/ VT 0.62.
k.	SunShield DSB No Grids: U-Factor 0.27/ R-Value 3.70/ SHGc 0.22/ VT 0.56.
l.	SunShield DSB With Grids: U-Factor 0.27/ R-Value 3.70/ SHGc 0.20/ VT 0.51
2.13	NEW CONSTRUCTION WINDOW ACCESSORIES
A.	Mullions:
1.	Common Jamb: Windows are contained within single frame and separated by a common mull post.
2.	Non-Structural Combination Mullion: horizontal or vertical members, factory or field applied.
B.	Casings: Factory installed casing options.
1.	Brick Mold: 2-3/8 inch (60 mm). Nominal thickness 0.080 inches (2 mm); 4 Sides.
2.	Brick Mold: 2-3/8 inch (60 mm). Nominal thickness 0.080 inches (2 mm); with 1 inch (25 mm) sill nosing.
3.	Flat Casing: 3 inch (76 mm). Nominal thickness: 0.080 inches (2 mm); 4 sides.
4.	Flat Casing: 3 inch (76 mm). Nominal thickness: 0.080 inches (2 mm); with 1 inch (25 mm) sill nosing.
C.	Extension Jambs:
1.	Finish: Pre-Primed.
2.	Finish: Clear Pine.
3.	Depth: 4-9/16 inch (116 mm) depth (2 x 4 wall construction).
4.	Depth: 6-9/16 inch (167 mm) depth (2 x 6 wall construction).
5.	Depth (inch/mm): __________.
2.14	SLIDING PATIO DOORS (Standard Size)
A.	Construction:
1.	Frame and sash: 0.080 inch (2 mm) thick polyvinyl chloride (PVC). Frame corners mechanically fastened/ Jamb Depth: 4-9/16 inches (116 mm). Fin is integral to master frame. Sash corners are miter cut and fusion welded.
2.	Color: White Vinyl.
3.	Color: Almond Vinyl.
4.	Color: Custom Exterior Finish - Painted. As determined by the Architect.
5.	Glazing: 1 inch (25 mm) Nominal thickness Insulating glass units secured to sash frame using a dual durometer glazing bead. Complies with ASTM E2190. 
6.	Locks and Hardware: Dual point Lock.
7.	Locks and Hardware: Multi-point locking system.
a.	Corrosion resistant stainless steel rollers.
8.	Weather stripping: In compliance with AAMA 701.2.
9.	Screens: Extruded aluminum frame. 18 x 16 charcoal finish fiberglass mesh.
10.	Grids: 5/8 inch (16 mm) Colonial contour grids between glass (GBG) dividers.
11.	Grids: 1 inch (25 mm) Colonial contour grids between glass (GBG) dividers.
12.	Grids: 5/8 inch (16 mm) Exterior Grid Package with GBG. 
13.	Grids: 1 inch (25 mm) Exterior Grid Package with GBG. 
B.	Performance:
1.	Structural Rating: SD-R35 (DP35) - Test Size: 96 inches x 80 inches (2438 mm x 2032 mm) in accordance with AAMA/WDMA/CSA 101/I.S.2/A440-17.
2.	Structural Rating: SD-R25 (DP25) - Test Size: 96 inches x 96 inches (2438 mm x 2438 mm) in accordance with AAMA/WDMA/CSA 101/I.S.2/A440-17.
3.	Structural Rating: SD-R35 (DP35) - Test Size: 143 3/4 inches x 79 5/8 inches 3-Lite OXO (3651 mm x 2022 mm) in accordance with AAMA/WDMA/CSA 101/I.S.2/A440-17.
4.	Forced Entry: Type A, Grade 10 in accordance with ASTM F 842.
5.	Sound Transmission Class (STC): 29.
6.	Glazing Type: Thermal transmittance in accordance with NFRC 100/200/500.
a.	Clear No Grids: U-Factor 0.45/ R-Value 2.22/ SHGc 0.57/ VT 0.60.
b.	Clear With Grids: U-Factor 0.45/ R-Value 2.22/ SHGc 0.50/ VT 0.52.
c.	Low-E No Grids: U-Factor 0.32/ R-Value 3.12/ SHGc 0.27/ VT 0.51.
d.	Low-E With Grids: U-Factor 0.32/ R-Value 3.12/ SHGc 0.24/ VT 0.45.
e.	ThermaLock Low-E/Argon No Grids: U-Factor 0.29/ R-Value 3.44/ SHGc 0.27/ VT 0.51.
f.	ThermaLock Low-E/Argon With Grids: U-Factor 0.29 / R-Value 3.44/ SHGc 0.24 / VT 0.45.
g.	Blinds Between Glass 2X Low-E No Grids: U-Factor 0.29/ R-Value 3.33/ SHGc 0.25/ VT 0.47.
h.	ThermaLock 2X Low-E/Argon No Grids: U-Factor 0.29/ R-Value 3.44/ SHGc 0.25/ VT 0.44.
i.	ThermaLock 2X Low-E/Argon With Grids: U-Factor 0.29/ R-Value 3.44/ SHGc 0.22/ VT 0.38.
j.	ThermaLock TG 2X Low-E /Argon No Grids:  U-Factor 0.24/ R-Value 4.16/ SHGc 0.23/ VT 0.40.
k.	ThermaLock TG 2X Low-E /Argon With Grids:  U-Factor 0.25/ R-Value 4.00/ SHGc 0.22/ VT 0.35.
l.	SunShield No Grids: U-Factor 0.29/ R-Value 3.44/ SHGc 0.24/ VT 0.56.
m.	SunShield With Grids: U-Factor 0.29/ R-Value 3.44/ SHGc 0.22/ VT 0.51
2.15	TRIBUTE LIGHT COMMERCIAL SERIES DOUBLE HUNG WINDOWS
A.	Construction:
1.	Frame: 0.065 inch (1.7 mm) thick polyvinyl chloride (PVC). Miter cut and fusion welded corners. Operable Sash: 0.070 inch (1.8 mm) thick. Fusion welded corners.
a.	New construction frame with optional jamb receiver. 
b.	Replacement frame.
2.	Color: White Vinyl.
3.	Color: White Vinyl with Dark Bronze Exterior Finish - Painted.
4.	Color: White Vinyl with Black Exterior Finish - Painted.
5.	Color: Custom Exterior Finish - Painted. As determined by the Architect.
6.	Glazing: Insulating glass units secured to sash frame using a silicone sealant and rigid PVC glazing bead. Complies with ASTM E2190.
7.	Sash Balances: Factory calibrated block and tackle, complying with AAMA-902. Balance cords shall be anchored to locking terminal housings that lock in place when the sash is tilted in. The locking terminal and pivot bar system shall provide accurate alignment of the sash and the frame during operation.
8.	Locks: Two low-profile sash locks anchored with screws driven through the sash rail and into extruded aluminum. 
9.	Weather Stripping: In compliance with AAMA 701.2.
10.	Screens: Extruded aluminum full screen. 18 x 16 charcoal finish fiberglass mesh.
11.	Screens: Extruded aluminum locking half screen. 18 x 16 charcoal finish fiberglass mesh.
12.	Screens: Extruded aluminum full screen. 16 x 16 VIEWS (Virtually Invisible Enhanced Window Screen) mesh.
13.	Screens: Extruded aluminum locking half screen. 16 x 16 VIEWS (Virtually Invisible Enhanced Window Screen) mesh
14.	Screens:  Premium FlexScreen full screen (Standard on Exterior Painted) 
15.	Screens: Premium FlexScreen half screen (Standard on Exterior Painted)
16.	Grids: 5/8 inch (16 mm) Colonial contour grids between glass (GBG) dividers.
17.	Grids: 1 inch (25 mm) Colonial contour grids between glass (GBG) dividers. 
18.	Grids: 5/8 inch (16 mm) SDL (Simulated Divided Lites).
19.	Grids: 1 inch (25 mm) SDL (Simulated Divided Lites).
B.	Performance:
1.	Structural Rating: H-C40 (DP 40) - Test Size: 54 inches x 91 inches (1372 mm x 2311 mm) in accordance with AAMA/WDMA/CSA 101/I.S.2 /A440-05.
2.	Structural Rating: H-LC 50 (DP 50) - Test Size: 42 inches x 77 inches (1067 mm x 1956 mm) in accordance with AAMA/WDMA/CSA 101/I.S.2 /A440-05.
3.	Forced Entry: Type B, Grade 10 in accordance with ASTM F 588.
4.	Glazing Type: Thermal transmittance in accordance with NFRC 100/200/500.
a.	ThermaGuard No Grids: U-Factor 0.30/ R-Value 3.33/ SHGc 0.30/ VT 0.53.
b.	ThermaGuard With Grids: U-Factor 0.30/ R-Value 3.33/ SHGc 0.27/ VT 0.47.
c.	ThermaLock RS No Grids: U-Factor 0.26/ R-Value 3.84/ SHGc 0.29/ VT 0.52.
d.	ThermaLock RS With Grids: U-Factor 0.26/ R-Value 3.84/ SHGc 0.26/ VT 0.46.
e.	ThermaLock 3X No Grids: U-Factor 0.24/ R-Value 4.16/ SHGc 0.24/ VT 0.44.
f.	ThermaLock 3X With Grids: U-Factor 0.24/ R-Value 4.16/ SHGc 0.21/ VT 0.39.
g.	SunGain No Grids U-Factor 0.31/ R-Value 3.22/ SHGc 0.48/ VT 0.58.
h.	SunGain With Grids U-Factor 0.31/ R-Value 3.22/ SHGc 0.43/ VT 0.51.
2.16	REPLACEMENT TRIBUTE DOUBLE HUNG WINDOWS
A.	Construction:
1.	Frame: 0.065 inch (1.7 mm) thick polyvinyl chloride (PVC). Miter cut and fusion welded corners. Contoured Sash Design: 0.070 inch (1.8 mm) thick. Fusion welded corners.
2.	Color: White Vinyl.
3.	Color: White Vinyl with Dark Bronze Exterior Finish - Painted.
4.	Color: White Vinyl with Black Exterior Finish - Painted.
5.	Color: Custom Exterior Finish - Painted. As determined by the Architect.
6.	Glazing: Insulating glass units are silicone glazed with an exterior glazing bead. Complies with ASTM E2190.
7.	Sash Balances: Factory calibrated block and tackle, complying with AAMA-902. Balance cords shall be anchored to locking terminal housings that lock in place when the sash is tilted in. The locking terminal and pivot bar system shall provide accurate alignment of the sash and the frame during operation.
8.	Two Sash Locks: unique low profile locks operate the tilt release latches allowing the sash to tilt-in.
9.	Weather Stripping: In compliance with AAMA 701.2.
10.	Screens: Extruded aluminum locking half screen. 16 x 16 VIEWS (Virtually Invisible Enhanced Window Screen) mesh.
11.	Screens: Extruded aluminum full screen. 16 x 16 VIEWS (Virtually Invisible Enhanced Window Screen) mesh.
12.	Screens:  Premium FlexScreen full screen (Standard on Exterior Painted) 
13.	Screens: Premium FlexScreen half screen (Standard on Exterior Painted)
14.	Grids: 5/8 inch (16 mm) Colonial contour grids between glass (GBG) dividers.
15.	Grids: 1 inch (25 mm) Colonial contour grids between glass (GBG) dividers. 
16.	Grids: 5/8 inch (16 mm) SDL (Simulated Divided Lites). 
17.	Grids: 1 inch (25 mm) SDL (Simulated Divided Lites).
B.	Performance:
1.	Structural Rating: H-LC35 (DP35) - Test Size: 48 inches x 84 inches (1219 mm x 2134 mm) in accordance with AAMA/WDMA/CSA 101/I.S.2/A440-05.
2.	Structural Rating: H-LC50 (DP50) - Test Size: 42 inches x 77 inches (1067 mm x 1956 mm) in accordance with AAMA/WDMA/CSA 101/I.S.2/A440-05.
3.	Forced Entry: Type A, Grade 10 in accordance with ASTM F 588-97.
4.	Glazing Type: Thermal transmittance in accordance with NFRC 100/200/500.
a.	ThermaGuard No Grids U-Factor 0.29/ R-Value 3.44/ SHGc 0.30/ VT 0.53.
b.	ThermaGuard With Grids U-Factor 0.29/ R-Value 3.44/ SHGc 0.27/ VT 0.47.
c.	ThermaLock RS No Grids: U-Factor 0.25/ R-Value 4.00/ SHGc 0.29/ VT 0.52.
d.	ThermaLock RS With Grids: U-Factor 0.25/ R-Value 4.00/ SHGc 0.26/ VT 0.46.
e.	ThermaLock 3X No Grids:  U-Factor 0.21/ R-Value 4.76/ SHGc 0.24/ VT 0.44.
f.	ThermaLock 3X With Grids:  U-Factor 0.22/ R-Value 4.54/ SHGc 0.21/ VT 0.39.
g.	SunGain No Grids U-Factor 0.30/ R-Value 3.33/ SHGc 0.48/ VT 0.58.
h.	SunGain With Grids U-Factor 0.30/ R-Value 3.33/ SHGc 0.43/ VT 0.51.
2.17	REPLACEMENT CLASSIC DOUBLE HUNG WINDOWS
A.	Construction:
1.	Frame: 0.065 inch (1.7 mm) thick polyvinyl chloride (PVC). Miter cut and fusion welded corners. Sash : 0.060 inch (1.5 mm) thick with fusion welded corners.
2.	Color: White Vinyl.
3.	Color: Almond Vinyl.
4.	Color: White Vinyl with Dark Bronze Exterior Finish - Painted.
5.	Color: White Vinyl with Black Exterior Finish - Painted.
6.	Color: Custom Exterior Finish - Painted. As determined by the Architect.
7.	Glazing: Insulating glass units secured to sash frame using a Silicone sealant exterior glazing bead. Complies with ASTM E2190.
8.	Sash Balances: Factory calibrated block and tackle, complying with AAMA-902. Balance cords shall be anchored to locking terminal housings that lock in place when the sash is tilted in. The locking terminal and pivot bar system shall provide accurate alignment of the sash and the frame during operation.
9.	Sash Locks: Cam type locks anchored with screws. Double locks when openings are 30 1/4 inches (768 mm) wide and greater.
10.	Weather Stripping: In compliance with AAMA 701.2.
11.	Screens: Extruded aluminum full screen. 18 x 16 charcoal finish fiberglass mesh.
12.	Screens: Extruded aluminum locking half screen. 18 x 16 charcoal finish fiberglass mesh.
13.	Screens:  FlexScreen full screen (Standard on Exterior Painted) 
14.	Screens: FlexScreen half screen (Standard on Exterior Painted)
15.	Grids: 5/8 inch (16 mm) Colonial contour grids between glass (GBG) dividers.
16.	Grids: 1 inch (25 mm) Colonial contour grids between glass (GBG) dividers.
17.	Grids: 5/8 inch (16 mm) SDL (Simulated Divided Lites).
18.	Grids: 1 inch (25 mm) SDL (Simulated Divided Lites).
B.	Performance:
1.	Structural Rating: H-LC40 (DP40) - Test Size: 46 inches x 77 inches (1168 mm x 1956 mm) in accordance with AAMA/WDMA/CSA 101/I.S.2/A440-08.
2.	Structural Rating: H-LC50 (DP50) - Test Size: 42 inches x 77 inches (1067 mm x 1956 mm) in accordance with AAMA/WDMA/CSA 101/I.S.2/A440-08.
3.	Structural Rating: H-R50 (DP50) - Test Size: 46 inches x 60 inches (1168 mm x 1524 mm) in accordance with AAMA/WDMA/CSA 101/I.S.2/A440-05.
4.	Sound Transmission Class (STC): 27.
5.	Sound Transmission Class (STC): 34. 
6.	Forced Entry: Type A, Grade 10 in accordance with ASTM F 588.
7.	Glazing Type: Thermal transmittance in accordance with NFRC 100/200/500.
a.	Clear No Grids: U-Factor 0.45/ R-Value 2.17/ SHGc 0.59/ VT 0.62.
b.	Clear With Grids: U-Factor 0.45/ R-Value 2.17/ SHGc 0.53 / VT 0.55.
c.	Low-E No Grids: U-Factor 0.32/ R-Value 3.03/ SHGc 0.31/ VT 0.55.
d.	Low-E With Grids: U-Factor 0.32/ R-Value 3.03/ SHGc 0.28/ VT 0.49.
e.	ThermaGuard No Grids: U-Factor 0.29/ R-Value 3.44/ SHGc 0.31/ VT 0.55.
f.	ThermaGuard With Grids: U-Factor 0.29/ R-Value 3.44/ SHGc 0.28/ VT 0.49.
g.	ThermaLock No Grids: U-Factor 0.27/ R-Value 3.70/ SHGc 0.29/ VT 0.49. 
h.	ThermaLock With Grids: U-Factor 0.27/ R-Value 3.70/ SHGc 0.26/ VT 0.44. 
i.	ThermaLock 3X No Grids U-Factor 0.21/ R-Value 4.76/ SHGc 0.25/ VT 0.46.
j.	ThermaLock 3X With Grids U-Factor 0.22/ R-Value 4.54/ SHGc 0.22/ VT 0.41.
k.	SunGain No Grids U-Factor 0.30/ R-Value 3.33/ SHGc 0.50/ VT 0.60.
l.	SunGain With Grids U-Factor 0.30/ R-Value 3.33/ SHGc 0.45/ VT 0.54.
m.	SunShield No Grids: U-Factor 0.28/ R-Value 3.57/ SHGc 0.21/ VT 0.49.
n.	SunShield With Grids: U-Factor 0.28/ R-Value 3.57/ SHGc 0.19/ VT 0.44.
2.18	REPLACEMENT SLIMLINE SINGLE HUNG WINDOWS 
A.	Construction: 
1.	Frame: 0.065 inch (1.7 mm) thick polyvinyl chloride (PVC),Miter cut and fusion welded corners. Sash: 0.065 inch (1.7 mm) thick. Fusion welded corners. 
2.	Color: White Vinyl. 
3.	Glazing: Insulating glass units secured to sash frame using a silicone sealant and dual durometer glazing bead. Complies with ASTM E 2190. 
4.	Sash Balances: Factory calibrated block and tackle, complying with AAMA-902. Balance cords shall be anchored to glass filled nylon terminal housings that lock in place once the sash is tilted in. The locking terminal and pivot bar system shall be designed to positively interlock, to provide accurate alignment of the sash and the frame during installation and operation. 
5.	Sash Locks: Knife type locks anchored with screws. Double locks when openings are 30 1/4 inches (768 mm) wide and greater. 
6.	Weather Stripping: In compliance with AAMA 701.2. 
7.	Screens: Extruded aluminum half screen. 18 x 16 charcoal finish fiberglass mesh. 
8.	Screens:  Rolled Form aluminum half screen. 18 x 16 charcoal finish fiberglass mesh. 
9.	Screens:  FlexScreen half screen. 18 x 16 charcoal finish fiberglass mesh. 
10.	Grids: 5/8 inch (16 mm) Colonial contour grids between glass (GBG) dividers. 
B.	Performance: 
1.	Structural Rating: H-R30 (DP30) - Test Size: 46 inches x 77 inches (1168 mm x 1956 mm) in accordance with AAMA/WDMA/CSA 101/I.S.2/A440-08 
2.	Structural Rating: H-C50 (DP50) - Test Size: 40 inches x 63 inches (1118 mm x 1524 mm) in accordance with AAMA/WDMA/CSA 101/I.S.2/A440-05. 
3.	Forced Entry: Type A, Grade 10 in accordance with ASTM F 588. 
4.	Sound Transmission Class (STC): 26. 
5.	Sound Transmission Class (STC): 34. 
6.	Glazing Type: Thermal transmittance in accordance with NFRC 100/200/500.
a.	Clear No Grids: U-Factor 0.46/ R-Value 2.17/ SHGc 0.61 / VT 0.64. 
b.	Clear With Grids: U-Factor 0.46/ R-Value 2.17/ SHGc 0.54 /  VT 0.57.
c.	Low-E No Grids: U-Factor 0.32/ R-Value 3.12/ SHGc 0.32/ VT 0.57. 
d.	Low-E With Grids: U-Factor 0.32/ R-Value 3.12/ SHGc 0.29/ VT 0.50.
e.	ThermaGuard No Grids: U-Factor 0.29/ R-Value 3.44/ SHGc 0.31/ VT 0.57. 
f.	ThermaGuard With Grids: U-Factor 0.29/ R-Value 3.44/ SHGc 0.28/ VT 0.50.
g.	ThermaLock RS No Grids: U-Factor 0.25/ R-Value 4.00/ SHGc 0.31/ VT 0.56. 
h.	ThermaLock RS With Grids: U-Factor 0.25/ R-Value 4.00/ SHGc 0.28/ VT 0.50. 
i.	SunGain No Grids: U-Factor 0.30/ R-Value 3.33/ SHGc 0.51/ VT 0.62.
j.	SunGain With Grids: U-Factor 0.30/ R-Value 3.33/ SHGc 0.46/ VT 0.55.
k.	SunShield No Grids:  U-Factor 0.28/ R-Value 3.57/ SHGc 0.22/ VT 0.51.
l.	SunShield With Grids:  U-Factor 0.28/ R-Value 3.57/ SHGc 0.20/ VT 0.45.
2.19	REPLACEMENT SLIMLINE DOUBLE HUNG WINDOWS 
A.	Construction: 
1.	Frame: 0.065 inch (1.7 mm) thick polyvinyl chloride (PVC). Miter cut and fusion welded corners. Sash: 0.065 inch (1.7 mm) thick. Fusion welded corners. 
2.	Color: White Vinyl. 
3.	Glazing: Insulating glass units secured to sash frame using a silicone sealant and dual durometer glazing bead. Complies with ASTM E 2190. 
4.	Sash Balances: Factory calibrated block and tackle, complying with AAMA-902. Balance cords shall be anchored to glass filled nylon terminal housings that lock in place once the sash is tilted in. The locking terminal and pivot bar system shall be designed to positively interlock, to provide accurate alignment of the sash and the frame during installation and operation. 
5.	Sash Locks: Knife type locks anchored with screws. Double locks when openings are 30 1/4 inches (768 mm) wide and greater. 
6.	Weather Stripping: In compliance with AAMA 701.2. 
7.	Screens: Extruded aluminum half screen. 18 x 16 charcoal finish fiberglass mesh. 
8.	Screens: Rolled Form aluminum half screen. 18 x 16 charcoal finish fiberglass mesh.
9.	Screens:  Extruded aluminum full screen. 18 x 16 charcoal finish fiberglass mesh. 
10.	Screens:  Rolled Form aluminum full screen. 18 x 16 charcoal finish fiberglass mesh.
11.	Screens:  FlexScreen full screen. 18 x 16 charcoal finish fiberglass mesh. 
12.	Screens:  FlexScreen half screen. 18 x 16 charcoal finish fiberglass mesh.
13.	Grids: 5/8 inch (16 mm) Colonial contour grids between glass (GBG) dividers. 
B.	Performance: 
1.	Structural Rating: H-R30 (DP30) - Test Size: 46 inches x 77 inches (1168 mm x 1956 mm) in accordance with AAMA/WDMA/CSA 101/I.S.2/A440-08 
2.	Structural Rating: H-R35 (DP35) - Test Size: 42 inches x 77 inches (1067 mm x 1956 mm) in accordance with AAMA/WDMA/CSA 101/I.S.2/A440-08. 
3.	Structural Rating: H-C50 (DP50) - Test Size: 40 inches x 63 inches (1118 mm x 1524 mm) in accordance with AAMA/WDMA/CSA 101/I.S.2/A440-05. 
4.	Forced Entry: Type A, Grade 10 in accordance with ASTM F 588. 
5.	Sound Transmission Class (STC): 26. 
6.	Sound Transmission Class (STC): 34. 
7.	Glazing Type: Thermal transmittance in accordance with NFRC 100/200/500.
a.	Clear No Grids: U-Factor 0.46/ R-Value 2.17/ SHGc 0.61 / VT 0.64. 
b.	Clear With Grids: U-Factor 0.46/ R-Value 2.17/ SHGc 0.54 /  VT 0.57. 
c.	Low-E No Grids: U-Factor 0.32/ R-Value 3.12/ SHGc 0.32/ VT 0.57.
d.	Low-E With Grids: U-Factor 0.32/ R-Value 3.12/ SHGc 0.29/ VT 0.50.
e.	ThermaGuard No Grids: U-Factor 0.29/ R-Value 3.44/ SHGc 0.31/ VT 0.57.
f.	ThermaGuard With Grids: U-Factor 0.29/ R-Value 3.44/ SHGc 0.28/ VT 0.50.
g.	ThermaLock RS No Grids: U-Factor 0.25/ R-Value 4.00/ SHGc 0.31/ VT 0.56.
h.	ThermaLock RS With Grids: U-Factor 0.25/ R-Value 4.00/ SHGc 0.28/ VT 0.50.
i.	SunGain No Grids U-Factor x0.30/ R-Value 3.33/ SHGc 0.51/ VT 0.62.
j.	SunGain With Grids U-Factor 0.30/ R-Value 3.33/ SHGc 0.46/ VT 0.55.
k.	SunShield No Grids: U-Factor 0.28/ R-Value 3.57/ SHGc 0.22/ VT 0.51.
l.	SunShield With Grids: U-Factor 0.28/ R-Value 3.57/ SHGc 0.20/ VT 0.45.
2.20	REPLACEMENT CASEMENT WINDOWS
A.	Construction:
1.	Frame and Sash: 0.070 inch (1.8 mm) thick polyvinyl chloride (PVC) with miter cut and fusion welded corners.
2.	Color: White Vinyl.
3.	Color: Almond Vinyl.
4.	Color: White Vinyl with Dark Bronze Exterior Finish - Painted.
5.	Color: White Vinyl with Black Exterior Finish - Painted.
6.	Color: Custom Exterior Finish - Painted. As determined by the Architect.
7.	Color: Custom Interior Finish - Painted. As determined by the Architect.
8.	Glazing: Insulating glass units secured to sash frame using a silicone sealant and rigid PVC glazing bead. Complies with ASTM E 2190. 
9.	Hinges: Maxim 14 series.
10.	Sash Locks: Sequentially locking multi-point type with single handle actuator.
11.	Operator: Encore series.
12.	Weather Stripping: In compliance with AAMA 701.2.
13.	Screens: Extruded aluminum frame. 18 x 16 charcoal finish fiberglass mesh.
14.	Screens: Extruded aluminum frame. 18 x 16 charcoal finish aluminum mesh.
15.	Grids: 5/8 inch (16 mm) Colonial contour grids between glass (GBG) dividers.
16.	Grids: 1 inch (25 mm) Colonial contour grids between glass (GBG) dividers. 
17.	Grids: 5/8 inch (16 mm) SDL (Simulated Divided Lites).
18.	Grids: 1 inch (25 mm) SDL (Simulated Divided Lites).
B.	Performance:
1.	Structural Rating: C-55 (DP55) - Test Size:  36 inches x 80 inches (914 mm x 2032 mm) in accordance with AAMA/WDMA/CSA 101/I.S.2/A440-17.
2.	Forced Entry: Type B, Grade 10 in accordance with ASTM F588.
3.	Sound Transmission Class (STC): 26.
4.	Sound Transmission Class (STC): 29.
5.	Sound Transmission Class (STC): 34. 
6.	Glazing Type: Thermal transmittance in accordance with NFRC 100/200/500.
a.	Clear No Grids: U-Factor 0.43/ R-Value 2.32/ SHGc 0.47/ VT 0.49.
b.	Clear With Grids: U-Factor 0.43/ R-Value 2.32/ SHGc 0.42/ VT 0.44.
c.	Low-E No Grids: U-Factor 0.31/ R-Value 3.22/ SHGc 0.25/ VT 0.44.
d.	Low-E With Grids: U-Factor 0.31/ R-Value 3.22/ SHGc 0.22/ VT 0.39.
e.	ThermaGuard No Grids: U-Factor 0.29/ R-Value 3.44/ SHGc 0.24/ VT 0.44.
f.	ThermaGuard With Grids: U-Factor 0.29/ R-Value 3.44/ SHGc 0.22/ VT 0.39.
g.	ThermaLock  RS No Grids: U-Factor 0.25/ R-Value 4.00/ SHGc 0.24/ VT 0.43. 
h.	ThermaLock  RS With Grids: U-Factor 0.25/ R-Value 4.00/ SHGc 0.22/ VT 0.38.
i.	ThermaLock TG 3X Grids: U-Factor 0.22/ R-Value 4.54/ SHGc 0.20/ VT 0.36. 
j.	ThermaLock TG 3X With Grids: U-Factor 0.23/ R-Value 4.34/ SHGc 0.18/ VT 0.32.
k.	SunGain No Grids U-Factor 0.29/ R-Value x.x/ SHGc 0.40/ VT 0.48.
l.	SunGain With Grids U-Factor 0.29/ R-Value x.x/ SHGc 0.36/ VT 0.43.
2.21	REPLACEMENT AWNING WINDOWS
A.	Construction:
1.	Frame and Sash: 0.070 inch (1.8 mm) thick polyvinyl chloride (PVC) with miter cut and fusion welded corners.
2.	Color: White Vinyl.
3.	Color: Almond Vinyl.
4.	Color: White Vinyl with Dark Bronze Exterior Finish - Painted.
5.	Color: White Vinyl with Black Exterior Finish - Painted.
6.	Color: Custom Exterior Finish - Painted. As determined by the Architect.
7.	Glazing: Insulating glass units secured to sash frame using a sealant and rigid PVC glazing bead. Complies with ASTM E2190. 
8.	Hinges: Maxim 13 series.
9.	Sash Locks: Maxim 24 Series single point locks.
10.	Weather stripping: In compliance with AAMA 701.2.
11.	Screens: Extruded aluminum frame. 18 x 16 charcoal finish fiberglass mesh.
12.	Grids: 5/8 inch (16 mm) Colonial contour grids between glass (GBG) dividers.
13.	Grids: 1 inch (25 mm) Colonial contour grids between glass (GBG) dividers. 
14.	Grids: 5/8 inch (16 mm) SDL (Simulated Divided Lites).
15.	Grids: 1 inch (25 mm) SDL (Simulated Divided Lites).
B.	Performance:
1.	Structural Rating: AP-LC40 (DP40) - Test Size: 60 inches x 42 inches (1524 mm x 1067 mm) in accordance with AAMA/WDMA/CSA 101/I.S.2/A440-05.
2.	Structural Rating: AP-LC75 (DP 75) - Size: 48 inches x 32 inches (1219.2 mm x 812.8 mm) in accordance with AAMA/WDMA/CSA 101/I.S.2/A440-05.
3.	Forced Entry: Type B, Grade 20 in accordance with ASTM F 588.
4.	Sound Transmission Class (STC): 26.
5.	Sound Transmission Class (STC): 29.
6.	Sound Transmission Class (STC): 34. 
7.	Glazing Type: Thermal transmittance in accordance with NFRC 100/200/500.
a.	Clear No Grids: U-Factor 0.43/ R-Value 2.32/ SHGc 0.47/ VT 0.49.
b.	Clear With Grids: U-Factor 0.43/ R-Value 2.32/ SHGc 0.42/ VT 0.44.
c.	Low-E No Grids: U-Factor 0.32/ R-Value 3.12/ SHGc 0.25/ VT 0.44.
d.	Low-E With Grids: U-Factor 0.32/ R-Value 3.12/ SHGc 0.22/ VT 0.39.
e.	ThermaGuard No Grids: U-Factor 0.29/ R-Value 3.44/ SHGc 0.24/ VT 0.44.
f.	ThermaGuard With Grids: U-Factor 0.29/ R-Value 3.44/ SHGc 0.22/ VT 0.39.
g.	ThermaLock RS No Grids:  U-Factor 0.26/ R-Value 3.84/ SHGc 0.24/ VT 0.43. 
h.	ThermaLock RS With Grids:  U-Factor 0.26/ R-Value 3.84/ SHGc 0.22/ VT 0.38.
i.	ThermaLock 3X No Grids: U-Factor 0.23/ R-Value 4.34/ SHGc 0.20/ VT 0.36. 
j.	ThermaLock 3X With Grids:  U-Factor 0.23/ R-Value 4.34/ SHGc 0.18/ VT 0.32.
k.	SunGain No Grids U-Factor 0.30/ R-Value 3.33/ SHGc 0.40/ VT 0.48.
l.	SunGain With Grids U-Factor 0.30/ R-Value 3.33/ SHGc 0.36/ VT 0.43.
2.22	REPLACEMENT HOPPER WINDOWS
A.	Construction:
1.	Frame: 0.065 inch (1.7 mm) thick polyvinyl chloride (PVC). Sash: 0.065 inch (1.7 mm). Miter cut and mechanically fastened sash and fusion welded frame.
2.	Color: White Vinyl.
3.	Color: Almond Vinyl.
4.	Color: White Vinyl with Dark Bronze Exterior Finish - Painted.
5.	Color: White Vinyl with Black Exterior Finish - Painted.
6.	Color: Custom Exterior Finish - Painted. As determined by the Architect.
7.	Glazing: 7/8 inch (22 mm) nominal thickness Insulating glass to be glazed utilizing a two leaf dual durometer glazing channel. Complies with ASTM E2190.
8.	Hinges: Maxim 13 series.
9.	Sash Locks: Knife type double locks when openings are 30 1/2 inches (774 mm) and wider.
10.	Weather stripping: In compliance with AAMA 701.2.
11.	Screens: Extruded aluminum frame. 18 x 16 charcoal finish fiberglass mesh.
12.	Screens: Extruded aluminum frame. 18 x 16 charcoal finish aluminum mesh.
13.	Grids: 5/8 inch (16 mm) Colonial contour grids between glass (GBG) dividers.
14.	Grids: 1 inch (25 mm) Colonial contour grids between glass (GBG) dividers.
B.	Performance:
1.	Structural Rating: AP-R15 - Test Size: 48 inches x 32 inches (1219 mm x 813 mm) in accordance with AAMA/WDMA/CSA 101/I.S.2/A440-05.
2.	Forced Entry: Type B, Grade 10 in accordance with ASTM F 588.
3.	Glazing Type: Thermal transmittance in accordance with NFRC 100/200/500.
a.	Clear No Grids: U-Factor 0.46/ R-Value 2.17/ SHGc 0.55/ VT 0.57.
b.	Clear With Grids: U-Factor 0.46/ R-Value 2.17/ SHGc 0.50/ VT 0.51.
c.	Low-E No Grids: U-Factor 0.34/ R-Value 2.94/ SHGc 0.29/ VT 0.51.
d.	Low-E With Grids: U-Factor 0.34/ R-Value 2.94/ SHGc 0.26/ VT 0.46.
e.	DSB Low-E/Argon No Grids: U-Factor 0.30/ R-Value 3.33/ SHGc 0.28/ VT 0.50.
f.	DSB Low-E/Argon With Grids: U-Factor 0.30/ R-Value 3.33/ SHGc 0.26/ VT 0.45.
g.	ThermaLock RS No Grids: U-Factor 0.27/ R-Value 3.70/ SHGc 0.28/ VT 0.50.
h.	ThermaLock RS With Grids: U-Factor 0.27/ R-Value 3.70/ SHGc 0.26/ VT 0.45.
i.	ThermaLock 3X No Grids U-Factor 0.23/ R-Value 4.34/ SHGc 0.23/ VT 0.42.
j.	ThermaLock 3X With Grids U-Factor 0.23/ R-Value 4.34/ SHGc 0.21/ VT 0.38.
k.	SunGain No Grids: U-Factor 0.30/ R-Value 3.33/ SHGc 0.46/ VT 0.55.
l.	SunGain With Grids: U-Factor 0.30/ R-Value 3.33/ SHGc 0.42/ VT 0.50.
2.23	REPLACEMENT ROLLING WINDOWS
A.	Construction:
1.	Frame: 0.090 inch (2.3 mm) thick polyvinyl chloride (PVC). Sash: 0.080 inch (2.0 mm) thick. Miter cut and fusion welded corners on frame and sash,
2.	Color: White Vinyl.
3.	Color: Almond Vinyl.
4.	Color: White Vinyl with Dark Bronze Exterior Finish - Painted.
5.	Color: White Vinyl with Black Exterior Finish - Painted.
6.	Color: Custom Exterior Finish - Painted. As determined by the Architect.
7.	Glazing: Insulating glass units secured to sash frame using a silicone sealant and a dual durometer glazing bead. Complies with ASTM E2190.
8.	Sash Locks: Cam type.
9.	Weather stripping: In compliance with AAMA 701.2.
10.	Screens: Extruded aluminum screen. 18 x 16 charcoal finish fiberglass mesh.
11.	Screens: Extruded aluminum screen. 18 x 16 charcoal finish aluminum mesh.
12.	Screens: FlexScreen (Standard on Exterior Painted)
13.	Grids: 5/8 inch (16 mm) Colonial contour grids between glass (GBG) dividers.
14.	Grids: 1 inch (25 mm) Colonial contour grids between glass (GBG) dividers. 
15.	Grids: 5/8 inch (16 mm) SDL (Simulated Divided Lites).
16.	Grids: 1 inch (25 mm) SDL (Simulated Divided Lites).
B.	Performance:
1.	Structural Rating: HS-LC35 (DP35) - Test Size: 72 inches x 62 1/2 inches (1829 mm x 1588 mm) in accordance with AAMA/WDMA/CSA 101/I.S.2/A440-11. 
2.	Structural Rating: HS-LC35 (DP 25) - Test Size: 120 inches x 62 1/2 inches (3048 mm x 1588 mm) in accordance with AAMA/WDMA/CSA 101/I.S.2/A440-11.
3.	Forced Entry: Type A, Grade 10 in accordance with ASTM F 588.
4.	Sound Transmission Class (STC): 26 Two Lite.
5.	Sound Transmission Class (STC): 33 Two Lite.
6.	Glazing Type: Thermal transmittance in accordance with NFRC 100/200/500.
a.	Clear No Grids: U-Factor 0.47/ R-Value 2.17/ SHGc - 0.60/ VT 0.62.
b.	Clear With Grids: U-Factor 0.47/ R-Value 2.17/ SHGc - 0.53/ VT 0.54.
c.	Low-E No Grids: U-Factor 0.33/ R-Value 3.03/ SHGc 0.31/ VT 0.55. 
d.	Low-E With Grids: U-Factor 0.33/ R-Value 3.03/ SHGc 0.28/ VT 0.49. 
e.	Low-E/Argon No Grids: U-Factor 0.30/ R-Value 3.33/ SHGc 0.31/ VT 0.55.
f.	Low-E/Argon With Grids: U-Factor 0.30/ R-Value 3.33/ SHGc 0.28/ VT 0.49.
g.	ThermaLock RS No Grids: U-Factor 0.26/ R-Value 3.84/ SHGc 0.30/ VT 0.55.
h.	ThermaLock RS With Grids: U-Factor 0.26/ R-Value 3.84/ SHGc 0.27/ VT 0.49.
i.	ThermaLock 3X No Grids: U-Factor 0.22/ R-Value 4.54/ SHGc 0.25/ VT 0.46.
j.	ThermaLock 3X With Grids: U-Factor 0.23/ R-Value 4.34/ SHGc 0.22/ VT 0.41.
k.	SunGain No Grids: U-Factor 0.30/ R-Value 3.33/ SHGc 0.50/ VT 0.61.
l.	SunGain With Grids: U-Factor 0.30/ R-Value 3.33/ SHGc 0.45/ VT 0.54.
m.	SunShield No Grids:  U-Factor 0.29/ R-Value 3.44/ SHGc 0.21/ VT 0.49. 
n.	SunShield With Grids:  U-Factor 0.29/ R-Value 3.44/ SHGc 0.19/ VT 0.44.
2.24	REPLACEMENT PICTURE WINDOWS
A.	Construction:
1.	Frame: 0.075 inch (1.9 mm) wall thickness polyvinyl chloride (PVC). Miter cut and fusion welded corners.
2.	Color: White Vinyl.
3.	Color: Almond Vinyl.
4.	Color: White Vinyl with Dark Bronze Exterior Finish - Painted.
5.	Color: White Vinyl with Black Exterior Finish - Painted.
6.	Color: Custom Exterior Finish - Painted. As determined by the Architect.
7.	Glazing: Insulating glass units secured to frame using sealant in the corners and a dual durometer glazing bead. Complies with ASTM E2190.
8.	Grids: 5/8 inch (16 mm) Colonial contour grids between glass (GBG) dividers.
9.	Grids: 1 inch (25 mm) Colonial contour grids between glass (GBG) dividers.
10.	Grids: 5/8 inch (16 mm) SDL (Simulated Divided Lites).
11.	Grids: 1 inch (25 mm) SDL (Simulated Divided Lites).
B.	Performance:
1.	Structural Rating: F-C55 (DP55) - Test Size: 72 inches x 72 inches (1829 mm x 1829 mm) in accordance with AAMA/WDMA/CSA 101/I.S.2/A440-11.
2.	Sound Transmission Class (STC):29.
3.	Sound Transmission Class (STC):32.
4.	Forced Entry: Type D, Grade 10 in accordance with ASTM F 588.
5.	Glazing Type: Thermal transmittance in accordance with NFRC 100/200/500.
a.	Clear No Grids: U-Factor 0.45/ R-Value 2.22/ SHGc 0.63/ VT 0.66.
b.	Clear With Grids: U-Factor 0.45/ R-Value 2.22/ SHGc 0.56/ VT 0.59.
c.	Low-E No Grids: U-Factor 0.30/ R-Value 3.33/ SHGc 0.33/ VT 0.59.
d.	Low-E With Grids: U-Factor 0.30/ R-Value 3.33/ SHGc 0.30/ VT 0.52.
e.	Low-E/Argon No Grids U-Factor 0.26/ R-Value 3.84/ SHGc 0.32/ VT 0.59.
f.	Low-E/Argon With Grids U-Factor 0.26/ R-Value 3.84/ SHGc 0.29/ VT 0.52.
g.	ThermaLock No Grids: U-Factor 0.26/ R-Value 3.84/ SHGc 0.30/VT 0.52.
h.	ThermaLock With Grids: U-Factor 0.26/ R-Value 3.84/ SHGc 0.28/ VT 0.47.
i.	ThermaLock 3X No Grids: U-Factor 0.19/ R-Value 5.26/ SHGc 0.26/ VT 0.49.
j.	ThermaLock 3X With Grids: U-Factor 0.20/ R-Value 5.00/ SHGc 0.24/ VT 0.43.
k.	SunGain No Grids U-Factor 0.27/ R-Value 3.70/ SHGc 0.53/ VT 0.64.
l.	SunGain With Grids U-Factor 0.27/ R-Value 3.70/ SHGc 0.47/ VT 0.57.
m.	SunShield No Grids: U-Factor 0.25/ R-Value 4.00/ SHGc 0.22/ VT 0.52.
n.	SunShield With Grids: U-Factor 0.25/ R-Value 4.00/ SHGc 0.20/ VT 0.47
2.25	REPLACEMENT DESIGNER SHAPES WINDOWS
A.	Construction:
1.	Frame: 0.1 inch (2.5 mm) wall thickness polyvinyl chloride (PVC) with miter cut and fusion welded corners.
2.	Color: White Vinyl.
3.	Color: Almond Vinyl.
4.	Color: White Vinyl with Dark Bronze Exterior Finish - Painted.
5.	Color: White Vinyl with Black Exterior Finish - Painted.
6.	Color: Custom Exterior Finish - Painted. As determined by the Architect.
7.	Glazing: Insulating glass units secured to frame using silicone sealant and a dual durometer glazing bead. Complies with ASTM E2190.
8.	Grids: Colonial contour grids between glass (GBG) dividers.
B.	Performance:
1.	Structural Rating: F-C50 (DP50) - Test Size:  78 inches x 85 1/4 inches (1981 mm x 2165 mm) in accordance with AAMA/WDMA/CSA 101/I.S.2/A440-17.
2.	Forced Entry: Type D, Grade 10 in accordance with ASTM F588.
3.	Glazing Type: The Thermal transmittance in accordance with NFRC 100/200/500.
a.	Clear DSB No Grids: U-Factor 0.46/ R-Value 2.17/ SHGc 0.68/ VT 0.72.
b.	Clear DSB With Grids: U-Factor 0.46/ R-Value 2.17/ SHGc 0.61/ VT 0.64.
c.	Low-E DSB No Grids: U-Factor 0.31/ R-Value 3.22/ SHGc 0.32/ VT 0.61.
d.	Low-E DSB With Grids: U-Factor 0.31/ R-Value 3.22/ SHGc 0.29/ VT
e.	Low-E/Argon DSB No Grids U-Factor 0.27/ R-Value 3.70/ SHGc 0.32/ VT 0.61.
f.	Low-E/Argon DSB With Grids U-Factor 0.27/ R-Value 3.70/ SHGc 0.29/ VT 0.55. 
g.	ThermaLock DSB No Grids: U-Factor 0.27/ R-Value 3.70/ SHGc 0.30/VT 0.52.
h.	ThermaLock DSB With Grids: U-Factor 0.27/ R-Value 3.70/ SHGc 0.27/ VT 0.47.
i.	SunGain DSB No Grids U-Factor 0.29/ R-Value 3.44/ SHGc 0.56/ VT 0.69.
j.	SunGain DSB With Grids U-Factor 0.29/ R-Value 3.44/ SHGc 0.51/ VT 0.62.
k.	SunShield DSB No Grids: U-Factor 0.27/ R-Value 3.70/ SHGc 0.24/ VT 0.57.
l.	SunShield DSB With Grids: U-Factor 0.27/ R-Value 3.70/ SHGc 0.22/ VT 0.51.
2.26	REPLACEMENT WINDOW ACCESSORIES
A.	Mullions:
1.	Common Jamb: Windows are contained within single frame and separated by a common mull post.
2.	Structural Mullion: DP 50 to 120 mph performance rated mullion for areas requiring conformance to increased wind loads (replacement windows only).
3.	Non-Structural Combination Mullion: Horizontal or vertical members formed by joining two or more window units. May be factory or field applied.
PART 3    EXECUTION
3.1	EXAMINATION
A.	Verify rough opening size is of sufficient size to receive window unit and complies with manufacturer's requirements for opening clearances. Verify sill plate is level.
B.	Notify Architect of unacceptable conditions before proceeding with installation.
3.2	INSTALLATION
A.	Install window unit in accordance with manufacturer's printed instructions including the following:
1.	Apply sealant around perimeter of window unit between nail fin and exterior sheathing of wall. Refer to Division 7 Section "Joint Sealants".
2.	Install window unit square, level and plumb. Center window unit in opening and secure window unit by nailing through nail fin and screw through jambs as indicated in manufacturer's instructions.
3.	Flash window in accordance with AAMA's "Standard Practice for Installation of Windows with a Mounting Flange in Stud Frame Construction".
4.	Insulate between window frame and rough opening with insulation. Refer to Division 7 Section "Building Insulation".
3.3	ADJUSTING
A.	Adjust units for smooth operation without binding or racking. Adjust sash locks and screens for smooth operation.
3.4	CLEANING AND PROTECTION
A.	Clean soiled surfaces and glass prior to substantial completion.
B.	Protect window unit from damage until substantial completion. Repair or replace damaged units.

END OF SECTION