SECTION 08 41 00.10

GENERATION 4 FOLDING GLASS WALLS BY NANAWALL - EXTERIOR AND INTERIOR

Display hidden notes to specifier. (Don't know how? Click Here) 
 Copyright 2021 -  2022 ARCAT, Inc. - All rights reserved

PART 1    GENERAL
1.1	SECTION INCLUDES
A.	Generation 4 Folding Glass Walls:
1.	Thermally-broken, sliding-folding aluminum-framed systems. (NW Aluminum 840)
2.	Thermally broken, sliding-folding, wood-framed system. (NW Wood 540)
3.	Thermally broken, sliding-folding, aluminum-framed system. (NW Aluminum 640)
4.	Thermally broken, sliding-folding acoustically rated, aluminum-framed system. (NW Acoustical 645)
5.	Thermally broken, sliding-folding, aluminum clad wood framed system. (NW Clad 740)
1.2	RELATED SECTIONS
A.	Section 06 10 00 - Rough Carpentry.O. and blocking.
B.	Section 06 20 00 - Finish Carpentry.
C.	Section 07 27 00 - Air Barriers.
D.	Section 07 62 00 - Sheet Metal Flashing and Trim.
E.	Section 07 90 00 - Joint Protection.
F.	Section 08 40 00 - Entrances, Storefronts, and Curtain Walls.
G.	Section 08 41 13 - Aluminum-Framed Entrances and Storefronts.
H.	Section 08 41 26 - All-Glass Entrances and Storefronts.
I.	Section 08 43 29 - Sliding Storefronts.
J.	Section 08 43 33 - Folding Glass Wall System.
K.	Section 08 51 13 - Aluminum Windows.
L.	Section 08 70 00 - Hardware.
M.	Section 08 83 13 - Mirrored Glass Glazing.
N.	Section 09 22 16 - Non-Structural Metal Framing.O. and reinforcement.
O.	Section 10 23 26 - Operable Glass Partition*.
1.3	REFERENCES
A.	American Architectural Manufacturer's Association (AAMA):
1.	AAMA 205-15, In-Plant Testing Guidelines for Manufacturers and Independent Laboratories.
2.	AAMA 502, Voluntary Specification for Field Testing of Newly Installed Fenestration Products.
3.	AAMA 611, Voluntary Specification for Anodized Architectural Aluminum.
4.	AAMA 920-11, Specification for Operating Cycle Performance of Side-Hinged Exterior Door System.
5.	AAMA 1304, Voluntary Specification for Forced Entry Resistance of Side-Hinged Door Systems.
6.	AAMA 2604, Voluntary Specifications, Performance Requirements and Test Procedures for High Performance Organic Coatings on Aluminum Extrusions and Panels.
7.	AAMA/WDMA/CSA 101/I.S.2/A440-17, NAFS, North American Fenestration Standard - Specification for Windows, Doors and Skylights.
B.	American National Standards Institute: ANSI Z97.1 - For Safety Glazing Materials Used in Buildings - Safety Performance Specifications and Methods of Test.
C.	ASTM International (ASTM):
1.	ASTM C1036, Standard Specification for Flat Glass.
2.	ASTM C1048, Standard Specification for Heat-Strengthened and Fully Tempered Flat Glass.
3.	ASTM E90-09, Standard Test Method for Laboratory Measurement of Airborne Sound Transmission Loss of Building Partitions and Elements.
4.	ASTM E283-04 (2012), Standard Test Method for Determining Rate of Air Leakage through Exterior Windows, Curtain Walls, and Doors Under Specified Pressure Difference Across the Specimen.
5.	ASTM E330-00 (2016), Standard Test Method for Structural Performance of Exterior Windows, Curtain Walls, and Doors by Uniform Static Air Pressure Difference.
6.	ASTM E331-00 (2016), Standard Test Method for Water Penetration of Exterior Windows, Skylights, Doors, and Curtain Walls by Uniform Statics Air Pressure Difference.
7.	ASTM E413-16, Classification for Rating Sound Insulation.
8.	ASTM E547-00 (2016), Standard Test Method for Water Penetration of Exterior Windows, Skylights, Curtain Walls, and Doors by Cyclic Static Air Pressure Differential.
9.	ASTM E2068-00 (2016), Standard Test Method for Determination of Operating Force of Sliding Windows and Doors.
10.	ASTM E987-88 (2017), Standard Test Methods for Deglazing Force of Fenestration Products.
11.	ASTM E1332, Standard Classification for Rating Outdoor-Indoor Sound Attenuation.
12.	ASTM F842, Standard Test Methods for Measuring the Forced Entry Resistance of Sliding Door Assemblies, Excluding Glazing Impact.
D.	Construction Product Directive (CPD), a legal mandate of the European Commission; CE Mark.
E.	Consumer Product Safety Commission (CPSC): CPSC 16CFR-1201, Safety Standard for Architectural Glazing Materials.
F.	CSA Group (Canadian Standards Association), CSA A440S1 - The Canadian supplement to North American (NAFS) standards.
G.	German Institute for Standardization (DIN) & International Organization for Standardization (ISO):
1.	DIN EN 1090, Manufacturing qualification for welding of supporting building components.
2.	DIN EN 1191, Windows and Pedestrian Doors - Resistance to repeated opening and closing - Mechanical Durability Test Method.
3.	DIN EN 1627, Pedestrian door sets, windows, curtain walling, grilles, and shutters - Burglar resistance - Requirements and classification.
4.	DIN EN 1630, Pedestrian door sets, windows, curtain walling, grilles, and shutters - Burglar resistance - Test method for the determination of resistance to manual burglary attempts.
5.	DIN EN ISO 717-1, Acoustics - Rating of sound insulation in buildings and building elements.
6.	DIN EN ISO 10140-1, 2, 4 and 5, Airborne sound measurement.
7.	DIN EN ISO 12400, Windows and pedestrian doors - Mechanical durability - Requirements and classification.
H.	National Fenestration Rating Council (NFRC):
1.	NFRC 100 - Procedure for Determining Fenestration Product U-factors.
2.	NFRC 200 - Procedure for Determining Fenestration Product Solar Heat Gain Coefficient and Visible Transmittance at Normal Incidence.
3.	NFRC 400 - Procedure for Determining Fenestration Product Air Leakage.
4.	NFRC 500 - Procedure for Determining Fenestration Product Condensation Resistance Rating Values.
I.	U.S. Environmental Protection Agency (EPA): Energy Star program.
1.4	SUBMITTALS
A.	Submit under provisions of Section 01 30 00.
B.	Product Data: Manufacturer's data sheets on each product to be used, including:
1.	Preparation instructions and recommendations.
2.	Storage and handling requirements and recommendations.
3.	Independently tested data listing performance criteria.
4.	Product literature for systems incorporated in the Work. Performance test results and details of construction relative to materials, dimensions of individual components, profiles, and colors.
5.	Manufacturers' Instructions: Owner's Manual from manufacturer which includes installation instructions, operation, and maintenance data.
6.	Certificates: CE Mark Certificate.
C.	Product Drawings: Including but not limited to the following.
1.	Indicate system component sizes, dimensions and framing R.O., configuration, swing panels, direction of swing, stacking layout, typical head jamb, side jambs and sill details, type of glazing material, handle height and field measurements.
2.	Elevations of rough opening requirements and details for field-applied components.
D.	Contract Closeout Submittal: Owner's Manual from manufacturer. Identify Owner's Manual with project name, location and completion date, type and size of unit installed.
1.5	QUALITY ASSURANCE
A.	Regulatory Requirements: CE Mark certified.
B.	Manufacturer: Complete, precision built, engineered, pre-fitted units by a single source manufacturer with 30-year experience in providing folding and sliding door systems for large openings in the North American market.
1.	ISO 9001: 2015 quality management system registration.
2.	ISO 14001: 2015 environmental management system registration.
C.	Installer Qualifications:
1.	Experienced in installation of manufacturer's products or similar products.
2.	Reference list of 3 projects of similar scale and complexity successfully completed in the last 3 years.
3.	Installer trained and certified by manufacturer.
D.	Single Source: Furnish system materials from one manufacturer for entire Project.
1.6	DELIVERY, STORAGE, AND HANDLING
A.	Deliver materials to job site in sealed, unopened cartons or crates.
1.	Upon receipt, inspect shipment. Ensure it is complete, in good condition and meets project requirements.
B.	Store products in manufacturer's unopened packaging until installation. Store flat in well ventilated area, no direct sunlight, in a clean and dry location. Protect units against weather and defacement or damage from construction activities, especially to panel edges.
1.7	PROJECT CONDITIONS
A.	Mark field measurements on Product Drawing submittal. Contractor shall field verify dimensions including but not limited to rough openings and inset components.
B.	Maintain environmental conditions (temperature, humidity, and ventilation) within limits recommended by manufacturer for optimum results. Do not install products under environmental conditions outside manufacturer's recommended limits.
1.8	WARRANTY
A.	Manufacturer's warranty against defects in materials and workmanship and as follows:
1.	Rollers: 10 years.
2.	Seal Failure of Insulated Glazing: 10 years.
3.	Other Components (excluding screens): Five years beginning with the earliest of 120 days from date of delivery by manufacturer or date of Substantial Completion.
4.	Other Components (excluding screens): 10 years beginning with the earliest of 120 days from date of delivery by manufacturer or Date of Substantial Completion if installed by manufacturer's specific system approved or certified trained installer.
PART 2    PRODUCTS
2.1	MANUFACTURERS
A.	Acceptable Manufacturer: Nana Wall Systems, Inc., which is located at: 100 Meadow Creek Dr. Suite 250; Corte Madera, CA 94925; ASD Toll Free Tel: 800-873-5673; Tel: 415-383-3148; Fax: 415-383-0312; Email: request info; Web: https://www.nanawall.com
B.	Substitutions: Not permitted.
C.	Requests for Substitutions: Considered in accordance with provisions of Section 01 60 00.
2.2	SLIDING-FOLDING THERMALLY-BROKEN ALUMINUM, WOOD AND ALUMINUM CLAD WOOD-FRAMED GLASS PANEL SYSTEMS
A.	Basis of Design: Model NW Aluminum 840 sliding-folding thermally broken aluminum-framed glass panel system as manufactured by Nana Wall Systems, Incorporated. Nominal frame stile width of 3-7/8 inch (99 mm) between folding panels, floor track supported system. Manufacturer's standard thermally broken frame and panel profiles, with head track, side jambs, sill and panels with dimensions as shown on Drawings.
1.	System Components: Aluminum frame, threshold. panels, sliding-folding and locking hardware, weather stripping, glass and glazing, panel catch, bionic turtle thermal break and accessories as required for a complete working installation.
2.	Performance Requirements (NW Aluminum 840): Lab tested.
a.	Sill and Opening Type: Hybrid Sill, Inward Opening:
1)	Folding Glass Door Units tested to AAMA/WDMA/CSA 101/ I.S.2/A440-17 (NAFS-17):
a)	Class CW-PG40 - FLD 157.5 x 102 inch (4000 x 2600 mm) and Class LC-PG50 - FLD 157.5 x 102 inch (4000 x 2600 mm) with 1L3R configuration.
2)	Air Infiltration per ASTM E283:
a)	Static air pressure difference of 1.57 psf (75 Pa): 0.04 cfm per sq ft (0.20 L per sec per sq m).
b)	Static air pressure difference of 6.24 psf (300 Pa): 0.11 cfm per sq ft (0.56 L per sec per sq m).
3)	Water Penetration per ASTM E331 and ASTM E547: No uncontrolled water leakage at static test pressure of 9 psf (450 Pa). Not applicable for even-even configurations.
4)	Structural Loading per ASTM E330: Wind load resistance.
a)	Design Pressure; Positive: 50 psf (2400 Pa).
b)	Design Pressure; Negative: 55 psf (2670 Pa).
c)	Uniform Load Deflection; L/175: Pass 40 psf (1945 Pa).
b.	Sill and Opening Type: Hybrid Sill, Outward Opening:
1)	Folding Glass Door Units test to AAMA/WDMA/CSA 101/I.S.2/A440-17 (NAFS-17):
a)	Class CW-PG40 - FLD 157.5 x 102 inch (4000 x 2600 mm) and Class LC-PG50 - FLD 157.5 x 102 inch (4000 x 2600 mm) with 1L3R configuration.
2)	Air Infiltration per ASTM E283:
a)	Static air pressure difference of 1.57 psf (75 Pa): 0.04 cfm per sq ft (0.20 L per sec per sq m).
b)	Static air pressure difference of 6.24 psf (300 Pa): 0.10 cfm per sq ft (0.5 L per sec per sq m).
3)	Water Penetration per ASTM E331 and ASTM E547: No uncontrolled water leakage at a static test pressure of 9 psf (450 Pa). Not applicable for even-even configurations.
4)	Structural Loading per ASTM E330: Wind load resistance.
a)	Design Pressure; Positive: 55 psf (2670 Pa).
b)	Design Pressure; Negative: 50 psf (2400 Pa).
c)	Uniform Load Deflection; L/175: Pass 45 psf (2150 Pa).
c.	Sill and Opening Type: Low Profile Saddle Sill, ADA Compliant, Inward Opening:
1)	Folding Glass Door Units test to AAMA/WDMA/CSA 101/I.S.2/A440-17 (NAFS-17):
a)	Class CW-PG35 - FLD 157.5 x 102 inch (4000 x 2600 mm) with 1L3R configuration.
2)	Air Infiltration per ASTM E283:
a)	Static air pressure difference of 1.57 psf (75 Pa): 0.12 cfm per sq ft (0.61 L per sec per sq m).
b)	Static air pressure difference of 6.24 psf (300 Pa): 0.30 cfm per sq ft (1.52 L per sec per sq m).
3)	Water Penetration per ASTM E331 and ASTM E547: No uncontrolled water leakage at a static, with weeps, test pressure of 5.43 psf (260 Pa). Not applicable for even-even configurations.
4)	Structural Loading per ASTM E330: Wind load resistance.
a)	Design Pressure; Positive and Negative: 50 psf (2400 Pa).
b)	Uniform Load Deflection, L/175: Pass 40 psf (1945 Pa).
d.	Sill and Opening Type:  Low Profile Saddle Sill, ADA Compliant, Outward Opening:
1)	Folding Glass Door Units test to AAMA/WDMA/CSA 101/I.S.2/A440-17 (NAFS-17):
a)	Class CW-PG35 - FLD 157.5 x 102 inch (4000 x 2600 mm) with 1L3R configuration.
2)	Air Infiltration per ASTM E283: 
a)	Static air pressure difference of 1.57 psf (75 Pa): 0.12 cfm per sq ft (0.61 L per sec per sq m).
b)	Static air pressure difference of 6.24 psf (300 Pa): 0.29 cfm per sq ft (1.5 L per sec per sq m).
3)	Water Penetration per ASTM E331 and ASTM E547: No uncontrolled water leakage at a static, with weeps, test pressure of 5.43 psf (260 Pa). Not applicable for even-even configurations.
4)	Structural Loading per ASTM E330: Wind load resistance.
a)	Design Pressure; Positive and Negative: 50 psf (2400 Pa).
b)	Uniform Load Deflection, L/175: Pass 40 psf (1945 Pa).
e.	Sill and Opening Type: Low Profile Saddle Sill with UniverSILL Insert, Outward Opening:
1)	Folding Glass Door Units test to AAMA/WDMA/CSA 101/I.S.2/A440-17 (NAFS-17):
a)	Class CW-PG40 - FLD 157.5 x 102 inch (4000 x 2600 mm) and Class LC-PG50 - FLD 157.5 x 102 inch (4000 x 2600 mm) with 1L3R configuration.
2)	Air Infiltration per ASTM E283:
a)	Static air pressure difference of 1.57 psf (75 Pa): 0.04 cfm per sq ft (0.20 L per sec per sq m).
b)	Static air pressure difference of 6.24 psf (300 Pa): 0.07 cfm per sq ft (0.36 L per sec per sq m).
3)	Water Penetration per ASTM E331 and ASTM E547: No uncontrolled water leakage at a static test pressure of 7.5 psf (360 Pa). Not applicable for even-even configurations.
4)	Structural Loading per ASTM E330: Wind load resistance.
a)	Design Pressure; Positive and Negative: 50 psf (2400 Pa).
b)	Uniform Load Deflection, L/175: Pass 40 psf (1945 Pa).
f.	Sill and Opening Type: Flush Sill, Inward Opening:
1)	Structural Loading per ASTM E330: Wind load resistance.
a)	Design Pressure; Positive and Negative: 50 psf (2400 Pa).
b)	Uniform Load Deflection, L/175: Pass 40 psf (1945 Pa).
2)	Air Infiltration per ASTM E283:
a)	Static air pressure difference of 1.57 psf (75 Pa): 0.12 cfm per sq ft (0.61 L per sec per sq m).
b)	Static air pressure difference of 6.24 psf (300 Pa): 0.30 cfm per sq ft (1.52 L per sec per sq m).
g.	Sill and Opening Type: Flush Sill, Outward Opening:
1)	Structural Loading per ASTM E330: Wind load resistance.
a)	Design Pressure; Positive and Negative: 50 psf (2400 Pa).
b)	Uniform Load Deflection, L/175: Pass 40 psf (1945 Pa).
2)	Air Infiltration per ASTM E283:
a)	Static air pressure difference of 1.57 psf (75 Pa): 0.12 cfm per sq ft (0.61 L per sec per sq m).
b)	Static air pressure difference of 6.24 psf (300 Pa): 0.29 cfm per sq ft (1.50 L per sec per sq m).
h.	Swing Panel - Operation / Cycling Performance (AAMA 920): 500,000 cycles.
i.	System - Life Cycle Testing Performance per EN 1191: Class 3; 20,000 cycles.
j.	Operating Force (ASTM E2068):
1)	Swing Panel: Open 1 lbf (2.8 N) & Close 1 lbf (3.9 N).
2)	Folding Panels:
a)	Initiate Motion: Open 4 lbf (20 N) & Close 3 lbf (15 N).
b)	Maintain Motion: Open 1 lbf (3 N) & Close 1 lbf (4 N).
k.	Forced Entry (AAMA 1304, DIN EN 1191): Pass.
l.	Forced Entry Resistance per ASTM F842, AAMA 1304, CAWM 300: Meets Grade 40; plus F2.
m.	Burglary Resistance Unit: EN 1627-30, Class RC2/ RC2N; Resistance Class 2 certified.
n.	Thermal Performance (U-factor): NFRC 100 rated, certified, and labeled.
o.	Solar Heat Gain Coefficient plus Visible Light Transmission: NFRC 200 rated, certified, and labeled.
p.	Air Leakage: NFRC 400 rated, certified, and labeled.
q.	Condensation Resistance Factor: NFRC 500 rated, certified, and labeled.
3.	Design Criteria:
a.	Sizes and Configurations: As indicated on Drawings for selected number and size of panels, location of swing panels, and number of panels stacking to the left and to the right.
b.	Operation: Adjustable sliding and folding hardware with top and bottom tracks.
c.	Panel Configuration: Straight.
d.	Panel Configuration: 90 degree angle turn.
e.	Panel Configuration: Window and door combination.
f.	Stack Storage Configuration: Inswing type.
g.	Stack Storage Configuration: Outswing type.
h.	Mounting Type: Floor track supported with upper guide track.
i.	Hinged Panels:
1)	Primary Swing Panel of Paired Swing Panels Looking from Inside: On the left.
2)	Primary Swing Panel of Paired Swing Panels Looking from Inside: On the right.
3)	Entry and Egress Panel: Hinged to bi-folding panels.
4)	Entry and Egress Panel: Hinged to side jamb.
5)	Entry and Egress Panel:  None.
j.	Panel Pairing Configuration: Bi-folding panels hinged to side jamb.
k.	Panel Pairing Configuration: Bi-folding panels unhinged FourFold or SixFold panel sets.
4.	Fabrication: Extruded aluminum frame and panel profiles, corner connectors, hinges, sliding and folding hardware, locking hardware, handles, glass and glazing, and weather stripping.
a.	Factory pre-assembled and shipped with system components, installation mounting plates, and instructions.
b.	Exposed work matched to produce continuity of line and design with joints.
c.	No raw edges visible at joints.
5.	Materials:
a.	Panels: Single lite; standard.
b.	Panels: Multiple lites with horizontal mullions at heights indicated on Drawings from bottom of panel.
c.	Panels: Single lite with simulated divided lites in pattern as shown on Drawings.
d.	Panel Size (W x H): ___ x ___ inches (___ x ___ mm).
e.	Rail Depth: 3-1/8 inch (84 mm).
f.	Top Rail Width: 2-5/8 inch (66 mm).
g.	Typical Stile Width: 1-3/4 inch (45 mm) on both stile or a nominal frame stile width of 3-7/8 inch (99 mm) between folding.
h.	Bottom Rail Width: 2-5/8 inch (67 mm).
i.	Bottom Rail Width: Manufacturer's standard kick-plate of 10 inches (254 mm).
6.	Frame:   
a.	 Thermally broken top track and side jambs with multi-purpose frame insert to hide anchoring connections.
b.	Thermally broken top track and side jambs without multi-purpose frame insert to hide anchoring connections.
c.	Frame Finish: To match panel finish.
d.	Frame Depth: Top Track and Side Jamb Depth; 3-9/16 inch (91 mm).
7.	Head Track Width: 2-13/16 inch (72 mm) standard.
8.	Head Track Width: 3-7/8 inch (99 mm) with anti-tilt feature for unhinged FourFold or SixFold panel set configurations.
9.	Side Jambs: 2-13/16 inch (72 mm) wide. Adjustment: Plus or minus 3/16 inch (5 mm).
10.	Sill Type: Hybrid sill, thermally broken with high heel protector insert.
11.	Sill Type: Low profile saddle sill, ADA compliant, thermally broken with high heel protector insert.
12.	Sill Type: Low profile saddle sill with UniverSILL, thermally broken with high heel protector insert.
13.	Sill Type: Flush sill, ADA compliant, thermally broken with high heel protector insert.
14.	Sill Finish: Aluminum with clear anodized finish.
15.	Sill Finish: Aluminum with black anodized finish.
16.	Aluminum Extrusions: AIMgSi0.5 alloy, 6063-T5; F-22 - European standard.
a.	Thickness: 0.078 inch (2.0 mm) nominal.
b.	Thermal Break: 1-15/16 inches (49 mm) wide specially designed and patented (Patent Number: US10550625B2) glass fiber reinforced (GFR) polyamide "Bionic Turtle" for panels. Standard thermal break elsewhere.
c.	Finish: One color inside and outside.
1)	Finish Type: Anodized per AAMA 611. Clear.
2)	Finish Type: Anodized per AAMA 611. Dark bronze.
3)	Finish Type: Powder coat per AAMA 2604.
a)	Color: Chosen from standard selection of 50 colors. Matte.
b)	Color: Chosen from full RAL selection. High gloss.
c)	Color: Chosen from full RAL selection. Matte.
4)	Finish Type: Custom finish.
d.	Finish: Different color inside and outside.
1)	Interior: Powder coat per AAMA 2604.
a)	Color: Chosen from standard selection of 50 colors. Matte.
b)	Color: Chosen from full RAL selection. High gloss.
c)	Color: Chosen from full RAL selection. Matte.
2)	Interior: Custom finish.
3)	Exterior: Powder coat per AAMA 2604.
a)	Color: Chosen from standard selection of 50 colors. Matte.
b)	Color: Chosen from full RAL selection. High gloss.
c)	Color: Chosen from full RAL selection. Matte.
4)	Exterior: Custom finish.
17.	Glass and Glazing: Safety Glazing per ASTM C1036, ASTM C1048, ANSI Z97.1 and CPSC 16CFR 1201 for NW Aluminum 840.
a.	Glazing Units, Double Insulated: Dry glazed with glass stops on the inside.
1)	Double IGU:  15/16 inch (24 mm), clear insulated tempered
a)	Insulated Glazing Unit Fill:  Air. 
b)	Insulated Glazing Unit Fill:  Argon. 
2)	Triple IGU:  1-9/16 inch (40 mm), Low E Insulated Tempered 176 No. 2 and No. 5. 
3)	Triple IGU:  1-9/16 inch (40 mm), Low E Insulated Tempered PL No. 2 and No. 5.
a)	Insulated Glazing Unit Fill: Air.
b)	Insulated Glazing Unit Fill: Argon.
18.	Glass Type: Reduced iron, standard.
19.	Glass Spacers: Gray finish with capillary tube.
20.	Glass Spacers: Black finish with capillary tubes.
21.	Glass Spacers: Gray finish without capillary tubes.
22.	Glass Spacers: Black finish without capillary tubes.
23.	Alarmed Glazing: Connection wiring to alarm system, position monitoring, locking detection and notification systems such as glass-breakage sensors by others.
24.	Locking Hardware and Handle for Sliding-Folding Systems: 
a.	Main Entry Panels:  Lockset with lockable latch, multi-point locking with deadbolt and rods at top and bottom on primary panels only. 
1)	Application:  Single swing panel. 
2)	Application:  Pair of swing panels. 
3)	Operation:  After turn of key or thumb turn, depression of handles withdraws latch. Lifting of handles engages rods and turn of key or thumb turn engages deadbolt and operates lock. 
4)	Rods:  Concealed, not edge mounted. 
5)	Lever Handles:  Lever handles on inside and outside. 
6)	Lever Handles:  Lever handles with return on inside and outside. 
7)	Lever Handle Finish:  Brushed satin stainless steel; standard. 
8)	Lever Handle Finish:  Black titanium stainless steel; standard. 
9)	Lever Handle Finish:  Copper-nickel stainless steel antiviral and antimicrobial. 
10)	Locking:  Standard profile cylinder. 
11)	Secondary Swing Panel:  Concealed two-point, edge locking. 
b.	Main Entry Panels:  Flat handle on inside only with concealed two-point locking hardware operated by 180 degrees turn of handle; the main entry panel is operable from inside only and there is no latch. 
c.	Main Entry Panels:  No hardware or locking provided by manufacturer; Field installed panic device from Section 08 71 00 prepped for commercial application. 
1)	Application:  Single swing panel. 
2)	Panic Hardware:  Von Duprin 33/35A Series Narrow Stile Rim Exit Devices. 
3)	Panic Hardware:  DORMA 9700 Series Narrow Stile Rim Exit Devices. 
d.	Pairs of Folding Panels:  Handles and concealed two-point locking hardware operated by 180 degrees turn of handle between each pair. Face applied flush bolt locking NOT acceptable. 
1)	Handles:  Manufacturer�s flat handles. 
a)	Flat Handle Finish:  Brushed satin stainless steel. 
b)	Flat Handle Finish:  Black titanium stainless steel. 
c)	Flat Handle Finish:  Copper-nickel stainless steel antiviral and antimicrobial. 
e.	Handle Height:  41-3/8 inch (105 cm) centered from bottom of panel unless otherwise indicated on Drawings. 
f.	Locking Rods:  End caps top and bottom:  Rod Stroke:  15/16 inch (24 mm). 
g.	Additional Profile Cylinders:  Keyed alike. 
h.	Additional Profile Cylinders:  Keyed differently. 
i.	Panel catch:  Panel catch to hold swing panel to adjacent folding panel to prevent incorrect operation when moving the panel. 
j.	Sliding-Folding Hardware:  Combination with top and bottom tracks and threshold. 
1)	Running carriages to have sealed, self-lubricating, double ball bearing multi-rollers. 
2)	Surface mounted hinges and running carriages not acceptable. 
3)	Lower Running Carriage Carrying Capacity:  240 lb. (110 kg); lower running carriage provided with two vertical stainless-steel wheels with double row of ball bearings and two horizontal polyamide wheels. 
4)	Vertical wheels with Gothic arch feature to ride on top of stainless-steel guide track covers over full length of sill track. Wheels on aluminum surfaces not acceptable. 
5)	Upper guide carriage with two horizontal polyamide guiding wheels. For configurations with pairs of panels that slide left or right, additional concealed, additional vertical tilt protection hardware. 
6)	Hinges and Rollers:  Anodized aluminum with stainless steel security hinge pins and set-screws. Concealed panel alignment with a tight seal through the patented (Patent Number:  US10711510B2) TwinX mechanism reinforced between panels for a tight seal. Double ball bearing stainless-steel wheel rollers match hinge finish. 
a)	Finish:  Clear. 
b)	Finish:  Black. 
7)	Spring-Loaded Pull Handle:  For outswing units with larger panel sizes, a spring loaded-pull handle is supplied for ease of closing the system. The pull handle is located above the flat handle. When not in use, the handle lays flat against the adjacent panel and is supplied with bumpers to avoid metal to metal contact. Handles are stainless steel  with the attachment to coordinate with the hinge hardware of the system. 
a)	Pull Handle Finish:  Brushed satin stainless steel or black titanium stainless steel. 
k.	Weather Stripping and Sound Gasketing:  Manufacturer�s double layer EPDM between panels and EPDM gasket, Q-Ion gasket, or brush seal between panel and frame, or brush seals with a two-layer fiberglass reinforced polyamide fin attached at both inner and outer edge of bottom of door panels with a recessed sill or on frame for sealing between panels and between panel and frame. 
l.	Fasteners:  Installation plates for connecting frame components made of stainless steel with sealing cushion to avoid thermal connectivity. 
m.	Insect Screen:  Fully retractable non-pleated screen. Ultra-strong, UV resistant fiberglass mesh housed in single cartridge riding on a single track. 
1)	Basis-of-Design Product by Manufacturer:  The Horizon by Wizard Industries, Inc. 
a)	Wizard Industries, Inc. which is located at:  4263 Phillips Ave, Burnaby, BC, Canada V5A 2X4; Toll Free:  (888) 949-3667; Telephone:  (604) 299-8878; Fax:  (604) 299-4496; Email:  sales@wizardindustries.com; Web:  https://www.wizardscreens.com. 
B.	Basis of Design: Model NW Wood 540 sliding-folding wood-framed glass panel system as manufactured by Nana Wall Systems, Incorporated. 3-3/8 inch (86 mm) thick, floor track supported system. Manufacturer's standard solid quadruple laminated wood panel profiles and wood clad thermally broken aluminum frame and profiles, with head and floor track, side jambs, sill and panels with dimensions as shown on Drawings.
1.	System Components: Cross-grained wood frame profile, threshold, wood-framed panels, sliding-folding and locking hardware, weather stripping, glass and glazing, panel catch, and accessories as required for a complete working installation.
2.	Performance Requirements (NW Wood 540): Lab tested.
a.	Sill and Opening Type: Hybrid Sill, Inward Opening:
1)	Folding Glass Door Units tested to AAMA/WDMA/CSA 101/I.S.2/A440-17 (NAFS-17):
a)	Class CW-PG35 - FLD 157.5 x 102 inch (4000 x 2600 mm) with 1L3R configuration.
2)	Air Infiltration per ASTM E283:
a)	Static air pressure difference of 1.57 psf (75 Pa): 0.06 cfm per sq ft (0.3 L per sec per sq m).
b)	Static air pressure difference of 6.24 psf (300 Pa): 0.14 cfm per sq ft (0.7 L per sec per sq m).
3)	Water Penetration per ASTM E331 and ASTM E547: No uncontrolled water leakage at static test pressure of 9 psf (450 Pa). Not applicable for even-even configurations.
4)	Structural Loading per ASTM E330: Wind load resistance.
a)	Design Pressure; Positive: 39 psf (1850 Pa).
b)	Design Pressure; Negative: 55 psf (2670 Pa)
c)	Uniform Load Deflection; L/175: Pass 45 psf (2150 Pa).
b.	Sill and Opening Type: Hybrid Sill, Outward Opening:
1)	Folding Glass Door Units test to AAMA/WDMA/CSA 101/I.S.2/A440-17 (NAFS-17):
a)	Class CW-PG35 - FLD 157.5 x 102 inch (4000 x 2600 mm) with 1L3R configuration.
2)	Air Infiltration per ASTM E283:
a)	Static air pressure difference of 1.57 psf (75 Pa): 0.06 cfm per sq ft (0.3 L per sec per sq m).
b)	Static air pressure difference of 6.24 psf (300 Pa): 0.14 cfm per sq ft (0.7 L per sec per sq m).
3)	Water Penetration per ASTM E331 and ASTM E547: No uncontrolled water leakage at a static test pressure of 9 psf (450 Pa). Not applicable for even-even configurations.
4)	Structural Loading per ASTM E330: Wind load resistance.
a)	Design Pressure; Positive: 55 psf (2670 Pa).
b)	Design Pressure; Negative: 39 psf (1850 Pa).
c)	Uniform Load Deflection; L/175: Pass 45 psf (2150 Pa).
c.	Sill and Opening Type: Low Profile Saddle Sill, ADA Compliant, Inward Opening:
1)	Folding Glass Door Units test to AAMA/WDMA/CSA 101/I.S.2/A440-17 (NAFS-17):
a)	Class CW-PG35 - FLD 157.5 x 102 inch (4000 x 2600 mm) with 1L3R configuration.
2)	Air Infiltration per ASTM E283:
a)	Static air pressure difference of 1.57 psf (75 Pa): 0.11 cfm per sq ft (0.6 L per sec per sq m).
b)	Static air pressure difference of 6.24 psf (300 Pa): 0.28 cfm per sq ft (1.50 L per sec per sq m).
3)	Water Penetration per ASTM E331 and ASTM E547: No uncontrolled water leakage at a static, with weeps, test pressure of 5.43 psf (260 Pa). Not applicable for even-even configurations.
4)	Structural Loading per ASTM E330: Wind load resistance.
a)	Design Pressure; Positive:40 psf (1945 Pa).
b)	Design Pressure; Negative: 45 psf (2150 Pa).
c)	Uniform Load Deflection, L/175: Pass 49 psf (2380 Pa).
d.	Sill and Opening Type:  Low Profile Saddle Sill, ADA Compliant, Outward Opening:
1)	Folding Glass Door Units test to AAMA/WDMA/CSA 101/I.S.2/A440-17 (NAFS-17):
a)	Class CW-PG35 - FLD 157.5 x 102 inch (4000 x 2600 mm) with 1L3R configuration.
2)	Air Infiltration per ASTM E283:
a)	Static air pressure difference of 1.57 psf (75 Pa): 0.13 cfm per sq ft (0.66 L per sec per sq m).
b)	Static air pressure difference of 6.24 psf (300 Pa): 0.25 cfm per sq ft (1.28 L per sec per sq m).
3)	Water Penetration per ASTM E331 and ASTM E547: No uncontrolled water leakage at a static, with weeps, test pressure of 5.43 psf (260 Pa). Not applicable for even-even configurations.
4)	Structural Loading per ASTM E330: Wind load resistance.
a)	Design Pressure; Positive: 45 psf (2150 Pa).
b)	Design Pressure; Negative: 40 psf (1945 Pa).
c)	Uniform Load Deflection, L/175: Pass 52 psf (2520 Pa).
e.	Sill and Opening Type: Low Profile Saddle Sill with UniverSILL Insert, Outward Opening:
1)	Folding Glass Door Units test to AAMA/WDMA/CSA 101/I.S.2/A440-17 (NAFS-17):
a)	Class CW-PG40 - FLD 157.5 x 102 inch (4000 x 2600 mm) with 1L3R configuration.
2)	Air Infiltration per ASTM E283:
a)	Static air pressure difference of 1.57 psf (75 Pa): 0.04 cfm per sq ft (0.20 L per sec per sq m).
3)	Static air pressure difference of 6.24 psf (300 Pa): 0.07 cfm per sq ft (0.36 L per sec per sq m).Water Penetration per ASTM E331 and ASTM E547: No uncontrolled water leakage at a static test pressure of 7.5 psf (360 Pa). Not applicable for even-even configurations.
4)	Structural Loading per ASTM E330: Wind load resistance.
a)	Design Pressure; Positive: 45 psf (2150 Pa).
b)	Design Pressure; Negative: 40 psf (1945 Pa).
c)	Uniform Load Deflection, L/175: Pass 52 psf (2520 Pa).
f.	Sill and Opening Type: Flush Sill, Inward Opening:
1)	Air Infiltration per ASTM E283:
a)	Static air pressure difference of 1.57 psf (75 Pa): 0.11 cfm per sq ft (0.6 L per sec per sq m).
b)	Static air pressure difference of 6.24 psf (300 Pa): 0.25 cfm per sq ft (1.28 L per sec per sq m).
2)	Structural Loading per ASTM E330: Wind load resistance.
a)	Design Pressure; Positive: 40 psf (1945 Pa).
b)	Design Pressure; Negative: 45 psf (2150 Pa).
c)	Uniform Load Deflection, L/175: Pass 49 psf (2380 Pa).
g.	Sill and Opening Type: Flush Sill, Outward Opening:
1)	Air Infiltration per ASTM E283:
a)	Static air pressure difference of 1.57 psf (75 Pa): 0.13 cfm per sq ft (0.66 L per sec per sq m).
b)	Static air pressure difference of 6.24 psf (300 Pa): 0.28 cfm per sq ft (1.5 L per sec per sq m).
2)	Structural Loading per ASTM E330: Wind load resistance.
a)	Design Pressure; Positive: 45 psf (2150 Pa).
b)	Design Pressure; Negative: 40 psf (1945 Pa).
c)	Uniform Load Deflection, L/175: Pass 52 psf (2520 Pa).
h.	Swing Panel - Operation / Cycling Performance (AAMA 920): 500,000 cycles.
i.	System - Life Cycle Performance per DIN EN 1191/12400: Class 3; 20,000 cycles.
j.	Operating Force (ASTM E2068): 
1)	Swing Panel: Open 1 lbf (2.8 N) & Close 1 lbf (3.9 N).
2)	Folding Panels:
a)	Initiate Motion - Open 4 lbf (20 N) & Close 3 lbf (15 N).
b)	Maintain Motion - Open 1 lbf (3 N) & Close 1 lbf (4 N).
k.	Forced Entry (AAMA 1304, DIN EN 1191): Pass.
l.	Forced Entry Resistance per ASTM F842, AAMA 1304, CAWM 300: Meets Grade 40; plus F2.
m.	Burglary Resistance Unit:  EN ISO 1627-30, Class RC2/ RC2N; Resistance Class 2 certified.
n.	Thermal Performance (U-factor): NFRC 100 rated, certified, and labeled.
o.	Solar Heat Gain Coefficient plus Visible Light Transmission: NFRC 200 rated, certified, and labeled.
p.	Air Leakage: NFRC 400 rated, certified, and labeled.
q.	Condensation Resistance Factor: NFRC 500 rated, certified, and labeled.
3.	Design Criteria:
a.	Sizes and Configurations: As indicated on Drawings for selected number and size of panels, location of swing panels, and number of panels stacking to the left and to the right.
b.	Operation: Adjustable folding sliding hardware with top and bottom tracks.
c.	Panel Configuration: Straight.
d.	Panel Configuration: 90 degree angle turn.
e.	Panel Configuration: Window and door combination.
f.	Stack Storage Configuration: Inswing type.
g.	Stack Storage Configuration: Outswing type.
h.	Mounting Type: Floor track supported with upper guide track.
i.	Hinged Panels:
1)	Primary Swing Panel of Paired Swing Panels Looking from Inside: On the left.
2)	Primary Swing Panel of Paired Swing Panels Looking from Inside: On the right.
3)	Entry and Egress Panel: Hinged to bi-folding panels.
4)	Entry and Egress Panel: Hinged to side jamb.
5)	Entry and Egress Panel: None.
j.	Panel Pairing Configuration: Bi-folding panels hinged to side jamb.
k.	Panel Pairing Configuration: Bi-folding panels unhinged FourFold or SixFold panel sets.
4.	Fabrication: Use thermally broken aluminum frame and running astragals with wood cladding, quad-layer, cross grained, solid wood for panel profiles, connected to hinges, sliding, folding hardware, locking hardware, handles, threshold and track, glass and glazing and weather stripping.
a.	Factory pre-assembled. Ship with system components and installation instructions.
b.	Exposed work matched to produce continuity of line and design with joints.
c.	Wood frame and panel components to be sealed with a clear sand sealer or primer.
d.	No raw edges visible at joints.
5.	Materials:
a.	Panels: Single lite; standard.
b.	Panels: Multiple lites with horizontal mullions at heights indicated on Drawings from bottom of panel.
c.	Panels: Single lite with simulated divided lites in pattern as shown on Drawings.
d.	Panel Size (W x H): ___ x ___ inches (___ x ___ mm).
e.	Rail Depth: 3-3/8 inch (86 mm).
f.	Top Rail Width: 3-1/4 inch (82 mm).
g.	Typical Stile Width: 2-5/8 inch (67 mm) for a total nominal frame stile width of 3-7/8 inch (143 mm) between folding panels.
h.	Bottom Rail Width: 3-1/4 inch (82 mm).
i.	Bottom Rail Width: Manufacturer's standard kick-plate of 10 inches (254 mm).
6.	Frame:  Including running astragals.
a.	Thermally broken top track and side jambs to hide anchoring connections.
b.	Wood cladding on both sides.
c.	For long-term tight, consistent sealing, provide a lateral patented (Patent Number: US10683688B2) adjustment feature at the side jambs capable of adjustment of plus or minus 3/16 inch (5 mm).
d.	Frame Finish: To match panel finish.
e.	Frame Depth: Top Track and Side Jamb Depth; 3-9/16 inch (91 mm).
7.	Head Track Width: 2-13/16 inch (72 mm) standard.
8.	Head Track Width: 3-7/8 inch (99 mm) with anti-tilt feature for unhinged FourFold or SixFold panel set configurations.
9.	Side Jamb Width: 2 inch (51 mm) wide. Adjustment: Plus or minus 3/16 inch (5 mm).
10.	Sill Type: Hybrid sill, thermally broken, with high heel protector insert.
11.	Sill Type: Low profile saddle sill, ADA compliant, thermally broken, with high heel protector insert.
12.	Sill Type: Low profile saddle sill with UniverSILL, thermally broken, with high heel protector insert.
13.	Sill Type: Flush sill, ADA compliant, thermally broken, with high heel protector insert.
14.	Wood Species Finish: FSC certified Sapeli Mahogany.
15.	Wood Species Finish: European Pine.
16.	Wood Species Finish: Spruce.
17.	Wood Species Finish: Western Hemlock.
18.	Wood Species Finish: Meranti.
19.	Wood Finish: Factory water-based, open pore clear sanding sealer for stain with one additional clear coat. See Section 09 90 00. 
20.	Wood Finish: Factory water-based, base coat applied for paint with one additional clear coat. See Section 09 90 00.
21.	Glass and Glazing: Safety Glazing per ASTM C1036, ASTM C1048, ANSI Z97.1 and CPSC 16CFR 1201.
a.	Glazing Units: Dry glazed with glass stops on the inside.
1)	Glass Lites: Tempered.
2)	Glass Lites: Laminated.
3)	Glass Lites: Tempered and Laminated.
4)	Double Insulated: 1-1/4 inch (32 mm), 6 mm + 6 mm or 15/16 inch (24 mm) 4 mm + 4 mm tempered glass depending on panel height.
5)	Double Insulated: 1-9/16 inch (40 mm), 12 mm + 10 mm STC 50 laminated glass to achieve unit STC of 42.
6)	Triple Insulated: 1-9/16 inch (40 mm), 6 mm + 4 mm + 6 mm or 1-1/2 inch (36 mm) 4 mm + 4 mm + 4 mm tempered glass depending on panel height.
22.	Insulated Glazing Unit Fill: Air.
23.	Insulated Glazing Unit Fill: Argon.
24.	Glass Type: Reduced iron.
25.	Glass Spacers: Gray finish with capillary tube.
26.	Glass Spacers: Black finish with capillary tubes.
27.	Glass Spacers: Gray finish without capillary tubes.
28.	Glass Spacers: Black finish without capillary tubes.
29.	Insulated Glass Unit Surfaces: Clear.
30.	Insulated Glass Unit Surfaces: Low- E coating on No. 2 surface of double IGU.
31.	Insulated Glass Unit Surfaces: Low-E coating on No. 2 and No. 4 surface of double IGU.
32.	Insulated Glass Unit Surfaces: Low-E coating on No. 2 and No. 5 surface of triple IGU.
33.	Alarmed Glazing: Connection wiring to alarm system, position monitoring, locking detection and notification systems such as glass-breakage sensors by others.
34.	Locking Hardware and Handle for Sliding-Folding Systems: 
a.	Main Entry Panels:  Lockset with lockable latch, multi-point locking with deadbolt and rods at top and bottom on primary panels only. 
1)	Application:  Single swing panel. 
2)	Application:  Pair of swing panels. 
3)	Operation:  After turn of key or thumb turn, depression of handles withdraws latch. Lifting of handles engages rods and turn of key or thumb turn engages deadbolt and operates lock. 
4)	Rods:  Concealed, not edge mounted. 
5)	Lever Handles:  Lever handles on inside and outside. 
6)	Lever Handles:  Lever handles with return on inside and outside. 
7)	Lever Handle Finish:  Brushed satin stainless steel; standard. 
8)	Lever Handle Finish:  Black titanium stainless steel; standard. 
9)	Lever Handle Finish:  Copper-nickel stainless steel antiviral and antimicrobial. 
10)	Locking:  Standard profile cylinder. 
11)	Secondary Swing Panel:  Concealed two-point, edge locking. 
b.	Main Entry Panels:  Flat handle on inside only with concealed two-point locking hardware operated by 180 degrees turn of handle; the main entry panel is operable from inside only and there is no latch. 
c.	Main Entry Panels:  No hardware or locking provided by manufacturer; Field installed panic device from Section 08 71 00 prepped for commercial application. 
1)	Application:  Single swing panel. 
2)	Application:  Pair of swing panels. 
d.	Pairs of Folding Panels:  Handles and concealed two-point locking hardware operated by 180 degrees turn of handle between each pair. Face applied flush bolt locking NOT acceptable. 
1)	Handles:  Manufacturer�s flat handles. 
a)	Flat Handle Finish:  Brushed satin stainless steel. 
b)	Flat Handle Finish:  Black titanium stainless steel. 
c)	Flat Handle Finish:  Copper-nickel stainless steel antiviral and antimicrobial. 
e.	Handle Height:  41-3/8 inch (105 cm) centered from bottom of panel unless otherwise indicated on Drawings.
f.	Locking Rods:  End caps top and bottom:  Rod Stroke:  15/16 inch (24 mm). 
g.	Additional Profile Cylinders:  Keyed alike. 
h.	Additional Profile Cylinders:  Keyed differently. 
i.	Panel catch:  Panel catch to hold swing panel to adjacent folding panel to prevent incorrect operation when moving the panel. 
j.	Sliding-Folding Hardware:  Combination with top and bottom tracks and threshold. 
1)	Running carriages to have sealed, self-lubricating, double ball bearing multi-rollers. 
2)	Surface mounted hinges and running carriages not acceptable. 
3)	Lower Running Carriage Carrying Capacity:  240 lb. (110 kg); lower running carriage provided with two vertical stainless-steel wheels with double row of ball bearings and two horizontal polyamide wheels. 
4)	Vertical wheels with Gothic arch feature to ride on top of stainless-steel guide track covers over full length of sill track. Wheels on aluminum surfaces not acceptable. 
5)	Upper guide carriage with two horizontal polyamide guiding wheels. For configurations with pairs of panels that slide left or right, additional concealed, additional vertical tilt protection hardware. 
6)	Hinges and Rollers:  Anodized aluminum with stainless steel security hinge pins and set-screws. Concealed panel alignment with a tight seal through the patented (Patent Number:  US10711510B2) TwinX mechanism reinforced between panels for a tight seal. Double ball bearing stainless-steel wheel rollers match hinge finish. 
a)	Finish:  Clear. 
b)	Finish:  Black. 
7)	Spring-Loaded Pull Handle:  For outswing units with larger panel sizes, a spring loaded-pull handle is supplied for ease of closing the system. The pull handle is located above the flat handle. When not in use, the handle lays flat against the adjacent panel and is supplied with bumpers to avoid metal to metal contact. Handles are stainless steel  with the attachment to coordinate with the hinge hardware of the system. 
a)	Pull Handle Finish:  Brushed satin stainless steel or black titanium stainless steel. 
k.	Weather Stripping and Sound Gasketing:  Manufacturer's double layer EPDM between panels and EPDM gasket, Q-Ion gasket, or brush seal between panel and frame, or brush seals with a two-layer fiberglass reinforced polyamide fin attached at both inner and outer edge of bottom of door panels with a recessed sill or on frame for sealing between panels and between panel and frame. 
l.	Fasteners:  Installation plates for connecting frame components made of stainless steel with sealing cushion to avoid thermal connectivity. 
m.	Insect Screen:  Fully retractable non-pleated screen. Ultra-strong, UV resistant fiberglass mesh housed in single cartridge riding on a single track. 
1)	Basis-of-Design Product by Manufacturer:  The Horizon by Wizard Industries, Inc. 
a)	Wizard Industries, Inc. which is located at:  4263 Phillips Ave, Burnaby, BC, Canada V5A 2X4; Toll Free:  (888) 949-3667; Telephone:  (604) 299-8878; Fax:  (604) 299-4496; Email:  sales@wizardindustries.com; Web:  https://www.wizardscreens.com.
C.	Basis of Design:  Model NW Aluminum 640 sliding-folding thermally broken, aluminum-framed glass panel system as manufactured by Nana Wall Systems, Incorporated. 2-5/8 inch (67 mm) thick, floor track supported system. Manufacturer's standard thermally broken panels and frame profiles, with head track, side jambs, sill and panels with dimensions as shown on Drawings.
1.	System Components: Aluminum framed panel, threshold, sliding-folding and locking hardware, weather stripping, bionic turtle thermal break, glass and glazing, panel catch, and accessories as required for a complete working installation.
2.	Performance Requirements:  Lab tested.
a.	Sill and Opening Type: Hybrid Sill, Inward Opening:
1)	Folding Glass Door Units tested to AAMA/WDMA/CSA 101/I.S.2/A440-17 (NAFS-17):
a)	Class CW-PG25 - FLD 157.5 x 102 inch (4000 x 2600 mm) and Class LC-PG50 - FLD 157.5 x 102 inch (4000 x 2600 mm) with 1L3R configuration.
2)	Air Infiltration per ASTM E283:
a)	Static air pressure difference of 1.57 psf (75 Pa): 0.03 cfm per sq ft (0.15 L per sec per sq m).
b)	Static air pressure difference of 6.24 psf (300 Pa): 0.07 cfm per sq ft (0.35 L per sec per sq m).
3)	Water Penetration per ASTM E331 and ASTM E547: No uncontrolled water leakage at static test pressure of 9 psf (450 Pa). Not applicable for even-even configurations.
4)	Structural Loading per ASTM E330: Wind load resistance.
a)	Design Pressure; Positive: 50 psf (2400 Pa).
b)	Design Pressure; Negative: 55 psf (2670 Pa)
c)	Uniform Load Deflection; L/175: Pass 25 psf (1190 Pa).
b.	Sill and Opening Type: Hybrid Sill, Outward Opening:
1)	Folding Glass Door Units test to AAMA/WDMA/CSA 101/I.S.2/A440-17 (NAFS-17):
a)	Class CW-PG25 - FLD 157.5 x 102 inch (4000 x 2600 mm) and Class LC-PG50 - FLD 157.5 x 102 inch (4000 x 2600 mm) with 1L3R configuration.
2)	Air Infiltration per ASTM E283:
a)	Static air pressure difference of 1.57 psf (75 Pa): 0.03 cfm per sq ft (0.15 L per sec per sq m).
b)	Static air pressure difference of 6.24 psf (300 Pa): 0.07 cfm per sq ft (0.35 L per sec per sq m).
3)	Water Penetration per ASTM E331 and ASTM E547: No uncontrolled water leakage at a static test pressure of 9 psf (450 Pa). Not applicable for even-even configurations.
4)	Structural Loading per ASTM E330: Wind load resistance.
a)	Design Pressure; Positive: 55 psf (2670 Pa).
b)	Design Pressure; Negative: 50 psf (2400 Pa).
c)	Uniform Load Deflection; L/175: Pass 25 psf (1190 Pa).
c.	Sill and Opening Type: Low Profile Saddle Sill, ADA Compliant, Inward Opening:
1)	Folding Glass Door Units test to AAMA/WDMA/CSA 101/I.S.2/A440-17 (NAFS-17):
a)	Class CW-PG25 - FLD 157.5 x 102 inch (4000 x 2600 mm) and Class LC-PG35 - FLD 157.5 x 102 inch (4000 x 2600 mm) with 1L3R configuration.
2)	Air Infiltration per ASTM E283: 
a)	Static air pressure difference of 1.57 psf (75 Pa): 0.12 cfm per sq ft (0.61 L per sec per sq m).
3)	Static air pressure difference of 6.24 psf (300 Pa): 0.30 cfm per sq ft (1.52 L per sec per sq m).Water Penetration per ASTM E331 and ASTM E547: No uncontrolled water leakage at a static, with weeps, test pressure of 5.43 psf (260 Pa). Not applicable for even-even configurations.
4)	Structural Loading per ASTM E330: Wind load resistance.
a)	Design Pressure; Positive and Negative: 50 psf (2400 Pa).
b)	Uniform Load Deflection, L/175: Pass 25 psf (1190 Pa).
d.	Sill and Opening Type:  Low Profile Saddle Sill, ADA Compliant, Outward Opening:
1)	Folding Glass Door Units test to AAMA/WDMA/CSA 101/I.S.2/A440-17 (NAFS-17):
a)	Class CW-PG25 - FLD 157.5 x 102 inch (4000 x 2600 mm) and Class LC-PG35 - FLD 157.5 x 102 inch (4000 x 2600 mm) with 1L3R configuration.
2)	Air Infiltration per ASTM E283: 
a)	Static air pressure difference of 1.57 psf (75 Pa): 0.12 cfm per sq ft (0.61 L per sec per sq m).
b)	Static air pressure difference of 6.24 psf (300 Pa): 0.28 cfm per sq ft (1.50 L per sec per sq m).
3)	Water Penetration per ASTM E331 and ASTM E547: No uncontrolled water leakage at a static, with weeps, test pressure of 5.43 psf (260 Pa). Not applicable for even-even configurations.
4)	Structural Loading per ASTM E330: Wind load resistance.
a)	Design Pressure; Positive and Negative: 50 psf (2400 Pa).
b)	Uniform Load Deflection, L/175: Pass 25 psf (1190 Pa).
e.	Sill and Opening Type: Low Profile Saddle Sill with UniverSILL Insert, Outward Opening:
1)	Folding Glass Door Units test to AAMA/WDMA/CSA 101/I.S.2/A440-17 (NAFS-17):
a)	Class CW-PG35 - FLD 157.5 x 102 inch (4000 x 2600 mm) and Class LC-PG50 - FLD 157.5 x 102 inch (4000 x 2600 mm) with 1L3R configuration.
2)	Air Infiltration per ASTM E283:
a)	Static air pressure difference of 1.57 psf (75 Pa): 0.04 cfm per sq ft (0.20 L per sec per sq m).
b)	Static air pressure difference of 6.24 psf (300 Pa): 0.07 cfm per sq ft (0.35 L per sec per sq m).
3)	Water Penetration per ASTM E331 and ASTM E547: No uncontrolled water leakage at a static test pressure of 7.5 psf (360 Pa). Not applicable for even-even configurations.
4)	Structural Loading per ASTM E330: Wind load resistance.
a)	Design Pressure; Positive and Negative: 50 psf (2400 Pa).
b)	Uniform Load Deflection, L/175: Pass 25 psf (1190 Pa).
f.	Sill and Opening Type: Flush Sill, Inward Opening:
1)	Air Infiltration per ASTM E283:
a)	Static air pressure difference of 1.57 psf (75 Pa): 0.12 cfm per sq ft (0.61 L per sec per sq m).
b)	Static air pressure difference of 6.24 psf (300 Pa): 0.30 cfm per sq ft (1.52 L per sec per sq m).
2)	Structural Loading per ASTM E330: Wind load resistance.
a)	Design Pressure; Positive and Negative: 50 psf (2400 Pa).
b)	Uniform Load Deflection, L/175: Pass 25 psf (1190 Pa).
g.	Sill and Opening Type: Flush Sill, Outward Opening:
1)	Air Infiltration per ASTM E283:
a)	Static air pressure difference of 1.57 psf (75 Pa): 0.12 cfm per sq ft (0.61 L per sec per sq m).
2)	Static air pressure difference of 6.24 psf (300 Pa): 0.28 cfm per sq ft (1.5 L per sec per sq m).Structural Loading per ASTM E330: Wind load resistance.
a)	Design Pressure; Positive and Negative: 50 psf (2400 Pa).
b)	Uniform Load Deflection, L/175: Pass 25 psf (1190 Pa).
h.	Swing Panel - Operation / Cycling Performance (AAMA 920): 500,000 cycles.
i.	System - Life Cycle Performance per DIN EN 1191/12400: Class 3; 20,000 cycles.
j.	Operating Force (ASTM E2068):
1)	Swing Panel: Open 1 lbf (2.8 N) & Close 1 lbf (3.9 N).
2)	Folding Panels:
a)	Initiate Motion: Open 4 lbf (20 N) & Close 3 lbf (15 N).
b)	Maintain Motion: Open 1 lbf (3 N) & Close 1 lbf (4 N).
k.	Forced Entry (AAMA 1304, DIN EN 1191): Pass.
l.	Forced Entry Resistance per ASTM F842, AAMA 1304, CAWM 300: Meets Grade 40; plus F2.
m.	Burglary Resistance Unit:  EN 1627-30, Class RC2/ RC2N; Resistance Class 2 certified.
n.	Thermal Performance (U-factor): NFRC 100 rated, certified, and labeled.
o.	Solar Heat Gain Coefficient plus Visible Light Transmission: NFRC 200 rated, certified, and labeled.
p.	Air Leakage: NFRC 400 rated, certified, and labeled.
q.	Condensation Resistance Factor: NFRC 500 rated, certified, and labeled.
3.	Design Criteria:
a.	Sizes and Configurations: As indicated on Drawings for selected number and size of panels, location of swing panels, and number of panels stacking to the left and to the right.
b.	Unit Operation: Adjustable sliding and folding hardware with top and bottom tracks.
c.	Panel Configuration: Straight.
d.	Panel Configuration: 90 degree angle turn.
e.	Panel Configuration: Window and door combination
f.	Stack Storage Configuration: Inswing type.
g.	Stack Storage Configuration: Outswing type.
h.	Mounting Type: Floor track supported with upper guide track.
i.	Hinged Panels:
1)	Primary Swing Panel of Paired Swing Panels Looking from Inside: On the left.
2)	Primary Swing Panel of Paired Swing Panels Looking from Inside: On the right.
3)	Entry and Egress Panel: Hinged to bi-folding panels.
4)	Entry and Egress Panel: Hinged to side jamb.
5)	Entry and Egress Panel: None.
j.	Panel Pairing Configuration: Bi-folding panels hinged to side jamb.
k.	Panel Pairing Configuration: Bi-folding panels unhinged FourFold or SixFold panel sets.
4.	Fabrication: Extruded aluminum frame and panel profiles, corner connectors, hinges, sliding and folding hardware, locking hardware, handles, glass and glazing, and weather stripping.
a.	Factory pre-assembled. Ship with system components and installation instructions.
b.	Exposed work matched to produce continuity of line and design with joints.
c.	No raw edges visible at joints.
5.	Materials:
a.	Panels: Single lite; standard.
b.	Panels: Multiple lites with horizontal mullions at heights indicated on Drawings from bottom of panel.
c.	Panels: Single lite with simulated divided lites in pattern as shown on Drawings.
d.	Panel Size (W x H): ___ x ___ inches (___ x ___ mm).
e.	Rail Depth: 2-5/8 inch (67 mm).
f.	Top Rail Width: 2-5/8 inch (66 mm).
g.	Typical Stile Width: 1-3/4 inch (45 mm) on both stiles for a nominal frame stile width of 3-7/8 inch (99 mm) between folding panels.
h.	Bottom Rail Width: 2-5/8 inch (66 mm).
i.	Bottom Rail Width: Manufacturer's standard kick-plate of 10 inches (254 mm).
6.	Frame:
a.	Thermally broken top track and side jambs to hide anchoring connections.
b.	For long-term tight, consistent sealing, provide a lateral patented (Patent Number: US10683688B2) adjustment feature at the side jambs capable of adjustment of plus or minus 3/16 inch (5 mm). 
c.	Frame Finish: To match panel finish.
d.	Frame Depth: Top Track and Side Jamb Depth; 2-15/16 inch (74 mm).
7.	Head Track Width: 2-13/16 inch (72 mm) standard.
8.	Head Track Width: 3-7/8 inch (99 mm) with anti-tilt feature for unhinged FourFold or SixFold panel set configurations.
9.	Side Jamb Width: 2 inch (51 mm) wide. Adjustment: Plus or minus 3/16 inch (5 mm).
10.	Sill Type: Hybrid sill, thermally broken, with high heel protector insert. Extruded Aluminum.
11.	Sill Type: Low profile saddle sill, ADA compliant, thermally broken, with high heel protector insert. Extruded Aluminum.
12.	Sill Type: Low profile saddle sill with UniverSILL, thermally broken, with high heel protector insert. Extruded Aluminum.
13.	Sill Type: Flush sill, ADA compliant, thermally broken, with high heel protector insert. Extruded Aluminum.
14.	Sill Finish: Aluminum with clear anodized finish.
15.	Sill Finish: Aluminum with black anodized finish.
16.	Aluminum Extrusion:  AlMgSi0.5 alloy, 6063-T5 (F-22 - European Standard).
a.	Thickness:  0.078 inch (2.0 mm) nominal. 
b.	Thermal Break:  1-15/16 inches (49 mm) wide specially designed and patented (Patent Number:  US10550625B2) glass fiber reinforced (GFR) polyamide �Bionic Turtle� for panels. Standard thermal break elsewhere. 
c.	Finish:  One color inside and outside. 
1)	Finish Type:  Anodized per AAMA 611. Clear 
2)	Finish Type:  Anodized per AAMA 611. Dark bronze. 
3)	Finish Type:  Powder coat per AAMA 2604 
a)	Color:  Chosen from standard selection of 50 colors. Matte. 
b)	Color:  Chosen from full RAL selection. High glass. 
c)	Color:  Chosen from full RAL selection. Matte. 
4)	Finish Type:  Custom finish. 
d.	Finish:  Different color inside and outside. 
1)	Interior:  Powder coat per AAMA 2604. 
a)	Color:  Chosen from standard selection of 50 colors. Matte. 
b)	Color:  Chosen from full RAL selection. High gloss. 
c)	Color:  Chosen from full RAL selection. Matte. 
2)	Exterior:  Powder coat per AAMA 2604.  
a)	Color:  Chosen from standard selection of 50 colors. Matte. 
b)	Color:  Chosen from full RAL selection. High gloss. 
c)	Color:  Chosen from full RAL selection. Matte. 
17.	Glass and Glazing: Safety Glazing per ASTM C1036, ASTM C1048, ANSI Z97.1 and CPSC 16 CFR 1201.
a.	Glazing Units, Double Insulated: Dry glazed with glass stops on the inside.
1)	Double IGU:  15/16 inch (24 mm), clear insulated tempered.
2)	Triple IGU:  1-3/8 inch (35 mm), Low E Insulated Tempered 176 #2 & #5. 
3)	Triple IGU:  1-3/8 inch (35 mm), Low E Insulated Tempered PL #2 & #5.
18.	Insulated Glazing Unit Fill: Air.
19.	Insulated Glazing Unit Fill: Argon.
20.	Glass Lite Type:  Reduced iron.
21.	Glass Spacers: Gray finish with capillary tube.
22.	Glass Spacers: Black finish with capillary tubes.
23.	Glass Spacers: Gray finish without capillary tubes.
24.	Glass Spacers: Black finish without capillary tubes.
25.	Alarmed Glazing: Connection wiring to alarm system, position monitoring, locking detection and notification systems such as glass-breakage sensors by others.
26.	Locking Hardware and Handle for Sliding-Folding Systems: 
a.	Main Entry Panels:  Lockset with lockable latch, multi-point locking with deadbolt and rods at top and bottom on primary panels only. 
1)	Application:  Single swing panel. 
2)	Application:  Pair of swing panels. 
3)	Operation:  After turn of key or thumb turn, depression of handles withdraws latch. Lifting of handles engages rods and turn of key or thumb turn engages deadbolt and operates lock. 
4)	Rods:  Concealed, not edge mounted. 
5)	Lever Handles:  Lever handles on inside and outside. 
6)	Lever Handle Finish:  Brushed satin stainless steel; standard. 
7)	Lever Handle Finish:  Black titanium stainless steel; standard. 
8)	Lever Handle Finish:  Copper-nickel stainless steel antiviral and antimicrobial. 
9)	Locking:  Standard profile cylinder. 
10)	Locking:  Adapter for Small Format Interchangeable Core. 
11)	Secondary Swing Panel:  Concealed two-point, edge locking. 
b.	Main Entry Panels:  Lockset with lockable latch, single point locking with a deadbolt on primary panel only.  
1)	Application:  Single swing panel. 
2)	Application:  Pair of swing panels. 
3)	Locking:  5 pin US rim cylinder. 
4)	Locking:  US mortise cylinder accommodating 5 - 7 pin, SFIC, FSIC or LFIC cores. 
5)	Lever Handles:  Accurate 18L on inside and outside. 
6)	Lever Handles:  Accurate 20L with return on inside and outside 
7)	Secondary Swing Panel:  Concealed two-point, edge locking. 
c.	Main Entry Panels:  Flat handle on inside only with concealed two-point locking hardware operated by 180 degrees turn of handle; the main entry panel is operable from inside only and there is no latch. 
d.	Main Entry Panels:  No hardware or locking provided by manufacturer; Field installed panic device from Section 08 71 00 prepped for commercial application. 
1)	Application:  Pair of swing panels. 
2)	Panic Hardware:  Von Duprin 33/35A Series Narrow Stile Rim Exit Devices. 
3)	Panic Hardware:  DORMA 9700 Series Narrow Stile Rim Exit Devices. 
e.	Pairs of Folding Panels:  Handles and concealed two-point locking hardware operated by 180 degrees turn of handle between each pair. Face applied flush bolt locking NOT acceptable. 
1)	Handles:  Manufacturer�s flat handles. 
a)	Flat Handle Finish:  Brushed satin stainless steel. 
b)	Flat Handle Finish:  Black titanium stainless steel. 
c)	Flat Handle Finish:  Copper-nickel stainless steel antiviral and antimicrobial. 
f.	Handle Height:  41-3/8 inch (105 cm) centered from bottom of panel unless otherwise indicated on Drawings.
g.	Locking Rods:  End caps top and bottom:  Rod Stroke:  15/16 inch (24 mm). 
h.	Additional Profile Cylinders:  Keyed alike. 
i.	Additional Profile Cylinders:  Keyed differently. 
j.	Panel catch:  Panel catch to hold swing panel to adjacent folding panel to prevent incorrect operation when moving the panel. 
k.	Sliding-Folding Hardware:  Combination with top and bottom tracks and threshold. 
1)	Running carriages to have sealed, self-lubricating, double ball bearing multi-rollers. 
2)	Surface mounted hinges and running carriages not acceptable. 
3)	Lower Running Carriage Carrying Capacity:  240 lb. (110 kg); lower running carriage provided with two vertical stainless-steel wheels with double row of ball bearings and two horizontal polyamide wheels. 
4)	Vertical wheels with Gothic arch feature to ride on top of stainless-steel guide track covers over full length of sill track. Wheels on aluminum surfaces not acceptable. 
5)	Upper guide carriage with two horizontal polyamide guiding wheels. For configurations with pairs of panels that slide left or right, additional concealed, additional vertical tilt protection hardware. 
6)	Hinges and Rollers:  Anodized aluminum with stainless steel security hinge pins and set-screws. Concealed panel alignment with a tight seal through the patented (Patent Number:  US10711510B2) TwinX mechanism reinforced between panels for a tight seal. Double ball bearing stainless-steel wheel rollers match hinge finish. 
a)	Finish:  Clear. 
b)	Finish:  Black. 
7)	Spring-Loaded Pull Handle:  For outswing units with larger panel sizes, a spring loaded-pull handle is supplied for ease of closing the system. The pull handle is located above the flat handle. When not in use, the handle lays flat against the adjacent panel and is supplied with bumpers to avoid metal to metal contact. Handles are stainless steel  with the attachment to coordinate with the hinge hardware of the system. 
a)	Pull Handle Finish:  Brushed satin stainless steel or black titanium stainless steel. 
l.	Weather Stripping and Sound Gasketing:  Manufacturer�s double layer EPDM between panels and EPDM gasket, Q-Ion gasket, or brush seal between panel and frame, or brush seals with a two-layer fiberglass reinforced polyamide fin attached at both inner and outer edge of bottom of door panels with a recessed sill or on frame for sealing between panels and between panel and frame. 
m.	Fasteners:  Installation plates for connecting frame components made of stainless steel with sealing cushion to avoid thermal connectivity. 
n.	Insect Screen:  Fully retractable non-pleated screen. Ultra-strong, UV resistant fiberglass mesh housed in single cartridge riding on a single track. 
1)	Basis-of-Design Product by Manufacturer:  The Horizon by Wizard Industries, Inc. 
a)	Wizard Industries, Inc. which is located at:  4263 Phillips Ave, Burnaby, BC, Canada V5A 2X4; Toll Free:  (888) 949-3667; Telephone:  (604) 299-8878; Fax:  (604) 299-4496; Email:  sales@wizardindustries.com; Web:  https://www.wizardscreens.com.
D.	Basis of Design: Model NW Acoustical 645 sliding-folding thermally broken, acoustically rated, aluminum-framed glass panel system as manufactured by Nana Wall Systems, Incorporated. Nominal frame stile width of 3-7/8 inch (99 mm), floor track supported system. Manufacturer's standard thermally broken panels and frame profiles, with head track, side jambs, sill and panels with dimensions as shown on Drawings.
1.	System Components: Aluminum framed panel, threshold, sliding-folding and locking hardware, sound gasketing, bionic turtle thermal break, panel catch, glass and glazing and accessories as required for a complete working installation.
2.	Performance  Requirements:	Lab tested. 
a.	Sill and Opening Type:  Minimal Surface Mounted Flush Sill and Flush Sill - Inward Opening. 
1)	Air Infiltration per ASTM E283:   
a)	Static air pressure difference of 1.57 psf (75 Pa):  0.12 cfm per sq ft (0.61 L per sec per sq m). 
b)	Static air pressure difference of 6.24 psf (300 Pa):  0.30 cfm per sq ft (1.52 L per sec per sq m). 
c)	Canadian Air Infiltration/ Exfiltration Level:  A2. 
b.	Sill and Opening Type:  Minimal Surface Mounted Flush Sill and Flush Sill - Outward Opening. 
1)	Air Infiltration per ASTM E283: 
a)	Static air pressure difference of 1.57 psf (75 Pa):  0.12 cfm per sq ft (0.61 L per sec per sq m). 
b)	Static air pressure difference of 6.24 psf (300 Pa):  0.28 cfm per sq ft (1.50 L per sec per sq m). 
c)	Canadian Air Infiltration/ Exfiltration Level:  A2. 
3.	Sizes and Configurations: As indicated on Drawings for selected number and size of panels, location of swing panels, and number of panels stacking to the left and to the right.
4.	Unit Operation: Adjustable sliding and folding hardware with top and bottom tracks.
5.	Panel Configuration: Straight.
6.	Stack Storage Configuration: Inswing type and stack storage inside jamb.
7.	Stack Storage Configuration: Outswing type and stack storage outside jamb.
8.	Mounting Type: Floor track supported with upper guide track.
9.	Panel Pairing Configuration: Bi-folding panels hinged to side jamb.
10.	Panel Pairing Configuration: Bi-folding panels unhinged FourFold or SixFold panel sets.
11.	Fabrication: Extruded aluminum frame and panel profiles, corner connectors, hinges, sliding and folding hardware, locking hardware, handles, glass and glazing, and sound gasketing.
a.	Each unit factory pre-assembled and shipped with complete system components and installation instructions.
b.	Exposed work to be carefully matched to produce continuity of line and design with all joints.
c.	No raw edges visible at joints.
12.	Materials:
a.	Panels: Single lite; standard.
b.	Panels: Multiple lites with horizontal mullions at heights indicated from bottom of the panel.
c.	Panels: Single lite with simulated divided lites in pattern as shown on Drawings.
d.	Panel Size (W x H): ___ x ___ inches (___ x ___ mm).
e.	Rail Depth: 2-5/8 inch (67 mm).
f.	Top Rail and Stile Width: 2-7/8 inch (73 mm).
g.	Bottom Rail Width: 2-5/8 inch (66 mm).
h.	Bottom Rail Width: Manufacturer's standard kick-plate of 10 inches (254 mm).
13.	Frame:
a.	Thermally broken top track and side jambs with multipurpose frame insert to hide anchoring connections.
b.	Thermally broken top track and side jambs without multipurpose frame insert to hide anchoring connections.
c.	For long-term tight, consistent sealing, provide a lateral patented (Patent Number: US10683688B2) adjustment feature at the side jambs capable of adjustment of plus or minus 3/16 inch (5 mm). 
d.	Frame Finish: To match panel finish.
e.	Frame Depth: Top Track and Side Jamb Depth; 2-15/16 inch (74 mm).
14.	Head Track Width: 2-13/16 inch (72 mm) standard.
15.	Head Track Width: 3-7/8 inch (99 mm) with anti-tilt feature for unhinged FourFold or SixFold panel set configurations.
16.	Side Jamb Width: 2 inch (51 mm) wide. Adjustment: Plus or minus 3/16 inch (5 mm).
17.	Sill Type: Minimal surface mounted flush sill - ADA compliant.
18.	Sill Type: Flush sill - ADA compliant with high heel protector insert.
19.	Sill Finish: Aluminum with clear anodized finish.
20.	Sill Finish: Aluminum with black anodized finish.
21.	Aluminum Extrusion:  AlMgSi0.5 alloy, 6063-T5; F-22 - European standard. 
a.	Thickness:  0.078 inch (2.0 mm) nominal. 
b.	Acoustical Break:  1-1/4 inches (32 mm) wide specially designed and patented (Patent Number:  US10550625B2) glass fiber reinforced (GFR) polyamide �Bionic Turtle� for panels. 
c.	Finish; One color inside and outside. 
1)	Finish Type:  Anodized per AAMA 611. Clear. 
2)	Finish Type:  Anodized per AAMA 611. Dark bronze. 
3)	Finish Type:  Powder coat per AAMA 2604. 
a)	Color:  Chosen from standard selection of 50 colors. Matte. 
b)	Color:  Chosen from full RAL selection. High gloss 
c)	Color:  Chosen from full RAL selection. Matte. 
d.	Finish:  Different color inside and outside. 
1)	Interior:  Powder coat per AAMA 2604. 
a)	Color:  Chosen from standard selection of 50 colors. Matte. 
b)	Color:  Chosen from full RAL selection. High gloss 
c)	Color:  Chosen from full RAL selection. Matte. 
2)	Exterior:  Powder coat per AAMA 2604. 
a)	Color:  Chosen from standard selection of 50 colors. Matte. 
b)	Color:  Chosen from full RAL selection. High gloss. 
c)	Color:  Chosen from full RAL selection. Matte. 
22.	Glass and Glazing: Safety Glazing per ASTM C1036, ASTM C1048, ANSI Z97.1 and CPSC 16 CFR 1201.
a.	Glazing Units, Double Insulated: Dry glazed with glass stops on the inside.
23.	Insulated Glass Unit (IGU): 1-9/16 inch (40 mm), 10 mm + 8 mm STC 48 enhanced laminated glass to achieve unit STC of 45 with head track recessed.
24.	Insulated Glass Unit (IGU): 1-9/16 inch (40 mm), 10 mm + 8 mm STC 48 enhanced laminated glass to achieve unit STC of 44.
25.	Insulated Glass Unit (IGU): 1-5/8 inch (42 mm), 8 mm + 8 mm STC 47 enhanced laminated glass to achieve unit STC of 44 with head track recessed.
26.	Insulated Glass Unit (IGU): 1-5/8 inch (42 mm), 8 mm + 8 mm STC 47 enhanced laminated glass to achieve unit STC of 43.
27.	Insulated Glass Unit (IGU): 1-7/16 inch (36 mm), 6 mm + 6 mm STC 42 enhanced laminated glass to achieve unit STC of 45.
28.	Insulated Glass Unit (IGU): 1-7/16 inch (36 mm), 6 mm + 6 mm STC 40 laminated glass to achieve unit STC of 42.
29.	Single Glass:  1/2 inch (12 mm) STC 39 enhanced laminated glass to achieve unit STC of 38. 
30.	Single Glass:  3/8 inch (10 mm) STC 38 enhanced laminated glass to achieve unit STC of 37. 
31.	Single Glass: 1/4 inch (6 mm) STC 36 enhanced laminated glass to achieve unit STC of 36.
32.	Single Glass: 1/4 inch (6 mm) STC 35 laminated glass to achieve unit STC of 35.
33.	Single Glass: 1/4 inch (6 mm) STC 31 tempered glass to achieve unit STC of 32.
34.	Insulated Glazing Unit Fill: Air.
35.	Glass Type:  Reduced iron.
36.	Glass Spacers: Gray finish with capillary tube.
37.	Glass Spacers: Black finish with capillary tubes.
38.	Glass Spacers: Gray finish without capillary tubes.
39.	Glass Spacers: Black finish without capillary tubes.
40.	Locking Hardware and Handle for Sliding-Folding Systems: 
a.	Main Entry Panels:  Lockset with lockable latch, multi-point locking with deadbolt and rods at top and bottom on primary panels only. 
1)	Application:  Single swing panel. 
2)	Application:  Pair of swing panels. 
3)	Operation:  After turn of key or thumb turn, depression of handles withdraws latch. Lifting of handles engages rods and turn of key or thumb turn engages deadbolt and operates lock. 
4)	Rods:  Concealed, not edge mounted. 
5)	Lever Handles:  Lever handles on inside and outside. 
6)	Lever Handle Finish:  Brushed satin stainless steel; standard. 
7)	Lever Handle Finish:  Black titanium stainless steel; standard. 
8)	Lever Handle Finish:  Copper-nickel stainless steel antiviral and antimicrobial. 
9)	Locking:  Standard profile cylinder. 
10)	Locking:  Adapter for Small Format Interchangeable Core. 
11)	Secondary Swing Panel:  Concealed two-point, edge locking. 
b.	Main Entry Panels:  Prepped for commercial applications with a single motion locking operated by lever handles with locking with a US mortise cylinder that can accommodate 5 -7 pin, SFIC, FSIC or LFIC cores. 
1)	Locking: Accurate 18L lever handle 
2)	Locking: Accurate 20L lever handle with return 
3)	Locking:  Yale 8808-2 Series with Mortise Lock 
4)	Locking:  L/LV9000 Series from Schlage with Mortise Lock 
5)	Locking:  Schlage ND Series Mechanical Lock 
6)	Secondary Swing Panel: Provide concealed two-point, edge locking. 
c.	Main Entry Panels:  Flat handle on inside only with concealed two-point locking hardware operated by 180 degrees turn of handle; the main entry panel is operable from inside only and there is no latch. 
d.	Main Entry Panels:  No hardware or locking provided by manufacturer; Field installed panic device from Section 08 71 00 prepped for commercial application.
1)	Application:  Single swing panel 
2)	Panic Hardware:  Von Duprin 33/35A Series Narrow Stile Rim Exit Devices. 
3)	Panic Hardware:  DORMA 9700 Series Narrow Stile Rim Exit Devices. 
e.	Pairs of Folding Panels:  Handles and concealed two-point locking hardware operated by 180 degrees turn of handle between each pair. Face applied flush bolt locking NOT acceptable. 
1)	Handles:  Manufacturer�s flat handles. 
a)	Flat Handle Finish:  Brushed satin stainless steel. 
b)	Flat Handle Finish:  Black titanium stainless steel. 
c)	Flat Handle Finish:  Copper-nickel stainless steel antiviral and antimicrobial. 
f.	Handle Height:  41-3/8 inch (105 cm) centered from bottom of panel unless otherwise indicated on Drawings. 
g.	Locking Rods:  End caps top and bottom:  Rod Stroke:  15/16 inch (24 mm). 
h.	Additional Profile Cylinders:  Keyed alike. 
i.	Additional Profile Cylinders:  Keyed differently. 
j.	Panel catch:  Panel catch to hold swing panel to adjacent folding panel to prevent incorrect operation when moving the panel. 
k.	Sliding-Folding Hardware:  Combination with top and bottom tracks and threshold. 
1)	Running carriages to have sealed, self-lubricating, double ball bearing multi-rollers. 
2)	Surface mounted hinges and running carriages not acceptable. 
3)	Lower Running Carriage Carrying Capacity:  240 lb. (110 kg); lower running carriage provided with two vertical stainless-steel wheels with double row of ball bearings and two horizontal polyamide wheels. 
4)	Vertical wheels with Gothic arch feature to ride on top of stainless-steel guide track covers over full length of sill track. Wheels on aluminum surfaces not acceptable. 
5)	Upper guide carriage with two horizontal polyamide guiding wheels. For configurations with pairs of panels that slide left or right, additional concealed, additional vertical tilt protection hardware. 
6)	Hinges and Rollers:  Anodized aluminum with stainless steel security hinge pins and set-screws. Concealed panel alignment with a tight seal through the patented (Patent Number:  US10711510B2) TwinX mechanism reinforced between panels for a tight seal. Double ball bearing stainless-steel wheel rollers match hinge finish. 
a)	Finish:  Clear. 
b)	Finish:  Black. 
7)	Spring-Loaded Pull Handle:  For outswing units with larger panel sizes, a spring loaded-pull handle is supplied for ease of closing the system. The pull handle is located above the flat handle. When not in use, the handle lays flat against the adjacent panel and is supplied with bumpers to avoid metal to metal contact. Handles are stainless steel  with the attachment to coordinate with the hinge hardware of the system. 
a)	Pull Handle Finish:  Brushed satin stainless steel or black titanium stainless steel. 
l.	Weather Stripping and Sound Gasketing:  Manufacturer�s double layer EPDM between panels and EPDM gasket, Q-Ion gasket, or brush seal between panel and frame, or brush seals with a two-layer fiberglass reinforced polyamide fin attached at both inner and outer edge of bottom of door panels with a recessed sill or on frame for sealing between panels and between panel and frame. 
m.	Fasteners:  Installation plates for connecting frame components made of stainless steel with sealing cushion to avoid thermal connectivity. 
n.	Insect Screen:  Fully retractable non-pleated screen. Ultra-strong, UV resistant fiberglass mesh housed in single cartridge riding on a single track. 
1)	Basis-of-Design Product by Manufacturer:  The Horizon by Wizard Industries, Inc. 
a)	Wizard Industries, Inc. which is located at:  4263 Phillips Ave, Burnaby, BC, Canada V5A 2X4; Toll Free:  (888) 949-3667; Telephone:  (604) 299-8878; Fax:  (604) 299-4496; Email:  sales@wizardindustries.com; Web:  https://www.wizardscreens.com.
E.	Basis of Design: Model NW Clad 740 sliding-folding, aluminum-clad wood framed glass panel system as manufactured by NanaWall Systems, Incorporated. Manufacturer's standard aluminum clad solid quad laminated wood panel profiles and interior wood clad thermally broken aluminum frame with head and floor track, side jambs with dimensions as shown on Drawings. 3-3/8 inch (86 mm) thick, floor track supported system.
1.	System Components: Interior wood clad aluminum frame and running astragals, threshold, exterior aluminum clad wood panels, sliding-folding and locking hardware, weather stripping, glass and glazing, panel catch, and accessories as required for a complete working installation.
2.	Performance Requirements: 
a.	Sill and Opening Type: Hybrid Sill, Inward Opening:
1)	Folding Glass Door Units tested to AAMA/WDMA/CSA 101/I.S.2/A440-17 (NAFS-17):
a)	Class CW-PG35 - FLD 157.5 x 102 inch (4000 x 2600 mm) with 1L3R configuration.
2)	Air Infiltration per ASTM E283:
a)	Static air pressure difference of 1.57 psf (75 Pa): 0.06 cfm per sq ft (0.3 L per sec per sq m).
b)	Static air pressure difference of 6.24 psf (300 Pa): 0.14 cfm per sq ft (0.7 L per sec per sq m).
3)	Water Penetration per ASTM E331 and ASTM E547: No uncontrolled water leakage at static test pressure of 9 psf (450 Pa). Not applicable for even-even configurations.
4)	Structural Loading per ASTM E330: Wind load resistance.
a)	Design Pressure; Positive: 39 psf (1850 Pa).
b)	Design Pressure; Negative: 55 psf (2670 Pa).
c)	Uniform Load Deflection; L/175: Pass 42 psf (2000 Pa).
b.	Sill and Opening Type: Hybrid Sill, Outward Opening:
1)	Folding Glass Door Units test to AAMA/WDMA/CSA 101/I.S.2/A440-17 (NAFS-17):
a)	Class CW-PG35 - FLD 157.5 x 102 inch (4000 x 2600 mm) with 1L3R configuration.
2)	Air Infiltration per ASTM E283:
a)	Static air pressure difference of 1.57 psf (75 Pa): 0.06 cfm per sq ft (0.3 L per sec per sq m).
b)	Static air pressure difference of 6.24 psf (300 Pa): 0.14 cfm per sq ft (0.7 L per sec per sq m).
3)	Water Penetration per ASTM E331 and ASTM E547: No uncontrolled water leakage at a static test pressure of 9 psf (450 Pa). Not applicable for even-even configurations.
4)	Structural Loading per ASTM E330: Wind load resistance.
a)	Design Pressure; Positive: 55 psf (2670 Pa).
b)	Design Pressure; Negative:39 psf (1850 Pa).
c)	Uniform Load Deflection; L/175: Pass 45 psf (2150 Pa).
c.	Sill and Opening Type: Low Profile Saddle Sill, ADA Compliant, Inward Opening:
1)	Folding Glass Door Units test to AAMA/WDMA/CSA 101/I.S.2/A440-17 (NAFS-17):
a)	Class CW-PG35 - FLD 157.5 x 102 inch (4000 x 2600 mm) with 1L3R configuration.
2)	Air Infiltration per ASTM E283: 
a)	Static air pressure difference of 1.57 psf (75 Pa): 0.12 cfm per sq ft (0.61 L per sec per sq m).
b)	Static air pressure difference of 6.24 psf (300 Pa): 0.29 cfm per sq ft (1.50 L per sec per sq m).
3)	Water Penetration per ASTM E331 and ASTM E547: No uncontrolled water leakage at a static, with weeps, test pressure of 5.43 psf (260 Pa). Not applicable for even-even configurations.
4)	Structural Loading per ASTM E330: Wind load resistance.
a)	Design Pressure; Positive: 40 psf (1945 Pa).
b)	Design Pressure; Negative: 45 psf (2150 Pa).
c)	Uniform Load Deflection, L/175: Pass 45 psf (2150 Pa).
d.	Sill and Opening Type: Low Profile Saddle Sill, ADA Compliant, Outward Opening:
1)	Folding Glass Door Units test to AAMA/WDMA/CSA 101/I.S.2/A440-17 (NAFS-17):
a)	Class CW-PG35 - FLD 157.5 x 102 inch (4000 x 2600 mm) with 1L3R configuration.
2)	Air Infiltration per ASTM E283:
a)	Static air pressure difference of 1.57 psf (75 Pa): 0.12 cfm per sq ft (0.61 L per sec per sq m).
b)	Static air pressure difference of 6.24 psf (300 Pa): 0.30 cfm per sq ft (1.52 L per sec per sq m).
3)	Water Penetration per ASTM E331 and ASTM E547: No uncontrolled water leakage at a static, with weeps, test pressure of 5.43 psf (260 Pa). Not applicable for even-even configurations.
4)	Structural Loading per ASTM E330: Wind load resistance.
a)	Design Pressure; Positive: 45 psf (2150 Pa).
b)	Design Pressure; Negative: 40 psf (1945 Pa).
c)	Uniform Load Deflection, L/175: Pass 45 psf (2150 Pa).
e.	Sill and Opening Type: Low Profile Saddle Sill with UniverSILL Insert, Outward Opening:
1)	Folding Glass Door Units test to AAMA/WDMA/CSA 101/I.S.2/A440-17 (NAFS-17):
a)	Class CW-PG40 - FLD 157.5 x 102 inch (4000 x 2600 mm) with 1L3R configuration.
2)	Air Infiltration per ASTM E283:
a)	Static air pressure difference of 1.57 psf (75 Pa): 0.04 cfm per sq ft (0.20 L per sec per sq m).
b)	Static air pressure difference of 6.24 psf (300 Pa): 0.07 cfm per sq ft (0.36 L per sec per sq m).
3)	Water Penetration per ASTM E331 and ASTM E547: No uncontrolled water leakage at a static test pressure of 7.5 psf (360 Pa). Not applicable for even-even configurations.
4)	Structural Loading per ASTM E330: Wind load resistance.
a)	Design Pressure; Positive: 45 psf (2150 Pa).
b)	Design Pressure; Negative: 40 psf (1945 Pa).
c)	Uniform Load Deflection, L/175: Pass 45 psf (2150 Pa).
f.	Sill and Opening Type: Flush Sill, Inward Opening:
1)	Structural Loading per ASTM E330: Wind load resistance.
a)	Design Pressure; Positive: 40 psf (1945 Pa).
b)	Design Pressure; Negative: 45 psf (2150 Pa).
c)	Uniform Load Deflection, L/175: Pass 45 psf (2150 Pa).
2)	Air Infiltration per ASTM E283:
a)	Static air pressure difference of 1.57 psf (75 Pa): 0.12 cfm per sq ft (0.61 L per sec per sq m).
b)	Static air pressure difference of 6.24 psf (300 Pa): 0.29 cfm per sq ft (1.50 L per sec per sq m).
g.	Sill and Opening Type: Flush Sill, Outward Opening:
1)	Structural Loading per ASTM E330: Wind load resistance.
a)	Design Pressure; Positive: 45 psf (2150 Pa).
b)	Design Pressure; Negative: 40 psf (1945 Pa).
c)	Uniform Load Deflection, L/175: Pass 45 psf (2150 Pa).
2)	Air Infiltration per ASTM E283:
a)	Static air pressure difference of 1.57 psf (75 Pa): 0.12 cfm per sq ft (0.61 L per sec per sq m).
b)	Static air pressure difference of 6.24 psf (300 Pa): 0.30 cfm per sq ft (1.52 L per sec per sq m).
h.	Swing Panel - Operation / Cycling Performance (AAMA 920): 500,000 cycles.
i.	System - Life Cycle Performance (DIN EN 1191/12400): Pass; 20,000 cycles.
j.	Operating Force (ASTM E2068):
1)	Swing Panel: Open 1 lbf (2.8 N) & Close 1 lbf (3.9 N).
2)	Folding Panel:
a)	Initiate Motion - Open 4 lbf (20 N) & Close 3 lbf (15 N).
b)	Maintain Motion - Open 1 lbf (3 N) & Close 1 lbf (4 N).
k.	Forced Entry (AAMA 1304): Meets 300 lb. (1330 N) point load requirement.
l.	Burglary Resistance Unit:  EN 1627-30, Class RC2/ RC2N; Resistance Class 2 certified.
m.	Thermal Performance (U-factor): NFRC 100 rated, certified, and labeled.
n.	Solar Heat Gain Coefficient plus Visible Light Transmission: NFRC 200 rated, certified, and labeled.
o.	Air Leakage: NFRC 400 rated, certified, and labeled.
p.	Condensation Resistance Factor: NFRC 500 rated, certified, and labeled.
3.	Design Criteria:
a.	Sizes and Configurations: As indicated on Drawings for selected number and size of panels, location of swing panels, and number of panels stacking to the left and to the right.
b.	Unit Operation: Adjustable sliding and folding hardware with top and bottom tracks.
c.	Panel Configuration: Straight.
d.	Panel Configuration: 90 degree angle turn.
e.	Panel Configuration: Window and door combination.
f.	Stack Storage Configuration: Inswing type.
g.	Stack Storage Configuration: Outswing type.
h.	Mounting Type: Floor track supported with upper guide track.
i.	Hinged Panels:
1)	Primary Swing Panel of Paired Swing Panels Looking from Inside: On the left.
2)	Primary Swing Panel of Paired Swing Panels Looking from Inside: On the right.
3)	Entry and Egress Panel: Hinged to bi-folding panels.
4)	Entry and Egress Panel: Hinged to side jamb.
5)	Entry and Egress Panel: None.
j.	Panel Pairing Configuration: Bi-folding panels hinged to side jamb.
k.	Panel Pairing Configuration: Bi-folding panels unhinged FourFold or SixFold panel sets.
4.	Fabrication: Thermally broken aluminum frame and running astragals with wood cladding, quad-layer, cross grained, solid wood for panels with aluminum cladding, connecting to hinges, sliding, and folding hardware, locking hardware and handles, glass and glazing, threshold and track and weather stripping.
a.	Factory pre-assembled. Ship with system components and installation instructions.
b.	Exposed work matched to produce continuity of line and design with all joints.
c.	No raw edges visible at joints.
d.	Wood frame and panel components to be sealed with a clear sand sealer or primer plus one additional coat.
5.	Materials:
a.	Panels: Single lite; standard.
b.	Panels: Multiple lites with horizontal mullions at heights indicated on Drawings from bottom of panel.
c.	Panels: Single lite with simulated divided lites in pattern as shown on Drawings.
d.	Panel Size (W x H): ___ x ___ inches (___ x ___ mm).
e.	Rail Depth: 3-3/8 inch (86 mm).
f.	Top Rail Width: 2-23/32 inch (69 mm).
g.	Typical Stile Width: 2-11/16 inch (68 mm) on both stiles for a nominal frame stile width of 5-5/8 inch (143 mm) between folding panels.
h.	Bottom Rail Width: 2-23/32 inch (69 mm).
i.	Bottom Rail Width: Manufacturer's standard kick-plate of 10 inches (254 mm).
6.	Frame:
a.	Thermally broken top track and side jambs to hide anchoring connections.
b.	For long-term tight, consistent sealing, provide a lateral patented (Patent Number: US10683688B2) adjustment feature at the side jambs capable of adjustment of plus or minus 3/16 inch (5 mm). 
c.	Frame Finish: Black anodized aluminum inside of top track and side jambs.
d.	Frame Depth: Top Track and Side Jamb Depth; 3 inch (76 mm).
7.	Head Track Width: 2-13/16 inch (72 mm) standard.
8.	Head Track Width: 3-7/8 inch (99 mm) with anti-tilt feature for unhinged FourFold or SixFold panel set configurations.
9.	Side Jamb Width: 2-13/16 inch (72 mm) wide. Adjustment: Plus or minus 3/16 inch (5 mm).
10.	Wood Species: FSC Sapeli Mahogany.
11.	Wood Species: European Pine.
12.	Wood Species: Spruce.
13.	Wood Species: Western Hemlock.
14.	Wood Species: Meranti.
15.	Wood Finish: Provide factory water-based, open pore clear base coat applied for paint with one additional clear coat; See Section 09 90 00
16.	Wood Finish: Provide factory water-based, open pore clear sanding sealer for stain with one additional clear coat; See Section 09 90 00.
17.	Aluminum Cladding and Frame Extrusion: AlMgSi0.5 alloy, 6063-T5 (F-22 - European standard).
a.	Thickness: 0.078 inch (2.0 mm) nominal.
b.	Alloy: AlMgSi0.5; 6063-T5 (F-22 - European standard).
18.	Panel Cladding Aluminum Finish:
a.	Finish: One color inside and outside.
1)	Finish Type: Anodized per AAMA 611. Clear.
2)	Finish Type: Anodized per AAMA 611. Dark bronze.
3)	Finish Type: Powder coat per AAMA 2604.
a)	Color: Chosen from standard selection of 50 colors. Matte.
b)	Color: Chosen from full RAL selection. High gloss.
c)	Color: Chosen from full RAL selection. Matte.
4)	Finish Type: Custom finish.
b.	Finish: Different color inside and outside.
1)	Interior: Powder coat per AAMA 2604.
a)	Color: Chosen from standard selection of 50 colors. Matte.
b)	Color: Chosen from full RAL selection. High gloss.
c)	Color: Chosen from full RAL selection. Matte.
2)	Interior: Custom finish.
3)	Exterior: Powder coat per AAMA 2604.
a)	Color: Chosen from standard selection of 50 colors. Matte.
b)	Color: Chosen from full RAL selection. High gloss.
c)	Color: Chosen from full RAL selection. Matte.
4)	Exterior:  Custom finish. 
19.	Sill Type: Hybrid sill, thermally broken, with high heel protector insert.
20.	Sill Type: Low profile saddle sill, ADA compliant, thermally broken, with high heel protector insert.
21.	Sill Type: Low profile saddle sill with UniverSILL, thermally broken, with high heel protector insert.
22.	Sill Type: Flush sill, ADA compliant, thermally broken, with high heel protector insert.
23.	Sill Finish: Aluminum with clear anodized finish.
24.	Sill Finish: Aluminum with black anodized finish.
25.	Glass and Glazing: Safety Glazing per ASTM C1036, ASTM C1048, ANSI Z97.1 and CPSC 16 CFR 1201 for NW Clad 740.
a.	Glazing Units: Dry glazed with glass stops on the inside.
1)	Glass Lites: Tempered.
2)	Glass Lites: Laminated.
3)	Glass Lites: Tempered and laminated.
4)	Double IGU: 1-1/4 inch (32 mm), 6 mm + 6 mm or 15/16 inch (24 mm) 4 mm + 4 mm tempered glass depending on panel height.
5)	Triple IGU: 1-9/16 inch (40 mm), 6 mm + 4 mm + 6 mm or 1-1/12 inch (36 mm) 4 mm + 4 mm + 4 mm tempered glass depending on panel height. 
26.	Insulated Glazing Unit Fill: Air.
27.	Insulated Glazing Unit Fill: Argon.
28.	Glass Type:  Reduced iron.
29.	Glass Spacers: Gray finish with capillary tube.
30.	Glass Spacers: Black finish with capillary tubes.
31.	Glass Spacers: Gray finish without capillary tubes.
32.	Glass Spacers: Black finish without capillary tubes.
33.	Insulated Glass Unit Surfaces: Clear.
34.	Insulated Glass Unit Surfaces: Low- E coating on No. 2 surface of double IGU.
35.	Insulated Glass Unit Surfaces: Low-E coating on No. 2 and No. 4 surface of double IGU.
36.	Insulated Glass Unit Surfaces: Low-E coating on No. 2 and No. 5 surface of triple IGU.
37.	Alarmed Glazing: Connection wiring to alarm system, position monitoring, locking detection and notification systems such as glass-breakage sensors by others.
38.	Locking Hardware and Handle for Sliding-Folding Systems:
a.	Main Entry Panels: Lockset with lockable latch, multi-point locking with deadbolt and rods at top and bottom on primary panels only.
1)	Application: Single swing panel.
2)	Application: Pair of swing panels.
3)	Operation:  After turn of key or thumb turn, depression of handles withdraws latch. Lifting of handles engages rods and turn of key or thumb turn engages deadbolt and operates lock.
4)	Rods: Concealed, not edge mounted.
5)	Lever Handles:  Lever handles on inside and outside.
6)	Lever Handles:  Lever handles with return on inside and outside.
7)	Lever Handle Finish: Brushed satin stainless steel; standard.
8)	Lever Handle Finish: Black titanium stainless steel; standard.
9)	Lever Handle Finish: Copper-nickel stainless steel antiviral and antimicrobial.
10)	Locking: Standard profile cylinder.
11)	Secondary Swing Panel: Concealed two-point, edge locking.
b.	Main Entry Panels: Flat handle on inside only with concealed two-point locking hardware operated by 180 degrees turn of handle; the main entry panel is operable from inside only and there is no latch.
c.	Main Entry Panels: No hardware or locking provided by manufacturer; Field installed panic device from Section 08 71 00 prepped for commercial application.
1)	Application: Single swing panel.
2)	Application: Pair of swing panels.
d.	Pairs of Folding Panels: Handles and concealed two-point locking hardware operated by 180 degrees turn of handle between each pair. Face applied flush bolt locking NOT acceptable.
1)	Handles: Manufacturer's flat handles.
a)	Flat Handle Finish: Brushed satin stainless steel.
b)	Flat Handle Finish: Black titanium stainless steel.
c)	Flat Handle Finish: Copper-nickel stainless steel antiviral and antimicrobial.
e.	Handle Height: 41-3/8 inch (105 cm) centered from bottom of panel unless otherwise indicated on Drawings.
f.	Locking Rods: End caps top and bottom: Rod Stroke: 15/16 inch (24 mm).
g.	Additional Profile Cylinders: Keyed alike.
h.	Additional Profile Cylinders: Keyed differently.
i.	Panel catch: Panel catch to hold swing panel to adjacent folding panel to prevent incorrect operation when moving the panel.
j.	Sliding-Folding Hardware: Combination with top and bottom tracks and threshold.
1)	Running carriages to have sealed, self-lubricating, double ball bearing multi-rollers.
2)	Surface mounted hinges and running carriages not acceptable.
3)	Lower Running Carriage Carrying Capacity:  240 lb. (110 kg); lower running carriage provided with two vertical stainless-steel wheels with double row of ball bearings and two horizontal polyamide wheels.
4)	Vertical wheels with Gothic arch feature to ride on top of stainless-steel guide track covers over full length of sill track. Wheels on aluminum surfaces not acceptable.
5)	Upper guide carriage with two horizontal polyamide guiding wheels. For configurations with pairs of panels that slide left or right, additional concealed, additional vertical tilt protection hardware.
6)	Hinges and Rollers:  Anodized aluminum with stainless steel security hinge pins and set-screws. Concealed panel alignment with a tight seal through the patented (Patent Number:  US10711510B2) TwinX mechanism reinforced between panels for a tight seal. Double ball bearing stainless-steel wheel rollers match hinge finish.
a)	Finish: Clear.
b)	Finish: Black.
7)	Spring-Loaded Pull Handle:  For outswing units with larger panel sizes, a spring loaded-pull handle is supplied for ease of closing the system. The pull handle is located above the flat handle. When not in use, the handle lays flat against the adjacent panel and is supplied with bumpers to avoid metal to metal contact. Handles are stainless steel  with the attachment to coordinate with the hinge hardware of the system.
a)	Pull Handle Finish:  Brushed satin stainless steel or black titanium stainless steel.
k.	Weather Stripping and Sound Gasketing: Manufacturer's double layer EPDM between panels and EPDM gasket, Q-Ion gasket, or brush seal between panel and frame, or brush seals with a two-layer fiberglass reinforced polyamide fin attached at both inner and outer edge of bottom of door panels with a recessed sill or on frame for sealing between panels and between panel and frame.
l.	Fasteners: Installation plates for connecting frame components made of stainless steel with sealing cushion to avoid thermal connectivity.
m.	Insect Screen:  Fully retractable non-pleated screen. Ultra-strong, UV resistant fiberglass mesh housed in single cartridge riding on a single track.
1)	Basis-of-Design Product by Manufacturer: The Horizon by Wizard Industries, Inc.
a)	Wizard Industries, Inc. which is located at:  4263 Phillips Ave, Burnaby, BC, Canada V5A 2X4; Toll Free:  (888) 949-3667; Telephone:  (604) 299-8878; Fax:  (604) 299-4496; Email:  sales@wizardindustries.com; Web:  https://www.wizardscreens.com. 
PART 3    EXECUTION
3.1	EXAMINATION AND PREPARATION
A.	Carefully examine rough openings with Installer present, for compliance with requirements affecting Work performance.
1.	Examine surfaces of openings and verify dimensions; verify rough openings are level, plumb, and square, with no unevenness, bowing, or bumps on floor and other conditions are required by the manufacturer for readiness to receive Work.
2.	Verify structural integrity of header; maximum deflection with both live and dead loads to be the lesser of L/720 of span or 1/4 inches (6 mm).
3.	Structural support for lateral loads, wind load, and eccentric load when panels are stacked open.
B.	Prepare openings using methods recommended by manufacturer for achieving the best result for the substrate under the project conditions.
1.	If preparation is the responsibility of another installer, notify Architect in writing of deviations from manufacturer's recommended installation tolerances and conditions.
C.	Do not proceed with installation until substrates are prepared using methods recommended by manufacturer. Commencement of installation constitutes acceptance of conditions.
3.2	INSTALLATION
A.	Install per Drawings, submittals, and manufacturer's installation instructions.
1.	Properly flash, seal, and waterproof around perimeter of opening.
2.	Attach anchorage devices in place, level, straight, plumb, and square. Install frame in proper elevation, plane, and location, and in proper alignment with other work.
3.	When lower track is designed to drain, provide connections to allow for drainage.
4.	Install panels, handles, lockset, screens, and other accessories in accordance with manufacturer's recommendations and instructions.
3.3	FIELD QUALITY CONTROL
A.	Field Inspection: Coordinate in accordance with appropriate sections in Division 01.
B.	Verify system operates and functions properly. Adjust hardware for proper operation.
C.	Non-Conforming Work: Repair or replace non-conforming work as directed by the Architect; see General and Supplementary Conditions, and Division 01, General Requirements.
3.4	CLEANING AND PROTECTION
A.	Protect installed products until completion of project. Keep units closed and protect installation against damage from construction activities.
B.	Remove protective coatings. Use manufacturer recommended methods to clean surfaces.

END OF SECTION