SECTION 03 11 16

FORMLINERS FOR ARCHITECTURAL CONCRETE.

Display hidden notes to specifier. (Don't know how? Click Here) 
 Copyright 2017 -  2024 ARCAT, Inc. - All rights reserved

PART 1    GENERAL.
1.1	SECTION INCLUDES.
A.	Reusable, elastomeric formliners for texturing architectural concrete with standard patterns.
B.	Reusable, elastomeric formliners for texturing architectural concrete with photo engraving.
C.	Reusable, elastomeric formliners for texturing architectural concrete with CNC graphic bas-relief patterns.
D.	Reusable, elastomeric formliners for texturing architectural concrete with custom designed patterns.
E.	Reusable, ABS plastic formliners for texturing architectural concrete with standard patterns.
F.	Single-use, HIPS plastic formliners for texturing architectural concrete with standard patterns.
G.	Architectural Stain for coloring concrete.
H.	Formliner accessories as required for complete installation.
1.2	RELATED SECTIONS.
A.	Section 03 10 00 - Concrete Forming and Accessories.
B.	Section 03 11 16 - Architectural Cast-in Place Concrete Forming.
C.	Section 03 45 13 - Faced Architectural Precast Concrete.
D.	Section 03 45 00 - Precast Architectural Concrete.
E.	Section 03 47 13 - Tilt-Up Concrete.
F.	Section 09 97 23 - Concrete and Masonry Coatings.
1.3	REFERENCES.
A.	American Concrete Institute (ACI): ACI 117 Tolerances for Concrete Construction and Materials.
B.	ASTM International (ASTM):
1.	ASTM D412: Standard Test Method for Tear Strength of Conventional Vulcanized Rubber and Thermoplastic Elastomers.
2.	ASTM D2240: Standard Test Method for Rubber Property - Durometer Hardness.
3.	ASTM D1456: Standard Test Method for Rubber Property - Elongation.
1.4	SUBMITTALS.
A.	Submit under provisions of Section 01 30 00.
B.	Product Data: Manufacturer's data sheets on each product to be used, including:
1.	Product sheets showing formliner name and model number.
2.	Formliner system preparation and installation procedures.
3.	Formliner application guide.
4.	Maintenance procedures.
5.	Storage and handling guidelines.
C.	Shop Drawings: Complete details of materials and installation, including but not limited to the following.
1.	Patterns.
2.	Formliner sheet sizes/accessory details.
3.	Joint locations.
4.	Installation sequence.
D.	Samples for Selection: For range of formliner types and patterns requested by Architect.
1.	Formliner sample, maximum 24 inches x 24 inches (610 mm x 610 mm) depicting textures and patterns.
2.	Renderings.
3.	Sample of release agents available for releasing of formliners from concrete.
E.	Verification Samples: For each formliner type and pattern specified.
1.	Formliner sample, maximum 24 inches x 24 inches (610 mm x 610 mm) depicting texture and pattern.
2.	Sample of release agent to be used for releasing of formliners from concrete.
F.	Quality Assurance Submittals: Copies of test reports conducted by independent laboratories verifying the characteristics of the formliner shall be submitted to the Architect upon request.
G.	Warranty: A copy of the manufacturer's product warranty shall be provided upon request.
1.5	QUALITY ASSURANCE.
A.	Single Source Requirements: Formliners, primary and secondary components necessary for the installation of the formliner shall be supplied from a single manufacturer, including but not limited to the following.
1.	Release agent.
2.	Formliner adhesive.
3.	Block outs/custom accessories.
B.	Manufacturer Qualifications: Manufacturer shall have a minimum of ten years experience manufacturing formliners.
C.	Installer Qualifications:
1.	If project is cast-in-place, installer shall have a minimum of three years experience working with formliners.
2.	If project is precast, precast manufacturer shall have a minimum of three years experience with fabricating with formliners.
D.	Project References: Upon request by Architect, manufacturer and installer shall submit a list of projects where formliners were used in the construction of concrete.
E.	Mock-Up: A mock-up panel shall be constructed to demonstrate the texture and pattern of formliners selected as well as the surface preparation techniques and craftsmanship of the installer and precast manufacturer.
1.	The mock-up panel shall accurately demonstrate the specified formliner textures, patterns, and conditions (corners, false joints, etc.) expected in the completed work.
2.	Provide representative mock-up panel in area designated by Architect.
3.	The exact procedures used in the full-scale construction of the concrete must also be used during the construction of the mock-up.
4.	Architect must approve the texture, pattern, color, and workmanship of the mock-up panel prior to the beginning of concrete construction. Do not proceed with remaining work until workmanship, installation and operation are approved by Architect.
5.	Mock-up panel must remain on-site for comparison during concrete construction or erection.
6.	The installer or precast manufacturer shall be responsible for the removal and disposal of the mock-up panel following completion of the project.
1.6	DELIVERY, STORAGE, AND HANDLING.
A.	Inspect the materials upon delivery to assure that specified products have been received. If there are any discrepancies upon inspection, the manufacturer must be immediately notified. Do not use damaged products.
B.	Deliver, store and handle materials and products in strict compliance with manufacturer's instructions and recommendations. Cover form liners when not in use to protect from water, oil, dirt, and UV exposure. If building storage is not available, formliners shall be raised from the ground and covered securely with non-transparent, non-translucent, waterproof covers.
C.	Store materials within absolute limits for temperature and humidity recommended by manufacturer. Liquid materials shall be stored in temperatures not exceeding 110 degrees F (43 degrees C) or falling below 32 degrees F (0 degrees C). Protect from damage.
1.7	PROJECT CONDITIONS.
A.	Maintain environmental conditions (temperature, humidity, and ventilation) within limits recommended by manufacturer for optimum results. Do not install products under environmental conditions outside manufacturer's absolute limits.
1.8	SEQUENCING.
A.	Ensure that products of this section are approved and supplied to affected trades in time to prevent interruption of construction progress.
B.	Pre-Installation/Pre-Manufacture Meeting: Convene minimum two weeks prior to starting work of this section.
1.9	WARRANTY.
A.	Manufacturer warranties formliners for specified usage as listed below.
1.	High Re-Use Elastomeric Formliners; Up to 100 uses.
2.	Low Use ABS Plastic Formliners: 2-5 uses.
3.	Single Use HIPS Plastic Formliners: Single use.
PART 2    PRODUCTS.
2.1	MANUFACTURERS.
A.	Acceptable Manufacturer: Architectural Polymers, which is located at:<BR />1220 Little Gap Rd.<BR />Palmerton, PA 18071<BR />Tel: 610-824-3322<BR />Fax: 610-824-3777<BR />Email: request info (Marshall@apformliner.com);Web: http://www.apformliner.com 
B.	Substitutions: Not permitted.
C.	Requests for substitutions will be considered in accordance with provisions of Section 01 60 00.
2.2	REUSABLE FORMLINERS FOR ARCHITECTURAL CONCRETE.
A.	Reusable Formliners: High Re-Use Elastomeric Formliners.
1.	Description: 100 prorated uses. Reusable elastomeric polyurethane formliners for creating textured surfaces on cast-in-place or precast concrete.
2.	Material Properties: As tested according to ASTM D2240.
a.	Specific Gravity: 1.05.
b.	Elongation at Break: 550.
c.	Shore A Hardness (DIN 53505): 65.
d.	Tensile Strength (DIN 53504): 520 PSI or 3.59 N/mm2.
e.	Tear Resistance (ASTM D624): 145 PLI or 25.44 kN/m.
3.	Manufacturing Tolerances:
a.	Height: Plus or minus 1/8 inch (3 mm).
b.	Width: Plus or minus 3/16 inch (5 mm) in length or width.
4.	Color: Grey.
5.	Pattern: As selected by Architect from manufacturer's standard range of available products.
6.	Pattern: From manufacturer's standard range of available products, as indicated on Drawings.
7.	Pattern: Brick Pattern 101A Modular Brick Velour (concave).
8.	Pattern: Brick Pattern 101B Modular Brick Velour (raked).
9.	Pattern: Brick Pattern 102A Utility Brick Wirecut (concave).
10.	Pattern: Brick Pattern 102B Utility Brick Wirecut (raked).
11.	Pattern: Brick Pattern 103A 1/3 Running Bond (concave).
12.	Pattern: Brick Pattern 103B 1/3 Running Bond (raked).
13.	Pattern: Brick Pattern 104 18th Century Brick.
14.	Pattern: Brick Pattern 105A Smooth Utility Brick (concave).
15.	Pattern: Brick Pattern 105B Smooth Utility Brick (raked).
16.	Pattern: Brick Pattern 107A Modular Brick Smooth (concave).
17.	Pattern: Brick Pattern 107B Modular Brick Smooth (raked).
18.	Pattern: Brick Pattern 108A Modular Brick Sand Finish (concave).
19.	Pattern: Brick Pattern 108B Modular Brick Sand Finish (raked).
20.	Pattern: Brick Pattern 109 Weathered Metric Brick.
21.	Pattern: Brick Pattern 110 8x8x1/2 inch Running Bond Tile (concave).
22.	Pattern: Brick Pattern 111 Ohio Sand Brick.
23.	Pattern: Brick Pattern 112 Modular Brick Wirecut (concave).
24.	Pattern: Brick Pattern 113 Closure Tumbled Brick (raked).
25.	Pattern: Brick Pattern 114 Long Format Brick.
26.	Pattern: Fractured Pattern 201 M&R Modified.
27.	Pattern: Fractured Pattern 202 Tree Bark.
28.	Pattern: Fractured Pattern 203 1 inch Standard Fractured Fin.
29.	Pattern: Fractured Pattern 204 1.5 inch Architectural Rib.
30.	Pattern: Fractured Pattern 205 Flat Fractured Rib.
31.	Pattern: Fractured Pattern 206 3/4 inch Standard Fractured Fin.
32.	Pattern: Fractured Pattern 207 1 inch Fractured Rope.
33.	Pattern: Fractured Pattern 208 Wavy Carolina Fractured Rib.
34.	Pattern: Fractured Pattern 209 1/2 inch Fractured Fin.
35.	Pattern: Fractured Pattern 210 NY Fractured Fin.
36.	Pattern: Fractured Pattern 210A Broome County Fin.
37.	Pattern: Fractured Pattern 211 Sound Absorptive Broken 1 ft Ribs.
38.	Pattern: Fractured Pattern 213 3 inch Fractured Flute.
39.	Pattern: Fractured Pattern 214 1/4 inch Standard Fractured Fin.
40.	Pattern: Fractured Pattern 215 Walpole Flute.
41.	Pattern: Fractured Pattern 216 Upton.
42.	Pattern: Fractured Pattern 217 Wavy Dover Rib.
43.	Pattern: Rhythmic Pattern 301 1/2 inch Sinewave.
44.	Pattern: Rhythmic Pattern 302 3/4 inch Fin.
45.	Pattern: Rhythmic Pattern 303 3 inch Fin.
46.	Pattern: Rhythmic Pattern 304 Wyeth Aherst Rib.
47.	Pattern: Rhythmic Pattern 305 3/8 inch Smooth Flute 1 O.C.
48.	Pattern: Rhythmic Pattern 306 1-1/2 inch Deep Smooth Rib.
49.	Pattern: Rhythmic Pattern 307 1-3/4 inch Smooth Flute 2-1/4 inch O.C.
50.	Pattern: Rhythmic Pattern 308 2 inch Deep Smooth Flute 2 inch O.C.
51.	Pattern: Rhythmic Pattern 309 1 inch Light Textured Flute 2 inch O.C.
52.	Pattern: Rhythmic Pattern 310 Pyramid Flute 8 inch O.C.
53.	Pattern: Rhythmic Pattern 311A Random Striated Rib.
54.	Pattern: Rhythmic Pattern 311B Random Striated Rib.
55.	Pattern: Rhythmic Pattern 311C Random Striated Rib.
56.	Pattern: Rhythmic Pattern 313 Salem.
57.	Pattern: Rhythmic Pattern 314 Geo Diamonds.
58.	Pattern: Rhythmic Pattern 315 Braintree.
59.	Pattern: Rhythmic Pattern 316 Random Board.
60.	Pattern: Rhythmic Pattern 317 1.25 inch Random Peak/Valley.
61.	Pattern: Rhythmic Pattern 319 3/4 inch Sinewave.
62.	Pattern: Rhythmic Pattern 321 Chelmsford.
63.	Pattern: Rhythmic Pattern 322 JFD Random Flute.
64.	Pattern: Rhythmic Pattern 323 Fine Scored Rib.
65.	Pattern: Rhythmic Pattern 324 Bellingham.
66.	Pattern: Rhythmic Pattern 325 Granby.
67.	Pattern: Flat Pattern 401 Exposed Aggregate.
68.	Pattern: Flat Pattern 403 Light Sand Finish.
69.	Pattern: Flat Pattern 404 Medium Sand Finish.
70.	Pattern: Flat Pattern 405 Smooth Finish.
71.	Pattern: Flat Pattern 406 Worm Stucco.
72.	Pattern: Flat Pattern 407 Broom.
73.	Pattern: Flat Pattern 408 Bush Hammered.
74.	Pattern: Flat Pattern 410 EIFS.
75.	Pattern: Flat Pattern 411 Heavy Sand Blast.
76.	Pattern: Flat Pattern 412 Venetian Stucco.
77.	Pattern: Flat Pattern 413 1/2 inch R-ver Gravel.
78.	Pattern: Flat Pattern 414 Travertine.
79.	Pattern: Wood Pattern 501 Barn Boards.
80.	Pattern: Wood Pattern 502 5 inch and 3 inch Cedar.
81.	Pattern: Wood Pattern 503 Cedar Stakes.
82.	Pattern: Wood Pattern 504 6 inch Shiplap.
83.	Pattern: Wood Pattern 505 Exaggerated Stakes.
84.	Pattern: Wood Pattern 506 Staggered Oak.
85.	Pattern: Wood Pattern 507 Staggered Oak Heavy.
86.	Pattern: Wood Pattern 508 1 inch Split Cedar Stakes.
87.	Pattern: Wood Pattern 509 5 inch Weathered Wood.
88.	Pattern: Wood Pattern 512 Hand Hewn Hemlock.
89.	Pattern: Wood Pattern 513 Bamboo Strips - Small.
90.	Pattern: Wood Pattern 514 2-1/2 inch Split Stakes.
91.	Pattern: Wood Pattern 515 Old Timber Form.
92.	Pattern: Wood Pattern 516 Medium Grain 7-5/8 inch Board.
93.	Pattern: Wood Pattern 517 Board and Batten.
94.	Pattern: Wood Pattern 518 6 inch Smooth Shiplap.
95.	Pattern: Wood Pattern 519 Cedar Shakes.
96.	Pattern: Wood Pattern 520 Weathered Fir.
97.	Pattern: Wood Pattern 521 7-1/2 inch Weathered Fir.
98.	Pattern: Wood Pattern 523 Cedar Shake.
99.	Pattern: Wood Pattern 524 Random Width Barn Boards.
100.	Pattern: Contemporary Pattern 701 Lowell.
101.	Pattern: Contemporary Pattern 702 Billerica.
102.	Pattern: Contemporary Pattern 703 Natick.
103.	Pattern: Contemporary Pattern 704 Dracut.
104.	Pattern: Contemporary Pattern 705 Haverhill.
105.	Pattern: Contemporary Pattern 706 Tewksbury.
106.	Pattern: Contemporary Pattern 707 Ipswich.
107.	Pattern: Contemporary Pattern 708 Saugus.
108.	Pattern: Contemporary Pattern 709 Sagaponack.
109.	Pattern: Contemporary Pattern 710 Pepperell.
110.	Pattern: Contemporary Pattern 711 Cambridge.
111.	Pattern: Contemporary Pattern 712 Marshfield.
112.	Pattern: Contemporary Pattern 713 Clicquot.
113.	Pattern: Contemporary Pattern 714 Lenox.
114.	Pattern: Contemporary Pattern 715 Roxbury.
115.	Pattern: Contemporary Pattern 716 Marblehead.
116.	Pattern: Contemporary Pattern 717 Peabody.
117.	Pattern: Contemporary Pattern 718 Reynold.
118.	Pattern: Contemporary Pattern 719 Longmeadow.
119.	Pattern: Contemporary Pattern 720 Chicopee.
120.	Pattern: Contemporary Pattern 721 Duxberry.
121.	Pattern: Stone and Block Pattern 888 9 inch Quarry Stone.
122.	Pattern: Stone and Block Pattern 889 8 inch Quarry Stone.
123.	Pattern: Stone and Block Pattern 890 14-3/4 inch Horseheads Quarry Stone.
124.	Pattern: Stone and Block Pattern 891A Riverstone.
125.	Pattern: Stone and Block Pattern 891C Riverstone.
126.	Pattern: Stone and Block Pattern 892 12 inch Quarry Stone.
127.	Pattern: Stone and Block Pattern 893 14 inch Quarry Stone.
128.	Pattern: Stone and Block Pattern 893A 15 inch Custom Quarry Stone.
129.	Pattern: Stone and Block Pattern 894 16 inch Quarry Stone.
130.	Pattern: Stone and Block Pattern 895 21 inch Quarry Stone.
131.	Pattern: Stone and Block Pattern 896 24 inch Quarry Stone.
132.	Pattern: Stone and Block Pattern 897A 14-3/4 inch Rustic Quarried 1-5/8 inch.
133.	Pattern: Stone and Block Pattern 897B 14-3/4 inch Rustic Quarried 3 inch.
134.	Pattern: Stone and Block Pattern 898 Rustic Ashlar Stone.
135.	Pattern: Stone and Block Pattern 898A Rustic Ashlar Stone.
136.	Pattern: Stone and Block Pattern 899 Northeast River Stone.
137.	Pattern: Stone and Block Pattern 900 2x8 Split Block.
138.	Pattern: Stone and Block Pattern 901A 8x16 Split Block Concave.
139.	Pattern: Stone and Block Pattern 901B 8x16 Split Block Raked.
140.	Pattern: Stone and Block Pattern 901C 8x16 Split Block Heavy Relief Concave.
141.	Pattern: Stone and Block Pattern 902 9x18 Split Block with Deep Mortar.
142.	Pattern: Stone and Block Pattern 903 8x8 Split Block.
143.	Pattern: Stone and Block Pattern 904 Ashlar Stone.
144.	Pattern: Stone and Block Pattern 904A Ashlar Stone.
145.	Pattern: Stone and Block Pattern 905 Small Aged Ashlar Stone.
146.	Pattern: Stone and Block Pattern 906 Ashlar Stone Heavy Cut.
147.	Pattern: Stone and Block Pattern 907 Coral Ashlar Stone.
148.	Pattern: Stone and Block Pattern 908 BQE Old Cut Ashlar Stone.
149.	Pattern: Stone and Block Pattern 909 Westmoreland Drystack.
150.	Pattern: Stone and Block Pattern 910 Median Barrier Drystack.
151.	Pattern: Stone and Block Pattern 910B Median Barrier Drystack.
152.	Pattern: Stone and Block Pattern 911 Large Stone Drystack.
153.	Pattern: Stone and Block Pattern 911A Large Stone Drystack.
154.	Pattern: Stone and Block Pattern 911B Large Stone Drystack.
155.	Pattern: Stone and Block Pattern 911O Large Stone Ohio Drystack.
156.	Pattern: Stone and Block Pattern 912 Valley Forge Fieldstone.
157.	Pattern: Stone and Block Pattern 912A Valley Forge Fieldstone 3/4 inch Relief.
158.	Pattern: Stone and Block Pattern 913 New York DOT Ashlar.
159.	Pattern: Stone and Block Pattern 914 Small Aged Ashlar with Thin Joints.
160.	Pattern: Stone and Block Pattern 916 Small Rustic Ashlar.
161.	Pattern: Stone and Block Pattern 917 8x8 Split Block Running Bond.
162.	Pattern: Stone and Block Pattern 918 12x24 Split Limestone Running Bond.
163.	Pattern: Stone and Block Pattern 919 Weathered Cut Ashlar.
164.	Pattern: Stone and Block Pattern 921 Split Slate.
165.	Pattern: Stone and Block Pattern 922 Cleaved Limestone.
166.	Pattern: Stone and Block Pattern 927 Atomic Ashlar.
167.	Pattern: Stone and Block Pattern 928 Slump Stone.
168.	Pattern: Stone and Block Pattern 929 8x16 Hand Chiseled Block.
169.	Pattern: Stone and Block Pattern 931 Dry Fit Ashlar.
170.	Pattern: Stone and Block Pattern 932 Random Coursed Ashlar.
171.	Pattern: Stone and Block Pattern 933 Ledgestone Drystack.
172.	Pattern: Stone and Block Pattern 934 Dry-Fit Paver.
173.	Pattern: Stone and Block Pattern 935 Castle Stone.
174.	Pattern: Stone and Block Pattern 936 3/8 inch Split Limestone.
175.	Pattern: Stone and Block Pattern 936B 3/4 inch Split Limestone.
176.	Pattern: Stone and Block Pattern 937 Mauch Chunk Drystack.
177.	Pattern: Stone and Block Pattern 938 Canal Lock Drystack.
2.3	LOW RE-USE ABS FORMLINERS FOR ARCHITECTURAL CAST-IN-PLACE CONCRETE.
A.	Reusable Formliners:
1.	Description: Up to 5 uses. ABS formliners for creating textured surfaces on cast-in-place or precast concrete.
2.	Material Properties: As tested according to ASTM D2240.
a.	Specific Gravity: 1.08 g/cm3.
b.	Shore A Hardness (DIN 53505): 98/65.
c.	Tensile Strength (DIN 53504): 30 to 40 MPa.
3.	Color: White.
4.	Pattern: As selected by Architect from manufacturer's standard range of available products.
5.	Pattern: From manufacturer's standard range of available products, as indicated on Drawings.
6.	Pattern: Brick Pattern 101A Modular Brick Velour (concave).
7.	Pattern: Brick Pattern 101B Modular Brick Velour (raked).
8.	Pattern: Brick Pattern 102A Utility Brick Wirecut (concave).
9.	Pattern: Brick Pattern 102B Utility Brick Wirecut (raked).
10.	Pattern: Brick Pattern 103A 1/3 Running Bond (concave).
11.	Pattern: Brick Pattern 103B 1/3 Running Bond (raked).
12.	Pattern: Brick Pattern 104 18th Century Brick.
13.	Pattern: Brick Pattern 105A Smooth Utility Brick (concave).
14.	Pattern: Brick Pattern 105B Smooth Utility Brick (raked).
15.	Pattern: Brick Pattern 107A Modular Brick Smooth (concave).
16.	Pattern: Brick Pattern 107B Modular Brick Smooth (raked).
17.	Pattern: Brick Pattern 108A Modular Brick Sand Finish (concave).
18.	Pattern: Brick Pattern 108B Modular Brick Sand Finish (raked).
19.	Pattern: Brick Pattern 109 Weathered Metric Brick.
20.	Pattern: Brick Pattern 110 8x8 1/2 inch Running Bond Tile (concave).
21.	Pattern: Brick Pattern 111 Ohio Sand Brick.
22.	Pattern: Brick Pattern 112 Modular Brick Wirecut (concave).
23.	Pattern: Brick Pattern 113 Closure Tumbled Brick (raked).
24.	Pattern: Fractured Pattern 201 M&R Modified.
25.	Pattern: Fractured Pattern 202 Tree Bark.
26.	Pattern: Fractured Pattern 203 1 inch Standard Fractured Fin.
27.	Pattern: Fractured Pattern 204 1.5 inch Architectural Rib.
28.	Pattern: Fractured Pattern 205 Flat Fractured Rib.
29.	Pattern: Fractured Pattern 206 3/4 inch Standard Fractured Fin.
30.	Pattern: Fractured Pattern 207 1 inch Fractured Rope.
31.	Pattern: Fractured Pattern 208 Wavy Carolina Fractured Rib.
32.	Pattern: Fractured Pattern 209 1/2 inch Fractured Fin.
33.	Pattern: Fractured Pattern 210 NY Fractured Fin.
34.	Pattern: Fractured Pattern 211 Sound Absorptive Broken 1 ft Ribs.
35.	Pattern: Fractured Pattern 213 3 inch Fractured Flute.
36.	Pattern: Fractured Pattern 214 1/4 inch Standard Fractured Fin.
37.	Pattern: Rhythmic Pattern 301 1/2 inch Sinewave.
38.	Pattern: Rhythmic Pattern 302 3/4 inch Fin.
39.	Pattern: Rhythmic Pattern 303 3 inch Fin.
40.	Pattern: Rhythmic Pattern 304 Wyeth Aherst Rib.
41.	Pattern: Rhythmic Pattern 305 3/8 inch Smooth Flute 1 O.C.
42.	Pattern: Rhythmic Pattern 307 1-3/4 inch Smooth Flute 2-1/4 inch O.C.
43.	Pattern: Rhythmic Pattern 309 1 inch Light Textured Flute 2 inch O.C.
44.	Pattern: Rhythmic Pattern 310 Pyramid Flute 8 inch O.C.
45.	Pattern: Rhythmic Pattern 311A Random Striated Rib.
46.	Pattern: Rhythmic Pattern 311C Random Striated Rib.
47.	Pattern: Rhythmic Pattern 313 Salem.
48.	Pattern: Rhythmic Pattern 314 Geo Diamonds.
49.	Pattern: Rhythmic Pattern 315 Braintree.
50.	Pattern: Rhythmic Pattern 317 1.25 inch Random Peak/Valley.
51.	Pattern: Rhythmic Pattern 319 3/4 inch Sinewave.
52.	Pattern: Flat Pattern 401 Exposed Aggregate.
53.	Pattern: Flat Pattern 403 Light Sand Finish.
54.	Pattern: Flat Pattern 404 Medium Sand Finish.
55.	Pattern: Flat Pattern 405 Smooth Finish.
56.	Pattern: Flat Pattern 406 Worm Stucco.
57.	Pattern: Flat Pattern 407 Broom.
58.	Pattern: Flat Pattern 408 Bush Hammered.
59.	Pattern: Flat Pattern 410 EIFS.
60.	Pattern: Flat Pattern 412 Venetian Stucco.
61.	Pattern: Wood Pattern 501 Barn Boards.
62.	Pattern: Wood Pattern 502 5 inch and 3 inch Cedar.
63.	Pattern: Wood Pattern 503 Cedar Stakes.
64.	Pattern: Wood Pattern 504 6 inch Shiplap.
65.	Pattern: Wood Pattern 505 Exaggerated Stakes.
66.	Pattern: Wood Pattern 506 Staggered Oak.
67.	Pattern: Wood Pattern 507 Staggered Oak Heavy.
68.	Pattern: Wood Pattern 508 1 inch Split Cedar Stakes.
69.	Pattern: Wood Pattern 509 5 inch Weathered Wood.
70.	Pattern: Wood Pattern 512 Hand Hewn Hemlock.
71.	Pattern: Wood Pattern 513 Bamboo Strips - Small.
72.	Pattern: Wood Pattern 514 2-1/2 inch Split Stakes.
73.	Pattern: Wood Pattern 515 Old Timber Form.
74.	Pattern: Wood Pattern 516 Medium Grain 7 5/8 inch Board.
75.	Pattern: Wood Pattern 517 Board and Batten.
76.	Pattern: Wood Pattern 518 6 inch Smooth Shiplap.
77.	Pattern: Wood Pattern 519 Cedar Shakes.
78.	Pattern: Wood Pattern 520 Weathered Fir.
79.	Pattern: Wood Pattern 521 7-1/2 inch Weathered Fir.
80.	Pattern: Contemporary Pattern 701 Lowell.
81.	Pattern: Contemporary Pattern 702 Billerica.
82.	Pattern: Contemporary Pattern 707 Ipswich.
83.	Pattern: Contemporary Pattern 708 Saugus.
84.	Pattern: Contemporary Pattern 709 Sagaponack.
85.	Pattern: Contemporary Pattern 710 Pepperell.
86.	Pattern: Contemporary Pattern 711 Cambridge.
87.	Pattern: Contemporary Pattern 712 Marshfield.
88.	Pattern: Contemporary Pattern 713 Clicquot.
89.	Pattern: Contemporary Pattern 716 Marblehead.
90.	Pattern: Contemporary Pattern 718 Reynold.
91.	Pattern: Contemporary Pattern 719 Longmeadow.
92.	Pattern: Contemporary Pattern 720 Chicopee.
93.	Pattern: Contemporary Pattern 721 Duxberry.
94.	Pattern: Contemporary Pattern 738 Holbrook.
95.	Pattern: Contemporary Pattern 739 Norwell.
96.	Pattern: Contemporary Pattern 740 Brocton.
97.	Pattern: Contemporary Pattern 741 Humarock.
98.	Pattern: Contemporary Pattern 742 Shrewsbury.
99.	Pattern: Contemporary Pattern 743 Rockland.
100.	Pattern: Contemporary Pattern 744 Wrentham].
101.	Pattern: Contemporary Pattern 745 Harwich.
102.	Pattern: Contemporary Pattern 746 Wayland.
103.	Pattern: Contemporary Pattern 747 Wellesley.
104.	Pattern: Contemporary Pattern 748 Watertown.
105.	Pattern: Contemporary Pattern 749 Athol.
106.	Pattern: Contemporary Pattern 750 Becket.
107.	Pattern: Contemporary Pattern 752 Quincy.
108.	Pattern: Stone and Block Pattern 888 9 inch Quarry Stone.
109.	Pattern: Stone and Block Pattern 889 8 inch Quarry Stone.
110.	Pattern: Stone and Block Pattern 891C Riverstone.
111.	Pattern: Stone and Block Pattern 892 12 inch Quarry Stone.
112.	Pattern: Stone and Block Pattern 893 14 inch Quarry Stone.
113.	Pattern: Stone and Block Pattern 893A 15 inch Custom Quarry Stone.
114.	Pattern: Stone and Block Pattern 894 16 inch Quarry Stone.
115.	Pattern: Stone and Block Pattern 897A 14-3/4 inch Rustic Quarried 1-5/8 inch.
116.	Pattern: Stone and Block Pattern 898 Rustic Ashlar Stone.
117.	Pattern: Stone and Block Pattern 898A Rustic Ashlar Stone.
118.	Pattern: Stone and Block Pattern 900 2x8 Split Block.
119.	Pattern: Stone and Block Pattern 901A 8x16 Split Block Concave.
120.	Pattern: Stone and Block Pattern 901B 8x16 Split Block Raked.
121.	Pattern: Stone and Block Pattern 901C 8x16 Split Block Heavy Relief Concave.
122.	Pattern: Stone and Block Pattern 902 9x18 Split Block with Deep Mortar.
123.	Pattern: Stone and Block Pattern 903 8x8 Split Block.
124.	Pattern: Stone and Block Pattern 904 Ashlar Stone.
125.	Pattern: Stone and Block Pattern 904A Ashlar Stone.
126.	Pattern: Stone and Block Pattern 905 Small Aged Ashlar Stone.
127.	Pattern: Stone and Block Pattern 906 Ashlar Stone Heavy Cut.
128.	Pattern: Stone and Block Pattern 907 Coral Ashlar Stone.
129.	Pattern: Stone and Block Pattern 908 BQE Old Cut Ashlar Stone.
130.	Pattern: Stone and Block Pattern 909 Westmoreland Drystack.
131.	Pattern: Stone and Block Pattern 910 Median Barrier Drystack.
132.	Pattern: Stone and Block Pattern 910B Median Barrier Drystack.
133.	Pattern: Stone and Block Pattern 911A Large Stone Drystack.
134.	Pattern: Stone and Block Pattern 911B Large Stone Drystack.
135.	Pattern: Stone and Block Pattern 911O Large Stone Ohio Drystack.
136.	Pattern: Stone and Block Pattern 912 Valley Forge Fieldstone.
137.	Pattern: Stone and Block Pattern 912A Valley Forge Fieldstone 3/4 inch Relief.
138.	Pattern: Stone and Block Pattern 913 New York DOT Ashlar.
139.	Pattern: Stone and Block Pattern 916 Small Rustic Ashlar.
140.	Pattern: Stone and Block Pattern 917 8x8 Split Block Running Bond.
141.	Pattern: Stone and Block Pattern 918 12x24 Split Limestone Running Bond.
142.	Pattern: Stone and Block Pattern 919 Weathered Cut Ashlar.
143.	Pattern: Stone and Block Pattern 921 Split Slate.
144.	Pattern: Stone and Block Pattern 922 Cleaved Limestone.
145.	Pattern: Stone and Block Pattern 927 Atomic Ashlar.
146.	Pattern: Stone and Block Pattern 928 Slump Stone.
147.	Pattern: Stone and Block Pattern 929 8x16 Hand Chiseled Block.
148.	Pattern: Stone and Block Pattern 931 Dry Fit Ashlar.
149.	Pattern: Stone and Block Pattern 932 Random Coursed Ashlar.
150.	Pattern: Stone and Block Pattern 933 Ledgestone Drystack.
151.	Pattern: Stone and Block Pattern 934 Dry-Fit Paver.
152.	Pattern: Stone and Block Pattern 935 Castle Stone.
153.	Pattern: Stone and Block Pattern 936 3/8 inch Split Limestone.
154.	Pattern: Stone and Block Pattern 936B 3/4 inch Split Limestone.
155.	Pattern: Stone and Block Pattern 937 Mauch Chunk Drystack.
156.	Pattern: Stone and Block Pattern 938 Canal Lock Drystack.
157.	Pattern: Stone and Block Pattern 939 Manassas Drystack.
158.	Pattern: Stone and Block Pattern 940 Winnipeg Quarry Stone.
159.	Pattern: Stone and Block Pattern 942 Ranger Split Stone.
160.	Pattern: Stone and Block Pattern 943 3/4 inch deep Drystack.
161.	Pattern: Stone and Block Pattern 944 Maryland Ashlar Stone.
162.	Pattern: Stone and Block Pattern 945 Montgomery Ashlar Stone.
163.	Pattern: Stone and Block Pattern 946 Smokey Mountain Drystack.
2.4	CUSTOM FORMLINERS FOR ARCHITECTURAL PRECAST AND CAST-IN-PLACE CONCRETE.
A.	Custom Reusable Formliners: As manufactured by Architectural Polymers, Inc.
1.	Description: Custom designed, formliners for creating textured surfaces on cast-in-place or precast concrete.
2.	Elastomeric High Re-Use Formliners: Up to 100 uses.
3.	Low Use ABS Plastic Formliners: 2 to 5 uses.
4.	Single Use HIPS Plastic Formliners: Single use.
5.	Pattern: Custom style, _____________.
6.	Pattern: Photo-engraving, _____________.
7.	Pattern: CNC graphic patterns, ___________.
8.	Pattern: As selected by Architect from manufacturer's custom range of available formliners.
9.	Pattern: From manufacturer's custom range of available formliners, as indicated on Drawings.
2.5	SINGLE-USE FORMLINERS FOR ARCHITECTURAL PRECAST OR CAST-IN-PLACE CONCRETE.
A.	Single Use Formliners: Single use HIPS plastic formliners as manufactured by Architectural Polymers, Inc.
1.	Description: Custom designed, single use formliners for creating textured surfaces on cast-in-place or precast concrete.
2.	Material Properties: As tested according to ASTM D2240.
a.	Specific Gravity: 1.06 g/cm3.
b.	Tensile Strength (DIN 53504): 20 MPa.
3.	Color: White.
4.	Pattern: As selected by Architect from manufacturer's standard range of available single use formliners.
5.	Pattern: From manufacturer's standard range of available single use formliners, as indicated on Drawings.
6.	Pattern: Brick Pattern 101A Modular Brick Velour (concave).
7.	Pattern: Brick Pattern 101B Modular Brick Velour (raked).
8.	Pattern: Brick Pattern 102A Utility Brick Wirecut (concave).
9.	Pattern: Brick Pattern 102B Utility Brick Wirecut (raked).
10.	Pattern: Brick Pattern 103A 1/3 Running Bond (concave).
11.	Pattern: Brick Pattern 103B 1/3 Running Bond (raked).
12.	Pattern: Brick Pattern 104 18th Century Brick.
13.	Pattern: Brick Pattern 105A Smooth Utility Brick (concave).
14.	Pattern: Brick Pattern 105B Smooth Utility Brick (raked).
15.	Pattern: Brick Pattern 107A Modular Brick Smooth (concave).
16.	Pattern: Brick Pattern 107B Modular Brick Smooth (raked).
17.	Pattern: Brick Pattern 108A Modular Brick Sand Finish (concave).
18.	Pattern: Brick Pattern 108B Modular Brick Sand Finish (raked).
19.	Pattern: Brick Pattern 109 Weathered Metric Brick.
20.	Pattern: Brick Pattern 110 8x8x1/2 inch Running Bond Tile (concave).
21.	Pattern: Brick Pattern 111 Ohio Sand Brick.
22.	Pattern: Brick Pattern 112 Modular Brick Wirecut (concave).
23.	Pattern: Brick Pattern 113 Closure Tumbled Brick (raked).
24.	Pattern: Fractured Pattern 201 M&R Modified.
25.	Pattern: Fractured Pattern 202 Tree Bark.
26.	Pattern: Fractured Pattern 203 1 inch Standard Fractured Fin.
27.	Pattern: Fractured Pattern 204 1.5 inch Architectural Rib.
28.	Pattern: Fractured Pattern 205 Flat Fractured Rib.
29.	Pattern: Fractured Pattern 206 3/4 inch Standard Fractured Fin.
30.	Pattern: Fractured Pattern 207 1 inch Fractured Rope.
31.	Pattern: Fractured Pattern 208 Wavy Carolina Fractured Rib.
32.	Pattern: Fractured Pattern 209 1/2 inch Fractured Fin.
33.	Pattern: Fractured Pattern 210 NY Fractured Fin.
34.	Pattern: Fractured Pattern 211 Sound Absorptive Broken 1 ft Ribs.
35.	Pattern: Fractured Pattern 213 3 inch Fractured Flute.
36.	Pattern: Fractured Pattern 214 1/4 inch Standard Fractured Fin.
37.	Pattern: Rhythmic Pattern 301 1/2 inch Sinewave.
38.	Pattern: Rhythmic Pattern 302 3/4 inch Fin.
39.	Pattern: Rhythmic Pattern 303 3 inch Fin.
40.	Pattern: Rhythmic Pattern 304 Wyeth Aherst Rib.
41.	Pattern: Rhythmic Pattern 305 3/8 inch Smooth Flute 1 O.C.
42.	Pattern: Rhythmic Pattern 307 1-3/4 inch Smooth Flute 2-1/4 inch O.C.
43.	Pattern: Rhythmic Pattern 309 1 inch Light Textured Flute 2 inch O.C.
44.	Pattern: Rhythmic Pattern 310 Pyramid Flute 8 inch O.C.
45.	Pattern: Rhythmic Pattern 311A Random Striated Rib.
46.	Pattern: Rhythmic Pattern 311C Random Striated Rib.
47.	Pattern: Rhythmic Pattern 313 Salem.
48.	Pattern: Rhythmic Pattern 314 Geo Diamonds.
49.	Pattern: Rhythmic Pattern 315 Braintree.
50.	Pattern: Rhythmic Pattern 317 1.25 inch Random Peak/Valley.
51.	Pattern: Rhythmic Pattern 319 3/4 inch Sinewave.
52.	Pattern: Flat Pattern 401 Exposed Aggregate.
53.	Pattern: Flat Pattern 403 Light Sand Finish.
54.	Pattern: Flat Pattern 404 Medium Sand Finish.
55.	Pattern: Flat Pattern 405 Smooth Finish.
56.	Pattern: Flat Pattern 406 Worm Stucco.
57.	Pattern: Flat Pattern 407 Broom.
58.	Pattern: Flat Pattern 408 Bush Hammered.
59.	Pattern: Flat Pattern 410 EIFS.
60.	Pattern: Flat Pattern 412 Venetian Stucco.
61.	Pattern: Wood Pattern 501 Barn Boards.
62.	Pattern: Wood Pattern 502 5 inch and 3 inch Cedar.
63.	Pattern: Wood Pattern 503 Cedar Stakes.
64.	Pattern: Wood Pattern 504 6 inch Shiplap.
65.	Pattern: Wood Pattern 505 Exaggerated Stakes.
66.	Pattern: Wood Pattern 506 Staggered Oak.
67.	Pattern: Wood Pattern 507 Staggered Oak Heavy.
68.	Pattern: Wood Pattern 508 1 inch Split Cedar Stakes.
69.	Pattern: Wood Pattern 509 5 inch Weathered Wood.
70.	Pattern: Wood Pattern 512 Hand Hewn Hemlock.
71.	Pattern: Wood Pattern 513 Bamboo Strips - Small.
72.	Pattern: Wood Pattern 514 2-1/2 inch Split Stakes.
73.	Pattern: Wood Pattern 515 Old Timber Form.
74.	Pattern: Wood Pattern 516 Medium Grain 7-5/8 inch Board.
75.	Pattern: Wood Pattern 517 Board and Batten.
76.	Pattern: Wood Pattern 518 6 inch Smooth Shiplap.
77.	Pattern: Wood Pattern 519 Cedar Shakes.
78.	Pattern: Wood Pattern 520 Weathered Fir.
79.	Pattern: Wood Pattern 521 7-1/2 inch Weathered Fir.
80.	Pattern: Contemporary Pattern 701 Lowell.
81.	Pattern: Contemporary Pattern 702 Billerica.
82.	Pattern: Contemporary Pattern 707 Ipswich.
83.	Pattern: Contemporary Pattern 708 Saugus.
84.	Pattern: Contemporary Pattern 709 Sagaponack.
85.	Pattern: Contemporary Pattern 710 Pepperell.
86.	Pattern: Contemporary Pattern 711 Cambridge.
87.	Pattern: Contemporary Pattern 712 Marshfield.
88.	Pattern: Contemporary Pattern 713 Clicquot.
89.	Pattern: Contemporary Pattern 716 Marblehead.
90.	Pattern: Contemporary Pattern 718 Reynold.
91.	Pattern: Contemporary Pattern 719 Longmeadow.
92.	Pattern: Contemporary Pattern 721 Duxberry.
93.	Pattern: Contemporary Pattern 752 Quincy.
94.	Pattern: Stone and Block Pattern 888 9 inch Quarry Stone.
95.	Pattern: Stone and Block Pattern 889 8 inch Quarry Stone.
96.	Pattern: Stone and Block Pattern 891C Riverstone.
97.	Pattern: Stone and Block Pattern 892 12 inch Quarry Stone.
98.	Pattern: Stone and Block Pattern 893 14 inch Quarry Stone.
99.	Pattern: Stone and Block Pattern 893A 15 inch Custom Quarry Stone.
100.	Pattern: Stone and Block Pattern 894 16 inch Quarry Stone.
101.	Pattern: Stone and Block Pattern 897A 14-3/4 inch Rustic Quarried 1-5/8 inch.
102.	Pattern: Stone and Block Pattern 898 Rustic Ashlar Stone.
103.	Pattern: Stone and Block Pattern 898A Rustic Ashlar Stone.
104.	Pattern: Stone and Block Pattern 900 2x8 Split Block.
105.	Pattern: Stone and Block Pattern 901A 8x16 Split Block Concave.
106.	Pattern: Stone and Block Pattern 901B 8x16 Split Block Raked.
107.	Pattern: Stone and Block Pattern 901C 8x16 Split Block Heavy Relief Concave.
108.	Pattern: Stone and Block Pattern 902 9x18 Split Block with Deep Mortar.
109.	Pattern: Stone and Block Pattern 903 8x8 Split Block.
110.	Pattern: Stone and Block Pattern 904 Ashlar Stone.
111.	Pattern: Stone and Block Pattern 904A Ashlar Stone.
112.	Pattern: Stone and Block Pattern 905 Small Aged Ashlar Stone.
113.	Pattern: Stone and Block Pattern 906 Ashlar Stone Heavy Cut.
114.	Pattern: Stone and Block Pattern 907 Coral Ashlar Stone.
115.	Pattern: Stone and Block Pattern 908 BQE Old Cut Ashlar Stone.
116.	Pattern: Stone and Block Pattern 909 Westmoreland Drystack.
117.	Pattern: Stone and Block Pattern 910 Median Barrier Drystack.
118.	Pattern: Stone and Block Pattern 910B Median Barrier Drystack.
119.	Pattern: Stone and Block Pattern 911A Large Stone Drystack.
120.	Pattern: Stone and Block Pattern 911B Large Stone Drystack.
121.	Pattern: Stone and Block Pattern 911O Large Stone Ohio Drystack.
122.	Pattern: Stone and Block Pattern 912 Valley Forge Fieldstone.
123.	Pattern: Stone and Block Pattern 912A Valley Forge Fieldstone 3/4 inch Relief.
124.	Pattern: Stone and Block Pattern 913 New York DOT Ashlar.
125.	Pattern: Stone and Block Pattern 916 Small Rustic Ashlar.
126.	Pattern: Stone and Block Pattern 917 8x8 Split Block Running Bond.
127.	Pattern: Stone and Block Pattern 918 12x24 Split Limestone Running Bond.
128.	Pattern: Stone and Block Pattern 919 Weathered Cut Ashlar.
129.	Pattern: Stone and Block Pattern 921 Split Slate.
130.	Pattern: Stone and Block Pattern 922 Cleaved Limestone.
131.	Pattern: Stone and Block Pattern 927 Atomic Ashlar.
132.	Pattern: Stone and Block Pattern 928 Slump Stone.
133.	Pattern: Stone and Block Pattern 929 8x16 Hand Chiseled Block.
134.	Pattern: Stone and Block Pattern 931 Dry Fit Ashlar.
135.	Pattern: Stone and Block Pattern 932 Random Coursed Ashlar.
136.	Pattern: Stone and Block Pattern 933 Ledgestone Drystack.
137.	Pattern: Stone and Block Pattern 934 Dry-Fit Paver.
138.	Pattern: Stone and Block Pattern 935 Castle Stone.
139.	Pattern: Stone and Block Pattern 936 3/8 inch Split Limestone.
140.	Pattern: Stone and Block Pattern 936B 3/4 inch Split Limestone.
141.	Pattern: Stone and Block Pattern 937 Mauch Chunk Drystack.
142.	Pattern: Stone and Block Pattern 938 Canal Lock Drystack.
2.6	ACCESSORY MATERIALS.
A.	Formliner Accessories: Form oil and adhesives as required for the complete form liner system as manufactured by Architectural Polymers, Inc.
1.	Release Agent: 2550 Form Oil release agent for pre-cast and cast-in-place concrete, solvent based.
2.	Filler: 75/65 RTV Urethane for repair of damaged formliners.
3.	Adhesive: Epoxy bond adhesive for fully adhering entire surfaces on steel or timber and equalizing rear of formliner.
PART 3    EXECUTION.
3.1	EXAMINATION AND PREPARATION.
A.	Verify that field measurements, surfaces, substrates, and conditions are as required, and ready to receive Work.
B.	Prepare substrates using the methods recommended by the manufacturer for achieving the best result for the substrate under the project conditions.
C.	Form Liner Preparation:
1.	Verify lines and levels of formwork and form liner patterns are within allowable tolerances.
2.	Clean liner before each use. Do not use damaged liner when continued use or repair would diminish the aesthetics of the work.
3.	The release agent to be used with the formliners should be Architectural Polymers 2550 Form Oil or Cresset Crete-Lease 880. Please take care that all sections, angles of the pattern are covered with the release agent. .
4.	Drying time for the release agents depends on ambient temperatures and air movement. Consumption is approximately 800 to 1200 sq/ft per gallon after the initial seasoning. .
D.	Do not proceed with installation until substrates have been properly prepared and deviations from manufacturer's recommended tolerances are corrected. Commencement of installation constitutes acceptance of conditions.
E.	If preparation is the responsibility of another installer, notify Architect in writing of deviations from manufacturer's recommended installation tolerances and conditions.
3.2	INSTALLATION.
A.	Install units within manufacturer's recommended tolerances. Comply with manufacturer's installation instructions and approved submittals. Refer to manufacturer's Application Guide for proper procedures for installing formliners.
B.	Store and use formliners at temperatures between 40 degrees F and 140 degrees F (4.4 degrees C and 60 degrees C).
C.	For applications where concrete temperatures will exceed 140 degrees F (60 degrees C) at the formliner face, reduce the temperature with methods as recommended by manufacturer.
D.	For applications involving multiple formliners butted together in a horizontal fashion, press the edges of the formliner together tightly to stop concrete bleeding between the formliners.
3.3	MAINTENANCE OF REUSABLE FORMLINERS.
A.	For applications with reusable formliners, comply with requirements of paragraph Delivery Storage and Handling when handling and storing units between uses. Prevent matrix build-up on the formliner surface. Excess release agent shall be removed before the form and liner is put back into service.
3.4	CLEANING AND PROTECTION.
A.	Clean exposed surfaces. Touch up, refinish, or replace damaged components in a manner acceptable to Architect.
B.	Protect installed products until completion of project.
C.	Repair or replace defective work as directed by Architect upon inspection.

END OF SECTION