SECTION 11 53 00

LABORATORY EQUIPMENT

Display hidden notes to specifier. (Don't know how? Click Here) 
 Copyright 2014 -  2018 ARCAT, Inc. - All rights reserved

PART 1    GENERAL
1.1	SECTION INCLUDES
A.	Laboratory equipment of the following types:
1.	Animal research products.
2.	Microbiological CO2 incubators.
3.	Custom biological incubators.
4.	Laminar airflow products.
5.	Compounding pharmacy equipment.
6.	Polypropylene fume hoods.
7.	Ultra-low temperature freezers.
8.	Laboratory centrifuges.
9.	Biological safety cabinets.
1.2	RELATED SECTIONS
A.	Section 26 05 00 - Common Work Results for Electrical.
1.3	REFERENCES
A.	ASTM E 84 - Standard Test Method for Surface Burning Characteristics of Building Materials.
1.4	SUBMITTALS
A.	Submit under provisions of Section 01 30 00 - Administrative Requirements.
B.	Product Data: Manufacturer's data sheets on each product to be used, including:
1.	Preparation instructions and recommendations.
2.	Storage and handling requirements and recommendations.
3.	Installation methods.
C.	Shop Drawings: provide schematics of mechanical and electrical connections.
D.	Verification Samples: For each finish product specified when different colors are available, two samples, minimum size 6 inches (150 mm) square representing actual product.
1.5	QUALITY ASSURANCE
A.	Manufacturer Qualifications: Minimum 5 years experience manufacturing similar products.
B.	Installer Qualifications: Minimum 2 years experience installing similar products.
C.	Mock-Up: Provide a mock-up for evaluation of surface preparation techniques and application workmanship.
1.	Finish areas designated by Architect.
2.	Do not proceed with remaining work until workmanship is approved by Architect.
3.	Rework mock-up area as required to produce acceptable work.
1.6	PRE-INSTALLATION MEETINGS
A.	Convene minimum two weeks prior to starting work of this section.
1.7	DELIVERY, STORAGE, AND HANDLING
A.	Deliver and store products in manufacturer's unopened packaging bearing the brand name and manufacturer's identification until ready for installation.
B.	Handling: Handle materials to avoid damage.
1.8	PROJECT CONDITIONS
A.	Maintain environmental conditions (temperature, humidity, and ventilation) within limits recommended by manufacturer for optimum results. Do not install products under environmental conditions outside manufacturer's recommended limits.
1.9	SEQUENCING
A.	Ensure that products of this section are supplied to affected trades in time to prevent interruption of construction progress.
1.10	WARRANTY
A.	Warranty: Manufacturer's warranty shall not apply to any product or part thereof which has been subject to misuse, abuse, accident, shipping damage, improper installation or service, or damage by fire, flood or acts of God. If the serial number of this product is altered, removed or defaced as to be illegible, the warranty shall be null and void in its entirety.
1.	Class II, Type A2 Bio-safety Cabinets with DC-ECM Motors:
a.	60 months (North America, Parts & Labor). 36 months parts and labor.
b.	72 months (International, Parts Only).
2.	Standard Airflow Products (BSCs) - 36 Months.
3.	Incubators - 24 Months.
4.	Freezers - 24 Months.
5.	Polypropylene Fume Hoods - 12 Months.
6.	Polypropylene Casework - 12 Months.
7.	Special Products (Determined by product built).
8.	International Warranty - 48 Months (Parts only).
9.	Refrigerated and Incubator products have a 24 month warranty.
10.	All Products sold internationally are covered with a 48 months Parts-Only warranty.
B.	Air Flow Products:
1.	Manufacturer warrants that it will repair F.O.B. its factory or furnish without charge, a similar part to replace any material in the equipment within 36 months after the date of sale:
a.	If proven to the satisfaction of the company to have been defective at the time it was sold.
b.	Failed during the covered period, provided that all parts claimed defective shall be returned, properly identified with a return authorization.
2.	Factory installed, customer specified equipment or accessories are warranted only to the extent guaranteed by the original manufacturer, and this warranty shall not apply to any portion of the equipment modified by the user/customer. Claims under this warranty should be directed to Manufacturer Technical Service Department setting forth in detail the nature of the defect, the date of the initial installation and the serial and model numbers of the equipment.
PART 2    GENERAL
2.1	MANUFACTURERS
A.	Acceptable Manufacturer: NuAire Laboratory Equipment Supply , which is located at:<BR />2100 Fernbrook Lane N.<BR />Plymouth, MN 55447 <BR />Toll Free Tel: 800-328-3352 <BR />Tel: 763-553-1270 <BR />Fax: 763-553-0459<BR />Email: request info (nuaire@nuaire.com);Web: http://www.nuaire.com 
B.	Substitutions: Not permitted.
C.	Requests for substitutions will be considered in accordance with provisions of Section 01 60 00 - Product Requirements.
2.2	ANIMAL RESEARCH PRODUCTS
A.	Animal Transfer Stations as manufactured by NuAire Laboratory Equipment Supply.
1.	AllerGard ES (Energy Saver) NU-619 Dual Access Animal Transfer Station.
a.	Model NU-619-300. 36-5/8 (930) W by 28-1/4 inches (718) D worktray dimensions.
b.	Model NU-619-400. 42-5/8 (1083) W by 28-1/4 inches (718) D worktray dimensions.
c.	Model NU-619-500. 54-5/8 (1387) W by 28-1/4 inches (718) D worktray dimensions.
d.	Provide Magnifying Glass Window.
e.	Provide One Sided Enclosure Panel w/ Stability Bracket.
f.	Provide Feed Hoppers.
g.	Provide Stainless Steel Folder Shelf.
h.	Provide Shelf Option for User Standing.
i.	Provide Light Timer.
j.	Provide Removable Divider Panel.
k.	Provide Automated Hand Sanitizer.
l.	Provide Mouse Guard.
m.	Provide Disposable Pre-filters.
n.	Provide Watering Systems.
o.	Provide Additional Outlets.
p.	Provide Custom Solutions as required or indicated.
2.	AllerGard ES (Energy Saver) NU-619 Innovive Edition Animal Transfer Station for INNOCAGE Mouse.
a.	Model NU-619-400. 42-5/8 (1083) W by 28-1/4 inches (718) D by 26 inches (659 mm) interior dimensions.
b.	Model NU-619-500. 54-5/8 (1387) W by 28-1/4 inches (718) D by 26 inches (659 mm ) interior dimensions.
c.	Provide AQUAVIVE Mouse Water Bottle Holder.
d.	Provide Magnifying Glass Window.
e.	Provide One Sided Enclosure Panel w/ Stability Bracket.
f.	Provide Feed Hoppers.
g.	Provide Stainless Steel Folder Shelf.
h.	Provide Light Timer.
i.	Provide Automated Hand Sanitizer.
j.	Provide Disposable Pre-filters.
k.	Provide Watering Systems.
l.	Additional Outlets.
m.	Provide Custom Solutions as required or indicated.
3.	AllerGard ES (Energy Saver) NU-620 High Containment Animal Transfer Station.
B.	Biological Safety Cabinets as manufactured by NuAire Laboratory Equipment Supply.
1.	LabGard ES (Energy Saver) NU-602 Class II, Type A2 Animal Handling Biosafety Cabinet.
a.	Model NU-602-400. 46-1/2 x 24-1/2 x 26-1/2 (1232 x 622 x 673) interior dimensions.
b.	Model NU-602-500. 58-1/2 x 24-1/2 x 26-1/2 (1486 x 622 x 673) interior dimensions.
c.	Model NU-602-600. 70-1/2 x 24-1/2 x 26-1/2 (1791 x 622 x 673) interior dimensions.
d.	Provide Germicidal UV Light.
e.	Provide Decorative Front Panel.
f.	Provide Metal Framed HEPA Filters.
g.	Provide Lay in Sorbent Exhaust Filter.
h.	Provide Base Stand Risers.
i.	Provide Additional Duplex Outlets.
j.	Provide GFI.
k.	Provide Exhaust Transitions.
l.	Provide Exhaust Interlocks.
m.	Provide Service Valves.
n.	Provide Water Systems.
o.	Provide IV Bar w/ 6 Hooks.
p.	Provide Custom Solutions as indicated or required.
2.	LabGard ES (Energy Saver) NU-610 Dual Access Class II, Type A2 Animal Handling Biosafety Cabinet.
a.	Model NU-610-500. 44 x 28-1/4 x 25 (1118 x 718 x 635) interior dimensions.
b.	Model NU-610-600. 64 x 28-1/4 x 25 (1626 x 718 x 635) interior dimensions.
c.	Provide Germicidal UV Light.
d.	Provide Exhaust Alarm Systems.
e.	Provide Service Valves.
f.	Provide Water Systems.
g.	Provide Exhaust Transitions.
h.	Provide Custom Solutions as indicated or required.
3.	LabGard ES (Energy Saver) NU-677 Class II, Type A2 Animal Handling Biological Safety Cabinet.
a.	Model NU-677-400. 46-3/8 x 28 x 25 (1178 x 718 x 635) Work Zone dimensions.
b.	Model NU-677-500. 58-3/8 x 28 x 25 (1483 x 718 x 635) Work Zone dimensions.
c.	Model NU-677-600. 70-3/8 x 28 x 25 (1788 x 718 x 635) Work Zone dimensions.
d.	Provide Germicidal UV Light.
e.	Provide Ground Fault Interrupter for Electrical System.
f.	Provide Additional Service Valves for Gas, Air, Vacuum.
g.	Provide Additional Outlet.
h.	Provide Alarm Systems.
i.	Provide Sinks with Hot/Cold or DI Water Faucets.
j.	Provide Storage Pull-Out Trays.
k.	Provide Lay in Sorbent Exhaust Filter.
l.	Provide Decorative Side Panels (hides plumbing fixture connections).
m.	Provide HEPA Filters 99.999% at 0.3 Micron.
n.	Provide Stainless Steel Armrest.
o.	Provide Custom Solutions as indicated or required.
C.	Bedding Waste Disposal Systems as manufactured by NuAire Laboratory Equipment Supply.
1.	AllerGard ES (Energy Saver) NU-607 Class I Animal Bedding Disposal Station.
2.	Interior Dimensions (W x D x H): 43-1/4 inches x 27-1/2 inches x 24 inches (1099 mm x 699 mm x 610 mm).
3.	Chute Design Configuration: Round.
4.	Chute Design Configuration: Rectangle.
5.	Chute Design Configuration: Double Rectangle.
6.	Exhaust HEPA Filter: 99.99% at 0.3 Micron.
7.	FlowGard Control System: A pressure monitor constantly inspects plenum pressure alerting to any imbalances in airflow.
8.	Energy Saver Motor: An ultra high efficiency motor saves on your energy bills while increasing filter life lowering your total cost of ownership.
9.	Dynamic Air Barrier: Strong inflow air velocity at 100 fpm (.51 m/s) creates personnel protection.
10.	Provide Spare Disposal Bags.
11.	Provide Spare Disposal Can.
12.	Provide Replacement Filters.
D.	Portable Animal Cleanroom Enclosure as manufactured by NuAire Laboratory Equipment Supply.
1.	LabGard NU-605 as manufactured by NuAire Laboratory Equipment Supply.
a.	Model NU-605-500: 66 inches W x 79 inches D x 78 inches H (1676 mm x 2007 mm x 1981 mm).
b.	Model NU-605-600: 78 inches W x 79 inches D x 78 inches H (1981 mm x 2007 mm x 1981 mm).
2.	Recycled Airflow: The LabGard 605 creates a mini clean room through recirculated airflow. The recycling feature produces ultra clean air for both personnel and animals.
3.	HEPEX Zero Leak Airflow System: The HEPEX plenum inflates to provide quiet uniform air without transferring vibration. Positive pressure chambers and ducts shall be surrounded by negative pressure eliminating potential leaks. HEPEX fabrics shall be durable and flameproof, provide a barrier against water, gases, fluid, and dust as well as resistance to chemicals, oils, and greases. It shall hold antibacterial properties and is impregnable meaning harmful materials become trapped in the filters.
4.	Provide Additional Stainless Steel Rack.
5.	Provide Additional Stainless Steel Shelves.
6.	Provide Clean Room Canopy.
E.	Clean Air Workstation as manufactured by NuAire Laboratory Equipment Supply.
1.	LabGard NU-603 Reverse Horizontal Flow Safety Cabinet.
a.	Model NU-603-424: 46-1/2 inches W x 24 inches D x 24 inches H (1181 mm x 610 mm x 610 mm) interior dimensions.
b.	Model NU-603-430: 46-1/2 inches W x 24 inches D x 30 inches H (1181 mm x 610 mm x 762 mm) interior dimensions.
c.	Model NU-603-624: 70-1/2 inches W x 24 inches D x 24 inches H (1791 mm x 610 mm x 610 mm) interior dimensions.
d.	Model NU-603-630: 70-1/2 inches W x 24 inches D x 30 inches H (1791 mm x 610 mm x 762 mm) interior dimensions.
2.	Dynamic Air Barrier: Strong inflow air velocity of 100 fpm (0.51 m/s) creates maximum personnel protection.
3.	Essentials Control System: Simple switches control the blower, lights, outlets while a magnehelic gauge measures plenum performance.
4.	Pre-filter System Extends Life of HEPA Filters: Air enters a pre-filtration system to capture animal hair, dander, and bedding before it enters the equipment's plenum extending the life of the exhaust and supply HEPA filters.
5.	Provide Germicidal UV Light.
6.	Provide Service Valves.
7.	Provide Watering Systems.
8.	Provide Stainless Steel Work Surface.
9.	Provide Storage Pull Out Trays.
10.	Provide Base Stands.
11.	Provide Custom Solutions as indicated or required.
2.3	MICROBIOLOGICAL CO2 INCUBATORS
A.	Direct Heat (Air Jacket) CO2 Incubators as manufactured by NuAire Laboratory Equipment Supply.
1.	In-VitroCell ES (Energy Saver) NU-5800 Direct Heat CO2 Incubator.
a.	Chamber Dimensions (W x D x H) in. (mm): 21 inches x 20 inches x 28-1/2 inches (540 x 509 x 724).
b.	NuTouch Intelligent Interface.
c.	Infrared (IR) Sensor.
d.	Constant Contamination Control (C3):
1)	Closed Loop HEPA Filtration.
2)	ISO Class 5 Cleanroom Conditions.
3)	Temperature Uniformity.
e.	Remote monitoring and communication 
1)	Remote alarm connection 
2)	4 to 20 mA connection 
3)	RS232 connection 
f.	Provide Copper Surfaces.
g.	Provide Automatic CO2 Tank Switch (External).
h.	Provide CO2 Tank Alarm.
i.	Provide Left Hinge Door Swing.
j.	Provide Additional Shelves with Slide Brackets.
k.	Provide CO2 Analyzer Fyrite Kit (Dry) 0-20%.
l.	Provide Replacement Fluid for CO2 Analyzer.
m.	Provide Surge Protector.
n.	Provide CO2 Regulator (2 Stage).
o.	Provide Gas tight 6 section door 
p.	Provide Custom Solutions as required or as indicated.
2.	In-VitroCell ES (Energy Saver) NU-5810 Direct Heat CO2 Incubator with Dual Sterilization Cycles.
a.	Chamber Dimensions (W x D x H) in. (mm): 21 inches x 20 inches x 28-1/2 inches (540 x 509 x 724).
b.	Dual Sterilization Cycles.
c.	NuTouch Intelligent Interface.
d.	Infrared (IR) Sensor.
e.	Closed Loop HEPA Filtration.
f.	ISO Class 5 Cleanroom Conditions.
g.	Single Beam, Dual Wave Infrared (IR) Sensor.
h.	Temperature Uniformity.
i.	Incubator Humidity.
j.	Remote monitoring and communication 
1)	Remote alarm connection 
2)	4 to 20 mA connection 
3)	RS232 connection 
k.	Provide Copper Surfaces.
l.	Provide Automatic CO2 Tank Switch (External).
m.	Provide CO2 Tank Alarm.
n.	Provide Left Hinge Door Swing.
o.	Provide Additional Shelves with Slide Brackets.
p.	Provide CO2 Analyzer Fyrite Kit (Dry) 0-20%.
q.	Provide Replacement Fluid for CO2 Analyzer.
r.	Provide Surge Protector.
s.	Provide CO2 Regulator (2 Stage).
t.	Provide Gas tight 6 section door 
u.	Provide Custom Solutions as required or as indicated.
3.	In-VitroCell ES (Energy Saver) NU-5820 Direct Heat CO2 Incubator featuring Relative Humidity (RH) Control.
a.	Chamber Dimensions (W x D x H) in. (mm): 21 inches x 20 inches x 28-1/2 inches (540 x 509 x 724).
b.	Relative Humidity (RH) Control.
c.	Dual Sterilization Cycles.
d.	NuTouch Intelligent Interface.
e.	Infrared (IR) Sensor.
f.	Closed Loop HEPA Filtration.
g.	ISO Class 5 Cleanroom Conditions.
h.	Single Beam, Dual Wave Infrared (IR) Sensor.
i.	Temperature Uniformity.
j.	Remote monitoring and communication 
1)	Remote alarm connection 
2)	4 to 20 mA connection 
3)	RS232 connection 
k.	Provide Copper Surfaces.
l.	Provide Automatic CO2 Tank Switch (External).
m.	Provide CO2 Tank Alarm.
n.	Provide Left Hinge Door Swing.
o.	Provide Additional Shelves with Slide Brackets.
p.	Provide CO2 Analyzer Fyrite Kit (Dry) 0-20%.
q.	Provide Replacement Fluid for CO2 Analyzer.
r.	Provide Surge Protector.
s.	Provide CO2 Regulator (2 Stage).
t.	Provide Gas tight 6 section door 
u.	Provide Custom Solutions as required or as indicated.
4.	In-VitroCell ES (Energy Saver) NU-5831 Direct Heat Hypoxic CO2 Incubator featuring Zirconia Oxygen Control.
a.	Chamber Dimensions (W x D x H) in. (mm): 21 inches x 20 inches x 28-1/2 inches (540 x 509 x 724).
b.	Hypoxic Zirconia Ceramic O2 Sensor Control.
c.	Dual Sterilization Cycles.
d.	NuTouch Intelligent Interface.
e.	Constant Contamination Control (C3):
1)	Closed Loop HEPA Filtration.
2)	ISO Class 5 Cleanroom Conditions.
3)	Temperature Uniformity.
f.	Single Beam, Dual Wave Infrared (IR) Sensor.
g.	Incubator Humidity.
h.	Remote monitoring and communication 
1)	Remote alarm connection 
2)	4 to 20 mA connection 
3)	RS232 connection 
i.	Provide Copper Surfaces.
j.	Provide Automatic CO2 Tank Switch (External).
k.	Provide CO2 Tank Alarm.
l.	Provide Left Hinge Door Swing.
m.	Provide Additional Shelves with Slide Brackets.
n.	Provide CO2 Analyzer Fyrite Kit (Dry) 0-20%.
o.	Provide Replacement Fluid for CO2 Analyzer.
p.	Provide Surge Protector.
q.	Provide CO2 Regulator (2 Stage).
r.	Provide Gas tight 6 section door 
s.	Provide Custom Solutions as required or as indicated.
5.	In-VitroCell ES (Energy Saver) NU-5841 Direct Heat Hypoxic CO2 Incubator featuring Humidity and Zirconia Oxygen Control.
a.	Chamber Dimensions (W x D x H) in. (mm): 21 inches x 20 inches x 28-1/2 inches (540 x 509 x 724).
b.	Hypoxic Zirconia Ceramic O2 Sensor Control.
c.	Dual Sterilization Cycles.
d.	NuTouch Intelligent Interface.
e.	Constant Contamination Control (C3):
1)	Closed Loop HEPA Filtration.
2)	ISO Class 5 Cleanroom Conditions.
3)	Temperature Uniformity.
f.	Single Beam, Dual Wave Infrared (IR) Sensor.
g.	Relative Humidity (RH) Control. 
h.	Incubator Humidity.
i.	Remote monitoring and communication 
1)	Remote alarm connection 
2)	4 to 20 mA connection 
3)	RS232 connection 
j.	Provide Copper Surfaces.
k.	Provide Automatic CO2 Tank Switch (External).
l.	Provide CO2 Tank Alarm.
m.	Provide Left Hinge Door Swing.
n.	Provide Additional Shelves with Slide Brackets.
o.	Provide CO2 Analyzer Fyrite Kit (Dry) 0-20%.
p.	Provide Replacement Fluid for CO2 Analyzer.
q.	Provide Surge Protector.
r.	Provide CO2 Regulator (2 Stage).
s.	Provide Gas tight 6 section door 
t.	Provide Custom Solutions as required or as indicated.
6.	In-VitroCell ES (Energy Saver) NU-5700 Direct Heat CO2 Incubator. 
a.	Chamber Dimensions (W x D x H) in. (mm): 20-1/4 inches x 20-11/16 inches x 24 inches (514 x 525 x 610). 
b.	NuTouch Intelligent Interface. 
c.	Infrared (IR) Sensor. 
d.	Constant Contamination Control  (C3): 
1)	Closed Loop HEPA Filtration. 
2)	ISO Class 5 Cleanroom Conditions. 
3)	Temperature Uniformity. 
e.	Remote monitoring and communication 
1)	Remote alarm connection 
2)	4 to 20 mA connection 
3)	RS232 connection 
f.	Provide Copper Surfaces. 
g.	Provide Automatic CO2 Tank Switch (External). 
h.	Provide CO2 Tank Alarm. 
i.	Provide Left Hinge Door Swing. 
j.	Provide Additional Shelves with Slide Brackets. 
k.	Provide CO2 Analyzer Fyrite Kit (Dry) 0-20%. 
l.	Provide Replacement Fluid for CO2 Analyzer. 
m.	Provide Surge Protector. 
n.	Provide CO2 Regulator (2 Stage). 
o.	Provide Gas tight 4 section door 
p.	Provide Custom Solutions as required or as indicated. 
7.	In-VitroCell ES (Energy Saver) NU-5710 Direct Heat CO2 Incubator with Dual Sterilization Cycles.
a.	Chamber Dimensions (W x D x H) in. (mm): 20-1/4 inches x 20-11/16 inches x 24 inches (514 x 525 x 610).
b.	Dual Sterilization Cycles.
c.	NuTouch Intelligent Interface.
d.	Infrared (IR) Sensor. 
e.	Closed Loop HEPA Filtration. 
f.	ISO Class 5 Cleanroom Conditions. 
g.	Single Beam, Dual Wave Infrared (IR) Sensor. 
h.	Temperature Uniformity. 
i.	Incubator Humidity.
j.	Remote monitoring and communication 
1)	Remote alarm connection 
2)	4 to 20 mA connection 
3)	RS232 connection 
k.	Provide Copper Surfaces. 
l.	Provide Automatic CO2 Tank Switch (External). 
m.	Provide CO2 Tank Alarm. 
n.	Provide Left Hinge Door Swing. 
o.	Provide Additional Shelves with Slide Brackets. 
p.	Provide CO2 Analyzer Fyrite Kit (Dry) 0-20%. 
q.	Provide Replacement Fluid for CO2 Analyzer. 
r.	Provide Surge Protector. 
s.	Provide CO2 Regulator (2 Stage). 
t.	Provide Gas tight 4 section door 
u.	Provide Custom Solutions as required or as indicated. 
8.	In-VitroCell ES (Energy Saver) NU-5720 Direct Heat CO2 Incubator featuring Relative Humidity (RH) Control.
a.	Chamber Dimensions (W x D x H) in. (mm): 20-1/4 inches x 20-11/16 inches x 24 inches (514 x 525 x 610). 
b.	Relative Humidity (RH) Control. 
c.	Dual Sterilization Cycles. 
d.	NuTouch Intelligent Interface. 
e.	Infrared (IR) Sensor. 
f.	Closed Loop HEPA Filtration.
g.	ISO Class 5 Cleanroom Conditions.
h.	Single Beam, Dual Wave Infrared (IR) Sensor.
i.	Temperature Uniformity.
j.	Remote monitoring and communication 
1)	Remote alarm connection 
2)	4 to 20 mA connection 
3)	RS232 connection
k.	Provide Copper Surfaces.
l.	Provide Automatic CO2 Tank Switch (External).
m.	Provide CO2 Tank Alarm.
n.	Provide Left Hinge Door Swing.
o.	Provide Additional Shelves with Slide Brackets.
p.	Provide CO2 Analyzer Fyrite Kit (Dry) 0-20%.
q.	Provide Replacement Fluid for CO2 Analyzer.
r.	Provide Surge Protector.
s.	Provide CO2 Regulator (2 Stage).
t.	Provide Gas tight 4 section door 
u.	Provide Custom Solutions as required or as indicated.
9.	In-VitroCell ES (Energy Saver) NU-5731 Direct Heat Hypoxic CO2 Incubator featuring Zirconia Oxygen Control. 
a.	Chamber Dimensions (W x D x H) in. (mm): 20-1/4 inches x 20-11/16 inches x 24 inches (514 x 525 x 610). 
b.	Hypoxic Zirconia Ceramic O2 Sensor Control. 
c.	Dual Sterilization Cycles. 
d.	NuTouch Intelligent Interface. 
e.	Constant Contamination Control (C3): 
1)	Closed Loop HEPA Filtration. 
2)	ISO Class 5 Cleanroom Conditions. 
3)	Temperature Uniformity. 
f.	Single Beam, Dual Wave Infrared (IR) Sensor. 
g.	Incubator Humidity. 
h.	Remote monitoring and communication 
1)	Remote alarm connection 
2)	4 to 20 mA connection 
3)	RS232 connection 
i.	Provide Copper Surfaces. 
j.	Provide Automatic CO2 Tank Switch (External). 
k.	Provide CO2 Tank Alarm. 
l.	Provide Left Hinge Door Swing. 
m.	Provide Additional Shelves with Slide Brackets. 
n.	Provide CO2 Analyzer Fyrite Kit (Dry) 0-20%. 
o.	Provide Replacement Fluid for CO2 Analyzer. 
p.	Provide Surge Protector. 
q.	Provide CO2 Regulator (2 Stage). 
r.	Provide Gas tight 4 section door 
s.	Provide Custom Solutions as required or as indicated.
10.	In-VitroCell ES (Energy Saver) NU-5741 Direct Heat Hypoxic CO2 Incubator featuring Humidity and Zirconia Oxygen Control.
a.	Chamber Dimensions (W x D x H) in. (mm): 20-1/4 inches x 20-11/16 inches x 24 inches (514 x 525 x 610).
b.	Hypoxic Zirconia Ceramic O2 Sensor Control.
c.	Dual Sterilization Cycles.
d.	NuTouch Intelligent Interface.
e.	Constant Contamination Control (C3):
1)	Closed Loop HEPA Filtration.
2)	ISO Class 5 Cleanroom Conditions.
3)	Temperature Uniformity.
f.	Single Beam, Dual Wave Infrared (IR) Sensor.
g.	Relative Humidity (RH) Control.
h.	Incubator Humidity.
i.	Remote monitoring and communication 
1)	Remote alarm connection 
2)	4 to 20 mA connection 
3)	RS232 connection 
j.	Provide Copper Surfaces.
k.	Provide Automatic CO2 Tank Switch (External).
l.	Provide CO2 Tank Alarm.
m.	Provide Left Hinge Door Swing.
n.	Provide Additional Shelves with Slide Brackets.
o.	Provide CO2 Analyzer Fyrite Kit (Dry) 0-20%.
p.	Provide Replacement Fluid for CO2 Analyzer.
q.	Provide Surge Protector.
r.	Provide CO2 Regulator (2 Stage).
s.	Provide Gas tight 4 section door 
t.	Provide Custom Solutions as required or as indicated
B.	Water Jacketed CO2 Incubators as manufactured by NuAire Laboratory Equipment Supply.
1.	In-VitroCell ES (Energy Saver) NU-8600 water Jacket CO2 Incubator.
a.	Chamber Dimensions (W x D x H) in. (mm): 20-3/8 inches x 20-5/8 inches x 24 inches (517x 524 x 610).
b.	NuTouch Intelligent Interface.
c.	Infrared (IR) Sensor.
d.	Constant Contamination Control (C3):
1)	Closed Loop HEPA Filtration. 
2)	ISO Class 5 Cleanroom Conditions. 
3)	Temperature Uniformity. 
e.	Single Beam, Dual Wave Infrared (IR) CO2 Sensor. 
f.	Incubator Humidity. 
g.	Remote monitoring and communication 
1)	Remote alarm connection 
2)	4 to 20 mA connection 
3)	RS232 connection 
h.	Provide Copper Surfaces. 
i.	Provide Automatic CO2 Tank Switch (External). 
j.	Provide CO2 Tank Alarm. 
k.	Provide Left Hinge Door Swing. 
l.	Provide Additional Shelves with Slide Brackets. 
m.	Provide CO2 Analyzer Fyrite Kit (Dry) 0-20%. 
n.	Provide Replacement Fluid for CO2 Analyzer. 
o.	Provide Surge Protector. 
p.	Provide CO2 Regulator (2 Stage). 
q.	Provide Humidity Display. 
r.	Provide Gas tight 4 section door 
s.	Provide water jacket cooling coil to control temperature down to 5 deg. C. 
t.	Provide Custom Solutions as required or as indicated. 
2.	In-VitroCell ES (Energy Saver) NU-8631 Water Jacket Hypoxic CO2 Incubator featuring Zirconia Oxygen Control. 
a.	Chamber Dimensions (W x D x H) in. (mm): 20-3/8 inches x 20-5/8 inches x 24 inches (517 x 524 x 610). 
b.	Hypoxic Zirconia Ceramic O2 Sensor Control. 
c.	NuTouch Intelligent Interface. 
d.	Constant Contamination Control (C3): 
1)	Closed Loop HEPA Filtration. 
2)	ISO Class 5 Cleanroom Conditions. 
3)	Temperature Uniformity. 
e.	Single Beam, Dual Wave Infrared (IR) CO2 Sensor. 
f.	Incubator Humidity. 
g.	Remote monitoring and communication 
1)	Remote alarm connection 
2)	4 to 20 mA connection 
3)	RS232 connection 
h.	Provide Copper Surfaces. 
i.	Provide Automatic CO2 Tank Switch (External). 
j.	Provide CO2 Tank Alarm. 
k.	Provide Left Hinge Door Swing. 
l.	Provide Additional Shelves with Slide Brackets. 
m.	Provide CO2 Analyzer Fyrite Kit (Dry) 0-20%. 
n.	Provide Replacement Fluid for CO2 Analyzer. 
o.	Provide Surge Protector. 
p.	Provide CO2 Regulator (2 Stage). 
q.	Provide Gas tight 4 sectioned door 
r.	Provide water jacket cooling coil to control temperature down to 5 deg. C. 
s.	Provide Custom Solutions as required or as indicated. 
2.4	CUSTOM BIOLOGICAL INCUBATORS
A.	Laminar Airflow Workstations as manufactured by NuAire Laboratory Equipment Supply.
1.	AireGard ES (Energy Saver) NU-101 Vertical Airflow Clean Workstation.
a.	Airflow Design: Total Exhaust.
b.	Airflow Design: Exhaust / Recirculation.
c.	Airflow Design: Open Base.
d.	Airflow Design: Wash Out.
e.	Airflow Design: Perforated Wash Through.
f.	Essentials Control System.
g.	HEPEX Zero Leak Airflow System.
h.	Attenumount: Vibration and sound control.
i.	Airflow System.
j.	99.99% HEPA Filtration.
k.	Air Intake Grill and Pre-Filter.
l.	Cool White Fluorescent Lighting.
m.	Centrally Located Control Center.
n.	Powder Coat Urethane Finish.
o.	Interior Cold-Rolled Finished Steel.
p.	Provide Duplex outlets.
q.	Provide Exhaust Chambers.
r.	Provide Exhaust Transitions.
s.	Provide Stainless Steel Interior.
t.	Provide IV Bar.
u.	Provide Ultraviolet Lights.
v.	Provide Service valves for Air, Gas, Vacuum.
w.	Provide Side Panels.
x.	Provide Tables and Table Tops.
y.	Provide Stainless Steel work Surfaces.
z.	Provide Increased work Zone Height.
aa.	Provide Custom Solutions.
B.	Biological Safety Cabinets as manufactured by NuAire Laboratory Equipment Supply.
1.	AutoLabGard ES (Energy Saver) NU-125 Mini-Room Class II, Type A2 Biosafety Cabinet.
a.	Model NU-125-436: 4 ft. (1.2 m).
b.	Model NU-125-636: 6 ft. (1.8 m).
c.	Model NU-125-648: 6 ft. (1.8 m).
d.	Model NU-125-836: 8 ft. (2.4 m).
e.	Model NU-125-848: 8 ft. (2.4 m).
f.	Model NU-125-1036: 10 ft. (3 m).
g.	Model NU-125-1048: 10 ft. (3 m).
h.	Model NU-125: Custom Dimensions.
i.	Essentials Control System.
j.	Energy Saver Motor.
k.	TruLaminar Airflow.
l.	Dynamic Air Barrier.
m.	HEPEX Zero Leak Airflow System.
n.	Attenumount: Vibration and sound control.
o.	Airflow System.
p.	Provide Stainless Steel Portable Table w/ Auto Life & Casters.
q.	Provide Exhaust Transitions.
r.	Provide Additional Duplex Outlets.
s.	Provide Service Valves.
t.	Provide Custom Solutions.
2.	LabGard ES (Energy Saver) NU-S425 Custom Designed Class II, Type A2 Biosafety Cabinet.
a.	Built for your Application.
b.	TruLaminar Airflow. 
c.	HEPEX Zero Leak Airflow System.
3.	LabGard ES (Energy Saver) NU-S430 Custom Designed Class II, Type B2 Biosafety Cabinet.
a.	Built for your Application.
b.	TruLaminar Airflow.
c.	HEPEX Zero Leak Airflow System.
2.5	LAMINAR AIRFLOW PRODUCTS
A.	Ceiling Mounted Air Showers as manufactured by NuAire Laboratory Equipment Supply.
1.	Model AireGard NU-105 Air Cleaning Ceiling Module.
a.	Size: NU-105-400.
b.	Size: NU-105-424.
c.	Size: NU-105-430.
d.	Size: NU-105-530.
e.	Size: NU-105-630.
f.	Cleanroom Creating Air Shower.
g.	Single-Pass Air Shower.
h.	Pre-filter System Extends Life of HEPA Filters.
i.	Exhaust HEPA Filter 99.99% at 0.3 Microns.
j.	Flow Control Valve.
k.	Bottom Filter Service.
l.	16 Gauge Welded Construction.
m.	Provide Fluorescent Lighting.
n.	Provide Duplex Outlets.
o.	Provide Custom Solutions.
B.	Horizontal Laminar Airflow Workstations as manufactured by NuAire Laboratory Equipment Supply.
1.	AireGard ES (Energy Saver) NU-201 Table Top Horizontal Airflow Workstation.
a.	Model/ Exterior Dimensions/ Interior Dimensions/ Weight.
b.	Model NU-201-224/ 2 ft. (0.6 m)/ 26 x 32 x 46 (660 x 813 x 1168) / 23 3/4 x 20 x 22 3/8 (603 x 508 x 568)/ 255 lbs. / 116 kg.
c.	Model NU-201-230/ 2 ft. (0.6 m)/ 26 x 32 x 52 (660 x 813 x 1321)/ 23 3/4 x 20 x 28 3/8 (603 x 508 x 721)/ 255 lbs. / 116 kg.
d.	Model NU-201-324/ 3 ft. (0.9 m)/ 38 x 32 x 46 (965 x 813 x 1168)/ 34 3/4 x 20 x 22 3/8 (883 x 508 x 568)/ 350 lbs. / 159 kg.
e.	Model NU-201-330/ 3 ft. (0.9 m)/ 38 x 32 x 52 (965 x 813 x 1321)/ 34 3/4 x 20 x 28 3/8 (883 x 508 x 721)/ 350 lbs. / 159 kg.
f.	Model NU-201-336/ 3 ft. (0.9 m)/ 38 x 32 x 58 (965 x 813 x 1473)/ 34 3/4 x 20 x 34 3/8 (883 x 508 x 873)/ 350 lbs. / 159 kg.
g.	Model NU-201-424/ 4 ft. (1.2 m)/ 50 x 32 x 46 (1270 x 813 x 1168)/ 46 3/4 x 20 x 22 3/8 (1187 x 508 x 568)/ 380 lbs. / 172 kg.
h.	Model NU-201-430/ 4 ft. (1.2 m)/ 50 x 32 x 52 (1270 x 813 x 1321)/ 46 3/4 x 20 x 28 3/8 (1187 x 508 x 721)/ 380 lbs. / 172 kg.
i.	Model NU-201-436/ 4 ft. (1.2 m) / 50 x 32 x 58 (1270 x 813 x 1473)/ 46 3/4 x 20 x 34 3/8 (1187 x 508 x 873)/ 380 lbs. / 172 kg.
j.	Model NU-201-524/ 5 ft. (1.5 m)/ 62 x 32 x 46 (1575 x 813 x 1168)/ 58 3/4 x 20 x 22 3/8 (1492 x 508 x 568)/ 520 lbs. / 236 kg.
k.	Model NU-201-530/ 5 ft. (1.5 m)/ 62 x 32 x 52 (1575 x 813 x 1321)/ 58 3/4 x 20 x 28 3/8 (1492 x 508 x 721)/ 520 lbs. / 236 kg.
l.	Model NU-201-536/ 5 ft. (1.5 m)/ 62 x 32 x 58 (1575 x 813 x 1473)/ 58 3/4 x 20 x 34 3/8 (1492 x 508 x 873)/ 520 lbs. / 236 kg.
m.	Model NU-201-624/ 6 ft. (1.8 m)/ 74 x 32 x 46 (1880 x 813 x 1168)/ 70 3/4 x 20 x 22 3/8 (1797 x 508 x 568)/ 550 lbs. / 249 kg.
n.	Model NU-201-630/ 6 ft. (1.8 m)/ 74 x 32 x 52 (1880 x 813 x 1321)/ 70 3/4 x 20 x 28 3/8 (1797 x 508 x 721)/ 550 lbs. / 249 kg.
o.	Model NU-201-636/ 6 ft. (1.8 m)/ 74 x 32 x 58 (1880 x 813 x 1473)/ 70 3/4 x 20 x 34 3/8 (1797 x 508 x 873)/ 550 lbs. / 249 kg.
p.	Model NU-201-830/ 8 ft. (2.4 m)/ 98 x 32 x 52 (2489 x 813 x 1321)/ 94 3/4 x 20 x 28 3/8 (2397 x 508 x 721)/ 760 lbs. / 345 kg.
q.	Essentials Control System.
r.	Energy Saver Motor.
s.	Experience Ergonomics.
t.	TruLaminar Airflow.
u.	HEPEX Zero Leak Airflow System.
v.	Class 100 Air Quality.
w.	Clear Top / Side Acrylic Panels.
x.	Textured Powder Coat Urethane Finish.
y.	Smooth White Formica Work Surface.
z.	Front Maintenance.
aa.	Florescent Lighting.
ab.	Protective Grill.
ac.	Glass Disposable Pre-filter.
ad.	Base Support Stands.
ae.	Germicidal UV Light.
af.	Vinyl Curtain - Front Closure for UV Light.
ag.	Duplex Outlets.
ah.	Service Valves.
ai.	GFI.
aj.	IV Bar w/ 6 Hooks.
ak.	Storage Trays.
al.	Stainless Steel Work Surface.
am.	Stainless Steel Sidewalls.
an.	Seismic Brackets.
ao.	Custom Solutions.
2.	AireGard ES (Energy Saver) NU-301 Console Horizontal Airflow Workstation.
a.	Model/ Exterior Dimensions/ Interior Dimensions/ Weight.
b.	NU-301-330/ 3 ft. (0.9 m)/ 38 x 32 x 72 1/2 in. (965 x 813 x 1842 mm)/ 34 3/4 x 20 x 28 3/8 in. (883 x 508 x 721 mm)/ 410 lbs. / 186 kg.
c.	NU-301-424/ 4 ft. (1.2 m)/ 50 x 32 x 66 1/2 in. (1270 x 813 x 1689 mm)/ 46 3/4 x 20 x 22 3/8 in. (1187 x 508 x 568 mm)/ 470 lbs. / 213 kg.
d.	NU-301-430/ 4 ft. (1.2 m)/ 50 x 32 x 72 1/2 in. (1270 x 813 x 1842 mm)/ 46 3/4 x 20 x 28 3/8 in. (1187 x 508 x 721 mm)/ 470 lbs. / 213 kg.
e.	NU-301-436/ 4 ft. (1.2 m)/ 50 x 32 x 78 1/2 in. (1270 x 813 x 1994 mm)/ 46 3/4 x 20 x 34 3/8 in. (1187 x 508 x 873 mm)/ 470 lbs. / 213 kg.
f.	NU-301-530/ 5 ft. (1.5 m)/ 62 x 32 x 72 1/2 in. (1575 x 813 x 1842 mm)/ 58 3/4 x 20 x 28 3/8 in. (1492 x 508 x 721 mm)/ 525 lbs. / 238 kg.
g.	NU-301-536/ 5 ft. (1.5 m)/ 62 x 32 x 78 1/2 in. (1575 x 813 x 1994 mm)/ 58 3/4 x 20 x 34 3/8 in. (1492 x 508 x 873 mm)/ 525 lbs. / 238 kg.
h.	NU-301-624/ 6 ft. (1.8 m)/ 74 x 32 x 66 1/2 in. (1880 x 813 x 1689 mm)/ 70 3/4 x 20 x 22 3/8 in. (1797 x 508 x 568 mm)/ 650 lbs. / 295 kg.
i.	NU-301-630/ 7 ft. (1.8 m)/ 74 x 32 x 72 1/2 in. (1880 x 813 x 1842 mm)/ 70 3/4 x 20 x 28 3/8 in. (1797 x 508 x 721 mm) 650 lbs. / 295 kg.
j.	NU-301-636/ 6 ft. (1.8 m)/ 74 x 32 x 78 1/2 in. (1880 x 813 x 1994 mm)/ 70 3/4 x 20 x 34 3/8 in. (1797 x 508 x 873 mm)/ 650 lbs. / 295 kg.
k.	NU-301-648/ 6 ft. (1.8 m)/ 74 x 32 x 90 1/2 in. (1880 x 813 x 2299 mm)/ 70 3/4 x 20 x 46 3/8 in. (1797 x 508 x 1178 mm)/ 650 lbs. / 295 kg.
l.	NU-301-830/ 8 ft. (2.4 m)/ 98 x 32 x 72 1/2 in. (2489 x 813 x 1841 mm)/ 94 3/4 x 20 x 28 3/8 in. (2397 x 508 x 721 mm)/ 940 lbs. / 426 kg.
m.	Essentials Control System.
n.	Energy Saver Motor.
o.	Experience Ergonomics.
p.	TruLaminar Airflow.
q.	HEPEX Zero Leak Airflow System Class 100 Air Quality.
r.	Clear Top / Side Acrylic Panels.
s.	Textured Powder Coat Urethane Finish.
t.	Smooth White Formica Work Surface.
u.	Front Maintenance.
v.	Florescent Lighting.
w.	Protective Grill.
x.	Glass Disposable Pre-filter.
y.	Leg Levelers.
z.	Provide Germicidal UV Light.
aa.	Provide Vinyl Curtain - Front Closure for UV Light.
ab.	Provide Casters.
ac.	Provide Duplex Outlets.
ad.	Provide Service Valves.
ae.	Provide GFI.
af.	Provide IV Bar w/ 6 Hooks.
ag.	Provide Storage Trays.
ah.	Provide Stainless Steel Work Surface.
ai.	Provide Stainless Steel Sidewalls.
aj.	Provide Seismic Brackets.
ak.	Provide Custom Solutions.
C.	Portable Mobile Filtration Units as manufactured by NuAire Laboratory Equipment Supply.
1.	AireGard ES (Energy Saver) NU-114 Portable Air Scrubber.
a.	Exterior Dimensions (W x D x H) in. (mm): 26 1/2 x 26 x 55 5/8 (673 x 660 x 1413).
b.	Weight: 270 lbs. / 122 kg.
c.	Inflow Velocity: 90 fpm (0.46 m/s).
d.	Quality Assurance: UL, UL-C.
D.	Vertical Laminar Airflow Workstation as manufactured by NuAire Laboratory Equipment Supply.
1.	Model AireGard ES (Energy Saver) NU-126 Vertical Airflow Workstation.
a.	Model NU-126-300.
b.	Model NU-126-400.
c.	Model NU-126-600.
d.	FlowGard Control System.
e.	Energy Saver Motor.
f.	Experience Ergonomics.
g.	TruLaminar Airflow.
h.	Class 5 Air Quality.
i.	Cool White Fluorescent Lighting.
j.	Clear Acrylic Side Walls.
k.	Hinged Clear Polycarbonate Viewing Window.
l.	Two Service Ports.
m.	99.99% at 0.3 Micron Supply HEPA Filter.
n.	Fiberglass Pre-Filter.
o.	White Formica Work Surface.
p.	Provide Germicidal UV Light w/ Front Enclosure.
q.	Provide Service Valves.
r.	Provide Stainless Steel Work Surface.
s.	Provide IV Bar w/ 6 Hooks.
t.	Provide Base Support Stands.
u.	Provide Seismic Brackets.
v.	Provide Custom Solution.
2.6	COMPOUNDING PHARMACY EQUIPMENT
A.	Compounding Aseptic (CAI) as manufactured by NuAire Laboratory Equipment Supply.
1.	Model PharmaGard ES (Energy Saver) NU-PR797 Compounding Aseptic Isolator.
a.	Model NU-PR797-400. 4 feet (1219 mm).
b.	Model NU-PR797-600. 6 feet (1829 mm).
c.	Experience Ergonomics.
d.	Quick Change Sharps and Waste.
e.	Counter Balance Inner Transfer Window.
f.	Sliding Work Tray.
g.	Energy Saver Motor.
h.	TruLaminar Airflow.
i.	HEPEX Zero Leak Airflow System.
j.	Attenumount: Vibration and sound control.
k.	Provide Bench Mount Support.
l.	Provide Telescoping Basestand.
m.	Provide Auto Lift Basestand.
n.	Provide Additional IV Bar w/ 6 Hooks.
o.	Provide Cord Pass Through.
p.	Provide Pull Out Stainless Steel Tray.
q.	Provide Storage Trays.
r.	Provide Right Side Transfer Compartment.
s.	Provide Dual Side Transfer Compartments (6 ft. Model Only).
t.	Provide Three or Four Glove Ports (6 ft. Model Only).
u.	Provide Additional Hospital Grade Duplex.
v.	Provide PharmaGard Digital Monitor.
w.	Provide Seismic Brackets.
x.	Provide Custom Solutions.
B.	Compounding Aseptic Containment (CACI) as manufactured by NuAire Laboratory Equipment Supply.
1.	PharmaGard ES (Energy Saver) NU-NR797 Recirculating Aseptic Containment Isolator.
a.	Model NU-NR797-400.
b.	Model NU-NR797-600.
c.	Experience Ergonomics.
d.	Quick Change Sharps and Waste.
e.	Counter Balance Inner Transfer Window.
f.	Energy Saver Motor.
g.	TruLaminar Airflow.
h.	HEPEX Zero Leak Airflow System.
i.	Attenumount: Vibration and sound control.
j.	Provide Bag-In Bag-Out Exhaust HEPA Filter.
k.	Provide Bench Mount Support.
l.	Provide Telescoping Basestand.
m.	Provide Auto Lift Basestand.
n.	Provide Additional IV Bar w/ 6 Hooks.
o.	Provide Cord Pass Through.
p.	Provide Pull Out Stainless Steel Tray.
q.	Provide Storage Trays.
r.	Provide Right Side Transfer Compartment.
s.	Provide Dual Side Transfer Compartments (6 ft. Model Only).
t.	Provide Three or Four Glove Ports (6 ft. Model Only).
u.	Provide Additional Hospital Grade Duplex.
v.	Provide PharmaGard Digital Monitor.
w.	Provide Seismic Brackets.
x.	Provide Custom Solutions.
2.	PharmaGard ES (Energy Saver) NU-NTE797 Total Exhaust Aseptic Containment Isolator.
a.	Model NU-NR797-400.
b.	Model NU-NR797-600.
c.	Quick Change Sharps and Waste.
d.	Counter Balance Inner Transfer Window.
e.	Sliding Work Tray.
f.	Energy Saver Motor.
g.	TruLaminar Airflow.
h.	HEPEX Zero Leak Airflow System.
i.	Attenumount: Vibration and sound control.
j.	Bag-In Bag-Out Exhaust HEPA Filter.
k.	Provide Bench Mount Support.
l.	Provide Telescoping Basestand.
m.	Provide Auto Lift Basestand.
n.	Provide Additional IV Bar w/ 6 Hooks.
o.	Provide Cord Pass Through.
p.	Provide Pull Out Stainless Steel Tray.
q.	Provide Storage Trays.
r.	Provide Right Side Transfer Compartment.
s.	Provide Dual Side Transfer Compartments (6 ft. Model Only).
t.	Provide Three or Four Glove Ports (6 ft. Model Only).
u.	Provide Additional Hospital Grade Duplex.
v.	Provide Seismic Brackets.
w.	Provide Custom Solutions.
2.7	POLYPROPYLENE FUME HOODS
A.	Vertical Laminar Airflow Fume Hood:
1.	Product: FumeGard NU-156 as manufactured by NuAire Laboratory Equipment Supply.
a.	Model: 4 feet (1232 mm) 24 inches (610 mm) work surface depth.
b.	Model: 4 feet (1232 mm) 30 inches (610 mm) work surface depth.
c.	Model: 5 feet (1524 mm) 24 inches (610 mm) work surface depth.
d.	Model: 5 feet (1524 mm) 30 inches (610 mm) work surface depth.
e.	Model: 6 feet (1829 mm) 24 inches (610 mm) work surface depth.
f.	Model: 6 feet (1829 mm) 30 inches (610 mm) work surface depth.
g.	Model: 8 feet (2438 mm) 24 inches (610 mm) work surface depth.
h.	Model: 8 feet (2438 mm) 30 inches (610 mm) work surface depth.
i.	Certification: NSF No. 49. Meet or exceed Federal Standard 209e, Class 10 air quality conditions, and have been independently tested for containment properties in accordance to ASHRAE Standard 110-1995 for Fume Hoods.
j.	Design: Constructed almost entirely of polypropylene, the fume hood contains the HePeX Zero Leak Airflow System, available only from NuAire. The HePeX system prevents uneven particulate loading by eliminating direct blasts to the HEPA filter, dispensing air over 100% of the surface. The system surrounds positive pressure airflow chambers and ducts with negative air pressure relative to the laboratory. This limits the possibility of leaks and guards against filter failure.
k.	Performance: Down Flow Velocity: 60 LFPM (0.30 m/s) Inflow Velocity: 105 LFPM (0.53 m/s) at 10 inch Access Opening.
B.	Conventional Fume Hood:
1.	Product: FumeGard NU-162 as manufactured by NuAire Laboratory Equipment Supply.
a.	Model: 4 feet (1232 mm) 24 inches (610 mm) work surface depth.
b.	Model: 4 feet (1232 mm) 30 inches (610 mm) work surface depth.
c.	Superstructure Constructed from 1/2 inch (13 mm) Stress Relieved, All Seam Welded Polypropylene.
d.	All Negative Pressure Interior.
e.	Cool White Fluorescent Lighting.
f.	Electronic Fluorescent Lamp Ballast.
g.	Counterbalanced Lexan View Screen Slides 18 inch (457 mm) Maximum Opening to Fully Closing.
h.	Flush Mounted Exterior/Interior Plumbing Chase Access Panels.
i.	Connection Provided for Venting a Base Cabinet.
j.	Removable Rear Baffle for Maintenance.
k.	Reinforced 1/2 inch (13 mm) Thick Polypropylene Work Surface.
l.	Lower Work Access Opening Airfoil.
m.	PVC Electrical Junction Box.
n.	Modular Electrical Component Construction.
o.	PVDF Lined Interior or Flame Retardant Polypropylene Fume Hood.
p.	Composition Stone/Modified Epoxy Resin Work Surfaces.
q.	Air Flow Alarm Systems.
r.	Remote Controlled Service Valves for Air, Vacuum, and/or N2.
s.	Cascade or Single Rinse Tanks with/without Nitrogen Purge.
t.	Rear Exhaust Duct Wash-down System.
u.	Polypropylene, Teflon or PVDF Gooseneck Faucets.
v.	Custom Polypropylene Sinks with Chemically Resistant "P"-Trap.
w.	Teflon, PVDF, or Polypropylene Dip Tanks with/without Drains.
x.	Polypropylene or PVDF Sinks with Hot/Cold or D.I. Water Faucets.
y.	Teflon Liquid/Air Aspirators to Syphon Chemicals.
z.	D.I. Water or N2 Teflon Spray Guns.
aa.	Exhaust Interlocks for Building Controls.
ab.	Polypropylene Exhaust Damper with Quadrant Lock.
ac.	Ground Fault Circuit Interrupter for Duplex Outlet(s).
ad.	Additional Duplex Outlet(s) with PVC Covers.
C.	By-Pass Fume Hood:
1.	Product: FumeGard NU-164 as manufactured by NuAire Laboratory Equipment Supply.
a.	Model: 4 feet (1232 mm) 24 inches (610 mm) work surface depth.
b.	Model: 4 feet (1232 mm) 30 inches (610 mm) work surface depth.
c.	Model: 5 feet (1524 mm) 24 inches (610 mm) work surface depth.
d.	Model: 5 feet (1524 mm) 30 inches (610 mm) work surface depth.
e.	Model: 6 feet (1829 mm) 24 inches (610 mm) work surface depth.
f.	Model: 6 feet (1829 mm) 30 inches (610 mm) work surface depth.
g.	Model: 8 feet (2438 mm) 24 inches (610 mm) work surface depth.
h.	Model: 8 feet (2438 mm) 30 inches (610 mm) work surface depth.
i.	Superstructure Constructed from 1/2 inch (13 mm) Stress Relieved, All Seam Welded Polypropylene.
j.	All Negative Pressure Interior.
k.	Air By-Pass for More Uniform Face Velocity During View Screen Manipulation.
l.	Cool White Fluorescent Lighting.
m.	Electronic Fluorescent Lamp Ballast.
n.	Counterbalanced Lexan View Screen Slides 18 inch (457 mm) Maximum Opening to Fully Closing.
o.	Flush Mounted Exterior/Interior Plumbing Chase Access Panels.
p.	Polypropylene Service Valves (Except Natural Gas).
q.	Connection Provided for Venting a Base Cabinet.
r.	Rear Baffle Removable for Maintenance.
s.	Reinforced 1/2 inch (13 mm) Polypropylene Work Surface.
t.	Lower Work Access Opening Airfoil.
u.	PVC Electrical Junction Box.
v.	Modular Electrical Component Construction.
w.	PVDF Lined Interior or Flame Retardant Polypropylene Fume Hood.
x.	Composition Stone/Modified Epoxy Resin Work Surfaces.
y.	Air Flow Alarm Systems.
z.	Remote Controlled Service Valves for Gas, Air, Vacuum.
aa.	Cascade or Single Rinse Tanks with/without Nitrogen Purge.
ab.	Rear Exhaust Duct Wash-Down System.
ac.	Polypropylene, Teflon or PVDF Gooseneck Faucets.
ad.	Custom Polypropylene Sinks with Chemically Resistant "P"-Trap.
ae.	Teflon, PVDF, or Polypropylene Dip Tanks with/without Drains.
af.	Polypropylene or PVDF Sinks with Hot/Cold or D.I. Water Faucets.
ag.	Teflon Liquid/Air Aspirators to Syphon Chemicals.
ah.	D.I. Water or N2 Teflon Spray Guns.
ai.	Exhaust Interlocks for Building Controls.
aj.	Polypropylene Exhaust Damper with Quadrant Lock.
ak.	Ground Fault Circuit Interrupter for Duplex Outlet(s).
al.	Additional Duplex Outlet(s) with PVC Covers.
2.8	ULTRA-LOW TEMPERATURE FREEZERS
A.	Upright Ultra-low Temperature Freezers:
1.	Model Glacier NU-9483 Upright Mid Capacity -86 degrees C Ultra-low Temperature Freezer.
a.	Interior Volume: 17.1 ft3 (487 L).
b.	GC model includes voltage booster.
c.	Access port.
d.	Heavy-gauge steel cabinet.
e.	Heavy-duty swivel casters.
f.	Key lock.
g.	Four compartments.
h.	Four shelves, three adjustable.
i.	Cobex temperature recorder.
j.	CO2 back-up system [NU-UB2].
k.	Painted steel interior.
l.	Floor anchor system.
m.	Inventory system.
2.	Model Glacier NU-9668 Upright Large Capacity -86 degrees C Ultra Low Freezer.
a.	Capacity: 3.5 cu.ft. (668 L).
b.	GC model includes voltage booster.
c.	Access port.
d.	Heavy-gauge steel cabinet.
e.	Heavy-duty swivel casters.
f.	Key lock.
g.	Four compartments.
h.	Four shelves, three adjustable.
i.	Cobex temperature recorder.
j.	CO2 back-up system [NU-UB2].
k.	Painted steel interior.
l.	Floor anchor system.
m.	Inventory system.
3.	Model Glacier Polar Edition -86 degrees C Ultra-low Temperature Freezer.
a.	Interior Volume: 25.7 ft3 (728 L).
b.	Insulated Inner Door: Steel frame, high impact plastic, w/ foam-in place insulation.
c.	Inner Door Configuration: Two (2).
d.	Door Gaskets: Multi-point compression gaskets.
e.	Condenser Filter: Electrostatic filter, front easy access, no tools.
f.	Interior Corners: Rounded for easy cleaning.
g.	Shelf Bracket: Adjustable.
h.	Casters: Four (4) Heavy Duty w/ leveling feet.
i.	Seismic Brackets: Standard; hard connection to facility wall.
j.	Access Ports: Multiple ports allow use of injection tubes, probes, leads, instrumentation.
2.9	LABORATORY CENTRIFUGES
A.	Ventilated Benchtop Centrifuge:
1.	Product: NuWind NU-C200V as manufactured by NuAire Laboratory Equipment Supply.
a.	Capacity of 4x500ml.
b.	Maximum speed of 4500RPM/4188xg with swing-out rotor.
c.	Maximum speed of 15300RPM/22380xg with fixed angle rotor.
d.	Full touchscreen display.
e.	Automatic lid lock.
f.	Rotor imbalance detector.
g.	Rotor recognition with automatic limitation of maximum speed.
h.	Power Factor Correction to filter and correct the incoming and outgoing line current.
i.	Control center for easy servicing.
j.	Motor accessible and removable from the top of the unit.
B.	Refrigerated Benchtop Centrifuge:
1.	Product: NuWind NU-C200R as manufactured by NuAire Laboratory Equipment Supply.
a.	Capacity of 4x500ml.
b.	Maximum speed of 5100RPM/5350xg with swing-out rotor.
c.	Maximum speed of 18000RPM/30980xg with fixed angle rotor.
d.	Full touchscreen display.
e.	Automatic lid lock.
f.	Rotor imbalance detector.
g.	Rotor recognition with automatic limitation of maximum speed.
h.	Power Factor Correction to filter and correct the incoming and outgoing line current.
i.	Control center for easy servicing.
j.	Motor accessible and removable from the top of the unit.
C.	High-Speed Centrifuges:
1.	Hitachi Koki himac CR22N High-Speed Refrigerated Centrifuge.
a.	Max RCF 55,200xg.
b.	Max Capacity 6 Litre.
D.	Ultracentrifuges:
1.	Hitachi Koki himac CP100NX Ultracentrifuge.
2.	Max Speed 100,000 rpm.
3.	Max RCF 803,000 xg (P100AT2 rotor).
E.	Micro Ultracentrifuges:
1.	Hitachi Koki himac CS150FNX Floor Standing Micro Ultracentrifuge.
a.	Max Speed 150,000 rpm.
b.	Max RCF 1,050,000 xg (S140AT rotor).
c.	Max Capacity (nominal) 30ml x 6 tubes (S50A rotor).
d.	Max Capacity (nominal) (Swinging Bucket Rotor) 7ml x 4 tubes (S50ST rotor).
2.	Hitachi Koki himac CS150NX Tabletop Micro Ultracentrifuge.
a.	Max Speed 150,000rpm.
b.	Max RCF 1,050,000 xg (S140AT rotor).
c.	Max Capacity (nominal) 30ml x 6 tubes (S50A rotor).
d.	Max Capacity (nominal) (Swinging Bucket Rotor) 7ml x 4 tubes (S50ST rotor).
F.	Mini-centrifuge:
1.	Prism LN-C1801 Mini Microcentrifuge.
a.	8 x 1.5 / 2.0 ml tube rotor.
b.	4 x 0.2 ml tube strip / 32 x PCR tube rotor.
G.	Micro-centrifuge:
1.	Prism LN-C2500 Micro Microcentrifuge.
a.	24 x 1.5 / 2.0 ml tube rotor.
b.	16 x 0.2 ml tube strip.
2.	Prism LN-C2500R Micro Microcentrifuge.
a.	24 x 1.5 / 2.0 ml tube rotor.
b.	16 x 0.2 ml tube strip.
H.	Provide the Following Accessories: ______.
2.10	BIOLOGICAL SAFETY CABINETS
A.	Biological Safety Cabinets Class I as manufactured by NuAire Laboratory Equipment Supply.
1.	Product: LabGard ES (Energy Saver) NU-813 Bench Top Class I Containment Cabinet.
a.	Model: NU-813-300/E. Interior: 34-3/8 inches (873 mm) W by 24 inches (610 mm) D by 28 inches (711 mm) H.
b.	Model: NU-813-400/E. Interior: 46-3/8 inches (1178 mm) W by 24 inches (610 mm) D by 28 inches (711 mm) H.
c.	Model: NU-813-600/E. Interior: 70-3/8 inches (1788 mm) W by 24 inches (610 mm) D by 28 inches (711 mm) H.
d.	Stand: 30 inches (762 mm) high.
e.	Stand: 36 inches (914 mm) high.
f.	Provide petcocks.
g.	Performance: ANSI/ASHRAE 110 - surrogate powder, NSF/ANSI 49 Class I. Sound Pressure Level of <62 dba.
h.	Exhaust: HEPA exhaust filter 99.995% (0.3 micron effective).
i.	Exhaust: Purafil exhaust filter 99.995% (0.3 micron effective).
j.	Exhaust: Charcoal exhaust filter 99.995% (0.3 micron effective).
k.	Work Access Opening: 8 inches (203 mm). Viewing panel raised to create a 24 inches (610 mm) opening.
l.	Lighting: Externally mounted fluorescent 50 to 150 fc (538 to 1600 lux).
m.	Average Inflow Velocity: Nominal 60 to 100 fpm (0.30 to 0.51 m/s).
n.	Control System: Constant monitoring and alarm set points for high/low air flow.
2.	Product: LabGard ES (Energy Saver) NU-819 Bench Top Class I Vented Enclosure.
a.	Model: NU-819-300. Interior: 34-1/4 inches (870 mm) W by 19-1/4 inches (489 mm) D by 17-3/4 inches (451 mm) H.
b.	Model: NU-819-400. Interior: 46-1/4 inches (1175 mm) W by 19-1/4 inches (489 mm) D by 17-3/4 inches (451 mm) H.
c.	Recommended Inflow Velocity: Nominal 75 to 100 fpm (0.38 to 0.51 m/s).
d.	Stand: 30 inches (762 mm) high.
e.	Stand: 36 inches (914 mm) high.
f.	Exhaust: HEPA Filter Blower Module exhaust filter 99.995% (0.3 micron effective).
g.	Low air flow alarm.
B.	Biological Safety Cabinets Class II Type A2 as manufactured by NuAire Laboratory Equipment Supply.
1.	Product: CellGard ES (Energy Saver) HD (Hazardous Drug) NU-481 Class II, Type A2 Biosafety Cabinet.
a.	Model: NU-481-400. Interior: 46-3/8 inches (1178 mm) W by 26-1/8 inches (664 mm) D by 28-1/2 inches (724 mm) H.
b.	Model: NU-481-500. Interior: 58-3/8 inches (1483 mm) W by 26-1/8 inches (664 mm) D by 28-1/2 inches (724 mm) H.
c.	Model: NU-481-600. Interior: 70-3/8 inches (1788 mm) W by 26-1/8 inches (664 mm) D by 28-1/2 inches (724 mm) H.
d.	Provide Germicidal UV Light w/ Window Interlock.
e.	Provide GFI.
f.	Provide Additional Duplex Outlets.
g.	Provide IV Bar w/ 6 Hooks.
h.	Provide Automatic Adjustable Support Stand.
i.	Provide Microscope Window.
j.	Provide Additional Service Valves.
k.	Provide ULPA Filters 99.999% at 0.12 Microns.
l.	Provide Storage Pull-Out Trays.
m.	Provide Decorative Side Panels.
n.	Provide Sinks w/ Hot/Cold or DI Faucets.
o.	Provide Heated Work Surface.
p.	Provide Seismic Brackets.
q.	Provide custom solutions as indicated or required.
2.	Product: LABGARD ES Energy Saver NU-540 Class II, Type A2 Biosafety Cabinet.
a.	Model: NU-540-300. Interior: 34-3/8 inches (873 mm) W by 25-3/4 inches (654 mm) D by 28-1/2 inches (724 mm) H.
b.	Model: NU-540-400. Interior: 46-3/8 inches (1178 mm) W by 25-3/4 inches (654 mm) D by 28-1/2 inches (724 mm) H.
c.	Model: NU-540-500. Interior: 58-3/8 inches (1483 mm) W by 25-3/4 inches (654 mm) D by 28-1/2 inches (724 mm) H.
d.	Model: NU-540-600. Interior: 70-3/8 inches (1788 mm) W by 25-3/4 inches (654 mm) D by 28-1/2 inches (724 mm) H.
e.	8 inch (203mm) Access Opening at 105fpm (.53 m/s) Inflow.
f.	Ultraviolet Light.
g.	LED Lighting.
h.	Additional Service Valves for Gas, Air, Vacuum.
i.	Additional Duplex Outlet.
j.	IV Bar with 6 Stainless Steel Hooks.
k.	Exhaust Transition Canopy.
l.	Base Support Stand (available as telescoping for work surface heights of 30 to 36 inches) (762 to 914mm) with or without Storage Shelves.
m.	Adjustable Control for Support Stand or Storage Cabinet.
n.	Sinks with Hot/Cold or DI Water Faucets.
o.	Storage Pull Out Trays.
p.	Lay in Sorbent Exhaust Filter.
q.	Decorative Side Panels (hides plumbing fixture connections).
r.	HEPA Filters 99.999% at 0.3 Micron.
s.	Arm Rest (Stainless Steel).
t.	GFI Outlets.
u.	Provide custom solutions as indicated or required.
3.	Product: LABGARD ES Energy Saver NU-540E Class II, Type A2 Biosafety Cabinet. 
a.	Model: NU-540E-300. Interior: 34-3/8 inches (873 mm) W by 25-3/4 inches (654 mm) D by 28-1/2 inches (724 mm) H. 
b.	Model: NU-540E-400. Interior: 46-3/8 inches (1178 mm) W by 25-3/4 inches (654 mm) D by 28-1/2 inches (724 mm) H. 
c.	Model: NU-540E-500. Interior: 58-3/8 inches (1483 mm) W by 25-3/4 inches (654 mm) D by 28-1/2 inches (724 mm) H. 
d.	Model: NU-540E-600. Interior: 70-3/8 inches (1788 mm) W by 25-3/4 inches (654 mm) D by 28-1/2 inches (724 mm) H. 
e.	8 inch (203mm) Access Opening at 105fpm (.53 m/s) Inflow. 
f.	Ultraviolet Light. 
g.	LED Lighting. 
h.	Additional Service Valves for Gas, Air, Vacuum. 
i.	Additional Duplex Outlet. 
j.	IV Bar with 6 Stainless Steel Hooks. 
k.	Exhaust Transition Canopy. 
l.	Base Support Stand (available as telescoping for work surface heights of 30 to 36 inches) (762 to 914mm) with or without Storage Shelves. 
m.	Adjustable Control for Support Stand or Storage Cabinet. 
n.	Sinks with Hot/Cold or DI Water Faucets. 
o.	Storage Pull Out Trays. 
p.	Lay in Sorbent Exhaust Filter. 
q.	Decorative Side Panels (hides plumbing fixture connections). 
r.	HEPA Filters 99.999% at 0.3 Micron. 
s.	Arm Rest (Stainless Steel). 
t.	GFI Outlets. 
u.	Provide custom solutions as indicated or required.
4.	Product: LABGARD ES Energy Saver NU-543 Class II, Type A2 Biosafety Cabinet.
a.	Model: NU-543-300. Interior: 34-3/8 inches (873 mm) W by 25-3/4 inches (654 mm) D by 28-1/2 inches (724 mm) H.
b.	Model: NU-543-400. Interior: 46-3/8 inches (1178 mm) W by 25-3/4 inches (654 mm) D by 28-1/2 inches (724 mm) H.
c.	Model: NU-543-500. Interior: 58-3/8 inches (1483 mm) W by 25-3/4 inches (654 mm) D by 28-1/2 inches (724 mm) H.
d.	Model: NU-543-600. Interior: 70-3/8 inches (1788 mm) W by 25-3/4 inches (654 mm) D by 28-1/2 inches (724 mm) H.
e.	8 inch (203mm) Access Opening at 105fpm (.53 m/s) Inflow.
f.	12 inch (305mm) Access Opening at 105fpm (.53mls) (400, 500, 600).
g.	Ultraviolet Light.
h.	LED Lighting.
i.	Additional Service Valves for Gas, Air, Vacuum.
j.	Additional Duplex Outlet.
k.	IV Bar with 6 Stainless Steel Hooks.
l.	Exhaust Transition Canopy.
m.	Base Support Stand (available as telescoping for work surface heights of 30 to 36 inches) (762 or 914mm) with or without Storage Shelves.
n.	Adjustable Control for Support Stand or Storage Cabinet.
o.	Sinks with Hot/Cold or DI Water Faucets.
p.	Storage PullOut Trays.
q.	Lay in Sorbent Exhaust Filter.
r.	Decorative Side Panels (hides plumbing fixture connections).
s.	HEPA Filters 99.999% at 0.3 Micron.
t.	Arm Rest (Stainless Steel).
u.	GFI Outlets.
v.	Provide custom solutions as indicated or required.
5.	Product: LABGARD ES Energy Saver NU-543E Class II, Type A2 Biosafety Cabinet. 
a.	Model: NU-543E-300. Interior: 34-3/8 inches (873 mm) W by 25-3/4 inches (654 mm) D by 28-1/2 inches (724 mm) H. 
b.	Model: NU-543E-400. Interior: 46-3/8 inches (1178 mm) W by 25-3/4 inches (654 mm) D by 28-1/2 inches (724 mm) H. 
c.	Model: NU-543E-500. Interior: 58-3/8 inches (1483 mm) W by 25-3/4 inches (654 mm) D by 28-1/2 inches (724 mm) H. 
d.	Model: NU-543E-600. Interior: 70-3/8 inches (1788 mm) W by 25-3/4 inches (654 mm) D by 28-1/2 inches (724 mm) H. 
e.	8 inch (203mm) Access Opening at 105fpm (.53 m/s) Inflow. 
f.	12 inch (305mm) Access Opening at 105fpm (.53mls) (400, 500, 600). 
g.	Ultraviolet Light. 
h.	LED Lighting. 
i.	Additional Service Valves for Gas, Air, Vacuum. 
j.	Additional Duplex Outlet. 
k.	IV Bar with 6 Stainless Steel Hooks. 
l.	Exhaust Transition Canopy. 
m.	Base Support Stand (available as telescoping for work surface heights of 30 to 36 inches) (762 or 914mm) with or without Storage Shelves. 
n.	Adjustable Control for Support Stand or Storage Cabinet. 
o.	Sinks with Hot/Cold or DI Water Faucets. 
p.	Storage PullOut Trays. 
q.	Lay in Sorbent Exhaust Filter. 
r.	Decorative Side Panels (hides plumbing fixture connections). 
s.	HEPA Filters 99.999% at 0.3 Micron. 
t.	Arm Rest (Stainless Steel). 
u.	GFI Outlets. 
v.	Provide custom solutions as indicated or required.
6.	Product: LABGARD ES Energy Saver NU-545 Class II, Type A2 Biosafety Cabinet.
a.	Model: NU-545-300. Interior: 34-3/8 inches (873 mm) W by 26 inches (660 mm) D by 28-1/2 inches (724 mm) H. 
b.	Model: NU-545-400. Interior: 46-3/8 inches (1178 mm) W by 26 inches (660 mm) D by 28-1/2 inches (724 mm) H. 
c.	Model: NU-545-500. Interior: 58-3/8 inches (1483 mm) W by 26 inches (660 mm) D by 28-1/2 inches (724 mm) H. 
d.	Model: NU-545-600. Interior: 70-3/8 inches (1788 mm) W by  26inches (660 mm) D by 28-1/2 inches (724 mm) H. 
e.	8 inch (203mm) Access Opening @ 105 (.53 m/s) Inflow 
f.	Ultraviolet Light 
g.	Additional Service Valves for Gas, Air, Vacuum 
h.	Additional Duplex Outlet 
i.	IV Bar with 6 Stainless Steel Hooks 
j.	Exhaust Transitions - Canopy 
k.	Base Support Stand (available in standard working  surface heights of 30 or 36 inches) (762 or 914mm) with or without Storage Shelves 
l.	Adjustable Control for Support Stand or Storage Cabinet 
m.	Sinks with Hot/Cold or DI Water Faucets 
n.	Storage Pull-Out Trays 
o.	Lay in Sorbent Exhaust Filter 
p.	Decorative Side Panels (hides plumbing fixture connections) 
q.	HEPA Filters 99.999% @ 0.3 Micron 
r.	Arm Rest (Stainless Steel) 
s.	Provide custom solutions as indicated or required. 
7.	Product: LabGard ES (Energy Saver) NU-677 Class II, Type A2 Animal Handling Biological Safety Cabinet.
C.	Biological Safety Cabinets Class II Type B1 as manufactured by NuAire Laboratory Equipment Supply.
1.	Product: LabGard ES (Energy Saver) NU-427 Class II, Type B1 Biological Safety Cabinet.
D.	Biological Safety Cabinets Class II Type B2 as manufactured by NuAire Laboratory Equipment Supply.
1.	Product: LabGard ES (Energy Saver) NU-430 Class II, Type B2 Biosafety Cabinet.
2.	Product: LabGard ES (Energy Saver) NU-435 Class II, Type B2 Biosafety Fume Hood.
E.	Biological Safety Cabinets Class III as manufactured by NuAire Laboratory Equipment Supply.
1.	Product: LabGard ES (Energy Saver) NU-704 Class III Biological Safety Cabinet.
PART 3    EXECUTION
3.1	EXAMINATION
A.	Do not begin installation until substrates have been properly prepared.
B.	If substrate preparation is the responsibility of another installer, notify Architect of unsatisfactory preparation before proceeding.
3.2	INSTALLATION
A.	Clean surfaces thoroughly prior to installation.
B.	Install in accordance with manufacturer's instructions and approved submittals. 
C.	Test for proper operation and adjust until proper operation is achieved.
3.3	PROTECTION
A.	Protect installed products until completion of project.
B.	Touch-up, repair or replace damaged products before Substantial Completion.

END OF SECTION