SECTION 12 20 00

WINDOW TREATMENT

Display hidden notes to specifier. (Don't know how? Click Here) 
 Copyright 2018 -  2019 ARCAT, Inc. - All rights reserved

PART 1    GENERAL
1.1	SECTION INCLUDES
A.	Roller Shades System Types:
1.	Manual operation systems.
2.	Motorized operation systems.
B.	Dual Roller Shade Systems:
1.	Manual operation systems.
2.	Motorized operation systems.
3.	A full line of fabrics.
C.	Vertical Blinds Systems:
1.	Manual operation systems.
2.	Motorized operation systems. 
3.	A full line of vertical fabrics.
4.	Vertical Aluminum coils.
D.	Sliding Panels Systems:
1.	Cord or wand operation systems.
2.	Motorized operation systems.
3.	Entire roller shade fabric collection.
E.	Cellular Shades Systems:
1.	Fabrics.
F.	Horizontal Blinds Systems:
1.	Cord or wand operation.
2.	Motorized operation.
3.	Bass wood collection.
4.	Aluminum blinds.
1.2	RELATED SECTIONS 
A.	Section 08 50 00 - Windows.
B.	Section 08 60 00 - Roof Windows and Skylights.
1.3	SUBMITTALS
A.	Submit under provisions of Section 01 30 00 - Administrative Requirements. 
B.	Product Data:  Manufacturer's data sheets on each product to be specified, including: 
1.	Style, dimensions, profiles, finishes and material descriptions.
C.	Shop Drawings:  Submit manufacturer's shop drawings, including plans, elevations, sections, product details, installation details, operational clearances, wiring diagrams, assembly and mounting details, typical installation details and recommendations and fit-up to adjacent work, finishes, options and accessories. 
D.	Window Treatment Schedule:  With same room designations indicated on the Drawings; including but not limited to opening sizes and key to typical mounting details. 
E.	Maintenance Data:  Instructions and precautions for cleaning shade cloth material, operating hardware and controls. 
F.	Verification Samples: 
1.	Fabric:  Submit 2 samples, minimum 8 x 11 inches (203 x 279 mm), representing actual products specified for shade cloth. 
2.	One complete shade assembly as specified herein. 
1.4	QUALITY ASSURANCE
A.	Manufacturer's Qualifications: Engaged in manufacturing of products of similar type to that specified, with a minimum of 20 years successful experience.
B.	Installer Qualifications: The installer shall be a firm qualified to install the product specified, as demonstrated by prior experience. Minimum 10 years successful experience installing like products.
C.	Single Source Requirements: To the greatest extent possible provide products specified in this section from a single manufacturer.
D.	Mock-Up: Provide a mock-up for evaluation of surface preparation techniques and application workmanship.
1.	Finish areas designated by Architect.
2.	Do not proceed with remaining work until workmanship, color, and sheen are approved by Architect or Owner.
3.	Rebuild mock-up area as required to produce acceptable work.
1.5	DELIVERY, STORAGE, AND HANDLING 
A.	Delivery: Deliver materials to site protected from damage.
B.	Storage: 
1.	Store materials in manufacturer's unopened packaging until ready for installation and in accordance with manufacturer's instructions.
2.	Materials shall be stored in a clean area free of corrosive fumes and dust, and away from construction activities.
3.	Materials shall be stacked horizontally using plastic or wood shims such that drainage and ventilation are provided for, and such that water cannot accumulate in, about, or upon the containers.
1.6	PROJECT CONDITIONS, COORDINATION AND SEQUENCING 
A.	Maintain environmental conditions (temperature, humidity, and ventilation) within limits recommended by manufacturer for optimum results. Do not install products under environmental conditions outside manufacturer's recommended limits.
B.	Conference: Convene a pre-installation conference to establish procedures to maintain optimum working conditions and to coordinate this work with related and adjacent work.
1.	Building shall be enclosed; windows, frames and sills shall be installed and glazed.
2.	Wet work shall be complete and dry; including but not limited to concrete, masonry, plaster, stucco, terrazzo, sheet rock, spackling, and taping (including sanding).
3.	Ceilings, window pockets, electrical and mechanical work above window treatments shall be complete.
1.7	WARRANTY
A.	Manufacturer's Warranty: Provide manufacturer's standard limited warranty against manufacturing defects in materials and workmanship.
1.	Shade:  10 years after completion of installation. 
2.	Fabric: For intended use - interior for 10 years, exterior for 5 years from date of shipment. 
3.	Motors: 5 years.
4.	Electronics and Accessories:  5 years. 
PART 2    PRODUCTS
2.1	MANUFACTURERS
A.	Acceptable Manufacturer: VERTILUX Ltd., which is located at:<BR />7753 N.W. 79th Place<BR />Medley, FL 33166<BR />Toll Free Tel: 800-356-8837<BR />Tel: 305-593-9494<BR />Fax: 800-275-1719<BR />Email: request info (craig.briggs@vertilux.com);Web: http://vertilux.com | http://www.specvertilux.com  
1.	Contact: Jason Schmucker Email: jason.schmucker@vertilux.com; http:// / Phone: 805-906-1199.
B.	Substitutions: Not permitted.
C.	Requests for substitutions will be considered in accordance with provisions of Section 01 60 00 - Product Requirements.
2.2	ROLLER SHADES
A.	Manual Roller Shade Systems:
1.	VTX Clutch System: Clutch made of high-impact nylon.
a.	Color: ________.
b.	Color: As selected by Architect from manufacturer's standard selections.
c.	Elegant Hook Mount Clutch: 1-1/8 in (28 mm).
d.	Elegant Hook Mount Clutch: 1-1/4 in (32 mm).
e.	Elegant Hook Mount Clutch: 1-1/2 in (38 mm).
f.	Designer Hook Mount Clutch: 1-1/8 in (28 mm).
g.	Designer Hook Mount Clutch: 1-1/4 in (32 mm).
h.	Designer Hook Mount Clutch: 1-1/2 in (38 mm).
i.	Elegant Tab Mount Clutch: 1-1/8 in (28 mm).
j.	Elegant Tab Mount Clutch: 1-1/4 in (32 mm).
k.	Elegant Tab Mount Clutch: 1-1/2 in (38 mm).
l.	Designer Tab Mount Clutch: 1-1/8 in (28 mm).
m.	Designer Tab Mount Clutch: 1-1/2 in (38 mm).
2.	Vertilux Rollershade Systems:
a.	Cassettes: 100 flat.
b.	Cassettes:  100 flat; projection. 
c.	Cassettes:  100 round. 
d.	Cassettes:  100 round; projection. 
e.	Cassettes: 120 flat.
f.	Cassettes:  120 flat; projection. 
g.	Cassettes:  120 round. 
h.	Cassettes:  120 round; projection. 
i.	Fascia: 3 in (76 mm) flat.
j.	Fascia: 3 in (76 mm) round.
k.	Fascia: 4 in (102 mm) flat.
l.	Fascia Headrail: Q Box system.
m.	EURO Brackets System:  Large.
n.	EURO Brackets System:  Large, projection. 
o.	EURO Brackets System:  Medium. 
p.	EURO Brackets System:  Medium, projection. 
q.	EURO Brackets System:  Small. 
r.	EURO Brackets System:  Small, projection. 
s.	FIT: Chainless system.
t.	FIT: Standard OM system.
u.	Atos Dropshade system.
v.	Atos Balcony system.
w.	Atos Windows system.
x.	Arion Roller Shade system.
y.	Z Box Guided System: Z Box, 3.93 in (100 mm).
z.	Z Box Guided System: Z Box, 2.12 in (54 mm).
3.	Steel Tubing:
a.	Tube: 2-1/2 in (63 mm) diameter galvanized grooved tube.
b.	Tube: 1-3/4 in (45 mm) Structural Tube for 1-1/2 in (38 mm).
4.	Aluminum Tubing:
a.	Tube: 1-1/2 in (38mm) diameter motor tube; mill finish.
b.	Tube: 1-1/8 in (28 mm) diameter with tape.
c.	Tube: 1-1/8 in (28 mm) diameter no tape.
d.	Tube: 1-1/4 in (32 mm) diameter tube with tape.
e.	Tube: 1-1/4 in (32 mm) iameter tube no tape.
f.	Tube: 1-1/2 in (38 mm) diameter tube with tape.
g.	Tube: 1-1/2 in (38 mm) diameter tube no tape.
h.	Tube: 2 in (50 mm) diameter tube with tape.
i.	Tube: 2 in (50 mm) diameter tube no tape.
j.	Tube: 2.16 in (55 mm) diameter tube flat groove; mill finish.
k.	Tube: 2-1/2 in (63 mm) diameter tube with tape.
l.	Tube: 2-1/2 in (63 mm) diameter tube no tape.
m.	Tube: 3-1/4 in (83 mm) diameter tube.
n.	Tube: 1-1/2 in (38 mm) diameter tube with tape.
o.	Tube: 1-1/2 in (38 mm) diameter tube no tape.
p.	Tube: 1-1/2 in (38 mm) diameter tube no tape; mill finish.
q.	Tube: 2 in (50 mm) diameter tube with tape, grooved; mill finish.
r.	Tube: 2 in (50 mm) diameter tube no tape, grooved.
s.	Tube: 2 in (50 mm) diameter heavy duty tube no tape.
t.	Tube: 1.73 in (45 mm) tube, 2 channels, mill finish with tape.
u.	Tube: 1.73 in (45 mm) tube, 2 channels, mill finish no tape.
5.	Bottom Rail: Euro slim.
6.	Bottom Rail: Slim.
7.	Bottom Rail: Contemporary.
8.	Bottom Rail: Elegant.
9.	Bottom Rail: Teardrop
10.	Bottom Rail: Classic.
11.	Bottom Rail: Supreme aluminum.
12.	Bottom Rail Color: ________.
13.	Bottom Rail Color: As selected by Architect from manufacturer's standard selections.
14.	Adapters: Colors as selected by the Architect from manufacturer's standard selections.
a.	For 1-3/4 in (45 mm) heavy duty structural tube, end plug side.
b.	For 1-3/4 in (45 mm) tube for VTX series.
c.	Rollux for 1-1/8 in (55 mm) tube. 
d.	For 2-1/2 in (63 mm) tube. 
15.	Chain and Chain Components:
a.	Safety device for cords and chains.
b.	Small cord and chain weight.
c.	large cord and chain weight.
d.	NPS chain connector for No. 10 chain.
e.	No. 10 plastic chain connector.
f.	No. 10 plastic peanut connector.
g.	No. 10 plastic chain stopper.
h.	Brass chain No.10.
i.	Nickel pleated Steel chain, No 10.
j.	No. 10 Stainless steel chain.
k.	No. 10 plastic chain.
l.	No. 10 plastic chain high density.
m.	Safety device with chain loop 2 ft (610 mm).
n.	No. 10 plastic chain loop high density 2 ft (610 mm).
o.	No. 10 plastic chain loop high density 3 ft (914 mm).
p.	No. 10 plastic chain loop high density 4 ft (1219 mm).
q.	No. 10 plastic chain loop high density 5 ft (1524 mm).
r.	No. 10 plastic chain loop high density 6 ft (1829 mm).
s.	No. 10 plastic chain loop high density 7 ft (2134 mm).
t.	Cord and chain tension device clear with Screws. 
u.	Continuous chain connector.
v.	No.10 metal chain splicing tool.
w.	Color: ________.
x.	Color: As selected by Architect from manufacturer's standard selections.
16.	Fiberglass insert rod.
17.	Miscellaneous Components:
a.	Silicone oil spray.
b.	Nylon monofilament transparent.
c.	Weather stripping 0.197 x 0.276 in (5 x 7 mm).
d.	Flexible nylon for fabric retainer, 1 in (25 mm).
e.	Narrow tube channel Insert.
f.	Screw for slim bottom rail.
g.	Flat internal hem bar 1 in (25 mm).
h.	Fray-A-Way spray.
i.	Double adhesive tape 3/4 in (19 mm).
j.	Double adhesive tape 1/2 in (13 mm).
k.	Welding tape 11/32 in (9 mm).
l.	Chain and cord tension device clear.
m.	Bottom rail Euro slim end cap.
n.	Bottom rail slim end cap.
o.	Bottom rail contemporary end cap.
p.	Bottom rail elegant end cap.
q.	Bottom rail Teardrop end cap.
r.	Bottom rail classic end cap.
s.	Supreme Bottom rail endcap set.
t.	Color: ________.
u.	Color: As selected by Architect from manufacturer's standard selections.
18.	Additional Field Application Details: Roller shade systems.
a.	________.
b.	________.
B.	Motorization:
1.	Tubular Roller Shade Motors: Fractional horsepower, asynchronous configuration with reversible capacitor designed for intermittent operation. Totally enclosed, thermally protected, temperature class A.
a.	6-700-CN-45E20: Celtic II RF Electronic Motor. For oversized roller shades and dual shades.
1)	Motor Diameter: 1-3/4 in (45mm). 
2)	Motor Length: 29 in (737 mm).
3)	Tube Size 2 in (50 mm). Capacity: 88 lbs (40 kg).
4)	Tube Size 2-1/2 in (63 mm). Capacity: 108 lbs (48 kg).
5)	Tube Size 2-3/4 in (70 mm). Capacity: 108 lbs (48 kg).
6)	Tube Size 3 in (78 mm). Capacity: 108 lbs (48 kg).
7)	Tube Size 3-1/4 in (83 mm). Capacity: 108 lbs (48 kg).
8)	Power: 220 Vac 50/60 Hz, 0.98 A. 
9)	Output: 177 in-lbs (20 Nm) at 33 rpm.
10)	Controls: Wall mount and remote control.
b.	6-700-CM-25E10: Celtic II RF Rechargeable Battery Motor. For roller shades (blackouts, screens, etc.) and dual shades. 
1)	Shade Size: Up to 120 x 96 in (3048 x 2438 mm).
2)	Motor Diameter: 1 in (25 mm).
3)	Motor Length: 22.8 in (579 mm).
4)	Tube Size: 1-3/4 in (45 mm). Capacity: 17 lbs (7.7 kg).
5)	Power: 12 Vdc internal battery, 0.90 A.
6)	Output: 15.93 in-lbs (1.8 Nm) at 30 rpm.
7)	Battery charger.
8)	Controls: Wall mount and remote control.
c.	6-700-CM-45EQ6: Celtic II RF Ultra Quiet Electronic Motor. Roller shades (blackouts, screens, etc.) and dual shades.
1)	Motor Diameter: 1-3/4 in (45 mm).
2)	Motor Length: 27.5 in (698 mm).
3)	Tube Size: 2 in (50 mm). Capacity: 26 lbs (12 kg).
4)	Tube Size: 2-1/2 in (63 mm). Capacity: 21.16 (9.53 kg).
5)	Power: 120 Vac, 50/60 Hz, 0.97 A.
6)	Output: 53 in-lbs (6 Nm) at 28 rpm.
d.	6-700-CN-35E06: Celtic II RF Electronic Motor. Roller shades (blackouts, screens, etc.) and dual shades
1)	Motor Diameter: Series (35mm). 
2)	Motor Length: 24 in (610 mm).
3)	Tube Size: 1-1/2 in (38mm). Capacity: 33 lbs (15 kg).
4)	Tube Size: 1-3/4 in (45mm). Capacity: 30 lbs (13.63 kg).
5)	Tube Size: 2 in (50mm). Capacity: 26.4 lbs (12 kg).
6)	Tube Size: 2-1/2 in (63mm). Capacity: 26.4 lbs (12 kg).
7)	Power: 220 Vac, 50/60 Hz, 0.96 A.
8)	Output: 53 in-lbs (6 Nm) at 33 rpm.
e.	6-700-CM-25E04: Celtic II RF Rechargeable Battery Motor. Roller shades (blackouts, screens, etc.) and dual shades.
1)	Motor Diameter: 1 in (25 mm). 
2)	Motor Length. 17.8 in (452 mm).
3)	Tube Size: 1-1/2 in (38 mm) keyed. Capacity: 11 lbs (4.9 kg).
4)	Power: 12 Vdc. Internal Battery, 0.90 A.
5)	Output: 10.62 in-lbs (1.2 Nm) at 30 rpm.
6)	Battery charger and remote control.
7)	Optional Accessories:
a)	Wall control.
b)	Solar battery charger.
8)	Controls: Wall mount and remote control.
f.	6-700-CM-35E06: Celtic II RF Electronic Motor. Roller shades (blackouts, screens, etc.) and dual shades.
1)	Motor diameter: 1-3/8 in (35 mm). 
2)	Motor Length: 24 in (610 mm).
3)	Tube Size: 1-1/2 in (38 mm). Capacity: 33 lbs (15 kg).
4)	Tube Size: 1-3/4 in (45 mm). Capacity: 30 lbs (13.63 kg).
5)	Tube Size: 2 in (50 mm). Capacity: 26.4 lbs (12 kg).
6)	Tube Size: 2-1/2 in (63 mm). Capacity:  26.4 lbs (12 kg).
7)	Power: 120 Vac 50/60 Hz, 0.96 A
8)	Output: 53 in-lbs (6 Nm) at 33 rpm.
9)	Controls: Wall mount and remote control.
g.	6-700-CN-45R20: Celtic II RF Motor. Oversize roller shades.
1)	Motor diameter: 1-3/4 in (45 mm). 
2)	Motor Length: 29 in (737 m).
3)	Tube Size: 2 in (50 mm). Capacity: 88 lbs (40 kg).
4)	Tube Size: 2-1/2 in (63 mm). Capacity: 108 lbs (48 kg).
5)	Tube Size: 2-3/4 in (70 mm). Capacity: 108 lbs (48 kg).
6)	Tube Size: 3 in (78 mm). Capacity: 108 lbs (48 kg).
7)	Tube Size: 3-1/4 in (83 mm). Capacity: 108 lbs (48 kg).
8)	Power: 220 Vac 50/60 Hz, 1.98 A.
9)	Output: 177 in-lbs (20 Nm) at 33 rpm.
10)	Controls: Wall mount and remote control.
h.	6-700-CN-35R06: Celtic II RF Motor. Roller shades (blackouts, screens, etc.) and dual shades.
1)	Motor Diameter: 1-3/8 in (35 mm).
2)	Motor Length: 24 in (610 mm).
3)	Tube Size: 1-1/2 in (38 mm). Capacity: 33 lbs (15 kg).
4)	Tube Size: 1-3/4 in (45 mm). Capacity: 30 lbs (13.63 kg).
5)	Tube Size: 2 in (50 mm). Capacity: 26.4 lbs (12 kg).
6)	Tube Size: 2-1/2 in (63 mm). Capacity: 26.4 lbs (12 kg).
7)	Maximum Limit Cycle: 33 rpm.
8)	Power: 220 Vac, 50/60 Hz, 0.96 A.
9)	Output: 53 in-lbs (6 Nm).
10)	Controls: Wall mount and remote control.
2.	Tubular Motors; Large Roller Shades:
a.	6-700-CN-45E20: Celtic II RF Electronic Motor. For oversized roller shades and dual shades.
1)	Motor Diameter: 1-3/4 in (45mm). 
2)	Motor Length: 29 in (734 mm).
3)	Tube Size: 2 in (50 mm). Capacity: 88 lbs (40 kg).
4)	Tube Size: 2-1/2 in (63 mm). Capacity: 108 lbs (48 kg).
5)	Tube Size: 2-3/4 in (70 mm). Capacity: 108 lbs (48 kg).
6)	Tube Size: 3 in (78 mm). Capacity: 108 lbs (48 kg).
7)	Tube Size: 3-1/4 in (83 mm). Capacity: 108 lbs (48 kg).
8)	Power: 220 Vac 50/60 Hz, 0.98 A. 
9)	Output: 177 in-lbs (20 Nm) at 33 rpm.
10)	Controls: Wall mount and remote control.
b.	6-700-CM-45E20: Celtic II RF Electronic Motor. Oversize roller shades.
1)	Motor Diameter: 1-3/4 in (45 mm). 
2)	Motor Length: 29 in (734 mm).
3)	Tube Size: 2 in (50 mm). Capacity: 88 lbs (40 kg).
4)	Tube Size: 2-1/2 in (63 mm) Capacity: 108 lbs (48 kg).
5)	Tube Size: 2-3/4 in (70 mm) Capacity: 108 lbs (48 kg).
6)	Tube Size: 3 in (78 mm) Capacity: 108 lbs (48 kg).
7)	Tube Size: 3-1/4 in (83 mm) Capacity: 108 lbs (48 kg).
8)	Power: 120 Vac 50/60 Hz, 0.98 A.
9)	Output: 177 in-lbs (20 Nm) at 33 rpm.
10)	Controls: Wall mounted and remote control.
c.	6-700-CN-45R20: Celtic II RF Motor. Oversize roller shades.
1)	Motor Diameter: 1-3/4 in (45 mm). 
2)	Motor Length: 29 in (734 mm).
3)	Tube Size: 2 in (50 mm). Capacity: 88 lbs (40 kg).
4)	Tube Size: 2-1/2 in (63 mm). Capacity: 108 lbs (48 kg).
5)	Tube Size: 2-3/4 in (70 mm). Capacity: 108 lbs (48 kg).
6)	Tube Size: 3 in (78 mm). Capacity: 108 lbs (48 kg).
7)	Tube Size: 3-1/4 in (83 mm). Capacity: 108 lbs (48 kg).
8)	Power: 220 Vac 50/60 Hz, 1.98 A.
9)	Output: 177 in-lbs (20 Nm) at 33 rpm.
10)	Controls: Wall mount and remote.
d.	6-700-Rc-00001: RF Ultra Quiet Mechanical Motor. Roller shades (blackouts, screens, etc.) and dual shades.
1)	Motor Diameter: (45 mm).
2)	Motor Length: 31 in (787 mm).
3)	Tube Size: 2 in (50 mm). Capacity: 26 lbs (12 kg).
4)	Tube Size: 2-1/2 in (63 mm). Capacity: 21.16 lbs (9.53 kg).
5)	Power: 120 Vac 50/60 Hz, 0.97 A.
6)	Output: 53 in-lbs (6 Nm) at 28 rpm/
7)	Controls: Wall mount and remote.
3.	Battery Motors:
a.	6-700-cM-25E10: Celtic II RF Rechargeable Battery Motor. For roller shades (blackouts, screens, etc.) and dual shades. Size: Up to 120 x 96 in.
1)	Motor Diameter: 1 in (25 mm). 
2)	Motor Length: 22.8 in (579 mm).
3)	Tube Size: 1-3/4 in (45 mm). Capacity: 17 lbs (7.7 kg)
4)	Power: 12 Vdc internal battery, 0.90 A.
5)	Output: 15.93 in-lbs (1.8 Nm) at 30 rpm.
6)	Battery charger.
7)	Controls: Wall mount and remote control.
b.	6-700-cM-25E04: Celtic II RF Rechargeable Battery Motor. Roller shades (blackouts, screens, etc.) and dual shades.
1)	Motor diameter: 1 in (25 mm). 
2)	Motor Length: 17.8 in (452 mm).
3)	Tube Size: 1-1/2 in (38 mm) keyed. Capacity: 11 lbs (4.9 kg).
4)	Power: 12 Vdc Internal Battery, 0.90 A.
5)	Output: 10.62 in-lbs (1.2 Nm) at 30 rpm.
6)	Battery charger and remote control.
7)	Optional Accessories:
a)	Wall control.
b)	Remote control.
c)	Solar battery charger.
4.	Additional Field Application Details: Motorization.
a.	________.
b.	________.
C.	Roller Shade Fabrics:
1.	Rollux DecoStyle Collection:
a.	Fabric: ________
b.	Color: ________
c.	Fabric and Color: As selected by the Architect from manufacturer's standard selections.
2.	Polyscreen Vision Collection:
a.	Fabric: ________
b.	Color: ________
c.	Fabric and Color: As selected by the Architect from manufacturer's standard selections.
3.	High Living 2.1 Collection:
a.	Fabric: ________
b.	Color: ________
c.	Fabric and Color: As selected by the Architect from manufacturer's standard selections.
4.	Eco-Contract Collection:
a.	Fabric: ________
b.	Color: ________
c.	Fabric and Color: As selected by the Architect from manufacturer's standard selections.
5.	Nightfall Blackout Collection:
a.	Fabric: ________
b.	Color: ________
c.	Fabric and Color: As selected by the Architect from manufacturer's standard selections.
6.	lntimate Blackout Collection:
a.	Fabric: ________
b.	Color: ________
c.	Fabric and Color: As selected by the Architect from manufacturer's standard selections.
7.	VX Screen:
a.	Fabric: ________
b.	Color: ________
c.	Fabric and Color: As selected by the Architect from manufacturer's standard selections.
8.	Urban-Chic Collection:
a.	Fabric: ________
b.	Color: ________
c.	Fabric and Color: As selected by the Architect from manufacturer's standard selections.
9.	Additional Field Application Details: Roller shade fabrics.
a.	________.
b.	________.
D.	Roller Shades Fabrication: Custom fabricated to size, color and material as indicated and required to provide light and privacy control.
1.	Configuration: Individual shades.
2.	Configuration: Banded shades.
3.	Configuration: Coupled shades.
4.	Roll Type: Regular single roll.
5.	Roll Type: Reverse single roll.
6.	Roll Type: Dual band.
7.	Clutch: Operate bi-directionally using an endless control loop. Sized to provide force to resist weight of shade and maintain shade position.
8.	Control Loop: Control shall be on right side as facing the shade unless indicated otherwise.
9.	Mounting: Brackets are configured to be ceiling, wall or jamb mounted as indicated or required. 
10.	Spring Lift Assist: Provide spring assist on oversized shades. The wound spring assists shall come in 36 in (914 mm) and 45 in (1143 mm) lengths, reducing lift force to 5 lbs (2.26 kg).
11.	Tube: Extruded aluminum sized per system selected for application.
12.	Fabric Attachment: The fabric shall be heat-welded to a soft vinyl interconnect and press-fit into a keyway, allowing for simple field adjustability, or change of shade band materials. 
13.	Hem Bar: The aluminum bar is inserted into the hem pocket and the fabric heat-welded at the top and sides of the bar to provide a refined unobtrusive appearance.
14.	Battens: Where required to maintain shade fabric flatness battens shall be placed at manufacturer's option. 
a.	Batten Placement: Align battens to horizontal window frame mullions or related architectural elements as indicated. All shades in a single elevation or room shall have battens if one or more require a batten.
15.	Seam Placement: Seam where needed for splicing shall be placed at manufacturer's option to minimize waste. 
16.	Seam Placement: Seam where needed for splicing shall align the seams with horizontal window frame mullions or related architectural elements as indicated. All shades in a single elevation or room shall be seamed if one or more require a splice.
17.	Additional Field Application Details: Roller shades fabrication.
a.	________.
b.	________.
E.	Exterior Roller Shades Fabrication: Operation by motorization or crank.
1.	Side Channels: Shades secured to side tracks with a zipper locking system. Weighted exposed hem bar has guide tracking into side channel. 
2.	Guide Cables: Shades secured to guide cables with cast aluminum eyes attached to ends of concealed stainless-steel hem bar in a welded seam pocket. 
3.	Provide closure plates and attachment as indicated or required to furnish application and product complying with design intent.
4.	Crank Operation:
a.	Gear Ratios: 3/1 to 14/1 shall be as required for size lift requirements.
b.	Handles and Poles: Natural gray finish with plastic sleeve. Universals shall be chromed brass and stainless steel. 
c.	Mounting with the shaft coming through the wall or directly from the bottom of the crank as indicated or required. 
d.	Handles permanently affixed or secured with hook and eye or bell coupler for removable handles as indicated or required.
5.	Additional Field Application Details: Exterior roller shade fabrication.
a.	________.
b.	________.
2.3	DUAL ROLLER SHADES SYSTEMS
A.	Dual Shade Systems: 
1.	VTX Clutch System: Clutch made of high-impact nylon.
a.	Color: ________.
b.	Color: As selected by the Architect from manufacturer's standard selections.
c.	Elegant Hook Mount: 1-1/8 in (28 mm).
d.	Elegant Hook Mount: 1-1/4 in (32 mm).
e.	Elegant Hook Mount: 1-1/2 in (38 mm).
f.	Designer Hook Mount: 1-1/8 in (28 mm).
g.	Designer Hook Mount: 1-1/4 in (32 mm).
h.	Designer Hook Mount: 1-1/2 in (38 mm).
i.	Elegant Tab Mount: 1-1/8 in (28 mm).
j.	Elegant Tab Mount: 1-1/4 in (32 mm).
k.	Elegant Tab Mount: 1-1/2 in (38 mm).
l.	Designer Tab Mount: 1-1/8 in (28 mm).
m.	Designer Tab Mount: 1-1/2 in (38 mm).
2.	Vertilux Rollershade Systems: 
a.	Cassettes: 100 flat.
b.	Cassettes:  100 flat; projection. 
c.	Cassettes:  100 round. 
d.	Cassettes:  100 round; projection. 
e.	Cassettes:  120 flat. 
f.	Cassettes:  120 flat; projection. 
g.	Cassettes:  120 round. 
h.	Cassettes: 120 flat round; projection. 
i.	Fascia:  3 in (76 mm) flat. 
j.	Fascia:  3 in (76 mm) round. 
k.	Fascia:  4 in (102 mm) flat. 
l.	Fascia Headrail:  Q Box system. 
m.	EURO Brackets System:  Large. 
n.	EURO Brackets System:  Large, projection. 
o.	EURO Brackets System:  Medium. 
p.	EURO Brackets System:  Medium, projection. 
q.	EURO Brackets System:  Small. 
r.	EURO Brackets System:  Small, projection. 
s.	FIT:  Chainless system. 
t.	FIT:  Standard OM system. 
u.	Atos Dropshade system. 
v.	Atos Balcony system. 
w.	Atos Windows system. 
x.	Arion Roller Shade system. 
y.	Z Box Guided System:  Z Box, 3.93 in (100 mm). 
z.	Z Box Guided System:  Z Box, 2.12 in (54 mm). 
3.	Steel Tubing: 
a.	Tube:  2-1/2 in (63 mm) diameter galvanized grooved tube. 
b.	Tube:  1-3/4 in (45 mm) Structural Tube for 1-1/2 in (38 mm). 
4.	Aluminum Tubing: 
a.	Tube:  1-1/2 in (38mm) diameter motor tube; mill finish. 
b.	Tube:  1-1/8 in (28 mm) diameter with tape. 
c.	Tube:  1-1/8 in (28 mm) diameter no tape. 
d.	Tube:  1-1/4 in (32 mm) diameter tube with tape. 
e.	Tube:  1-1/4 in (32 mm) iameter tube no tape. 
f.	Tube:  1-1/2 in (38 mm) diameter tube with tape. 
g.	Tube:  1-1/2 in (38 mm) diameter tube no tape. 
h.	Tube:  2 in (50 mm) diameter tube with tape. 
i.	Tube:  2 in (50 mm) diameter tube no tape. 
j.	Tube:  2.16 in (55 mm) diameter tube flat groove; mill finish. 
k.	Tube:  2-1/2 in (63 mm) diameter tube with tape. 
l.	Tube:  2-1/2 in (63 mm) diameter tube no tape. 
m.	Tube:  3-1/4 in (83 mm) diameter tube. 
n.	Tube:  1-1/2 in (38 mm) diameter tube with tape. 
o.	Tube:  1-1/2 in (38 mm) diameter tube no tape. 
p.	Tube:  1-1/2 in (38 mm) diameter tube no tape; mill finish. 
q.	Tube:  2 in (50 mm) diameter tube with tape, grooved; mill finish. 
r.	Tube:  2 in (50 mm) diameter tube no tape, grooved. 
s.	Tube:  2 in (50 mm) diameter heavy duty tube no tape. 
t.	Tube:  1.73 in (45 mm) tube, 2 channels, mill finish with tape. 
u.	Tube:  1.73 in (45 mm) tube, 2 channels, mill finish no tape.
5.	Bottom Rails and Bottom Rail End Caps: 
a.	Color: As selected by the Architect from manufacturer's standard selections.
b.	Aluminum Bottom rail I and end caps.
c.	Bottom rail II and end caps.
d.	Aluminum inside tube.
e.	Aluminum tube II.
f.	Bottom rail and end caps.
g.	Supreme aluminum bottom rail and end caps.
h.	Bottom Rail: Tube I cover - grey.
i.	Bottom Rail: Euro Slim.
j.	Bottom Rail: Slim.
k.	Bottom Rail: Contemporary.
l.	Bottom Rail: Elegant.
m.	Bottom Rail: Teardrop.
n.	Bottom Rail: Classic. 
6.	Additional Field Application Details: Dual shade systems.
a.	________.
b.	________.
B.	Motorization:
1.	Tubular Roller Shade Motors: Fractional horsepower, asynchronous configuration with reversible capacitor designed for intermittent operation. Totally enclosed, thermally protected, temperature class A.
a.	6-700-CN-45E20: Celtic II RF Electronic Motor. For oversized roller shades and dual shades.
1)	Motor Diameter: (45mm). 
2)	Motor Length: 29 in (734 mm).
3)	Tube Size 2 in (50 mm). Capacity: 88 lbs (40 kg).
4)	Tube Size 2-1/2 in (63 mm). Capacity: 108 lbs (48 kg).
5)	Tube Size 2-3/4 in (70 mm). Capacity: 108 lbs (48 kg).
6)	Tube Size 3 in (78 mm). Capacity: 108 lbs (48 kg).
7)	Tube Size 3-1/4 in (83 mm). Capacity: 108 lbs (48 kg).
8)	Power: 220 Vac 50/60 Hz, 0.98 A. 
9)	Output: 177 in-lbs (20 Nm) at 33 rpm.
10)	Controls: Wall mount and remote control.
b.	6-700-CM-25E10: Celtic II RF Rechargeable Battery Motor. For roller shades (blackouts, screens, etc.) and dual shades. 
1)	Shade Size: Up to 120 x 96 in (3048 x 2438 mm).
2)	Motor Diameter: 1 in (25 mm).
3)	Motor Length: 22.8 in (579 mm).
4)	Tube Size: 1-3/4 in (45 mm). Capacity: 17 lbs (7.7 kg).
5)	Power: 12 Vdc internal battery, 0.90 A.
6)	Output: 15.93 in-lbs (1.8 Nm) at 30 rpm.
7)	Battery charger.
8)	Controls: Wall mount and remote control.
c.	6-700-CM-45EQ6: Celtic II RF Ultra Quiet Electronic Motor. Roller shades (blackouts, screens, etc.) and dual shades.
1)	Motor Diameter: 1-3/4 in (45 mm).
2)	Motor Length: 27.5 in (698 mm).
3)	Tube Size: 2 in (50 mm). Capacity: 26 lbs (12 kg).
4)	Tube Size: 2-1/2 in (63 mm). Capacity: 21.16 (9.53 kg).
5)	Power: 120 Vac, 50/60 Hz, 0.97 A.
6)	Output: 53 in-lbs (6 Nm) at 28 rpm.
d.	6-700-CN-35E06: Celtic II RF Electronic Motor. Roller shades (blackouts, screens, etc.) and dual shades
1)	Motor Diameter: 1-3/8 in (35mm). 
2)	Motor Length: 24 in (610 mm).
3)	Tube Size: 1-1/2 in (38 mm). Capacity: 33 lbs (15 kg).
4)	Tube Size: 1-3/4 in (45 mm). Capacity: 30 lbs (13.63 kg).
5)	Tube Size: 2 in (50 mm). Capacity: 26.4 lbs (12 kg).
6)	Tube Size: 2-1/2 in (63 mm). Capacity: 
7)	Power: 220 Vac, 50/60 Hz, 0.96 A.
8)	Output: 53 in-lbs (6 Nm) at 33 rpm.
e.	6-700-CM-25E04: Celtic II RF Rechargeable Battery Motor. Roller shades (blackouts, screens, etc.) and dual shades.
1)	Motor Diameter: 1 in (25 mm). 
2)	Motor Length. 17.8 in (452 mm).
3)	Tube Size: 1-1/2 in (38 mm) keyed. Capacity: 11 lbs (4.9 kg).
4)	Power: 12 Vdc. Internal Battery, 0.90 A.
5)	Output: 10.62 in-lbs (1.2 Nm) at 30 rpm.
6)	Battery charger and remote control.
7)	Optional Accessories:
a)	Wall control.
b)	Solar battery charger.
f.	6-700-CM-35E06: Celtic II RF Electronic Motor. Roller shades (blackouts, screens, etc.) and dual shades.
1)	Motor diameter: 1-3/8 in (35 mm). 
2)	Motor Length: 24 in (610 mm).
3)	Tube Size: 1-1/2 in (38 mm). Capacity: 33 lbs (15 kg).
4)	Tube Size: 1-3/4 in (45 mm). Capacity: 30 lbs (13.63 kg).
5)	Tube Size: 2 in (50 mm). Capacity: 26.4 lbs (12 kg).
6)	Tube Size: 2-1/2 in (63 mm). Capacity:  26.4 lbs (12 kg).
7)	Power: 120 Vac 50/60 Hz, 0.96 A.
8)	Output: 53 in-lbs (6 Nm) at 33 rpm.
9)	Controls: Wall mount and remote control.
g.	6-700-CN-45R20: Celtic II RF Motor. Oversize Roller Shades.
1)	Motor diameter: 1-3/4 in (45 mm). 
2)	Motor Length: 29 in (737 m).
3)	Tube Size: 2 in (50 mm). Capacity: 88 lbs (40 kg).
4)	Tube Size: 2-1/2 in (63 mm). Capacity: 108 lbs (48 kg).
5)	Tube Size: 2-3/4 in (70 mm). Capacity: 108 lbs (48 kg).
6)	Tube Size: 3 in (78 mm). Capacity: 108 lbs (48 kg).
7)	Tube Size: 3-1/4 in (83 mm). Capacity: 108 lbs (48 kg).
8)	Power: 220 Vac 50/60 Hz, 1.98 A.
9)	Output: 177 in-lbs (20 Nm) at 33 rpm.
10)	Controls: Wall mount and remote control.
h.	6-700-CN-35R06: Celtic II RF Motor. Roller shades (blackouts, screens, etc.) and dual shades.
1)	Motor Diameter: 1-3/8 in (35 mm).
2)	Motor Length: 24 in (610 mm).
3)	Tube Size: 1-1/2 in (38 mm). Capacity: 33 lbs (15 kg).
4)	Tube Size: 1-3/4 in (45 mm). Capacity: 30 lbs (13.63 kg).
5)	Tube Size: 2 in (50 mm). Capacity: 26.4 lbs (12 kg).
6)	Tube Size: 2-1/2 in (63 mm). Capacity: 26.4 lbs (12 kg).
7)	Maximum Limit Cycle: 33 rpm.
8)	Power: 220 Vac, 0.96 A.
9)	Output: 53 in-lbs (6 Nm).
i.	6-700-CM-35R06: Celtic II RF Motor. Roller shades (blackouts, screens, etc.) and dual shades.
1)	Motor diameter: (35 mm). 
2)	Motor Length: 24 in (610 mm).
3)	Tube Size: 1-1/2 in (38 mm). Capacity: 33 lbs (15 kg).
4)	Tube Size: 1-3/4 in (45 mm). Capacity: 30 lbs (13.63 kg).
5)	Tube Size: 2 in (50 mm). Capacity: 26.4 lbs (12 kg).
6)	Tube Size: 2-1/2 in (63 mm). Capacity: 26.4 lbs (12 kg).
7)	Power: 20 Vac 50/60 Hz, 0.96 A.
8)	Output: 53 in-lbs (6 Nm) at 33 rpm.
2.	Additional Field Application Details: Dual shade motorization.
a.	________.
b.	________.
C.	Dual Roller Shade Fabrics:
1.	Neolux Essence:
a.	Fabric: ________
b.	Color: ________.
c.	Fabric and Color: As selected by the Architect from manufacturer's standard selections.
2.	Neolux Avant:
a.	Fabric: ________
b.	Color: ________.
c.	Fabric and Color: As selected by the Architect from manufacturer's standard selections.
3.	Additional Field Application Details: Dual roller shade fabrics.
a.	________.
b.	________.
D.	Roller Shades Fabrication: Custom fabricated to size, color and material as indicated and required to provide light and privacy control.
1.	Configuration: Individual shades.
2.	Configuration: Banded shades.
3.	Configuration: Coupled shades.
4.	Roll Type: Regular single roll.
5.	Roll Type: Reverse single roll.
6.	Roll Type: Dual band.
7.	Clutch: Operate bi-directionally using an endless control loop. Sized to provide force to resist weight of shade and maintain shade position.
8.	Control Loop: Control shall be on right side as facing the shade unless indicated otherwise.
9.	Mounting: Brackets are configured to be ceiling, wall or jamb mounted as indicated or required. 
10.	Spring Lift Assist: Provide spring assist on oversized shades. The wound spring assists shall come in 36 in (914 mm) and 45 in (1143 mm) lengths, reducing lift force to 5 lbs (2.26 kg).
11.	Tube: Extruded aluminum sized per system selected for application.
12.	Fabric Attachment: The fabric shall be heat-welded to a soft vinyl interconnect and press-fit into a keyway, allowing for simple field adjustability, or change of shade band materials. 
13.	Hem Bar: The aluminum bar is inserted into the hem pocket and the fabric heat-welded at the top and sides of the bar to provide a refined unobtrusive appearance.
14.	Battens: Where required to maintain shade fabric flatness battens shall be placed at manufacturer's option. 
a.	Batten placement: Align battens to horizontal window frame mullions or related architectural elements as indicated. All shades in a single elevation or room shall have battens if one or more require a batten.
15.	Seam Placement: Seam where needed for splicing shall be placed at manufacturer's option to minimize waste. 
16.	Seam Placement: Seam where needed for splicing shall align the seams with horizontal window frame mullions or related architectural elements as indicated. All shades in a single elevation or room shall be seamed if one or more require a splice.
17.	Additional Field Application Details: Roller shades fabrication.
a.	________.
b.	________.
2.4	VERTICAL BLIND SYSTEMS
A.	Basis of Design: 3 and 8 Prong systems by Vertilux Limited.
1.	Components:
a.	Control set, 3 prong.
b.	Control end set, notchless, 8 prong.
c.	No. 2 Nylon cord, medium.
d.	No. 2 Nylon cord, hard.
e.	Tension pulley.
f.	No. 6 metal NPB chain connectors.
g.	NPB bead for No. 2 Nylon cord 5/32 in (4 mm).
h.	No. 3 metal NPB chain connector.
i.	Clear plastic cleat for cords.
j.	Plastic chain connector.
k.	No. 6 NPS chain.
l.	Plastic chain 1/8 in (3.2 mm).
m.	No. 6 NPB chain.
n.	No. 3 brass chain.
o.	No. 3 steel chain.
p.	No. 3 plastic chain clear.
q.	Brass chain and clip clear clip.
r.	Steel chain and clip white clip.
s.	Chain and clip plastic - metal weights.
t.	Chain and clip plastic - plastic weights.
u.	NPS chain connector for No. 10 chain.
v.	No. 10 plastic chain connector.
w.	No. 10 brass chain.
x.	No. 10 nickel plated steel, qualified 50/51.
y.	No. 10 stainless steel chain (50/51).
z.	No. 10 plastic chain.
aa.	No. 10 plastic chain, high density.
ab.	Cord weight pulley.
ac.	Two, 7-8 in (178-203 mm) L brackets regular.
ad.	Two, 7-8 in (178-203 mm) L brackets and valance holder.
ae.	Two, 7-8 in (178-203 mm) L brackets, valance holder and snap for V and T tops.
af.	Two, 7-8 in (178-203 mm) L bracket and snap.
ag.	"L" brackets regular, 4 in (102 mm).
ah.	Flat extension brackets, 4 in (102 mm).
ai.	"L" bracket and valance holder, 4 in (102 mm).
aj.	"L" bracket, valance holder and snap for v and T tops, 4 in (102 mm).
ak.	"L" bracket and snap regular, 4 in (102 mm).
al.	Snap in bracket.
am.	Plastic carrier heavy duty, 3 prong.
an.	Carrier self-alignment (scissor), 3 prong.
ao.	Dummy carrier, 3 prong.
ap.	Plastic self-alignment carrier, 8 prong.
aq.	Dummy carrier, 8 prong.
ar.	Plastic louver weight, 3-1/2 in (89 mm).
as.	Metal louver weight, 3-1/2 in (89 mm).
at.	Sew-in weights.
au.	Plastic louver weight (chainless), 3-1/2 in (89 mm).
av.	Aluminum track T-top 16 ft (4877 mm) carton.
aw.	Aluminum track V-top 16 ft (4877 mm) carton.
2.	Motor for vertical blinds, left side.
3.	Additional Field Application Details:
a.	________.
b.	________.
B.	Basis of Design: MX93, 4 Prong Strap System by Vertilux Limited.
1.	Components:
a.	Control for square track.
b.	Cord drive runner for strap system.
c.	Control for hook and wand operation.
d.	Ceiling mount snap in bracket.
e.	Aluminum square flat for vertical blinds.
f.	"L" Bracket and Snap. 2-7/8 in (73 mm).
g.	"L" Bracket and Snap. 4 in (102 mm).
h.	Connector for strap carriers.
i.	Individual 4 prong carrier.
j.	Linked carriers right 3-1/8 in (79 mm).
k.	Linked carriers Left 3-1/8 in (79 mm).
l.	Linked carriers right 2-7/8 in (73 mm).
m.	Linked carriers Left 2- 7/8 in (73 mm).
n.	Plastic strap for carriers. 2-7/8 in (73 mm).
o.	Plastic strap for carriers. 3-1/8 in (79 mm).
p.	Master carrier for strap system.
q.	Dummy carrier for strap system, 4 prong.
r.	Connector for scissor carriers.
2.	Motor for vertical blinds, left side.
a.	Controls: Wall mounted.
3.	Additional Field Application Details:
a.	________.
b.	________.
C.	Basis of Design: Tiltrak Systems by Vertilux Limited.
1.	Components:
a.	End control set, fixed wand.
1)	Endcap set, wand control.
2)	Wand hook
3)	Wand knob
4)	Wand clip
5)	Aluminum Wand
b.	End control set for chain operation.
1)	Cord lock and cord brake.
c.	Center support.
d.	Fixed friction rod support.
e.	Plastic louver weight. 3-1/2 in (89 mm).
f.	Metal louver weight. 3-1/2 in (89 mm).
g.	Sew-in weights.
h.	Plastic louver weight (chainless). 3-1/2 in (89 mm).
i.	Carrier.
j.	Lead carrier.
k.	Lead carrier, center open.
l.	Linked carrier with 3-1/8 in (80 mm) strap.
m.	Linked carrier with 2 7/8 in (73 mm) strap.
n.	Slope angle carrier
2.	Motor for vertical blinds, left side.
a.	Controls: Wall mounted.
3.	Additional Field Application Details:
a.	________.
b.	________.
D.	Basis of Design: Matrix Systems by Vertilux Limited.
1.	Matrix 4 Prong Pantographic System Square Track.
a.	Components:
1)	Control for square track.
2)	Control for hook and wand operation.
3)	Aluminum square flat for vertical blinds.
4)	"L" Bracket and Snap. 2-7/8 in (73 mm).
5)	"L" Bracket and Snap. 4 in (102 mm).
6)	Ceiling mount snap in bracket for valance.
7)	Ceiling mount snap in bracket.
8)	Self-aligning scissor carrier.
a)	Tiltrod support for scissor carrier.
b)	Magnetic tiltrod support for scissor carrier.
c)	Rivets for adding scissor carriers. 1/8 x 1/4 (2.5 x 5.5 mm).
d)	Connector for scissor carriers (scissor carriers only).
e)	Cord drive master carrier for scissor carrier.
f)	Cord drive runner for scissor carrier.
b.	Motor for vertical blinds, left side.
1)	Controls: Wall mounted.
2.	Matrix 4 Prong Pantographic System Ellipse Track.
a.	Components:
1)	Control for rounded track
2)	Aluminum ellipse track for vertical blinds
3)	"L" Bracket and Snap. 2-7/8 in (73 mm).
4)	"L" Bracket and Snap. 4 in (102 mm).
5)	Ceiling mount snap in bracket for valance.
6)	Ceiling mount snap in bracket.
7)	Self-aligning scissor carrier.
a)	Cord drive master carrier for scissor carrier.
b)	Cord drive runner for scissor carrier.
c)	Tiltrod support for scissor carrier.
d)	Magnetic tiltrod support for scissor carrier.
e)	Rivets for adding scissor carriers. 1/8 x 1/4 (2.5 x 5.5 mm).
b.	Motor for vertical blinds, left side.
1)	Controls: Wall mounted.
3.	Additional Field Application Details:
a.	________.
b.	________.
E.	Vertical Blinds, Fabrics:
1.	Basis of Design: Evolution Vertical Blinds by Vertilux Limited.
a.	Fabric: ________
b.	Color: ________.
c.	Fabric and Color: As selected by the Architect from manufacturer's standard selections.
2.	Additional Field Application Details: Vertical blinds, fabrics.
a.	________.
b.	________.
F.	Vertical Blinds, Aluminum:
1.	Basis of Design: 3.5 in (89 mm) aluminum.
a.	Color: ______.
b.	Color: As selected by the Architect from manufacturer's standard selections.
2.	Additional Field Application Details: Vertical blinds, aluminum.
a.	________.
b.	________.
G.	Vertical Blind Systems Fabrication: Custom fabricated to size, color and material as indicated and required to provide light and privacy control. 
1.	Bottom hems shall have plated steel weights sonically welded and sealed into folded fabric on 3 sides.
2.	Configuration: Straight.
3.	Configuration: Curved - 90 degree.
4.	Configuration: Continuous curve.
5.	Draw: Center.
6.	Draw: One way.
7.	Draw: Off set.
8.	Operation: Hand.
9.	Operation: Wand.
10.	Operation: Cord.
11.	Operation: Motor.
12.	Additional Field Application Details: Vertical blind systems fabrication.
a.	________.
b.	________.
2.5	SLIDING PANELS SYSTEMS
A.	Basis of Design: Zen Sliding Panel Systems by Vertilux Limited.
1.	Components:
a.	End Plug right.
b.	End Plug left.
c.	Flat Weight 1 x 1-8 in (25 x 25-203 mm) mill finish.
d.	Hook for vertical wand control carrier, white.
e.	Wand hook.
f.	Wand knob.
g.	Wand clip.
h.	Aluminum wand.
i.	Cord locking nut.
j.	Cord, 0.14 in (3.5 mm).
k.	Installation clip 4 and 5 channels.
l.	Installation clip 2 and 3 channels.
m.	Adjustable "L" bracket 3-3/8 to 5-3/4 in (85 to 145 mm).
n.	"L" bracket angle.
o.	Double "L" bracket angle.
p.	Double "L" bracket angle front installation.
q.	Aluminum track, 2 channel.
r.	Aluminum track, 3 channel.
s.	Aluminum track, 4 channel.
t.	Aluminum track, 5 channel.
u.	Channel guide left/right, 2.
v.	Channel guide left/right, 3.
w.	Channel guide left/right, 4.
x.	Channel guide left/right, 5.
y.	Channel stop screw with hook fastener.
z.	Support with needle and screw.
aa.	Double support with needle and screw.
ab.	Double support with needle and screw front installation.
ac.	Motor set for sliding panels, 4 channel, right side.
ad.	Motor set for sliding panels, 4 channel, left side.
ae.	Motor set for sliding panels, 5 channel, right side.
af.	Motor set for sliding panels, 5 channel, left side.
2.	Additional Field Application Details: 
a.	________.
b.	________.
B.	Sliding Panel Fabrics by Vertilux Limited:
1.	Deco-Styles Collection:
a.	Fabric: ________
b.	Color: ________.
c.	Fabric and Color: As selected by the Architect from manufacturer's standard selections.
2.	Polyscreen Vision Collection:
a.	Fabric: ________
b.	Color: ________.
c.	Fabric and Color: As selected by the Architect from manufacturer's standard selections.
3.	High Living 2.1 Collection:
a.	Fabric: ________
b.	Color: ________.
c.	Fabric and Color: As selected by the Architect from manufacturer's standard selections.
4.	Nightfall Blackout Collection:
a.	Fabric: ________
b.	Color: ________.
c.	Fabric and Color: As selected by the Architect from manufacturer's standard selections.
5.	Additional Field Application Details: 
a.	________.
b.	________.
C.	Sliding Panel System Fabrication: Custom fabricated to size, color and material as indicated and required to provide light and privacy control. Provide top hung fabric panels in multi-track configurations.
1.	Tracks: 2, 3, 4, and 5 channel tracks 1-9/16 x 3-7/16 in (40 to 87 mm) deep by 3/4 in (19 mm) high. Refer to drawings for track type or provide track type required for configuration indicated.
2.	Draw: One way draw.
3.	Draw: Center draw.
4.	Draw: Center opening draw.
5.	Draw: Staggered draw.
6.	Draw: As indicated on drawings.
7.	Overlap: 2-1/2 in (64 mm) approximate panel overlap.
8.	Edge Banding: As indicated or required.
9.	Fabric Attachment: Velcro hook and loop on panel runner and sewed to fabric.
10.	Operation: Hand.
11.	Operation: Wand.
12.	Operation: Cord.
13.	Operation: Motor.
14.	Additional Field Application Details: 
a.	________.
b.	________.
2.6	CELLULAR SHADES SYSTEMS
A.	Basis of Design: Elitepleat Systems by Vertilux Limited.
1.	PVC profile with adhesive tape.
2.	PVC profile bushing.
3.	Aluminum track anodized.
4.	"L" installation bracket.
5.	Cord 0.055 in (1.4 mm).
6.	Cord tassel.
7.	Lift cord 0.047 in (1.2 mm).
8.	Aluminum cord connector.
9.	Cord lock right.
10.	Cord lock left.
11.	Return cord 0.031 in (0.8 mm).
12.	Ribbon.
13.	Clear plastic tags.
14.	Arch clips with pin set (2 pcs).
15.	Steel weight with tape.
16.	Plastic end cap.
17.	Plastic end cap with hole.
18.	Ladder.
19.	Installation clip for hexagonal screw.
20.	Low gap installation clip for flat head screw.
21.	Clear plastic bottom arch support.
22.	Clear plastic bottom support extension for large shades.
23.	Double adhesive tape 3/4 in (19 mm).
24.	Double adhesive tape 1/2 in (13 mm).
25.	Additional Field Application Details: 
a.	________.
b.	________.
B.	Basis of Design: Versarails Systems by Vertilux Limited.
1.	Components:
a.	Cellular system clutch set, 1 in (25 mm).
b.	Cellular system gearbox, 1 in (25 mm).
c.	Cellular system headrail 14 ft (4267 mm) x 24 pc white.
d.	Cellular system interior plug set for bottom rail, 1 in (25 mm).
e.	Cellular system exterior plug set for bottom rail, 1 in (25 mm).
f.	Cellular system mounting bracket, 1 in (25 mm).
g.	Cellular system lift set, 1 in (25 mm).
h.	Cellular system insert strip, 1 in (25 mm).
i.	Cellular system ferrules, 1 in (25 mm).
j.	Fiberglass shaft 3/8 in (10 mm).
k.	Pleated-cord 0.031 in (0.8 mm).
l.	Ivory control cord loops.
m.	White control cord loops.
n.	Cellular system cord loop vanilla, 1 in (25 mm).
o.	Cord/chain tension device clear with screws.
p.	Long spears 5.7 in (145 mm).
q.	Short spears 4.6 in (117 mm).
2.	Additional Field Application Details: 
a.	________.
b.	________.
C.	Cellular Fabrics:
1.	High Living by Vertilux Limited.
a.	Fabric: ________
b.	Color: ________.
c.	Fabric and Color: As selected by the Architect from manufacturer's standard selections.
2.	Additional Field Application Details: 
a.	________.
b.	________.
D.	Cellular Shades Systems Fabrication: Custom fabricated to size, color and material as indicated and required to provide light and privacy control.
1.	Additional Field Application Details: 
a.	________.
b.	________.
2.7	HORIZONTAL BLINDS SYSTEMS
A.	Basis of Design: Horizontal Blinds 2 in (51 mm) Systems by Vertilux Limited.
1.	Components:
a.	Headrail, touch wood, 2 in (50 mm).
b.	Headrail, high profile, 2 in (50 mm).
c.	Center support bracket for headrail, 2 in (50 mm).
d.	Blind metal hold down bracket, 2 in (50 mm).
e.	Hidden, 2 in (50 mm) installation bracket wall/ceiling.
f.	Hidden, 2 in (50 mm) installation bracket.
g.	Installation brackets, 2 in (50 mm).
h.	Lift cord, 0.07 in (1.8 mm).
i.	Lift cord, (0.10 in (2.6 mm).
j.	Cord equalizer large.
k.	Swing cord lock, 2 in (50 mm).
l.	Small flange cord lock (high back), 2 in (50 mm).
m.	Large flange cord lock (high back), 2 in (50 mm).
n.	Cord tilter large flange, 2 in (50 mm)."
o.	Cord tilter small flange, 2 in (50 mm)."
p.	Plastic drum for ladder or tape, 2 in (50 mm).
q.	Metal drum and support for ladder, 2 in (50 mm).
r.	Metal drum and support for tape, 2 in (50 mm).
s.	Braided ladder 1.73 in (44 mm).
t.	Braided ladder clip
u.	Ladder Buttons, 2 in (50 mm).
2.	Motor: Celtic II RF Electric Motor.
a.	Motor Diameter: 1-3/8 in (35 mm).
b.	Motor Length: 24 in (610 mm).
c.	Time of Operation: 4 Minutes.
d.	Power: 120 Vac 50/60 Hz, 0.96 A.
e.	Output: 88.5 in-lbs (10 Nm) at 17 rpm.
f.	Controls: Wall mounted and remote.
3.	Additional Field Application Details: 
a.	________.
b.	________.
B.	Basis of Design: Horizontal Blinds 1 in (25 mm) Signum Systems by Vertilux Limited.
1.	Components:
a.	Tilter.
b.	"D" tilt rod.
c.	Head rail end plug, 1 in (25 mm).
d.	"C" type bottom rail end plug, 1 in (25 mm).
e.	Cord lock.
f.	Cord connector.
g.	Cord lock cover.
h.	Tilter cover.
i.	Cord lock tilter cover.
j.	Cord connector cover.
k.	Cord/wand bottom cover.
l.	Louverlux, 1 in (25 mm) plastic slat clip.
m.	Standard "O" ring (1/8 in ID x 1/4 in OD) for "D" tilt rod.
n.	Drum support.
o.	Ladder drum.
p.	Tilt wand 15/64 in (5.8 mm).
q.	Cord/wand inside bottom.
2.	Motor: Celtic II RF Electric Motor.
a.	Motor Diameter: 1-3/8 in (35 mm).
b.	Motor Length: 24 in (610 mm).
c.	Time of Operation: 4 minutes.
d.	Power: 120 Vac 50/60 Hz, 0.96 A.
e.	Output: 88.5 in-lbs (10 Nm) at 17 rpm.
f.	Controls: Wall mounted and remote.
3.	Additional Field Application Details: 
a.	________.
b.	________.
C.	Horizontal Blinds; Aluminum:
1.	Basis of Design: Louverlux by Vertilux Limited.
a.	Perforated 1 in (25 mm):
1)	Color: ______.
2)	Color: As selected by the Architect from manufacturer's standard selections.
b.	Solid Colors 1 in (25 mm):
1)	Color: ______.
2)	Color: As selected by the Architect from manufacturer's standard selections.
c.	Touch of Wood 1 in (25 mm):
1)	Color: ______.
2)	Color: As selected by the Architect from manufacturer's standard selections.
d.	Perforated, 2 in (50 mm):
1)	Color: ______.
2)	Color: As selected by the Architect from manufacturer's standard selections.
e.	Solid colors, 2 in (50 mm):
1)	Color: ______.
2)	Color: As selected by the Architect from manufacturer's standard selections.
f.	Touch of wood, 2 in (50 mm):
1)	Color: ______.
2)	Color: As selected by the Architect from manufacturer's standard selections.
2.	Additional Field Application Details: 
a.	________.
b.	________.
D.	Horizontal Blinds; Wood:
1.	Basis of Design: Horizontal Blinds, 2 in (50 mm) by Vertilux Limited.
a.	Bass Wood Slat, 2 in (50 mm):
1)	Color: ______.
2)	Color: As selected by the Architect from manufacturer's standard selections.
b.	Bass Wood Modern Valance, 2-1/2 in (63 mm):
1)	Color: ______.
2)	Color: As selected by the Architect from manufacturer's standard selections.
c.	Bass Wood Modern Bottom Rail, 2 in (50 mm):
1)	Color: ______.
2)	Color: As selected by the Architect from manufacturer's standard selections.
2.	Additional Field Application Details: 
a.	________.
b.	________.
E.	Horizontal Blinds Systems Fabrication: Custom fabricated to size, color and material as indicated and required to provide light and privacy control.
1.	Additional Field Application Details: 
a.	________.
b.	________.
PART 3    EXECUTION
3.1	EXAMINATION AND PREPARATION
A.	Do not proceed with installation until substrates have been properly prepared and deviations from manufacturer's recommended tolerances are corrected. Commencement of installation constitutes acceptance of conditions.
B.	If preparation is the responsibility of another installer, notify Architect in writing of deviations from manufacturer's recommended installation tolerances and conditions.
C.	Additional Field Application Details: 
1.	________.
2.	________.
3.2	INSTALLATION 
A.	Install in accordance with manufacturer's instructions, approved submittals and in proper relationship with adjacent construction. 
1.	Install support brackets and with clearance sufficient to permit unencumbered operation of shade and hardware as recommended by manufacturer. 
2.	Test for proper operation and adjust until satisfactory results are obtained. 
B.	Fabric: Install straight and flat without buckling or distortion. Shade fabric shall not telescope on the roll.
C.	Demonstration: Installer shall demonstrate shade to be in uniform and smooth working order.
D.	Additional Field Application Details: 
1.	________.
2.	________.
3.3	PROTECTION 
A.	Protect installed products until completion of project.
B.	Touch-up, repair or replace damaged products before Substantial completion.
C.	Additional Field Application Details: 
1.	________.
2.	________.

END OF SECTION