SECTION 10 71 13.13

EXTERIOR SHUTTERS

Display hidden notes to specifier. (Don't know how? Click Here) 
 Copyright 2021 -  2021 ARCAT, Inc. - All rights reserved

PART 1    GENERAL
1.1	RELATED SECTIONS
A.	Functional exterior shutters.
B.	Exterior shutter hardware.
1.2	RELATED SECTIONS
A.	Section 09 90 00 - Painting and Coating.
1.3	REFERENCES
A.	ASTM International (ASTM):
1.	ASTM C177 - Standard Test Method for Steady-State Heat Flux Measurements and Thermal Transmission Properties by Means of the Guarded-Hot-Plate Apparatus.
B.	American Architectural Manufacturers Association (AAMA):
1.	AAMA 2605 - Superior Performance Metal Finishes.
1.4	SUBMITTALS
A.	Submit under provisions of Section 01 30 00 - Administrative Requirements.
B.	Shop Drawings: Show materials, layout, dimensions, profiles, fasteners and anchors, hardware, finishes, and interface with adjacent construction.
C.	Product Data: Manufacturer's data sheets on each product to be used, including:
1.	Preparation instructions and recommendations.
2.	Storage and handling requirements and recommendations.
3.	Installation methods.
D.	Selection Samples: For each finish product specified, two complete sets of color chips representing manufacturer's 26 standard colors or Custom Colors.
E.	Verification Samples: For each finish product specified, one sample, minimum size 12 inches (305 mm) square, representing actual product, color, and textures.
1.5	QUALITY ASSURANCE
A.	Manufacturer Qualifications: Company specializing in manufacturing products specified in this section with a minimum five years documented experience.
B.	Installer Qualifications: Company specializing in performing Work of this section with minimum two years documented experience with projects of similar scope and complexity.
C.	Source Limitations: Provide each type of product from a single manufacturing source to ensure uniformity.
D.	Mock-Up: Construct a mock-up with actual materials in sufficient time for Architect's review and to not delay construction progress. Locate mock-up as acceptable to Architect and provide temporary foundations and support.
1.	Intent of mock-up is to demonstrate quality of workmanship and visual appearance.
2.	If mock-up is not acceptable, rebuild mock-up until satisfactory results are achieved.
3.	Retain mock-up during construction as a standard for comparison with completed work. 
4.	Do not alter or remove mock-up until work is completed or removal is authorized.
1.6	DELIVERY, STORAGE, AND HANDLING
A.	Deliver materials to site in manufacturer's original, unopened packaging, with labels clearly identifying product name and manufacturer.
B.	Store materials in a clean, cool, and dry area in an upright position and in accordance with manufacturer's instructions. Do not leave unopened shutters in extreme heat and direct sunlight.
C.	Protect materials during handling and installation to prevent damage.
1.7	PROJECT CONDITIONS
A.	Maintain environmental conditions (temperature, humidity, and ventilation) within limits recommended by manufacturer for optimum results. Do not install products under environmental conditions outside manufacturer's absolute limits.
1.8	WARRANTY
A.	Warranty is limited to original purchaser. This is not to supersede warranty available on our website.
1.	Residential Application Warranty:
a.	Deep South Architectural Series Shutters:
1)	Limited Lifetime Warranty: Structural components and finish under normal weather conditions.
b.	Artisan Architectural Series Shutters:
1)	Limited Lifetime Warranty: Structural components and finish under normal weather conditions.
c.	Classic Architectural Series Shutters:
1)	Limited Lifetime Warranty: Structural components and finish under normal weather conditions.
d.	E-Class Series Shutters:
1)	Warranty: 15 years on structural components and finish under normal weather conditions. 
2.	Commercial and Rental Application Warranty:
a.	Warranty: 10 years on structural components and finish under normal weather conditions. 
PART 2    PRODUCTS
2.1	MANUFACTURERS
A.	Acceptable Manufacturer: New Horizon Shutters International, LLC, which is located at:<BR />7259 Spa Rd., Suite A<BR />North Charleston, SC 29418<BR />Tel: 843-797-7762<BR />Email: request info (info+arcat@newhorizonshutters.com);Web: https://www.newhorizonshutters.com 
B.	Substitutions: Not permitted.
C.	Requests for substitutions will be considered in accordance with provisions of Section 01 60 00 - Product Requirements.
2.2	PERFORMANCE AND DESIGN REQUIREMENTS
A.	Thermal Stability: High impact polystyrene (HIPS) and/or aluminum structural louvers finished with Sherwin Williams two-part Polyurethane Enamel are thermally stable up to 200 degrees F (94 degrees C). 
B.	Thermal Stability: reinforced aluminum structural louvers for wider spans up to 48 inches ( mm) and vertical stiles finished with Sherwin Williams two-part Polyurethane Enamel thermally stable up to 800 degrees F (427 degrees C).
C.	Shutter Finish: Certified to AAMA 2605 specifications.
D.	Thermal Stability: Structural Expanded Foam PVC horizontal rails and shutter core finished with Sherwin Williams two-part Polyurethane Enamel thermally stable up to 200 degrees F (94 degrees C) withASTM C177 and class A fire rating.
2.3	SHUTTERS
A.	Shutter Style: Raised Panel by New Horizon Shutters International LLC. 
1.	Fabrication: Structural Expanded Foam PVC.
a.	Sheet machined and interlocked with reinforced aluminum structural vertical stiles.
2.	Finish: Sherwin Williams 2-part Polyurethane Enamel, certified to AAMA 2605 specifications.
3.	Series: Deep South Architectural.
a.	Thickness of Finished Shutter: 1-3/4 inch (44.5 mm).
b.	Vertical Stile Width: 2 inch (51 mm).
c.	Options:
1)	Standard two panel.
2)	Single panel.
3)	Extra panel (3 panel or 4 panel).
4)	Recessed flat panel.
5)	Custom rail location. 
6)	Custom rail sizes.
7)	Arch or radius top.
8)	V-Groove flat panel.
9)	V-Groove framed recessed panel. Vertical V-Groove.
10)	V-Groove framed recessed panel. Diagonal V-Groove.
11)	Cut out.
12)	Vertical Stile Width: 4 inch (102 mm).
13)	Bifold.
14)	Copper cap.
15)	Vertical center stile.
16)	Custom make.
4.	Series: Artisan Architectural.
a.	Thickness of Finished Shutter: 1-1/4 inch (32 mm).
b.	Vertical Stile Width: 2-1/2 (64 mm).
c.	Options:
1)	Standard two panel.
2)	Single panel.
3)	Extra panel (3 panel or 4 panel).
4)	Recessed flat panel.
5)	Custom rail location. 
6)	Custom rail sizes.
7)	Arch or radius top.
8)	V-Groove framed recessed panel. Vertical V-Groove.
9)	V-Groove framed recessed panel. Diagonal V-Groove.
10)	Cut out.
11)	Rabbeted stile.
12)	Bifold.
13)	Horns: 3/4 inch (19 mm).
14)	Copper cap.
15)	Vertical center stile.
16)	Custom make.
5.	Series: Classic Architectural.
a.	Thickness of Finished Shutter: 1-1/4 inch (32 mm).
b.	Vertical Stile Width: 2-1/2 (64 mm).
c.	Options:
1)	Standard two panel.
2)	Single panel.
3)	Extra panel (3 panel or 4 panel).
4)	Recessed flat panel.
5)	Custom rail location.
6)	Custom rail sizes.
7)	Arch or radius top.
8)	V-Groove flat panel.
9)	V-Groove framed recessed panel. Vertical V-Groove.
10)	V-Groove framed recessed panel. Diagonal V-Groove.
11)	Cut out.
12)	Rabbeted stile.
13)	Bifold.
14)	Horns: 3/4 inch (19 mm).
15)	Impact rated.
16)	Copper cap.
17)	Vertical center stile.
18)	Custom make.
6.	Series: E-Class:
a.	Thickness of Finished Shutter: 1 inch (25 mm).
b.	Vertical Stile Width: 2 inch (51 mm).
c.	Options:
1)	Standard two panel.
2)	Single panel.
3)	Extra panel (3 panel).
4)	Custom rail location. 
5)	Custom rail sizes.
6)	Arch or radius top.
7)	Cut out. 
8)	Bifold.
9)	Horns: 3/4 inch (19 mm).
7.	Width: _____ inch (____ mm).
8.	Width: As indicated on the Drawings.
9.	Height: _____ inch (____ mm).
10.	Height: As indicated on the Drawings.
11.	Color: Bahama Blue 113.
12.	Color: Black 125.
13.	Color: Black Forest Green 122.
14.	Color: Board and Batten Red 110.
15.	Color: Bordeaux 111.
16.	Color: Charleston Green (New) 123.
17.	Color: Charleston Green (Old) 124.
18.	Color: Chelsea Gray 105.
19.	Color: Classic White 101.
20.	Color: Deep Sea Blue 116.
21.	Color: Driftwood 103.
22.	Color: Essex Green 119.
23.	Color: Evergreen 120.
24.	Color: Federal Brown 109.
25.	Color: Forest Green 118.
26.	Color: Hamilton Blue 115.
27.	Color: Hunter Green 117.
28.	Color: Pewter 104.
29.	Color: Polished Mahogany 112.
30.	Color: Quaker Bronze 108.
31.	Color: Roycroft Bottle Green 121.
32.	Color: Roycroft Pewter 106.
33.	Color: Stratford Blue 114.
34.	Color: Tricorn Black 126.
35.	Color: Weathered Shingle 107.
36.	Color: White 102.
37.	Color: Custom color as selected.
B.	Shutter Style: Louver Shutters by New Horizon Shutters International LLC.
1.	Fabrication:
a.	Structural Vertical Stiles: Reinforced aluminum.
b.	Horizontal Rails: Structural expanded foam PVC horizontal rails.
1)	Machined and interlocked with structural vertical stiles.
c.	Structural Louvers: High impact polystyrene and/or aluminum.
2.	Finish: Sherwin Williams 2-part Polyurethane Enamel, certified to AAMA 2605 specifications.
3.	Series: Deep South Architectural.
a.	Thickness of Finished Shutter: 1-3/4 inch (44.5 mm).
b.	Louver Size: 2 inch (51 mm). Rounded.
c.	Vertical Stile Width: 2 inch (51 mm).
d.	Options:
1)	Standard two panel.
2)	Single panel.
3)	Extra panel (3 panel or 4 panel).
4)	Custom rail location.
5)	Custom rail sizes.
6)	Custom louver spacing.
7)	Full louver or solid panel arch or radius top.
8)	Vertical Stile Width: 4 inch (102 mm).
9)	Decorative tilt rod.
10)	Bifold.
11)	Copper cap.
12)	Vertical center stile.
13)	Custom make.
4.	Series: Artisan Architectural.
a.	Thickness of Finished Shutter: 1-1/4 inch (32 mm).
b.	Louver Size: 2 inch (51 mm). Flat-edged.
c.	Vertical Stile Width: 2 inch (51 mm).
d.	Options:
1)	Standard two panel.
2)	Single panel.
3)	Extra panel (3 panel or 4 panel).
4)	Custom rail location.
5)	Custom rail sizes.
6)	Custom louver spacing.
7)	Full louver or solid panel arch or radius top.
8)	Rabbeted stile.
9)	Bifold.
10)	Horns: 3/4 inch (19 mm).
11)	Copper cap.
12)	Vertical center stile.
13)	Bead surrounding louver sections.
14)	Diagonal louver.
15)	Custom make.
5.	Series: Classic Architectural.
a.	Thickness of Finished Shutter: 1-1/4 inch (32 mm).
b.	Louver Size: 1-1/2 inch (51 mm), Rounded.
c.	Vertical Stile Width: 2-1/2 (64 mm).
d.	Options:
1)	Standard two panel.
2)	Single panel.
3)	Extra panel (3 panel or 4 panel).
4)	Custom rail location.
5)	Custom rail sizes.
6)	Custom louver spacing.
7)	Full louver or solid panel arch or radius top.
8)	Decorative tilt rod.
9)	Rabbeted stile.
10)	Bifold.
11)	Horns: 3/4 inch (19 mm).
12)	Impact rated.
13)	Copper cap.
14)	Vertical center stile.
15)	Custom make.
6.	Series: E-Class.
a.	Thickness of Finished Shutter: 1 inch (25 mm).
b.	Louver Size: 1-1/4 inch (32 mm). Rounded.
c.	Vertical Stile Width: 2 inch (51 mm).
d.	Options:
1)	Standard two panel.
2)	Single panel.
3)	Extra panel (3 panel).
4)	Custom rail location. 
5)	Custom rail sizes.
6)	Solid panel arch or radius top.
7)	Decorative tilt rod.
8)	Bifold.
9)	Horns: 3/4 inch (19 mm).
7.	Width: _____ inch (____ mm).
8.	Width: As indicated on the Drawings.
9.	Height: _____ inch (____ mm).
10.	Height: As indicated on the Drawings.
11.	c Bahama Blue 113.
12.	Color: Black 125.
13.	Color: Black Forest Green 122.
14.	Color: Board & Batten Red 110.
15.	Color: Bordeaux 111.
16.	Color: Charleston Green (New) 123.
17.	Color: Charleston Green (Old) 124.
18.	Color: Chelsea Gray 105.
19.	Color: Classic White 101.
20.	Color: Deep Sea Blue 116.
21.	Color: Driftwood 103.
22.	Color: Essex Green 119.
23.	Color: Evergreen 120.
24.	Color: Federal Brown 109.
25.	Color: Forest Green 118.
26.	Color: Hamilton Blue 115.
27.	Color: Hunter Green 117.
28.	Color: Pewter 104.
29.	Color: Polished Mahogany 112.
30.	Color: Quaker Bronze 108.
31.	Color: Roycroft Bottle Green 121.
32.	Color: Roycroft Pewter 106.
33.	Color: Stratford Blue 114.
34.	Color: Tricorn Black 126.
35.	Color: Weathered Shingle 107.
36.	Color: White 102.
37.	Color: Custom color as selected by the Architect.
C.	Shutter Style: Board and Batten Shutters by New Horizon Shutters International LLC.
1.	Fabrication: Structural Expanded Foam PVC sheet machined.
a.	Structural Vertical Stiles: Reinforced aluminum.
2.	Finish: Sherwin Williams 2-part Polyurethane Enamel, certified to AAMA 2605 specifications.
3.	Series: Deep South Architectural.
a.	Thickness of Finished Shutter: 2-1/4 inch (57 mm).
b.	Vertical Stile Width: 2 inch (51 mm).
c.	Options:
1)	Standard panel.
2)	Z-bar (cross buck).
3)	Extra batten.
4)	No battens.
5)	Arch or radius top.
6)	Cut out.
7)	4 inch (102 mm) width vertical stile.
8)	Bifold.
9)	Copper Cap.
4.	Series: Classic Architectural.
a.	Thickness of Finished Shutter: 1-3/4 inch (44.5 mm).
b.	Vertical Stile Width: 2-1/2 (64 mm).
c.	Options:
1)	Standard panel.
2)	Z-bar (cross buck).
3)	Extra batten.
4)	No battens.
5)	Arch or radius top.
6)	Cut out.
7)	Rabbeted stile.
8)	Bifold.
9)	Horns: 3/4 inch (19 mm).
10)	Impact rated.
11)	Copper cap.
5.	Series: E-Class.
a.	Thickness of Finished Shutter: 2 inch (51 mm).
b.	Options: 
1)	Standard panel.
2)	Z-bar (cross buck).
3)	Extra batten.
4)	No battens.
5)	Arch or radius top.
6)	Cut out.
7)	Bifold.
8)	Horns: 3/4 inch (19 mm).
6.	Width: _____ inch (____ mm).
7.	Width: As indicated on the Drawings.
8.	Height: _____ inch (____ mm).
9.	Height: As indicated on the Drawings.
10.	Color: Bahama Blue 113.
11.	Color: Black 125.
12.	Color: Black Forest Green 122.
13.	Color: Board & Batten Red 110.
14.	Color: Bordeaux 111.
15.	Color: Charleston Green (New) 123.
16.	Color: Charleston Green (Old) 124.
17.	Color: Chelsea Gray 105.
18.	Color: Classic White 101.
19.	Color: Deep Sea Blue 116.
20.	Color: Driftwood 103.
21.	Color: Essex Green 119.
22.	Color: Evergreen 120.
23.	Color: Federal Brown 109.
24.	Color: Forest Green 118.
25.	Color: Hamilton Blue 115.
26.	Color: Hunter Green 117.
27.	Color: Pewter 104.
28.	Color: Polished Mahogany 112.
29.	Color: Quaker Bronze 108.
30.	Color: Roycroft Bottle Green 121.
31.	Color: Roycroft Pewter 106.
32.	Color: Stratford Blue 114.
33.	Color: Tricorn Black 126.
34.	Color: Weathered Shingle 107.
35.	Color: White 102.
36.	Color: Custom as selected.
D.	Shutter Style: Combination Shutters by New Horizon Shutters International LLC. 
1.	Fabrication: 
a.	Structural Vertical Stiles: Reinforced aluminum. 
b.	Horizontal Rails: Structural expanded foam PVC horizontal rails. 
1)	Machined and interlocked with structural vertical stiles.
c.	Structural Louvers: High impact polystyrene and/or aluminum. 
2.	Finish: Sherwin Williams 2-part Polyurethane Enamel, certified to AAMA 2605 specifications.
3.	Series: Deep South Architectural.
a.	Thickness of Finished Shutter: 1-3/4 inch (44.5 mm).
b.	Louver Size: 2 inch (51 mm). Rounded.
c.	Vertical Stile Width: 2 inch (51 mm).
d.	Options:
1)	Standard two panel.
2)	Single panel.
3)	Extra panel (3 panel or 4 panel).
4)	Custom rail location.
5)	Custom rail sizes.
6)	Custom louver spacing.
7)	Full louver or solid panel arch or radius top.
8)	Vertical Stile Width: 4 inch (102 mm).
9)	Decorative tilt rod.
10)	Bifold.
11)	Copper cap.
12)	Vertical center stile.
13)	Custom make.
4.	Series: Artisan Architectural.
a.	Thickness of Finished Shutter: 1-1/4 inch (32 mm).
b.	Louver Size: 2 inch (51 mm). Flat-edged.
c.	Vertical Stile Width: 2 inch (51 mm).
d.	Options: 
1)	Standard two panel.
2)	Single panel.
3)	Extra panel (3 panel or 4 panel).
4)	Custom rail location. 
5)	Custom rail sizes.
6)	Custom louver spacing.
7)	Full louver or solid panel arch or radius top.
8)	Decorative tilt rod.
9)	Rabbeted stile.
10)	Bifold.
11)	Horns: 3/4 inch (19 mm).
12)	Copper cap.
13)	Vertical center stile.
14)	Bead surrounding louver sections.
15)	Diagonal louver.
16)	Custom make.
5.	Series: Classic Architectural.
a.	Thickness of Finished Shutter: 1-1/4 inch (32 mm).
b.	Louver Size: 1-1/2 inch (51 mm), Rounded.
c.	Vertical Stile Width: 2-1/2 (64 mm).
d.	Options:
1)	Standard two panel.
2)	Single panel.
3)	Extra panel (3 panel or 4 panel).
4)	Custom rail location. 
5)	Custom rail sizes.
6)	Custom louver spacing.
7)	Full louver or solid panel arch or radius top.
8)	Decorative tilt rod.
9)	Rabbeted stile.
10)	Bifold.
11)	Horns: 3/4 inch (19 mm) horns.
12)	Impact rated.
13)	Copper Cap.
14)	Vertical center stile.
15)	Custom make.
6.	Width: _____ inch (____ mm).
7.	Width: As indicated on the Drawings.
8.	Height: _____ inch (____ mm).
9.	Height: As indicated on the Drawings.
10.	Color: Bahama Blue 113.
11.	Color: Black 125.
12.	Color: Black Forest Green 122.
13.	Color: Board & Batten Red 110.
14.	Color: Bordeaux 111.
15.	Color: Charleston Green (New) 123.
16.	Color: Charleston Green (Old) 124.
17.	Color: Chelsea Gray 105.
18.	Color: Classic White 101.
19.	Color: Deep Sea Blue 116.
20.	Color: Driftwood 103.
21.	Color: Essex Green 119.
22.	Color: Evergreen 120.
23.	Color: Federal Brown 109.
24.	Color: Forest Green 118.
25.	Color: Hamilton Blue 115.
26.	Color: Hunter Green 117.
27.	Color: Pewter 104.
28.	Color: Polished Mahogany 112.
29.	Color: Quaker Bronze 108.
30.	Color: Roycroft Bottle Green 121.
31.	Color: Roycroft Pewter 106.
32.	Color: Stratford Blue 114.
33.	Color: Tricorn Black 126.
34.	Color: Weathered Shingle 107.
35.	Color: White 102.
36.	Color: Custom color as selected.
E.	Shutter Style: Bahama (Bermuda) Shutters by New Horizon Shutters International LLC. 
1.	Fabrication:
a.	Structural Vertical Stiles: Reinforced aluminum.
b.	Vertical Mullions: Structural expanded foam PVC sheet.
1)	Machined and interlocked with reinforced aluminum structural vertical stiles.
c.	Horizontal Rails: Structural expanded foam PVC
d.	Structural Louvers: High impact polystyrene and/or aluminum
2.	Finish: Sherwin Williams 2-part Polyurethane Enamel, certified to AAMA 2605 specifications.
3.	Series: Deep South Architectural.
a.	Thickness of Finished Shutter: 1-3/4 inch (44.5 mm).
b.	Louver Size: 2 inch (51 mm). Rounded.
c.	Vertical Stile Width: 2 inch (51 mm).
d.	Options:
1)	Additional rail.
2)	Additional vertical mullions.
3)	Custom louver spacing.
4)	Custom louver angles.
5)	Full louver arch or radius top.
6)	Vertical Stiles 4 inch (102 mm) wide.
7)	Decorative tilt rod.
8)	Custom make.
4.	Series: Artisan Architectural.
a.	Thickness of Finished Shutter: 1-1/4 inch (32 mm).
b.	Louver Size: 2 inch (51 mm). Flat-edged.
c.	Vertical Stile Width: 2 inch (51 mm).
d.	Bead surrounding louver sections
e.	Options: 
1)	Additional rail.
2)	Additional vertical mullions.
5.	Series: Classic Architectural.
a.	Thickness of Finished Shutter: 1-1/4 inch (32 mm).
b.	Louver Size: 1-1/2 inch (51 mm), Rounded.
c.	Vertical Stile Width: 2-1/2 (64 mm).
d.	Options:
1)	Additional rail.
2)	Additional vertical mullions.
3)	Custom louver spacing.
4)	Custom louver angles.
5)	Full louver arch or radius top.
6)	Decorative tilt rod.
7)	Custom make.
6.	Width:
7.	Width; Single Panel: _____ inch (____ mm).
8.	Width; Double Panel with Vertical Mullion: _____ inch (____ mm).
9.	Width; Triple Panel with Vertical Mullions: _____ inch (____ mm).
10.	Width; Four Panel with Vertical Mullions: _____ inch (____ mm).
11.	Width; As indicated on the Drawings.
12.	Height:
13.	Height: _____ inch (____ mm).
14.	Height: As indicated on the Drawings.
15.	Color: Bahama Blue 113.
16.	Color: Black 125.
17.	Color: Black Forest Green 122.
18.	Color: Board & Batten Red 110.
19.	Color: Bordeaux 111.
20.	Color: Charleston Green (New) 123.
21.	Color: Charleston Green (Old) 124.
22.	Color: Chelsea Gray 105.
23.	Color: Classic White 101.
24.	Color: Deep Sea Blue 116.
25.	Color: Driftwood 103.
26.	Color: Essex Green 119.
27.	Color: Evergreen 120.
28.	Color: Federal Brown 109.
29.	Color: Forest Green 118.
30.	Color: Hamilton Blue 115.
31.	Color: Hunter Green 117.
32.	Color: Pewter 104.
33.	Color: Polished Mahogany 112.
34.	Color: Quaker Bronze 108.
35.	Color: Roycroft Bottle Green 121.
36.	Color: Roycroft Pewter 106.
37.	Color: Stratford Blue 114.
38.	Color: Tricorn Black 126.
39.	Color: Weathered Shingle 107.
40.	Color: White 102.
41.	Color: Custom color as selected.
2.4	HARDWARE
A.	Hardware: Raised Panel, Louver, Combination, or Board and Batten Shutters.
1.	Pintel Plate Size: 1-1/2 x 1/8 inch (38 x 3 mm). Provide in same size pairs.
a.	Pin Diameter: 3/8 inch (10 mm).
b.	Material: Type 304 Stainless Steel. Finish: Matte black powder coat.
c.	Offsets: 1/2 inch (13 mm).
d.	Offsets: 1-1/2 inch (38 mm).
e.	Offsets: 2-1/4 inch (57 mm).
f.	Offsets: 3-1/4 inch (83 mm).
2.	Pintel Plate Size: 3/4 x 1/8 inch (19 x 3 mm). Provide in same size pairs.
a.	Pin Diameter: 3/8 inch (10 mm).
b.	Material: Type 304 Stainless Steel. Finish: Matte black powder coat.
c.	Offsets: 1/2 inch (13 mm).
d.	Offsets: 1-1/2 inch (38 mm).
e.	Offsets: 2-1/4 inch (57 mm).
f.	Offsets: 3-1/4 inch (83 mm).
3.	Lag Pintel: 6 inch (152 mm). Provide in same size pairs.
a.	Material: Type 304 Stainless Steel. Finish: Matte black powder coat.
b.	Jamb Pintel (Leaf Pintel): Provide in same size pairs.
c.	Material: Type 304 Stainless Steel. Finish: Matte black powder coat.
d.	Offsets: 1-1/4 inch (32 mm).
e.	Offsets: 2-1/4 inch (57 mm).
4.	L-Hinge: 6 inch (152 mm). Provide in same size pairs.
a.	Material: Type 304 Stainless Steel. Finish: Matte black powder coat.
b.	Offsets: 0 inch (flat).
c.	Offsets: 1/2 inch (13 mm).
d.	Offsets: 1-1/2 inch (38 mm).
e.	Offsets: 1-3/4 inch (45 mm). 
f.	Offsets: 2-1/4 inch (57 mm).
5.	Strap Hinge: 10 inch (254 mm): Provide in same size pairs.
a.	Material: Type 304 Stainless Steel. Finish: Matte black powder coat.
b.	Offsets: 0 inch (flat).
c.	Offsets: 1/2 inch (13 mm).
d.	Offsets: 1-1/2 inch (38 mm).
e.	Offsets: 1-3/4 inch (45 mm). 
f.	Offsets: 2-1/4 inch (57 mm).
6.	Strap Hinge: 12-inch (305 mm). Provide in same size pairs.
a.	Material: Type 304 Stainless Steel. Finish: Matte black powder coat.
b.	Offsets: 1/2 inch (13 mm).
7.	Flat Hinge (center hinge): Provide in same size pairs.
a.	Material: Type 304 Stainless Steel. Finish: Matte black powder coat.
b.	Offsets: 0 inch (flat).
c.	Offsets: 1/2 inch (13 mm).
d.	Offsets: 1-3/4 inch (45 mm).
e.	Offsets: 2-1/4 inch (57 mm).
8.	Holdback: S style.
a.	Material: Type 304 Stainless Steel. Finish: Matte black powder coat.
b.	Material: Type 304 Stainless Steel lag bolt.
9.	Holdback: Acorn style.
a.	Material: Type 304 Stainless steel.
10.	Holdback: Rat Tail style.
a.	Material: Type 304 Stainless Steel. Finish: Matte black powder coat.
11.	Holdback: Propeller style.
a.	Material: Type 304 Stainless Steel. Finish: Matte black powder coat.
12.	Holdback: 15 inch Hook and Eye Screw
a.	Material: Galvanized Carbon steel.
13.	Holdback: 22 inch Hook and Eye Plate Mount.
a.	Material: Type 304 Stainless Steel. Finish: Matte black powder coat.
14.	Shutter Lock: Slide Bolt, 12-inch (305 mm). 
a.	Material: Type 304 Stainless Steel. Finish: Matte black powder coat.
15.	Shutter Lock: Barrel Bolt, 4 inch (102 mm).
a.	Material: Type 304 Stainless Steel. Finish: Matte black powder coat.
16.	Shutter Lock: Cane Bolt.
a.	Type 304 Stainless Steel.
17.	Shutter Lock: 4 inch Hook and Eye Plate Mount.
a.	Material: Type 304 Stainless Steel. Finish: Matte black powder coat.
18.	Pull Ring: 
a.	Material: Type 304 Stainless Steel. Finish: Matte black powder coat.
b.	Plate mount.
19.	Fixed Mounting Bracket: Material: Clear polycarbonate,
20.	Pintel Shim: Stackable, black polyamide plastic, 1/4 inch (6 mm) thick.
B.	Hardware: Bahama Shutters.
1.	Male Hinge: Plate size: 1-1/8 inch (28 mm) backplate.
2.	Female Hinge: Standard.
a.	Plate Size: 1-1/4 inch (32 mm) with 1/4 inch (6 mm) lip.
b.	Projection: 2-3/8 inch (60 mm).
3.	Female Hinge: One inch build out.
a.	Plate Size: 1-1/4 inch (32 mm) with 1/4 inch (6 mm) lip.
b.	Projection: 3-3/8 inch (86 mm).
4.	Female Hinge: Lintel.
a.	Plate Size: 3-3/8 inch (86 mm) with 1/4 inch (6 mm) lip.
b.	Projection: 0 inch (0 mm).
5.	Standoff Rods: Material: Aluminum. 
a.	End Caps: Nylon
b.	End Caps: Type 304 stainless steel.
c.	Deck hinges. Eye end sets.
6.	Standoff Rods: Telescoping. Material: Aluminum .
7.	Standoff Rods: Square. Material: Aluminum. Deck Hinges: Aluminum with pin or bolt.
8.	Standoff Rods: Material: Type 304 Stainless steel. Clevis pins. 
PART 3    EXECUTION
3.1	EXAMINATION
A.	Do not begin installation until shutters have been properly prepared.
3.2	PREPARATION
A.	Clean surfaces thoroughly prior to installation.
3.3	INSTALLATION
A.	Install in accordance with manufacturer's instructions.
B.	Adjust operable units for smooth unobstructed operation.
3.4	PROTECTION
A.	Protect installed products from damage by weather and other work until Date of Substantial Completion.
B.	Touch-up and repair damaged products before Date of Substantial Completion.

END OF SECTION