SECTION 10 31 00.10

CUSTOM GAS BURNING FIREPLACES

Display hidden notes to specifier. (Don't know how? Click Here) 
 Copyright 2015 -  2022 ARCAT, Inc. - All rights reserved

PART 1    GENERAL
1.1	SECTION INCLUDES
A.	Custom Manufactured Gas Fireplaces.
1.2	RELATED SECTIONS
A.	Section 04 22 00.16 - Surface-Bonded Concrete Unit Masonry.
B.	Section 06 10 00 - Rough Carpentry.
C.	Section 09 29 00 - Gypsum Board.
D.	Section 22 10 00 - Plumbing Piping.
E.	Section 26 05 00 - Common Work Results for Electrical
1.3	REFERENCES
A.	ANSI Z21.50b - Vented Gas Fireplaces.
B.	CSA 2.22b - Vented Gas Fireplaces.
1.4	SUBMITTALS
A.	Submit under provisions of Section 01 30 00 - Administrative Requirements.
B.	Product Data: Manufacturer's data sheets on each product to be used, including:
1.	Storage and handling requirements and recommendations.
2.	Preparation instructions and recommendations.
3.	Framing sizes and requirements.
4.	Installation methods.
1.5	DELIVERY, STORAGE, AND HANDLING
A.	Store products in manufacturer's unopened packaging until ready for installation.
B.	Store products in covered area, well protected from weather.
PART 2    PRODUCTS
2.1	MANUFACTURERS
A.	Acceptable Manufacturer: DaVinci Custom Fireplaces - a division of Travis Industries, which is located at:<BR />12521 Harbour Reach Dr.<BR />Mukilteo, WA 98275<BR />Toll Free Tel: 800-654-1177<BR />Tel: 425-609-2500<BR />Fax: 425-609-2781<BR />Email: request info (b.barber@travisindustries.com);Web: https://www.davincifireplace.com 
B.	Substitutions: Not permitted.
C.	Requests for substitutions will be considered in accordance with provisions of Section 01 60 00 - Product Requirements.
2.2	CUSTOM GAS BURNING FIREPLACES / CATEGORY 1
A.	Description: DaVinci custom, decorative gas burning fireplace.
1.	Decorative Fireplace Rated ANSI Z21.50b-2014 / CSA 2.22b-2014
2.	Safe Touch Glass: Hi-tech air flow system keeps the glass cool to the touch.
3.	Zero clearance 
4.	Multi-color interior LED lighting
5.	Outside air direct vent.
6.	Heat Optional, HeatSmart kit (heat exchanger)
B.	DaVinci Single-Sided Custom Linear Fireplace: 
1.	Category 1: 
a.	Nominal Opening Size: 
1)	24 inches W by 12 inches H by 20 inches D
2)	24 inches W by 20 inches H by 20 inches D
3)	24 inches W by 30 inches H by 20 inches D
4)	24 inches W by 36 inches H by 20 inches D
5)	24 Inches W by 48 inches H by 20 inches D
6)	24 inches W by 58 inches H by 20 inches D
7)	36 inches W by 12 inches H by 20 inches D
8)	36 inches W by 20 inches H by 20 inches D
9)	36 inches W by 30 inches H by 20 inches D
10)	36 inches W by 36 inches H by 20 inches D
11)	36 Inches W by 48 inches H by 20 inches D
12)	36 inches W by 58 inches H by 20 inches D 
13)	48 inches W by 12 inches H by 20 inches D
14)	48 inches W by 20 inches H by 20 inches D
15)	48 inches W by 30 inches H by 20 inches D
16)	48 inches W by 36 inches H by 20 inches D
17)	48 inches W by 48 inches H by 20 inches D
18)	48 inches W by 58 inches H by 20 inches D 
19)	60 inches W by 12 inches H by 20 inches D
20)	60 inches W by 20 inches H by 20 inches D
21)	60 inches W by 30 inches H by 20 inches D
22)	60 inches W by 36 inches H by 20 inches D
23)	60 inches W by 48 inches H by 20 inches D 
24)	60 inches W by 58 inches H by 20 inches D 
2.	Category 2: 
a.	Nominal Opening Size: 
1)	72 inches W by 12 inches H by 20 inches D
2)	72 inches W by 20 inches H by 20 inches D
3)	72 inches W by 30 inches H by 20 inches D
4)	72 inches W by 36 inches H by 20 inches D
5)	72 inches W by 48 inches H by 20 inches D
6)	72 inches W by 58 inches H by 20 inches D 
7)	84 inches W by 12 inches H by 20 inches D
8)	84 inches W by 20 inches H by 20 inches D
9)	84 inches W by 30 inches H by 20 inches D
10)	84 inches W by 36 inches H by 20 inches D
11)	84 inches W by 48 inches H by 20 inches D 
12)	84 inches W by 58 inches H by 20 inches D 
13)	96 inches W by 12 inches H by 20 inches D
14)	96 inches W by 20 inches H by 20 inches D
15)	96 inches W by 30 inches H by 20 inches D
16)	96 inches W by 36 inches H by 20 inches D
17)	96 inches W by 48 inches H by 20 inches D 
18)	96 inches W by 58 inches H by 20 inches D 
19)	108 inches W by 12 inches H by 20 inches D
20)	108 inches W by 20 inches H by 20 inches D
21)	108 inches W by 30 inches H by 20 inches D
22)	108 inches W by 36 inches H by 20 inches D
23)	108 inches W by 48 inches H by 20 inches D
24)	108 inches W by 58 inches H by 20 inches D 
25)	120 inches W by 12 inches H by 20 inches D
26)	120 inches W by 20 inches H by 20 inches D
27)	120 inches W by 30 inches H by 20 inches D
28)	120 inches W by 36 inches H by 20 inches D
29)	120 inches W by 48 inches H by 20 inches D
30)	120 inches W by 58 inches H by 20 inches D 
3.	Category 3: 
a.	Nominal Opening Size: 
1)	132 inches W by 12 inches H by 20 inches D
2)	132 inches W by 20 inches H by 20 inches D
3)	132 inches W by 30 inches H by 20 inches D
4)	132 inches W by 36 inches H by 20 inches D
5)	132 inches W by 48 inches H by 20 inches D
6)	132 inches W by 58 inches H by 20 inches D 
7)	144 inches W by 12 inches H by 20 inches D
8)	144 inches W by 20 inches H by 20 inches D
9)	144 inches W by 30 inches H by 20 inches D
10)	144 inches W by 36 inches H by 20 inches D
11)	144 inches W by 48 inches H by 20 inches D
12)	144 inches W by 58 inches H by 20 inches D 
13)	156 inches W by 12 inches H by 20 inches D
14)	156 inches W by 20 inches H by 20 inches D
15)	156 inches W by 30 inches H by 20 inches D
16)	156 inches W by 36 inches H by 20 inches D
17)	156 inches W by 48 inches H by 20 inches D
18)	156 inches W by 58 inches H by 20 inches D 
19)	168 inches W by 12 inches H by 20 inches D
20)	168 inches W by 20 inches H by 20 inches D
21)	168 inches W by 30 inches H by 20 inches D
22)	168 inches W by 36 inches H by 20 inches D
23)	168 inches W by 48 inches H by 20 inches D
24)	168 inches W by 58 inches H by 20 inches D 
25)	180 inches W by 12 inches H by 20 inches D
26)	180 inches W by 20 inches H by 20 inches D
27)	180 inches W by 30 inches H by 20 inches D
28)	180 inches W by 36 inches H by 20 inches D
29)	180 inches W by 48 inches H by 20 inches D
30)	180 inches W by 58 inches H by 20 inches D 
4.	Category 4: 
a.	Nominal Opening Size: 
1)	192 inches W by 12 inches H by 20 inches D
2)	192 inches W by 20 inches H by 20 inches D
3)	192 inches W by 30 inches H by 20 inches D
4)	192 inches W by 36 inches H by 20 inches D
5)	192 inches W by 48 inches H by 20 inches D
6)	192 inches W by 58 inches H by 20 inches D 
7)	204 inches W by 12 inches H by 20 inches D
8)	204 inches W by 20 inches H by 20 inches D
9)	204 inches W by 30 inches H by 20 inches D
10)	204 inches W by 36 inches H by 20 inches D
11)	204 inches W by 48 inches H by 20 inches D
12)	204 inches W by 58 inches H by 20 inches D 
13)	216 inches W by 12 inches H by 20 inches D
14)	216 inches W by 20 inches H by 20 inches D
15)	216 inches W by 30 inches H by 20 inches D
16)	216 inches W by 36 inches H by 20 inches D
17)	216 inches W by 48 inches H by 20 inches D
18)	216 inches W by 58 inches H by 20 inches D 
19)	228 inches W by 12 inches H by 20 inches D
20)	228 inches W by 20 inches H by 20 inches D
21)	228 inches W by 30 inches H by 20 inches D
22)	228 inches W by 36 inches H by 20 inches D
23)	228 inches W by 48 inches H by 20 inches D
24)	228 inches W by 58 inches H by 20 inches D 
25)	240 inches W by 12 inches H by 20 inches D
26)	240 inches W by 20 inches H by 20 inches D
27)	240 inches W by 30 inches H by 20 inches D
28)	240 inches W by 36 inches H by 20 inches D
29)	240 inches W by 48 inches H by 20 inches D
30)	240 inches W by 58 inches H by 20 inches D 
5.	Vent:
6.	a. 10 inch B-Vent Chimney, quantity as recommended by the installer
7.	b.8 Inch B-Vent Chimney, quantity as recommended by the installer
8.	Peak and Valley Burner
9.	Gas Input: Up to 14,500 BTUs/foot with natural gas or propane
10.	Power Exhaust Fan: 
a.	RS12 Low Volume External Power Exhaust Fan
b.	RSIF 160 Low Volume Inline Power Exhaust Fan
c.	RS16 High Volume External Power Exhaust Fan
d.	RSIF 180 High Volume Inline Power Exhaust Fan
11.	Touch Smart wall control:
a.	Black Glass with timer
b.	Black Glass with variable blower speed (for use with heat exchanger)
c.	White Glass with timer
d.	White Glass with variable blower speed (for use with heat exchanger)
12.	Touch Smart Wall Switch Wire Harness:
a.	25 foot 
b.	50 foot
c.	100 foot
13.	Power Exhaust Fan Wire Harness:
a.	50 foot
b.	150 foot
c.	250 foot 
14.	Fireback:
a.	Silver Painted
b.	Matte Black Painted
c.	Gloss Black Enamel 
d.	Black Glass
15.	Burner Decor:
a.	Platinum Crushed Glass 
b.	Black Crushed Glass 
c.	Rock Embers 
16.	Interior Fire Art: 
a.	Twigs & Stones 
b.	Traditional Logs 
c.	Driftwood 
d.	Tumbled Stones 
e.	Tumbled Stones
f.	Birch
17.	Trim: 
a.	Flat 2 inch Black Trim 
b.	IronWorks Trim, Painted Charcoal 
c.	IronWorks Trim, Black Metalic 
18.	Accessories: 
a.	Tile Stop, 1/2 inch. 
b.	Heat Exchanger
c.	Outdoor Window Kit
d.	Carbon Monoxide Detector
e.	Home Automation Breakout Board
f.	Dehumidifier 
C.	DaVinci Left Side Corner Custom Linear Fireplace: 
1.	Category 1: 
a.	Nominal Opening Size: 
1)	30 inches W by 12 inches H by 20 inches D
2)	30 inches W by 20 inches H by 20 inches D
3)	30 inches W by 30 inches H by 20 inches D
4)	30 inches W by 36 inches H by 20 inches D
5)	30 inches W by 48 inches H by 20 inches D 
6)	30 inches W by 58 inches H by 20 inches D
7)	42 inches W by 12 inches H by 20 inches D
8)	42 inches W by 20 inches H by 20 inches D
9)	42 inches W by 30 inches H by 20 inches D
10)	42 inches W by 36 inches H by 20 inches D
11)	42 inches W by 48 inches H by 20 inches D
12)	42 inches W by 58 inches H by 20 inches D 
13)	54 inches W by 12 inches H by 20 inches D
14)	54 inches W by 20 inches H by 20 inches D
15)	54 inches W by 30 inches H by 20 inches D
16)	54 inches W by 36 inches H by 20 inches D
17)	54 inches W by 48 inches H by 20 inches D 
18)	54 inches W by 58 inches H by 20 inches D 
19)	66 inches W by 12 inches H by 20 inches D
20)	66 inches W by 20 inches H by 20 inches D
21)	66 inches W by 30 inches H by 20 inches D
22)	66 inches W by 36 inches H by 20 inches D
23)	66 inches W by 48 inches H by 20 inches D 
24)	66 inches W by 58 inches H by 20 inches D 
2.	Category 2: 
a.	Nominal Opening Size: 
1)	78 inches W by 12 inches H by 20 inches D
2)	78 inches W by 20 inches H by 20 inches D
3)	78 inches W by 30 inches H by 20 inches D
4)	78 inches W by 36 inches H by 20 inches D
5)	78 inches W by 48 inches H by 20 inches D
6)	78 inches W by 58 inches H by 20 inches D 
7)	90 inches W by 12 inches H by 20 inches D
8)	90 inches W by 20 inches H by 20 inches D
9)	90 inches W by 30 inches H by 20 inches D
10)	90 inches W by 36 inches H by 20 inches D
11)	90 inches W by 48 inches H by 20 inches D
12)	90 inches W by 58 inches H by 20 inches D 
13)	102 inches W by 12 inches H by 20 inches D
14)	102 inches W by 20 inches H by 20 inches D
15)	102 inches W by 30 inches H by 20 inches D
16)	102 inches W by 36 inches H by 20 inches D
17)	102 inches W by 48 inches H by 20 inches D
18)	102 inches W by 58 inches H by 20 inches D 
19)	114 inches W by 12 inches H by 20 inches D
20)	114 inches W by 20 inches H by 20 inches D
21)	114 inches W by 30 inches H by 20 inches D
22)	114 inches W by 36 inches H by 20 inches D
23)	114 inches W by 48 inches H by 20 inches D
24)	114 inches W by 58 inches H by 20 inches D 
25)	126 inches W by 12 inches H by 20 inches D
26)	126 inches W by 20 inches H by 20 inches D
27)	126 inches W by 30 inches H by 20 inches D
28)	126 inches W by 36 inches H by 20 inches D
29)	126 inches W by 48 inches H by 20 inches D
30)	126 inches W by 58 inches H by 20 inches D 
3.	Category 3: 
a.	Nominal Opening Size: 
1)	138 inches W by 12 inches H by 20 inches D
2)	138 inches W by 20 inches H by 20 inches D
3)	138 inches W by 30 inches H by 20 inches D
4)	138 inches W by 36 inches H by 20 inches D
5)	138 inches W by 48 inches H by 20 inches D
6)	138 inches W by 58 inches H by 20 inches D
7)	150 inches W by 12 inches H by 20 inches D
8)	150 inches W by 20 inches H by 20 inches D
9)	150 inches W by 30 inches H by 20 inches D
10)	150 inches W by 36 inches H by 20 inches D
11)	150 inches W by 48 inches H by 20 inches D
12)	150 inches W by 58 inches H by 20 inches D
13)	162 inches W by 12 inches H by 20 inches D
14)	162 inches W by 20 inches H by 20 inches D
15)	162 inches W by 30 inches H by 20 inches D
16)	162 inches W by 36 inches H by 20 inches D
17)	162 inches W by 48 inches H by 20 inches D
18)	162 inches W by 58 inches H by 20 inches D
19)	174 inches W by 12 inches H by 20 inches D
20)	174 inches W by 20 inches H by 20 inches D
21)	174 inches W by 30 inches H by 20 inches D
22)	174 inches W by 36 inches H by 20 inches D
23)	174 inches W by 48 inches H by 20 inches D
24)	174 inches W by 58 inches H by 20 inches D
25)	186 inches W by 12 inches H by 20 inches D
26)	186 inches W by 20 inches H by 20 inches D
27)	186 inches W by 30 inches H by 20 inches D
28)	186 inches W by 36 inches H by 20 inches D
29)	186 inches W by 48 inches H by 20 inches D
30)	186 inches W by 58 inches H by 20 inches D
4.	Category 4: 
a.	Nominal Opening Size: 
1)	198 inches W by 12 inches H by 20 inches D
2)	198 inches W by 20 inches H by 20 inches D
3)	198 inches W by 30 inches H by 20 inches D
4)	198 inches W by 36 inches H by 20 inches D
5)	198 inches W by 48 inches H by 20 inches D
6)	198 inches W by 58 inches H by 20 inches D
7)	210 inches W by 12 inches H by 20 inches D
8)	210 inches W by 20 inches H by 20 inches D
9)	210 inches W by 30 inches H by 20 inches D
10)	210 inches W by 36 inches H by 20 inches D
11)	210 inches W by 48 inches H by 20 inches D
12)	210 inches W by 58 inches H by 20 inches D
13)	222 inches W by 12 inches H by 20 inches D
14)	222 inches W by 20 inches H by 20 inches D
15)	222 inches W by 30 inches H by 20 inches D
16)	222 inches W by 36 inches H by 20 inches D
17)	222 inches W by 48 inches H by 20 inches D
18)	222 inches W by 58 inches H by 20 inches D
19)	234 inches W by 12 inches H by 20 inches D
20)	234 inches W by 20 inches H by 20 inches D
21)	234 inches W by 30 inches H by 20 inches D
22)	234 inches W by 36 inches H by 20 inches D
23)	234 inches W by 48 inches H by 20 inches D
24)	234 inches W by 58 inches H by 20 inches D
25)	246 inches W by 12 inches H by 20 inches D
26)	246 inches W by 20 inches H by 20 inches D
27)	246 inches W by 30 inches H by 20 inches D
28)	246 inches W by 36 inches H by 20 inches D
29)	246 inches W by 48 inches H by 20 inches D
30)	246 inches W by 58 inches H by 20 inches D
5.	Vent:
6.	a.10 inch B-Vent Chimney, quantity as recommended by the installer
7.	b.8 Inch B-Vent Chimney, quantity as recommended by the installer
8.	Peak and Valley Burner
9.	Gas Input: Up to 14,500 BTUs/foot with natural gas or propane
10.	Power Exhaust Fan: 
a.	RS12 Low Volume External Power Exhaust Fan
b.	RSIF 160 Low Volume Inline Power Exhaust Fan
c.	RS16 High Volume External Power Exhaust Fan
d.	RSIF 180 High Volume Inline Power Exhaust Fan
11.	Touch Smart wall control:
a.	Black Glass with timer
b.	Black Glass with variable blower speed (for use with heat exchanger)
c.	White Glass with timer
d.	White Glass with variable blower speed (for use with heat exchanger)
12.	Touch Smart Wire Harness:
a.	25 foot 
b.	50 foot
c.	100 foot
13.	Power Exhaust Fan Wire Harness:
a.	50 foot
b.	150 foot
c.	250 foot 
14.	Fireback:
a.	Silver Painted
b.	Matte Black Painted
c.	Gloss Black Enamel 
d.	Black Glass
15.	Burner Decor: 
a.	Platinum Crushed Glass 
b.	Black Crushed Glass 
c.	Rock Embers 
16.	Interior Fire Art: 
a.	Twigs & Stones 
b.	Traditional Logs 
c.	Driftwood 
d.	Tumbled Stones 
e.	Tumbled Stones
f.	Birch
17.	Trim: 
a.	Flat 2 inch Black Trim 
b.	IronWorks Trim, Painted Charcoal 
c.	IronWorks Trim, Black Metalic 
18.	Accessories: 
a.	Tile Stop, 1/2 inch. 
b.	Heat Exchanger
c.	Carbon Monoxide Detector
d.	Home Automation Breakout Board
e.	Dehumidifier 
D.	DaVinci Right Side Corner Custom Linear Fireplace: 
1.	Category 1: 
a.	Nominal Opening Size: 
1)	30 inches W by 12 inches H by 20 inches D
2)	30 inches W by 20 inches H by 20 inches D
3)	30 inches W by 30 inches H by 20 inches D
4)	30 inches W by 36 inches H by 20 inches D
5)	30 inches W by 48 inches H by 20 inches D 
6)	30 inches W by 58 inches H by 20 inches D
7)	42 inches W by 12 inches H by 20 inches D
8)	42 inches W by 20 inches H by 20 inches D
9)	42 inches W by 30 inches H by 20 inches D
10)	42 inches W by 36 inches H by 20 inches D
11)	42 inches W by 48 inches H by 20 inches D
12)	42 inches W by 58 inches H by 20 inches D 
13)	54 inches W by 12 inches H by 20 inches D
14)	54 inches W by 20 inches H by 20 inches D
15)	54 inches W by 30 inches H by 20 inches D
16)	54 inches W by 36 inches H by 20 inches D
17)	54 inches W by 48 inches H by 20 inches D 
18)	54 inches W by 58 inches H by 20 inches D 
19)	66 inches W by 12 inches H by 20 inches D
20)	66 inches W by 20 inches H by 20 inches D
21)	66 inches W by 30 inches H by 20 inches D
22)	66 inches W by 36 inches H by 20 inches D
23)	66 inches W by 48 inches H by 20 inches D 
24)	66 inches W by 58 inches H by 20 inches D 
2.	Category 2: 
a.	Nominal Opening Size: 
1)	78 inches W by 12 inches H by 20 inches D
2)	78 inches W by 20 inches H by 20 inches D
3)	78 inches W by 30 inches H by 20 inches D
4)	78 inches W by 36 inches H by 20 inches D
5)	78 inches W by 48 inches H by 20 inches D
6)	78 inches W by 58 inches H by 20 inches D 
7)	90 inches W by 12 inches H by 20 inches D
8)	90 inches W by 20 inches H by 20 inches D
9)	90 inches W by 30 inches H by 20 inches D
10)	90 inches W by 36 inches H by 20 inches D
11)	90 inches W by 48 inches H by 20 inches D
12)	90 inches W by 58 inches H by 20 inches D 
13)	102 inches W by 12 inches H by 20 inches D
14)	102 inches W by 20 inches H by 20 inches D
15)	102 inches W by 30 inches H by 20 inches D
16)	102 inches W by 36 inches H by 20 inches D
17)	102 inches W by 48 inches H by 20 inches D
18)	102 inches W by 58 inches H by 20 inches D 
19)	114 inches W by 12 inches H by 20 inches D
20)	114 inches W by 20 inches H by 20 inches D
21)	114 inches W by 30 inches H by 20 inches D
22)	114 inches W by 36 inches H by 20 inches D
23)	114 inches W by 48 inches H by 20 inches D
24)	114 inches W by 58 inches H by 20 inches D 
25)	126 inches W by 12 inches H by 20 inches D
26)	126 inches W by 20 inches H by 20 inches D
27)	126 inches W by 30 inches H by 20 inches D
28)	126 inches W by 36 inches H by 20 inches D
29)	126 inches W by 48 inches H by 20 inches D
30)	126 inches W by 58 inches H by 20 inches D 
3.	Category 3: 
a.	Nominal Opening Size: 
1)	138 inches W by 12 inches H by 20 inches D
2)	138 inches W by 20 inches H by 20 inches D
3)	138 inches W by 30 inches H by 20 inches D
4)	138 inches W by 36 inches H by 20 inches D
5)	138 inches W by 48 inches H by 20 inches D
6)	138 inches W by 58 inches H by 20 inches D
7)	150 inches W by 12 inches H by 20 inches D
8)	150 inches W by 20 inches H by 20 inches D
9)	150 inches W by 30 inches H by 20 inches D
10)	150 inches W by 36 inches H by 20 inches D
11)	150 inches W by 48 inches H by 20 inches D
12)	150 inches W by 58 inches H by 20 inches D
13)	162 inches W by 12 inches H by 20 inches D
14)	162 inches W by 20 inches H by 20 inches D
15)	162 inches W by 30 inches H by 20 inches D
16)	162 inches W by 36 inches H by 20 inches D
17)	162 inches W by 48 inches H by 20 inches D
18)	162 inches W by 58 inches H by 20 inches D
19)	174 inches W by 12 inches H by 20 inches D
20)	174 inches W by 20 inches H by 20 inches D
21)	174 inches W by 30 inches H by 20 inches D
22)	174 inches W by 36 inches H by 20 inches D
23)	174 inches W by 48 inches H by 20 inches D
24)	174 inches W by 58 inches H by 20 inches D
25)	186 inches W by 12 inches H by 20 inches D
26)	186 inches W by 20 inches H by 20 inches D
27)	186 inches W by 30 inches H by 20 inches D
28)	186 inches W by 36 inches H by 20 inches D
29)	186 inches W by 48 inches H by 20 inches D
30)	186 inches W by 58 inches H by 20 inches D
4.	Category 4: 
a.	Nominal Opening Size: 
1)	198 inches W by 12 inches H by 20 inches D
2)	198 inches W by 20 inches H by 20 inches D
3)	198 inches W by 30 inches H by 20 inches D
4)	198 inches W by 36 inches H by 20 inches D
5)	198 inches W by 48 inches H by 20 inches D
6)	198 inches W by 58 inches H by 20 inches D
7)	210 inches W by 12 inches H by 20 inches D
8)	210 inches W by 20 inches H by 20 inches D
9)	210 inches W by 30 inches H by 20 inches D
10)	210 inches W by 36 inches H by 20 inches D
11)	210 inches W by 48 inches H by 20 inches D
12)	210 inches W by 58 inches H by 20 inches D
13)	222 inches W by 12 inches H by 20 inches D
14)	222 inches W by 20 inches H by 20 inches D
15)	222 inches W by 30 inches H by 20 inches D
16)	222 inches W by 36 inches H by 20 inches D
17)	222 inches W by 48 inches H by 20 inches D
18)	222 inches W by 58 inches H by 20 inches D
19)	234 inches W by 12 inches H by 20 inches D
20)	234 inches W by 20 inches H by 20 inches D
21)	234 inches W by 30 inches H by 20 inches D
22)	234 inches W by 36 inches H by 20 inches D
23)	234 inches W by 48 inches H by 20 inches D
24)	234 inches W by 58 inches H by 20 inches D
25)	246 inches W by 12 inches H by 20 inches D
26)	246 inches W by 20 inches H by 20 inches D
27)	246 inches W by 30 inches H by 20 inches D
28)	246 inches W by 36 inches H by 20 inches D
29)	246 inches W by 48 inches H by 20 inches D
30)	246 inches W by 58 inches H by 20 inches D
5.	Vent:
6.	a.10 inch B-Vent Chimney, quantity as recommended by the installer. 
7.	b.8 Inch B-Vent Chimney, quantity as recommended by the installer. 
8.	Peak and Valley Burner
9.	Gas Input: Up to 14,500 BTUs/foot with natural gas or propane 
10.	Power Exhaust Fan: 
a.	RS12 Low Volume External Power Exhaust Fan
b.	RSIF 160 Low Volume Inline Power Exhaust Fan
c.	RS16 High Volume External Power Exhaust Fan
d.	RSIF 180 High Volume Inline Power Exhaust Fan
11.	Touch Smart wall control:
a.	Black Glass with timer
b.	Black Glass with variable blower speed (for use with heat exchanger)
c.	White Glass with timer
d.	White Glass with variable blower speed (for use with heat exchanger)
12.	Touch Smart Wire Harness:
a.	25 foot 
b.	50 foot
c.	100 foot
13.	Power Exhaust Fan Wire Harness:
a.	50 foot
b.	150 foot
c.	250 foot 
14.	Fireback:
a.	Silver Painted
b.	Matte Black Painted
c.	Gloss Black Enamel 
d.	Black Glass
15.	Burner Decor: 
a.	Platinum Crushed Glass 
b.	Black Crushed Glass 
c.	Rock Embers 
16.	Interior Fire Art: 
a.	Twigs & Stones 
b.	Traditional Logs 
c.	Driftwood 
d.	Tumbled Stones 
e.	Tumbled Stones
f.	Birch
17.	Trim: 
a.	Flat 2 inch Black Trim 
b.	IronWorks Trim, Painted Charcoal 
c.	IronWorks Trim, Black Metalic 
18.	Accessories: 
a.	Tile Stop, 1/2 inch. 
b.	Heat Exchanger
c.	Carbon Monoxide Detector
d.	Home Automation Breakout Board
e.	Dehumidifier 
E.	DaVinci Bay Window Custom Linear Fireplace: 
1.	Category 1: 
a.	Nominal Opening Size: 
1)	36 inches W by 12 inches H by 20 inches D
2)	36 inches W by 20 inches H by 20 inches D
3)	36 inches W by 30 inches H by 20 inches D
4)	36 inches W by 36 inches H by 20 inches D
5)	36 Inches W by 48 inches H by 20 inches D
6)	36 inches W by 58 inches H by 20 inches D 
7)	48 inches W by 12 inches H by 20 inches D
8)	48 inches W by 20 inches H by 20 inches D
9)	48 inches W by 30 inches H by 20 inches D
10)	48 inches W by 36 inches H by 20 inches D
11)	48 inches W by 48 inches H by 20 inches D
12)	48 inches W by 58 inches H by 20 inches D 
13)	60 inches W by 12 inches H by 20 inches D
14)	60 inches W by 20 inches H by 20 inches D
15)	60 inches W by 30 inches H by 20 inches D
16)	60 inches W by 36 inches H by 20 inches D
17)	60 inches W by 48 inches H by 20 inches D 
18)	60 inches W by 58 inches H by 20 inches D 
19)	72 inches W by 12 inches H by 20 inches D
20)	72 inches W by 20 inches H by 20 inches D
21)	72 inches W by 30 inches H by 20 inches D
22)	72 inches W by 36 inches H by 20 inches D
23)	72 inches W by 48 inches H by 20 inches D 
24)	72 inches W by 58 inches H by 20 inches D 
2.	Category 2: 
a.	Nominal Opening Size: 
1)	84 inches W by 12 inches H by 20 inches D
2)	84 inches W by 20 inches H by 20 inches D
3)	84 inches W by 30 inches H by 20 inches D
4)	84 inches W by 36 inches H by 20 inches D
5)	84 inches W by 48 inches H by 20 inches D 
6)	84 inches W by 58 inches H by 20 inches D 
7)	96 inches W by 12 inches H by 20 inches D
8)	96 inches W by 20 inches H by 20 inches D
9)	96 inches W by 30 inches H by 20 inches D
10)	96 inches W by 36 inches H by 20 inches D
11)	96 inches W by 48 inches H by 20 inches D 
12)	96 inches W by 58 inches H by 20 inches D 
13)	108 inches W by 12 inches H by 20 inches D
14)	108 inches W by 20 inches H by 20 inches D
15)	108 inches W by 30 inches H by 20 inches D
16)	108 inches W by 36 inches H by 20 inches D
17)	108 inches W by 48 inches H by 20 inches D
18)	108 inches W by 58 inches H by 20 inches D 
19)	120 inches W by 12 inches H by 20 inches D
20)	120 inches W by 20 inches H by 20 inches D
21)	120 inches W by 30 inches H by 20 inches D
22)	120 inches W by 36 inches H by 20 inches D
23)	120 inches W by 48 inches H by 20 inches D
24)	120 inches W by 58 inches H by 20 inches D
25)	132 inches W by 12 inches H by 20 inches D
26)	132 inches W by 20 inches H by 20 inches D
27)	132 inches W by 30 inches H by 20 inches D
28)	132 inches W by 36 inches H by 20 inches D
29)	132 inches W by 48 inches H by 20 inches D
30)	132 inches W by 58 inches H by 20 inches D 
3.	Category 3: 
a.	Nominal Opening Size: 
1)	144 inches W by 12 inches H by 20 inches D
2)	144 inches W by 20 inches H by 20 inches D
3)	144 inches W by 30 inches H by 20 inches D
4)	144 inches W by 36 inches H by 20 inches D
5)	144 inches W by 48 inches H by 20 inches D
6)	144 inches W by 58 inches H by 20 inches D 
7)	156 inches W by 12 inches H by 20 inches D
8)	156 inches W by 20 inches H by 20 inches D
9)	156 inches W by 30 inches H by 20 inches D
10)	156 inches W by 36 inches H by 20 inches D
11)	156 inches W by 48 inches H by 20 inches D
12)	156 inches W by 58 inches H by 20 inches D 
13)	168 inches W by 12 inches H by 20 inches D
14)	168 inches W by 20 inches H by 20 inches D
15)	168 inches W by 30 inches H by 20 inches D
16)	168 inches W by 36 inches H by 20 inches D
17)	168 inches W by 48 inches H by 20 inches D
18)	168 inches W by 58 inches H by 20 inches D 
19)	180 inches W by 12 inches H by 20 inches D
20)	180 inches W by 20 inches H by 20 inches D
21)	180 inches W by 30 inches H by 20 inches D
22)	180 inches W by 36 inches H by 20 inches D
23)	180 inches W by 48 inches H by 20 inches D
24)	180 inches W by 58 inches H by 20 inches D 
25)	192 inches W by 12 inches H by 20 inches D
26)	192 inches W by 20 inches H by 20 inches D
27)	192 inches W by 30 inches H by 20 inches D
28)	192 inches W by 36 inches H by 20 inches D
29)	192 inches W by 48 inches H by 20 inches D
30)	192 inches W by 58 inches H by 20 inches D 
4.	Category 4: 
a.	Nominal Opening Size: 
1)	204 inches W by 12 inches H by 20 inches D
2)	204 inches W by 20 inches H by 20 inches D
3)	204 inches W by 30 inches H by 20 inches D
4)	204 inches W by 36 inches H by 20 inches D
5)	204 inches W by 48 inches H by 20 inches D
6)	204 inches W by 58 inches H by 20 inches D 
7)	216 inches W by 12 inches H by 20 inches D
8)	216 inches W by 20 inches H by 20 inches D
9)	216 inches W by 30 inches H by 20 inches D
10)	216 inches W by 36 inches H by 20 inches D
11)	216 inches W by 48 inches H by 20 inches D
12)	216 inches W by 58 inches H by 20 inches D 
13)	228 inches W by 12 inches H by 20 inches D
14)	228 inches W by 20 inches H by 20 inches D
15)	228 inches W by 30 inches H by 20 inches D
16)	228 inches W by 36 inches H by 20 inches D
17)	228 inches W by 48 inches H by 20 inches D
18)	228 inches W by 58 inches H by 20 inches D 
19)	240 inches W by 12 inches H by 20 inches D
20)	240 inches W by 20 inches H by 20 inches D
21)	240 inches W by 30 inches H by 20 inches D
22)	240 inches W by 36 inches H by 20 inches D
23)	240 inches W by 48 inches H by 20 inches D
24)	240 inches W by 58 inches H by 20 inches D 
25)	252 inches W by 12 inches H by 20 inches D
26)	252 inches W by 20 inches H by 20 inches D
27)	252 inches W by 30 inches H by 20 inches D
28)	252 inches W by 36 inches H by 20 inches D
29)	252 inches W by 48 inches H by 20 inches D
30)	252 inches W by 58 inches H by 20 inches D 
5.	Vent:
6.	a. 10 inch B-Vent Chimney, quantity as recommended by the installer
7.	b.8 Inch B-Vent Chimney, quantity as recommended by the installer
8.	Peak and Valley Burner
9.	Gas Input: Up to 14,500 BTUs/foot with natural gas or propane 
10.	Power Exhaust Fan: 
a.	RS12 Low Volume External Power Exhaust Fan
b.	RSIF 160 Low Volume Inline Power Exhaust Fan
c.	RS16 High Volume External Power Exhaust Fan
d.	RSIF 180 High Volume Inline Power Exhaust Fan
11.	Touch Smart wall control:
a.	Black Glass with timer
b.	Black Glass with variable blower speed (for use with heat exchanger)
c.	White Glass with timer
d.	White Glass with variable blower speed (for use with heat exchanger)
12.	Touch Smart Wire Harness:
a.	25 foot 
b.	50 foot
c.	100 foot
13.	Power Exhaust Fan Wire Harness:
a.	50 foot
b.	150 foot
c.	250 foot 
14.	Fireback:
a.	Silver Painted
b.	Matte Black Painted
c.	Gloss Black Enamel 
d.	Black Glass
15.	Burner Decor: 
a.	Platinum Crushed Glass 
b.	Black Crushed Glass 
c.	Rock Embers 
16.	Interior Fire Art: 
a.	Twigs & Stones 
b.	Traditional Logs 
c.	Driftwood 
d.	Tumbled Stones 
e.	Tumbled Stones
f.	Birch
17.	Trim: 
a.	Flat 2 inch Black Trim 
b.	IronWorks Trim, Painted Charcoal 
c.	IronWorks Trim, Black Metalic 
18.	Accessories: 
a.	Stop, 1/2 inch.
b.	Heat Exchanger
c.	Carbon Monoxide Detector
d.	Home Automation Breakout Board
e.	Dehumidifier 
F.	DaVinci See-Thru Custom Linear Fireplace: 
1.	Category 1: 
a.	Nominal Opening Size: 
1)	24 inches W by 12 inches H by 20 inches D
2)	24 inches W by 20 inches H by 20 inches D
3)	24 inches W by 30 inches H by 20 inches D
4)	24 inches W by 36 inches H by 20 inches D
5)	24 Inches W by 48 inches H by 20 inches D
6)	24 inches W by 58 inches H by 20 inches D
7)	36 inches W by 12 inches H by 20 inches D
8)	36 inches W by 20 inches H by 20 inches D
9)	36 inches W by 30 inches H by 20 inches D
10)	36 inches W by 36 inches H by 20 inches D
11)	36 Inches W by 48 inches H by 20 inches D
12)	36 inches W by 58 inches H by 20 inches D 
13)	48 inches W by 12 inches H by 20 inches D
14)	48 inches W by 20 inches H by 20 inches D
15)	48 inches W by 30 inches H by 20 inches D
16)	48 inches W by 36 inches H by 20 inches D
17)	48 inches W by 48 inches H by 20 inches D
18)	48 inches W by 58 inches H by 20 inches D 
19)	60 inches W by 12 inches H by 20 inches D
20)	60 inches W by 20 inches H by 20 inches D
21)	60 inches W by 30 inches H by 20 inches D
22)	60 inches W by 36 inches H by 20 inches D
23)	60 inches W by 48 inches H by 20 inches D 
24)	60 inches W by 58 inches H by 20 inches D 
2.	Category 2: 
a.	Nominal Opening Size: 
1)	72 inches W by 12 inches H by 20 inches D
2)	72 inches W by 20 inches H by 20 inches D
3)	72 inches W by 30 inches H by 20 inches D
4)	72 inches W by 36 inches H by 20 inches D
5)	72 inches W by 48 inches H by 20 inches D
6)	72 inches W by 58 inches H by 20 inches D 
7)	84 inches W by 12 inches H by 20 inches D
8)	84 inches W by 20 inches H by 20 inches D
9)	84 inches W by 30 inches H by 20 inches D
10)	84 inches W by 36 inches H by 20 inches D
11)	84 inches W by 48 inches H by 20 inches D 
12)	84 inches W by 58 inches H by 20 inches D 
13)	96 inches W by 12 inches H by 20 inches D
14)	96 inches W by 20 inches H by 20 inches D
15)	96 inches W by 30 inches H by 20 inches D
16)	96 inches W by 36 inches H by 20 inches D
17)	96 inches W by 48 inches H by 20 inches D 
18)	96 inches W by 58 inches H by 20 inches D 
19)	108 inches W by 12 inches H by 20 inches D
20)	108 inches W by 20 inches H by 20 inches D
21)	108 inches W by 30 inches H by 20 inches D
22)	108 inches W by 36 inches H by 20 inches D
23)	108 inches W by 48 inches H by 20 inches D
24)	108 inches W by 58 inches H by 20 inches D 
25)	120 inches W by 12 inches H by 20 inches D
26)	120 inches W by 20 inches H by 20 inches D
27)	120 inches W by 30 inches H by 20 inches D
28)	120 inches W by 36 inches H by 20 inches D
29)	120 inches W by 48 inches H by 20 inches D
30)	120 inches W by 58 inches H by 20 inches D 
3.	Category 3: 
a.	Nominal Opening Size: 
1)	132 inches W by 12 inches H by 20 inches D
2)	132 inches W by 20 inches H by 20 inches D
3)	132 inches W by 30 inches H by 20 inches D
4)	132 inches W by 36 inches H by 20 inches D
5)	132 inches W by 48 inches H by 20 inches D
6)	132 inches W by 58 inches H by 20 inches D 
7)	144 inches W by 12 inches H by 20 inches D
8)	144 inches W by 20 inches H by 20 inches D
9)	144 inches W by 30 inches H by 20 inches D
10)	144 inches W by 36 inches H by 20 inches D
11)	144 inches W by 48 inches H by 20 inches D
12)	144 inches W by 58 inches H by 20 inches D 
13)	156 inches W by 12 inches H by 20 inches D
14)	156 inches W by 20 inches H by 20 inches D
15)	156 inches W by 30 inches H by 20 inches D
16)	156 inches W by 36 inches H by 20 inches D
17)	156 inches W by 48 inches H by 20 inches D
18)	156 inches W by 58 inches H by 20 inches D 
19)	168 inches W by 12 inches H by 20 inches D
20)	168 inches W by 20 inches H by 20 inches D
21)	168 inches W by 30 inches H by 20 inches D
22)	168 inches W by 36 inches H by 20 inches D
23)	168 inches W by 48 inches H by 20 inches D
24)	168 inches W by 58 inches H by 20 inches D 
25)	180 inches W by 12 inches H by 20 inches D
26)	180 inches W by 20 inches H by 20 inches D
27)	180 inches W by 30 inches H by 20 inches D
28)	180 inches W by 36 inches H by 20 inches D
29)	180 inches W by 48 inches H by 20 inches D
30)	180 inches W by 58 inches H by 20 inches D 
4.	Category 4: 
a.	Nominal Opening Size: 
1)	192 inches W by 12 inches H by 20 inches D
2)	192 inches W by 20 inches H by 20 inches D
3)	192 inches W by 30 inches H by 20 inches D
4)	192 inches W by 36 inches H by 20 inches D
5)	192 inches W by 48 inches H by 20 inches D
6)	192 inches W by 58 inches H by 20 inches D 
7)	204 inches W by 12 inches H by 20 inches D
8)	204 inches W by 20 inches H by 20 inches D
9)	204 inches W by 30 inches H by 20 inches D
10)	204 inches W by 36 inches H by 20 inches D
11)	204 inches W by 48 inches H by 20 inches D
12)	204 inches W by 58 inches H by 20 inches D 
13)	216 inches W by 12 inches H by 20 inches D
14)	216 inches W by 20 inches H by 20 inches D
15)	216 inches W by 30 inches H by 20 inches D
16)	216 inches W by 36 inches H by 20 inches D
17)	216 inches W by 48 inches H by 20 inches D
18)	216 inches W by 58 inches H by 20 inches D 
19)	228 inches W by 12 inches H by 20 inches D
20)	228 inches W by 20 inches H by 20 inches D
21)	228 inches W by 30 inches H by 20 inches D
22)	228 inches W by 36 inches H by 20 inches D
23)	228 inches W by 48 inches H by 20 inches D
24)	228 inches W by 58 inches H by 20 inches D 
25)	240 inches W by 12 inches H by 20 inches D
26)	240 inches W by 20 inches H by 20 inches D
27)	240 inches W by 30 inches H by 20 inches D
28)	240 inches W by 36 inches H by 20 inches D
29)	240 inches W by 48 inches H by 20 inches D
30)	240 inches W by 58 inches H by 20 inches D 
5.	Vent:
6.	a. 10 inch B-Vent Chimney, quantity as recommended by the installer
7.	b.8 Inch B-Vent Chimney, quantity as recommended by the installer
8.	Peak and Valley Burner
9.	Gas Input: Up to 14,500 BTUs/foot with natural gas or propane 
10.	Power Exhaust Fan: 
a.	RS12 Low Volume External Power Exhaust Fan
b.	RSIF 160 Low Volume Inline Power Exhaust Fan
c.	RS16 High Volume External Power Exhaust Fan
d.	RSIF 180 High Volume Inline Power Exhaust Fan
11.	Touch Smart wall control:
a.	Black Glass with timer
b.	Black Glass with variable blower speed (for use with heat exchanger)
c.	White Glass with timer
d.	White Glass with variable blower speed (for use with heat exchanger)
12.	Touch Smart Wire Harness:
a.	25 foot 
b.	50 foot
c.	100 foot
13.	Power Exhaust Fan Wire Harness:
a.	50 foot
b.	150 foot
c.	250 foot 
14.	Fireback:
a.	Silver Painted
b.	Matte Black Painted
c.	Gloss Black Enamel 
15.	Burner Decor: 
a.	Platinum Crushed Glass 
b.	Black Crushed Glass 
c.	Rock Embers 
16.	Interior Fire Art: 
a.	Twigs & Stones 
b.	Traditional Logs 
c.	Driftwood 
d.	Tumbled Stones 
e.	Tumbled Stones
f.	Birch
17.	Trim: 
a.	Flat 2 inch Black Trim 
b.	IronWorks Trim, Painted Charcoal 
c.	IronWorks Trim, Black Metalic 
18.	Accessories: 
a.	Tile Stop, 1/2 inch. 
b.	Heat Exchanger
c.	Outdoor Window Kit
d.	Carbon Monoxide Detector
e.	Home Automation Breakout Board
f.	Dehumidifier 
G.	DaVinci Pier Custom Linear Fireplace: (Posted OR Post-less)
1.	Category 1: 
a.	Nominal Opening Size: 
1)	30 inches W by 12 inches H by 20 inches D
2)	30 inches W by 20 inches H by 20 inches D
3)	30 inches W by 30 inches H by 20 inches D
4)	30 inches W by 36 inches H by 20 inches D
5)	30 inches W by 48 inches H by 20 inches D 
6)	30 inches W by 58 inches H by 20 inches D
7)	42 inches W by 12 inches H by 20 inches D
8)	42 inches W by 20 inches H by 20 inches D
9)	42 inches W by 30 inches H by 20 inches D
10)	42 inches W by 36 inches H by 20 inches D
11)	42 inches W by 48 inches H by 20 inches D
12)	42 inches W by 58 inches H by 20 inches D 
13)	54 inches W by 12 inches H by 20 inches D
14)	54 inches W by 20 inches H by 20 inches D
15)	54 inches W by 30 inches H by 20 inches D
16)	54 inches W by 36 inches H by 20 inches D
17)	54 inches W by 48 inches H by 20 inches D 
18)	54 inches W by 58 inches H by 20 inches D 
19)	66 inches W by 12 inches H by 20 inches D
20)	66 inches W by 20 inches H by 20 inches D
21)	66 inches W by 30 inches H by 20 inches D
22)	66 inches W by 36 inches H by 20 inches D
23)	66 inches W by 48 inches H by 20 inches D 
24)	66 inches W by 58 inches H by 20 inches D 
2.	Category 2: 
a.	Nominal Opening Size: 
1)	78 inches W by 12 inches H by 20 inches D
2)	78 inches W by 20 inches H by 20 inches D
3)	78 inches W by 30 inches H by 20 inches D
4)	78 inches W by 36 inches H by 20 inches D
5)	78 inches W by 48 inches H by 20 inches D
6)	78 inches W by 58 inches H by 20 inches D 
7)	90 inches W by 12 inches H by 20 inches D
8)	90 inches W by 20 inches H by 20 inches D
9)	90 inches W by 30 inches H by 20 inches D
10)	90 inches W by 36 inches H by 20 inches D
11)	90 inches W by 48 inches H by 20 inches D
12)	90 inches W by 58 inches H by 20 inches D 
13)	102 inches W by 12 inches H by 20 inches D
14)	102 inches W by 20 inches H by 20 inches D
15)	102 inches W by 30 inches H by 20 inches D
16)	102 inches W by 36 inches H by 20 inches D
17)	102 inches W by 48 inches H by 20 inches D
18)	102 inches W by 58 inches H by 20 inches D 
19)	114 inches W by 12 inches H by 20 inches D
20)	114 inches W by 20 inches H by 20 inches D
21)	114 inches W by 30 inches H by 20 inches D
22)	114 inches W by 36 inches H by 20 inches D
23)	114 inches W by 48 inches H by 20 inches D
24)	114 inches W by 58 inches H by 20 inches D 
25)	126 inches W by 12 inches H by 20 inches D
26)	126 inches W by 20 inches H by 20 inches D
27)	126 inches W by 30 inches H by 20 inches D
28)	126 inches W by 36 inches H by 20 inches D
29)	126 inches W by 48 inches H by 20 inches D
30)	126 inches W by 58 inches H by 20 inches D 
3.	Category 3: 
a.	Nominal Opening Size: 
1)	138 inches W by 12 inches H by 20 inches D
2)	138 inches W by 20 inches H by 20 inches D
3)	138 inches W by 30 inches H by 20 inches D
4)	138 inches W by 36 inches H by 20 inches D
5)	138 inches W by 48 inches H by 20 inches D
6)	138 inches W by 58 inches H by 20 inches D
7)	150 inches W by 12 inches H by 20 inches D
8)	150 inches W by 20 inches H by 20 inches D
9)	150 inches W by 30 inches H by 20 inches D
10)	150 inches W by 36 inches H by 20 inches D
11)	150 inches W by 48 inches H by 20 inches D
12)	150 inches W by 58 inches H by 20 inches D
13)	162 inches W by 12 inches H by 20 inches D
14)	162 inches W by 20 inches H by 20 inches D
15)	162 inches W by 30 inches H by 20 inches D
16)	162 inches W by 36 inches H by 20 inches D
17)	162 inches W by 48 inches H by 20 inches D
18)	162 inches W by 58 inches H by 20 inches D
19)	174 inches W by 12 inches H by 20 inches D
20)	174 inches W by 20 inches H by 20 inches D
21)	174 inches W by 30 inches H by 20 inches D
22)	174 inches W by 36 inches H by 20 inches D
23)	174 inches W by 48 inches H by 20 inches D
24)	174 inches W by 58 inches H by 20 inches D
25)	186 inches W by 12 inches H by 20 inches D
26)	186 inches W by 20 inches H by 20 inches D
27)	186 inches W by 30 inches H by 20 inches D
28)	186 inches W by 36 inches H by 20 inches D
29)	186 inches W by 48 inches H by 20 inches D
30)	186 inches W by 58 inches H by 20 inches D
4.	Category 4: 
a.	Nominal Opening Size: 
1)	198 inches W by 12 inches H by 20 inches D
2)	198 inches W by 20 inches H by 20 inches D
3)	198 inches W by 30 inches H by 20 inches D
4)	198 inches W by 36 inches H by 20 inches D
5)	198 inches W by 48 inches H by 20 inches D
6)	198 inches W by 58 inches H by 20 inches D
7)	210 inches W by 12 inches H by 20 inches D
8)	210 inches W by 20 inches H by 20 inches D
9)	210 inches W by 30 inches H by 20 inches D
10)	210 inches W by 36 inches H by 20 inches D
11)	210 inches W by 48 inches H by 20 inches D
12)	210 inches W by 58 inches H by 20 inches D
13)	222 inches W by 12 inches H by 20 inches D
14)	222 inches W by 20 inches H by 20 inches D
15)	222 inches W by 30 inches H by 20 inches D
16)	222 inches W by 36 inches H by 20 inches D
17)	222 inches W by 48 inches H by 20 inches D
18)	222 inches W by 58 inches H by 20 inches D
19)	234 inches W by 12 inches H by 20 inches D
20)	234 inches W by 20 inches H by 20 inches D
21)	234 inches W by 30 inches H by 20 inches D
22)	234 inches W by 36 inches H by 20 inches D
23)	234 inches W by 48 inches H by 20 inches D
24)	234 inches W by 58 inches H by 20 inches D
25)	246 inches W by 12 inches H by 20 inches D
26)	246 inches W by 20 inches H by 20 inches D
27)	246 inches W by 30 inches H by 20 inches D
28)	246 inches W by 36 inches H by 20 inches D
29)	246 inches W by 48 inches H by 20 inches D
30)	246 inches W by 58 inches H by 20 inches D
5.	Vent:
6.	a. 10 inch B-Vent Chimney, quantity as recommended by the installer 
7.	b.8 Inch B-Vent Chimney, quantity as recommended by the installer
8.	Peak and Valley Burner
9.	Gas Input: Up to 14,500 BTUs/foot with natural gas or propane 
10.	Power Exhaust Fan: 
a.	RS12 Low Volume External Power Exhaust Fan
b.	RSIF 160 Low Volume Inline Power Exhaust Fan
c.	RS16 High Volume External Power Exhaust Fan
d.	RSIF 180 High Volume Inline Power Exhaust Fan
11.	Touch Smart wall control:
a.	Black Glass with timer
b.	Black Glass with variable blower speed (for use with heat exchanger)
c.	White Glass with timer
d.	White Glass with variable blower speed (for use with heat exchanger)
12.	Touch Smart Wire Harness:
a.	25 foot 
b.	50 foot
c.	100 foot
13.	Power Exhaust Fan Wire Harness:
a.	50 foot
b.	150 foot
c.	250 foot 
14.	Fireback: 
a.	Silver Painted
b.	Matte Black Painted
c.	Gloss Black Enamel 
15.	Posts: Painted to match Fireback 
16.	Burner Decor: 
a.	Platinum Crushed Glass 
b.	Black Crushed Glass 
c.	Rock Embers 
17.	Interior Fire Art: 
a.	Twigs & Stones 
b.	Traditional Logs 
c.	Driftwood 
d.	Tumbled Stones 
e.	Tumbled Stones
f.	Birch
18.	Trim: 
a.	Flat 2 inch Black Trim 
b.	IronWorks Trim, Painted Charcoal 
c.	IronWorks Trim, Black Metalic 
19.	Accessories: 
a.	On/Off 24 Hour Timer Switch 
b.	Tile Stop, 1/2 inch. 
c.	Heat Exchanger
d.	Carbon Monoxide Detector
e.	Home Automation Breakout Board
f.	Dehumidifier 
H.	DaVinci Island Custom Linear Fireplace: (With Posts) 
1.	Category 1: 
2.	Category 1: 
a.	Nominal Opening Size: 
1)	36 inches W by 12 inches H by 20 inches D
2)	36 inches W by 20 inches H by 20 inches D
3)	36 inches W by 30 inches H by 20 inches D
4)	36 inches W by 36 inches H by 20 inches D
5)	36 Inches W by 48 inches H by 20 inches D
6)	36 inches W by 58 inches H by 20 inches D 
7)	48 inches W by 12 inches H by 20 inches D
8)	48 inches W by 20 inches H by 20 inches D
9)	48 inches W by 30 inches H by 20 inches D
10)	48 inches W by 36 inches H by 20 inches D
11)	48 inches W by 48 inches H by 20 inches D
12)	48 inches W by 58 inches H by 20 inches D 
13)	60 inches W by 12 inches H by 20 inches D
14)	60 inches W by 20 inches H by 20 inches D
15)	60 inches W by 30 inches H by 20 inches D
16)	60 inches W by 36 inches H by 20 inches D
17)	60 inches W by 48 inches H by 20 inches D 
18)	60 inches W by 58 inches H by 20 inches D 
19)	72 inches W by 12 inches H by 20 inches D
20)	72 inches W by 20 inches H by 20 inches D
21)	72 inches W by 30 inches H by 20 inches D
22)	72 inches W by 36 inches H by 20 inches D
23)	72 inches W by 48 inches H by 20 inches D 
24)	72 inches W by 58 inches H by 20 inches D 
3.	Category 2: 
a.	Nominal Opening Size: 
1)	84 inches W by 12 inches H by 20 inches D
2)	84 inches W by 20 inches H by 20 inches D
3)	84 inches W by 30 inches H by 20 inches D
4)	84 inches W by 36 inches H by 20 inches D
5)	84 inches W by 48 inches H by 20 inches D 
6)	84 inches W by 58 inches H by 20 inches D 
7)	96 inches W by 12 inches H by 20 inches D
8)	96 inches W by 20 inches H by 20 inches D
9)	96 inches W by 30 inches H by 20 inches D
10)	96 inches W by 36 inches H by 20 inches D
11)	96 inches W by 48 inches H by 20 inches D 
12)	96 inches W by 58 inches H by 20 inches D 
13)	108 inches W by 12 inches H by 20 inches D
14)	108 inches W by 20 inches H by 20 inches D
15)	108 inches W by 30 inches H by 20 inches D
16)	108 inches W by 36 inches H by 20 inches D
17)	108 inches W by 48 inches H by 20 inches D
18)	108 inches W by 58 inches H by 20 inches D 
19)	120 inches W by 12 inches H by 20 inches D
20)	120 inches W by 20 inches H by 20 inches D
21)	120 inches W by 30 inches H by 20 inches D
22)	120 inches W by 36 inches H by 20 inches D
23)	120 inches W by 48 inches H by 20 inches D
24)	120 inches W by 58 inches H by 20 inches D
25)	132 inches W by 12 inches H by 20 inches D
26)	132 inches W by 20 inches H by 20 inches D
27)	132 inches W by 30 inches H by 20 inches D
28)	132 inches W by 36 inches H by 20 inches D
29)	132 inches W by 48 inches H by 20 inches D
30)	132 inches W by 58 inches H by 20 inches D 
4.	Category 3: 
a.	Nominal Opening Size: 
1)	144 inches W by 12 inches H by 20 inches D
2)	144 inches W by 20 inches H by 20 inches D
3)	144 inches W by 30 inches H by 20 inches D
4)	144 inches W by 36 inches H by 20 inches D
5)	144 inches W by 48 inches H by 20 inches D
6)	144 inches W by 58 inches H by 20 inches D 
7)	156 inches W by 12 inches H by 20 inches D
8)	156 inches W by 20 inches H by 20 inches D
9)	156 inches W by 30 inches H by 20 inches D
10)	156 inches W by 36 inches H by 20 inches D
11)	156 inches W by 48 inches H by 20 inches D
12)	156 inches W by 58 inches H by 20 inches D 
13)	168 inches W by 12 inches H by 20 inches D
14)	168 inches W by 20 inches H by 20 inches D
15)	168 inches W by 30 inches H by 20 inches D
16)	168 inches W by 36 inches H by 20 inches D
17)	168 inches W by 48 inches H by 20 inches D
18)	168 inches W by 58 inches H by 20 inches D 
19)	180 inches W by 12 inches H by 20 inches D
20)	180 inches W by 20 inches H by 20 inches D
21)	180 inches W by 30 inches H by 20 inches D
22)	180 inches W by 36 inches H by 20 inches D
23)	180 inches W by 48 inches H by 20 inches D
24)	180 inches W by 58 inches H by 20 inches D 
25)	192 inches W by 12 inches H by 20 inches D
26)	192 inches W by 20 inches H by 20 inches D
27)	192 inches W by 30 inches H by 20 inches D
28)	192 inches W by 36 inches H by 20 inches D
29)	192 inches W by 48 inches H by 20 inches D
30)	192 inches W by 58 inches H by 20 inches D 
5.	Category 4: 
a.	Nominal Opening Size: 
1)	204 inches W by 12 inches H by 20 inches D
2)	204 inches W by 20 inches H by 20 inches D
3)	204 inches W by 30 inches H by 20 inches D
4)	204 inches W by 36 inches H by 20 inches D
5)	204 inches W by 48 inches H by 20 inches D
6)	204 inches W by 58 inches H by 20 inches D 
7)	216 inches W by 12 inches H by 20 inches D
8)	216 inches W by 20 inches H by 20 inches D
9)	216 inches W by 30 inches H by 20 inches D
10)	216 inches W by 36 inches H by 20 inches D
11)	216 inches W by 48 inches H by 20 inches D
12)	216 inches W by 58 inches H by 20 inches D 
13)	228 inches W by 12 inches H by 20 inches D
14)	228 inches W by 20 inches H by 20 inches D
15)	228 inches W by 30 inches H by 20 inches D
16)	228 inches W by 36 inches H by 20 inches D
17)	228 inches W by 48 inches H by 20 inches D
18)	228 inches W by 58 inches H by 20 inches D 
19)	240 inches W by 12 inches H by 20 inches D
20)	240 inches W by 20 inches H by 20 inches D
21)	240 inches W by 30 inches H by 20 inches D
22)	240 inches W by 36 inches H by 20 inches D
23)	240 inches W by 48 inches H by 20 inches D
24)	240 inches W by 58 inches H by 20 inches D 
25)	252 inches W by 12 inches H by 20 inches D
26)	252 inches W by 20 inches H by 20 inches D
27)	252 inches W by 30 inches H by 20 inches D
28)	252 inches W by 36 inches H by 20 inches D
29)	252 inches W by 48 inches H by 20 inches D
30)	252 inches W by 58 inches H by 20 inches D 
6.	Vent:
7.	a. 10 inch B-Vent Chimney, quantity as recommended by the installer.
8.	b.8 Inch B-Vent Chimney, quantity as recommended by the installer
9.	Peak and Valley Burner
10.	Gas Input: Up to 14,500 BTUs/foot with natural gas or propane 
11.	Power Exhaust Fan: 
a.	RS12 Low Volume External Power Exhaust Fan
b.	RSIF 160 Low Volume Inline Power Exhaust Fan
c.	RS16 High Volume External Power Exhaust Fan
d.	RSIF 180 High Volume Inline Power Exhaust Fan
12.	Touch Smart wall control:
a.	Black Glass with timer
b.	Black Glass with variable blower speed (for use with heat exchanger)
c.	White Glass with timer
d.	White Glass with variable blower speed (for use with heat exchanger)
13.	Touch Smart Wire Harness:
a.	25 foot 
b.	50 foot
c.	100 foot
14.	Power Exhaust Fan Wire Harness:
a.	50 foot
b.	150 foot
c.	250 foot 
15.	Posts:
a.	Silver Painted.
16.	Burner Decor: 
a.	Platinum Crushed Glass 
b.	Black Crushed Glass 
c.	Rock Embers 
17.	Interior Fire Art: 
a.	Twigs & Stones 
b.	Traditional Logs 
c.	Driftwood 
d.	Tumbled Stones 
e.	Tumbled Stones
f.	Birch
18.	Accessories: 
a.	On/Off 24 Hour Timer Switch 
b.	Tile Stop, 1/2 inch.
c.	Heat Exchanger
d.	Carbon Monoxide Detector
e.	Home Automation Breakout Board
f.	Dehumidifier 
PART 3    EXECUTION
3.1	EXAMINATION
A.	Do not begin installation until substrates have been properly prepared.
B.	Verify framed opening sizes and clearances.
C.	If substrate preparation is the responsibility of another installer, notify Architect of unsatisfactory preparation before proceeding.
D.	Verify proper power supply and fuel source are available.
3.2	PREPARATION
A.	Clean surfaces thoroughly prior to installation.
B.	Prepare surfaces using the methods recommended by the manufacturer for achieving the best result for the substrate under the project conditions.
3.3	INSTALLATION
A.	Install in accordance with manufacturer's instructions, ANSI Z21.44 and the requirements of authorities having jurisdiction.
B.	Use manufacturer's guidelines for minimum clearances to combustibles, walls, and finishes.
C.	Anchor all components firmly in position for long life under hard use.
D.	Upon completion of installation, visually inspect all exposed surfaces. Touch up scratches and abrasions with touch up paint recommended by the manufacturer; make imperfections invisible to the unaided eye from a distance of 5 feet (1.5 m).
3.4	PROTECTION
A.	Protect installed products until completion of project.
B.	Touch-up, repair or replace damaged products before Substantial Completion.

END OF SECTION