SECTION 10 57 00

COAT RACK SYSTEMS

Display hidden notes to specifier. (Don't know how? [Click Here](https://www.arcat.com/sd/display_hidden_notes.shtml))

*Copyright 2021 - 2023 ARCAT, Inc. - All rights reserved*

\*\* NOTE TO SPECIFIER \*\* HangSafe Hooks; coat hooks, coat racks, shelving.
This section is based on the products of HangSafe Hooks, which is located at:165 E. Hwy. CCNixa, MO 65714Toll Free Tel: 888-803-7403Tel: 417-725-8900Fax: 417-725-8901Email: [request info (sales@hangsafehooks.com)](https://arcat.com/rfi?action=email&company=HangSafe%252BHooks&message=RE%253A%2520Spec%2520Question%2520(10900hsh)%253A%2520&coid=43213&spec=10900hsh&rep=&fax=417-725-8901)
Web: <https://www.hangsafehooks.com>
 [ [Click Here](https://arcat.com/company/hangsafe-hooks-43213) ] for additional information.
We provide flat-profile, virtually unbreakable coat hooks and fully-assembled, wall mounted coat racks for interior or exterior use. Specifying HangSafe Hooks for your project is simple. In addition to the resources below, contact us for custom design assistance.

1. GENERAL
	1. SECTION INCLUDES

\*\* NOTE TO SPECIFIER \*\* Delete items below not required for project.

* + 1. HangSafe Vibrant Racks - Coat and Backpack Racks with high density recycled polyethene mounting boards.
		2. HangSafe Racks - Coat and Backpack Racks with solid wood mounting boards.
	1. RELATED SECTIONS

\*\* NOTE TO SPECIFIER \*\* Delete any sections below not relevant to this project; add others as required.

* + 1. Section 04 20 00 - Unit Masonry.
		2. Section 06 10 00 - Rough Carpentry.
		3. Section 09 28 13 - Cementitious Backing Boards.
	1. SUBMITTALS
		1. Submit under provisions of Section 01 30 00 - Administrative Requirements.
		2. Product Data:
			1. Manufacturer's data sheets on each product to be used.
			2. Preparation instructions and recommendations.
			3. Storage and handling requirements and recommendations.
			4. Typical installation methods.
		3. Shop Drawings: For each type. Include spacing of mounting holes.
	2. QUALITY ASSURANCE
		1. Source Limitations: Provide each type of product from a single manufacturing source to ensure uniformity.
	3. DELIVERY, STORAGE, AND HANDLING
		1. Store and handle in strict compliance with manufacturer's written instructions and recommendations.
		2. Protect from damage due to weather, excessive temperature, and construction operations.
	4. PROJECT CONDITIONS
		1. Maintain environmental conditions (temperature, humidity, and ventilation) within limits recommended by manufacturer for optimum results.
		2. Do not install products under environmental conditions outside manufacturer's recommended limits.
	5. WARRANTY
		1. Manufacturer's Warranty: Provide manufacturer's standard lifetime warranty against defects in manufacturing.
1. PRODUCTS
	1. MANUFACTURERS
		1. Acceptable Manufacturer: HangSafe Hooks, which is located at:165 E. Hwy. CCNixa, MO 65714Toll Free Tel: 888-803-7403Tel: 417-725-8900Fax: 417-725-8901Email: [request info (sales@hangsafehooks.com)](https://arcat.com/rfi?action=email&company=HangSafe%252BHooks&message=RE%253A%2520Spec%2520Question%2520(10900hsh)%253A%2520&coid=43213&spec=10900hsh&rep=&fax=417-725-8901);Web: <https://www.hangsafehooks.com>

\*\* NOTE TO SPECIFIER \*\* Delete one of the following two paragraphs; coordinate with requirements of Division 1 section on product options and substitutions.

* + 1. Substitutions: Not permitted.
		2. Requests for substitutions will be considered in accordance with provisions of Section 01 60 00 - Product Requirements.

\*\* NOTE TO SPECIFIER \*\* Delete if not required.

* 1. HANGSAFE VIBRANT RACKS - COAT AND BACKPACK RACKS WITH RECYCLED HIGH DENSITY POLYETHYLENE MOUNTING BOARD
		1. Coat and Backpack Racks with Recycled High Density Polyethylene Mounting Board: Vibrant Racks by HangSafe Hooks.

\*\* NOTE TO SPECIFIER \*\* Delete application not required.

* + - 1. Application: Indoor.
			2. Application: Outdoor.
			3. Hooks: Polycarbonate plastic with polished rounded ends and eased edges.

\*\* NOTE TO SPECIFIER \*\* Hook spacing of 5-1/3 inches is the most economical choice, 6.4 inch spacing allows for bigger backpacks and bulky coats (most popular choice), 8 inch spacing is for larger coats and heavy backpacks, 10-2/3 inch spacing is the most spacious option. Delete hook spacings not required.

* + - 1. Hook Spacing: 5-1/3 inches (135 mm).
			2. Hook Spacing: 6.4 inches. (162 mm).
			3. Hook Spacing: 8 inches (203 mm).
			4. Hook Spacing: 10-2/3 inches (270 mm).
			5. Attachment: No. 14 by 2 inch (51 mm) stainless steel Philips oval head screws and finishing washers. Provide finishing button to conceal screws.
			6. Mounting Boards: High density recycled polyethylene with solid color throughout and UV inhibitors, approximately 1-9/16 inches (40 mm) by 3-1/2 inches (89 mm). Provide manufacturer's standard connectors for continuous lengths.

\*\* NOTE TO SPECIFIER \*\* Delete colors not required.

* + - 1. Recycled Polyethylene Color: Antique Mahogany.
			2. Recycled Polyethylene Color: Aqua Blue.
			3. Recycled Polyethylene Color: Birchwood.
			4. Recycled Polyethylene Color: Black.
			5. Recycled Polyethylene Color: Cardinal Red.
			6. Recycled Polyethylene Color: Cedar.
			7. Recycled Polyethylene Color: Driftwood.
			8. Recycled Polyethylene Color: Dark Brown.
			9. Recycled Polyethylene Color: Dark Green.
			10. Recycled Polyethylene Color: Ivory.
			11. Recycled Polyethylene Color: Light Brown.
			12. Recycled Polyethylene Color: Light Grey.
			13. Recycled Polyethylene Color: Lime Green.
			14. Recycled Polyethylene Color: Maroon.
			15. Recycled Polyethylene Color: Orange.
			16. Recycled Polyethylene Color: Patriot Blue.
			17. Recycled Polyethylene Color: Purple.
			18. Recycled Polyethylene Color: Royal Blue.
			19. Recycled Polyethylene Color: Slat Grey.
			20. Recycled Polyethylene Color: White.
			21. Recycled Polyethylene Color: Yellow.

\*\* NOTE TO SPECIFIER \*\* Delete if not required.

* + - 1. Individual Hook Numbering: Required.

\*\* NOTE TO SPECIFIER \*\* Delete if not required.

* 1. HANGSAFE RACKS - COAT AND BACKPACK RACKS WITH SOLID WOOD MOUNTING BOARD
		1. Coat Racks with Solid Wood Mounting Board: Solid Wood Racks by HangSafe Hooks.
			1. Application: Indoor (only).
			2. Hooks: Polycarbonate plastic with polished rounded ends and eased edges.

\*\* NOTE TO SPECIFIER \*\* Hook spacing of 5-1/3 inches is the most economical choice, 6.4 inch spacing allows for bigger backpacks and bulky coats (most popular choice), 8 inch spacing is for larger coats and heavy backpacks, 10-2/3 inch spacing is the most spacious option. Delete hook spacings not required.

* + - 1. Hook Spacing: 5-1/3 inches (135 mm).
			2. Hook Spacing: 6.4 inches. (162 mm).
			3. Hook Spacing: 8 inches (203 mm).
			4. Hook Spacing: 10-2/3 inches (270 mm).
			5. Attachment: No. 14 by 2 inch (51 mm) stainless steel Philips oval head screws and finishing washers. Provide finishing button to conceal screws.

\*\* NOTE TO SPECIFIER \*\* Delete mounting boards option not required.

* + - 1. Mounting Boards: Two layers of 3/4 inch (19 mm) maple, approximately 1-9/16 inches (40 mm) by 3-1/2 inches (89 mm). Provide manufacturer's standard connectors for continuous lengths.
				1. Finish: Two protective coats of polyurethane.
			2. Mounting Boards: Two layers of 3/4 inch (19 mm) solid oak, approximately 1-9/16 inches (40 mm) by 3-1/2 inches (89 mm). Provide manufacturer's standard connectors for continuous lengths.
				1. Finish: Stain and two protective coats of polyurethane.

\*\* NOTE TO SPECIFIER \*\* Delete stain colors not required.

* + - * 1. Stain Color: Cherry.
				2. Stain Color: Classic Grey.
				3. Stain Color: Dark Walnut.
				4. Stain Color: Ebony.
				5. Stain Color: English Chestnut.
				6. Stain Color: Golden Oak.
				7. Stain Color: Maple.
				8. Stain Color: Natural.
				9. Stain Color: Pickled Oak.
				10. Stain Color: Red Mahogany.

\*\* NOTE TO SPECIFIER \*\* Delete if not required.

* + - * 1. Individual Hook Numbering: Required.
1. EXECUTION
	1. INSTALLATION
		1. Install in accordance with manufacturer's written instructions, approved submittals and in proper relationship with adjacent construction.
			1. Tighten attachments to eliminate all movement.
			2. Place finishing button in mounting pocket.
	2. CLEANING AND PROTECTION
		1. Clean and protect products in accordance with the manufacturer's recommendations.
		2. Touch-up, repair or replace damaged products before Substantial Completion.

END OF SECTION