SECTION 32 31 23

VINYL FENCING AND GATES

Display hidden notes to specifier. (Don't know how? Click Here) 
 Copyright 2017 -  2020 ARCAT, Inc. - All rights reserved

PART 1    GENERAL
1.1	SECTION INCLUDES
A.	Wood Tone Fence.
B.	Yard Fence 
C.	Privacy Fence 
D.	Post and Rail Fence 
E.	Vinyl Picket Fence 
F.	Post Caps 
G.	Gates 
H.	Gate Hardware
I.	Lawn and Garden Accessories
1.2	RELATED SECTIONS
A.	Section 02 20 00 - Assessment.
B.	Section 03 30 00 - Cast-in-Place Concrete.
1.3	REFERENCES
A.	ASTM D 1784 - Standard Specification for Rigid Poly(Vinyl Chloride) (PVC) Compounds and Chlorinated Poly (Vinyl Chloride) (CPVC) Compounds.
1.4	DESIGN / PERFORMANCE REQUIREMENTS
A.	Provide pool fencing to meet applicable code requirements.
1.5	SUBMITTALS
A.	Submit under provisions of Section 01 30 00 - Administrative Requirements.
B.	Product Data: Manufacturer's data sheets on each product to be used, including:
1.	Preparation instructions and recommendations.
2.	Storage and handling requirements and recommendations.
3.	Installation methods.
C.	Shop Drawings: Submit shop drawings for each product and accessory required. Include information not fully detailed in manufacturer's standard product data.
D.	Selection Samples: For each finish product specified, two complete sets of color chips representing manufacturer's full range of available colors and patterns.
E.	Verification Samples: For each finish product specified, two samples, minimum size 3 inches (76 mm) square, representing actual product, color, and patterns.
F.	Manufacturer's Certificates: Certify products meet or exceed specified requirements.
G.	Closeout Submittals: Provide manufacturer's maintenance instructions that include recommendations for periodic cleaning and maintenance of all components.
1.6	QUALITY ASSURANCE
A.	Manufacturer Qualifications: A firm engaged in the manufacture of vinyl fence and gates of types and sizes specified, and whose products have been in satisfactory use in similar service for a minimum of five years.
B.	Installer Qualifications: A firm with a minimum of two years of successful installation experience with projects utilizing vinyl fence and gates similar in type and scope to that required for this Project.
C.	Mock-Up: Provide a mock-up for evaluation of surface preparation techniques and application workmanship.
1.	Finish areas designated by Architect.
2.	Do not proceed with remaining work until workmanship, color, and sheen are approved by Architect.
3.	Refinish mock-up area as required to produce acceptable work.
4.	Accepted mock-ups shall be comparison standard for remaining Work
D.	Pre-Installation Conference: Conduct pre-installation conference in accordance with Section 01 20 00 - Price and Payment Procedures. Date and time of the pre-installation conference shall be acceptable to the Owner and the Architect.
1.	Prior to commencing the installation, meet at the Project site to review the material selections, installation procedures, and coordination with other trades. 
2.	Mock-ups shall be reviewed during the pre-installation conference. 
3.	Pre-installation conference shall include the Contractor, the Installer, and any trade that requires coordination with the work. 
1.7	DELIVERY, STORAGE, AND HANDLING
A.	Deliver materials to the Project site in manufacturer's original wrappings and containers, labeled with supplier's or manufacturer's name, material or product brand name, and lot number, if any.
B.	Store materials in their original, undamaged packages and containers, inside a well-ventilated area protected from weather, moisture, soiling, extreme temperatures, and humidity.
1.8	SEQUENCING
A.	Ensure that locating templates and other information required for installation of products of this section are furnished to affected trades in time to prevent interruption of construction progress.
B.	Ensure that products of this section are supplied to affected trades in time to prevent interruption of construction progress.
1.9	PROJECT CONDITIONS
A.	Maintain environmental conditions (temperature, humidity, and ventilation) within limits recommended by manufacturer for optimum results. Do not install products under environmental conditions outside manufacturer's absolute limits.
1.10	WARRANTY
A.	Lifetime Limited, Non-Prorated Warranty on Material and 5 Year Prorated Labor Warranty.
PART 2    PRODUCTS
2.1	MANUFACTURERS
A.	Acceptable Manufacturer: Key-Link, which is located at:<BR />110 Peters Rd.<BR />New Holland, PA 17557<BR />Toll Free Tel: 888-704-7130<BR />Tel: 717-435-3196<BR />Fax: 717-355-7129<BR />Email: request info (jsurovi@keylinkonline.com);Web: https://keylinkonline.com 
B.	Substitutions: Not permitted.
C.	Requests for substitutions will be considered in accordance with provisions of Section 01 60 00 - Product Requirements.
2.2	MATERIALS
A.	PVC: Poly Vinyl Chloride (PVC) formulated to resist impact and for Ultra Violet (UV) stabilization. Extruded products meets or exceeds ASTM D I784.
2.3	WOOD TONE FENCE
A.	Style: Classic Picket with pinched top, 3 inch straight picket.
1.	Heights: 
a.	36 inch
b.	48 inch
c.	57 inch (pool)
2.	Width: 8 foot wide Sections
3.	Notched Pickets: 7/8 inch 3 inch max spacing 3-1/4 inch
4.	Gates and Posts: 
a.	Matching fence style.
5.	Colors: 
a.	White Pine.
b.	Seasoned Pine.
B.	Style: Manor Privacy Fence
1.	Heights: 
a.	48 inch
b.	60 inch (pool)
c.	72 inch (pool)
2.	Width: 8 foot wide Sections
3.	Panels: 7/8 inch by 6.8 inch Tongue & Groove Panels 
4.	Posts: 5 inch by 5 inch Posts
5.	Gates and Posts: 
a.	Matching fence style.
6.	Colors: 
a.	White Pine.
b.	Seasoned Pine.
C.	Style: Post and Rail Sections
1.	Heights: 
a.	36 inch
b.	48 inch
2.	Rail Option:
a.	2
b.	3 
c.	4
3.	Width: 8 foot wide Sections
4.	Rail Size: 2 inch by 6 inch by 8 foot rails.
5.	Gates and Posts: 
a.	Matching fence style.
6.	Colors: 
a.	White Pine.
b.	Seasoned Pine.
D.	Style: Nantucket Privacy Fence
1.	Height:
a.	48 inch
b.	60 inch with Lattice (pool)
c.	66 inch (pool)
d.	66 inch with Lattice (pool)
e.	66 inch with New England Accent (pool)
f.	72 inch (pool) 
g.	72 inch with Lattice (pool) 
h.	84 inch (pool)
i.	84 inch with Lattice (pool)
j.	96 inch (pool)
k.	96 inch with Lattice (pool)
2.	Section Width: 
a.	8 foot 
3.	Nantucket Classic: 
a.	Top and Bottom Horizontal Rails: 1-3/4 inch by 7 inch
b.	Vertical Panels: 3/4 inch by 10 inch interlocking.
4.	Nantucket Smooth: 
a.	Top and Bottom Horizontal Rails: 2 inch by 7 inch
b.	Vertical Panels: 3/4 inch by 10 inch interlocking.
5.	Nantucket Smooth: 
a.	Top and Bottom Horizontal Rails: 1-3/4 inch by 5-1/2 inch
b.	Vertical Panels: 3/4 inch by 10 inch interlocking.
6.	Posts: 5 inch by 5 inch.
7.	Gates and Posts: 
a.	Matching fence style.
8.	Colors: 
a.	White 
b.	Almond
c.	Clay
d.	White Pine
e.	Seasoned Pine
2.4	YARD FENCE SYSTEMS 
A.	Style: Model Yard Fence
1.	Height: 48 inch (pool)
2.	Section Width: 
a.	6 foot 
b.	8 foot 
3.	Rails: 1-3/4 inch by 3-1/2 inch routed 
4.	Midrail: Provide for 60 inch and 72 inch high fence sections. 
5.	Gates and Posts: 
a.	Matching fence style.
6.	Colors: 
a.	White 
b.	Almond
c.	Clay
d.	Black (With UV stabilizers to resist fading and chalking)
B.	Style: Victorian Yard Fence
1.	Height:
a.	36 inch
b.	48 inch (pool)
c.	60 inch (pool)
d.	72 inch (pool)
2.	Section Width: 
a.	6 foot 
b.	8 foot 
3.	Rails: 1-3/4 inch by 3-1/2 inch routed 
4.	Midrail: Provide for 60 inch and 72 inch high fence sections.
5.	Gates and Posts: 
a.	Matching fence style.
6.	Colors: 
a.	White 
b.	Almond
c.	Clay
C.	Style: Baron Yard Fence
1.	Height:
a.	36 inch
b.	48 inch (pool)
c.	60 inch (pool)
d.	72 inch (pool)
2.	Section Width: 
a.	6 foot 
b.	8 foot 
3.	Notched Pickets: 7/8 inch 3 inch maximum spacing 3-1/4 inch
4.	Rails: 1-3/4 inch by 3-1/2 inch routed 
5.	Midrail: Provide for 60 inch and 72 inch high fence sections.
6.	Gates and Posts: 
a.	Matching fence style.
7.	Colors: 
a.	White 
b.	Almond
c.	Clay
D.	Style: Ramada Yard Fence
1.	Height:
a.	36 inch
b.	48 inch (pool)
c.	60 inch (pool)
d.	72 inch (pool)
2.	Section Width: 
a.	6 foot 
b.	8 foot 
3.	Pickets: 7/8 inch 1-1/2 inch maximum spacing 1-3/4 inch
4.	Rails: 1-3/4 inch by 3-1/2 inch routed 
5.	Midrail: Provide for 60 inch and 72 inch high fence sections.
6.	Gates and Posts: 
a.	Matching fence style.
7.	Colors: 
a.	White 
b.	Almond
c.	Clay
E.	Style: Imperial Yard Fence
1.	Height:
a.	36 inch
b.	48 inch (pool)
c.	60 inch (pool)
d.	60 inch with lattice upper section
e.	72 inch (pool)
f.	72 inch with lattice upper section
2.	Section Width: 
a.	6 foot 
b.	8 foot 
3.	Pickets: 7/8 inch 1-1/2 inch maximum spacing 11/16 inch
4.	Rails: 1-3/4 inch by 3-1/2 inch routed 
5.	Midrail: Provide for 60 inch and 72 inch high fence sections.
6.	Gates and Posts: 
a.	Matching fence style.
7.	Colors: 
a.	White 
b.	Almond
c.	Clay
2.5	PRIVACY FENCE
A.	Style: Boston Privacy Fence.
1.	Height:
a.	48 inch
b.	60 inch (pool)
c.	60 inch with Lattice (pool)
d.	66 inch (pool)
e.	66 inch with Lattice (pool)
f.	66 inch with New England Accent (pool)
g.	72 inch (pool) 
h.	72 inch with Lattice (pool) 
i.	84 inch (pool)
j.	84 inch with Lattice (pool)
k.	96 inch (pool)
l.	96 inch with Lattice (pool)
2.	Section Width: 
a.	6 foot 
b.	8 foot 
3.	Deco Rails: 2 inch by 6-1/2 
4.	Midrail: Provide for 64 inch, 84 inch and 72 inch high fence sections.
5.	Tongue and Groove Panels: 7/8 inch by 8-1/2 inch with 4 inch appearance.
6.	Posts: 5 inch by 5 inch.
7.	Gates and Posts: 
a.	Matching fence style.
8.	Colors: 
a.	White 
b.	Almond
c.	Clay
B.	Style: Manor Privacy Fence.
1.	Height:
a.	48 inch
b.	60 inch with Lattice (pool)
c.	66 inch (pool)
d.	66 inch with Lattice (pool)
e.	66 inch with New England Accent (pool)
f.	72 inch (pool) 
g.	72 inch with Lattice (pool) 
h.	84 inch (pool)
i.	84 inch with Lattice (pool)
j.	96 inch (pool)
k.	96 inch with Lattice (pool)
2.	Section Width: 
a.	6 foot 
b.	8 foot 
3.	Deco Rails: 2 inch by 6-1/2 
4.	Midrail: Provide for 64 inch, 84 inch and 72 inch high fence sections.
5.	Tongue and Groove Panels: 7/8 inch by 6.8 inch.
6.	Posts: 5 inch by 5 inch.
7.	Gates and Posts: 
a.	Matching fence style.
8.	Colors: 
a.	White 
b.	Almond
c.	Clay
d.	White Pine
e.	Seasoned pine
C.	Style: Cambridge Privacy Fence
1.	Height:
a.	48 inch
b.	60 inch with Lattice (pool)
c.	66 inch (pool)
d.	66 inch with Lattice (pool)
e.	66 inch with New England Accent (pool)
f.	72 inch (pool) 
g.	72 inch with Lattice (pool) 
h.	84 inch (pool)
i.	84 inch with Lattice (pool)
j.	96 inch (pool)
k.	96 inch with Lattice (pool)
2.	Section Width: 
a.	8 foot 
3.	Cambridge Classic: 
a.	Top and Bottom Horizontal Rails: 1-3/4 inch by 7 inch
b.	Vertical Panels: 3/4 inch by 10 inch interlocking.
4.	Cambridge Smooth: 
a.	Top and Bottom Horizontal Rails: 2 inch by 7 inch
b.	Vertical Panels: 3/4 inch by 10 inch interlocking.
5.	Cambridge Smooth: 
a.	Top and Bottom Horizontal Rails: 1-3/4 inch by 5-1/2 inch
b.	Vertical Panels: 3/4 inch by 10 inch interlocking.
6.	Posts: 5 inch by 5 inch.
7.	Gates and Posts: 
a.	Matching fence style.
8.	Colors: 
a.	White 
b.	Almond
D.	Style: Nantucket Privacy Fence
1.	Height:
a.	48 inch
b.	60 inch with Lattice (pool)
c.	66 inch (pool)
d.	66 inch with Lattice (pool)
e.	66 inch with New England Accent (pool)
f.	72 inch (pool) 
g.	72 inch with Lattice (pool) 
h.	84 inch (pool)
i.	84 inch with Lattice (pool)
j.	96 inch (pool)
k.	96 inch with Lattice (pool)
2.	Section Width: 
a.	8 foot 
3.	Nantucket Classic: 
a.	Top and Bottom Horizontal Rails: 1-3/4 inch by 7 inch
b.	Vertical Panels: 3/4 inch by 10 inch interlocking.
4.	Nantucket Smooth: 
a.	Top and Bottom Horizontal Rails: 2 inch by 7 inch
b.	Vertical Panels: 3/4 inch by 10 inch interlocking.
5.	Nantucket Smooth: 
a.	Top and Bottom Horizontal Rails: 1-3/4 inch by 5-1/2 inch
b.	Vertical Panels: 3/4 inch by 10 inch interlocking.
6.	Posts: 5 inch by 5 inch.
7.	Gates and Posts: 
a.	Matching fence style.
8.	Colors: 
a.	White 
b.	Almond
c.	Clay
d.	White Pine
e.	Seasoned Pine
E.	Newbury Shadowbox Privacy Fence
1.	Height:
a.	48 inch
b.	60 inch with Lattice (pool)
c.	66 inch (pool)
d.	66 inch with Lattice (pool)
e.	66 inch with New England Accent (pool)
f.	72 inch (pool) 
g.	72 inch with Lattice (pool) 
h.	84 inch (pool)
i.	84 inch with Lattice (pool)
j.	96 inch (pool)
k.	96 inch with Lattice (pool)
2.	Section Width: 
a.	8 foot 
3.	Top and Bottom Horizontal Rails: 2 inch by 6-1/2 inch
4.	Vertical Panels: 7/8 inch by 8-1/4 inch T & G Panels.
5.	New England Accent:
6.	Lattice Accent:
7.	Scotland Accent:
8.	Posts: 5 inch by 5 inch.
9.	Gates and Posts: 
a.	Matching fence style.
10.	Colors: 
a.	White 
b.	Almond
2.6	POST AND RAIL FENCE
A.	Style: Post and Rail Sections
1.	Heights: 
a.	34-1/2 inch
b.	48 inch
c.	57 inch
2.	Rail Option:
a.	2
b.	3 
c.	4
3.	Width: 8 foot wide Sections
4.	Rail Size: 1-1/2 inch by 5-1/2 inch by 8 foot rails.
5.	Posts: 5 inch by 5 inch.
6.	Gates and Posts: 
a.	Matching fence style.
7.	Colors: 
a.	White 
b.	Almond
c.	Clay
d.	Black (With UV stabilizers to resist fading and chalking)
8.	Post Caps: 
a.	Size: 
1)	5 inch
b.	Material/Color: 
1)	White
2)	Almond
3)	Clay
4)	Black
5)	White Pine
6)	Seasoned Pine
B.	Style: Post and Rail Horse Fence
1.	Styles:
a.	2 Rail, 1-1/2 inch by 5-1/2 inch, approximate height 36.75 inch.
b.	2 Rail, 2 inch by 6 inch, approximate height 36.75 inch. 
c.	3 Rail, 1-1/2 inch by 5-1/2 inch, approximate height 51.00 inch.
d.	3 Rail, 2 inch by 6 inch, approximate height 51.00 inch.
e.	4 Rail, 1-1/2 inch by 5-1/2 inch, approximate height 58.75 inch.
f.	4 Rail, 2 inch by 6 inch, approximate height 59.25 inch.
2.	Rail Sections: 
a.	8 foot wide Lengths
b.	16 foot wide Lengths
3.	Posts: 
a.	5 inch by 5 inch with flat cap.
b.	8 foot O.C. 
4.	Gates and Posts: 
a.	Matching fence style.
5.	Colors: 
1)	White (1-1/2 inch by 5-1/2 inch)
2)	Almond (1-1/2 inch by 5-1/2 inch)
3)	Clay (2 inch by 6 inch)
4)	Black (2 inch by 6 inch)
5)	White Pine (2 inch by 6 inch)
6)	Seasoned Pine (2 inch by 6 inch)
2.7	PICKET FENCE
A.	Columbia Picket Fence
1.	Style:
a.	Straight 
b.	Concave 
2.	Heights: 
a.	36 inch
b.	48 inch
c.	57 inch (pool)
3.	Notched Pickets:
a.	7/8 inch 3 inch max spacing 3-1/4 inch.
4.	Rails: 1-3/4 inch by 3-1/2 inch routed
5.	Rail Section: 
a.	6 foot 
b.	8 foot 
6.	Posts: 
a.	5 inch.
7.	Gates and Posts: 
a.	Matching fence style.
8.	Colors: 
a.	White 
b.	Almond
c.	Clay
d.	Black
B.	Classic Picket Fence 1-1/2 inch
1.	Style:
a.	Straight 
b.	Concave 
2.	Heights: 
a.	36 inch
b.	48 inch
c.	57 inch (pool)
3.	Notched Pickets:
a.	7/8 inch 1-1/2 inch max spacing 2-1/8 inch.
4.	Rails: 1-3/4 inch by 3-1/2 inch routed
5.	Rail Section: 
a.	6 foot 
b.	8 foot 
6.	Posts: 
a.	5 inch.
7.	Gates and Posts: 
a.	Matching fence style.
8.	Colors: 
a.	White 
b.	Almond
c.	Clay
d.	Black
e.	White Pine
f.	Seasoned Pine
C.	Classic Picket Fence 3 inch
1.	Style:
a.	Straight 
b.	Concave 
2.	Heights: 
a.	36 inch
b.	48 inch
c.	57 inch (pool)
3.	Notched Pickets:
a.	7/8 inch 3 inch max spacing 3-1/4 inch.
4.	Rails: 1-3/4 inch by 3-1/4 inch routed
5.	Rail Section: 
a.	6 foot 
b.	8 foot 
6.	Posts: 
a.	5 inch.
7.	Gates and Posts: 
a.	Matching fence style.
8.	Colors: 
a.	White 
b.	Almond
c.	Clay
d.	Black
e.	White Pine
f.	Seasoned Pine
D.	New England Picket 1-1/2 inch
1.	Style:
a.	Straight 
b.	Concave 
2.	Heights: 
a.	36 inch
b.	48 inch
3.	Notched Pickets:
a.	1-1/2 inch square maximum spacing 1-3/4 inch.
4.	Rails: 
a.	Top Rail: 2 inch by 4 inch routed.
b.	Bottom Rail: 2 inch by 6 4inch routed.
5.	Rail Section: 
a.	6 foot 
b.	8 foot 
6.	Posts: 
a.	5 inch.
7.	Gates and Posts: 
a.	Matching fence style.
8.	Colors: 
a.	White 
b.	Almond
c.	Clay
E.	Deluxe Picket Fence: 
1.	Style:
a.	Straight 
b.	Concave 
2.	Heights: 
a.	36 inch
b.	48 inch (pool)
c.	57 inch (pool with 1-3/4 inch picket specing)
3.	Face Mounted Pickets: Pinched tops:
a.	7/8 inch by 3 inch maximum spacing 3-1/4 inch.
4.	Rails: 1-3/4 inch by 3-1/2 inch routed
5.	Rail Section: 
a.	6 foot 
6.	Posts: 
a.	5 inch.
7.	Gates and Posts: 
a.	Matching fence style.
8.	Colors: 
a.	White 
b.	Almond
2.8	POST CAPS
A.	Vinyl Post Cap
1.	Size:
a.	4 inch Flat (White, Almond, Clay, Black)
b.	4 inch New England (White, Almond, Clay)
c.	4 inch Spade (White, Almond, Clay)
d.	4 inch King (White, Almond, Clay)
e.	4 inch Queen (White, Almond, Clay)
f.	4inch Ball (White, Almond, Clay)
g.	4 inch New York (White, Almond, Clay)
h.	4 inch Copper (Haven)
i.	5 inch Flat (White, Almond, Clay, Black)
j.	5 inch New England (White, Almond, Clay)
k.	5 inch Ball (White, Almond, Clay)
l.	5 inch Spade (White, Almond, Clay)
m.	5 inch King (White)
n.	5 inch Queen (White)
o.	5 inch Horses Head (White)
p.	5 inch Copper (Haven)
q.	6 inch New England (White, Almond, Clay, Black)
r.	6 inch Flat (White, Almond, Clay, Black)
s.	6 inch Dental Molding (White, Almond, Clay)
t.	6 inch Ball (White)
u.	6 inch Federation (White)
v.	8 inch New England Cap (White, Almond, Clay)
w.	8 inch New York Cap (White)
B.	LED Post Cap Lights: UL approved with low voltage power supply.
1.	Style:
a.	Pyramid Style Post Cap Light: 4 inch (White, Almond, Clay, Black)
b.	Decorative Style Post Cap Light: 4 inch (White, Almond, Clay, Black)
c.	Pyramid Style Post Cap Downlight: 4 inch (White, Almond, Clay, Black)
d.	Decorative Style Post Cap Downlight: 4 inch (White, Almond, Clay, Black)
e.	Adapters to fit 4 inch cap on 5 inch Post
C.	Woodtone Post Caps
1.	Size: 
a.	4 inch 
b.	5 inch
2.	Material/Color: 
a.	Vinyl White Pine
b.	Vinyl Seasoned Pine
2.9	GATE HARDWARE
A.	"Select" Gate Hardware: 
1.	Latch: Stainless steel with aluminum latch clapper
2.	Aluminum Handle
3.	Hinge Set - Select
4.	Drop Pin Kit - Select
5.	2 Way Latch Set
6.	Finish/Color: Powder coated
a.	White
b.	Black
B.	Gate Hardware: Stainless steel with aluminum latch clappers.
1.	Aluminum Gate Handle.
2.	Gate Wheel.
3.	Aluminum Gate Brace.
4.	Hinge Set
5.	Residential Latch: Stainless steel with aluminum latch clapper.
a.	Drop Pin Kit- Residential
6.	Commercial Latch: Stainless steel with aluminum latch clapper.
a.	Drop Pin Kit - Commercial
b.	Spring Set - Commercial
7.	Finish/Color: Powder coated
a.	Black
2.10	LAWN AND GARDEN ACCESSORIES
A.	Vinyl Pergolas:
1.	Size/Color: 
a.	8 foot by 8 foot 
b.	8 foot by 12 foot 
c.	10 foot by 10 foot 
d.	10 foot by 12 foo
e.	10 foot by 16 foot
f.	12 foot by 12 foot 
g.	12 foot by 12 foot, arched 
h.	12 foot by 16 foot
i.	12 foot by 16 foot, arched
2.	Support Column: 
a.	6 inch Square Pergola Post
b.	8 inch Tapered Round Column 
c.	10 inch Tapered Round Column
d.	8 inch Square Column
e.	6 inch Savannah Column
f.	8 inch Savannah Column
3.	Roof Style:
a.	Straight Rafters 
b.	Arched Rafters (12 foot by 12 foot maximum)
4.	Shade Cover Type:
a.	Square 1-1/2 inch 
b.	Square 1-3/4 inch 
c.	Lattice 
d.	Louvered 7/8 inch by 3 inch (12 foot by 12 foot maximum)
5.	Color: 
a.	White
b.	Almond
c.	Clay
d.	Black
B.	Aluminum Pergolas:
1.	Size/Color: 
a.	8 foot by 8 foot 
b.	8 foot by 12 foot 
c.	10 foot by 10 foot 
d.	10 foot by 12 foot
e.	10 foot by 16 foot
f.	12 foot by 12 foot 
g.	12 foot by 12 foot, arched 
h.	12 foot by 16 foot
i.	12 foot by 16 foot, arched
2.	Support Column: 
a.	4 inch Square Pergola Post
3.	Roof Style:
a.	Straight Rafters 
b.	Arched Rafters (12 foot by 12 foot maximum)
4.	Shade Cover Type:
a.	Square Rail 1-1/2 inch by 3-1/4 inch
b.	Square Rail 1-3/8 inch by 5-1/4 inch
c.	Louvered 7/8 inch by 3 inch (12 foot by 12 foot maximum)
5.	Color: Powder coated
a.	Gloss Bronze
b.	Gloss Black
C.	Vinyl Arbors:
1.	Plymouth Arbor
a.	50 inches W by 88 inches H by 32 inches D White
2.	Pergola Arbor
a.	50 inches W by 81 inches H by 36 inches D White 
b.	66 inches W by 81 inches H by 36 inches D White 
c.	50 inches W by 81 inches H by 36 inches D Almond
d.	66 inches W by 81 inches H by 36 inches D Almond
3.	Kingston Arbor
a.	50 inches or 66 inches W by 84 inches H by 32 inches D White
b.	50 inches or 66 inches W by 84 inches H by 32 inches D White
4.	Madison Arbor
a.	50 inches W by 84 inches H by 32 inches D White 
b.	66 inches W by 84 inches H by 32 inches D White 
c.	50 inches W by 84 inches H by 32 inches D Almond
d.	66 inches W by 84 inches H by 32 inches D Almond
5.	Jefferson Arbor
a.	50 inches W by 80 inches H by 32 inches D White
b.	66 inches W by 80 inches H by 32 inches D White
6.	2 Hoop Arbor
a.	36 inches W by 82 inches H by 26 inches D White 
b.	48 inches W by 87 inches H by 26 inches D White
c.	48 inches W by 87 inches H by 26 inches D Almond
D.	Aluminum Arbors:
1.	Durham Arbor
a.	47 inches W by 91 inches H by 32 inches D
2.	Fairway Arbor
a.	47 inches W by 90 inches H by 37-1/2 inches D White 
3.	Color: Powder coated
a.	Black
b.	Bronze
E.	Mailbox Posts: Lettering not included
1.	Fluted Mailbox Post White
2.	Classic Mailbox Post White
3.	Recessed Panel Mailbox Post White
4.	Regular Mailbox Post White
5.	Regular Mailbox Post Almond
6.	Regular Mailbox Post Black
7.	Aluminum Mailbox Post 4 inch Black
8.	Aluminum Mailbox Post 4 inch Bronze
F.	Lamp Posts 4 inch: Includes internal aluminum pipe for added strength.
1.	Classic Post White
2.	Classic Post Almond
3.	Classic Post Clay
4.	Traditional Post White
5.	Traditional Post Almond
6.	Traditional Post Clay
7.	Manchester Post White, w/ lamp cap
8.	Manchester Post Clay, w/ lamp cap
G.	Trellises:
1.	Square Top Trellis
a.	26 inches W by 60 inches H, White
2.	Arch Top Trellis
a.	26 inches W by 74 inches H White
3.	Sheffield
a.	26 inches W by 60 inches H by 15 inches D White
4.	5 Spoke Trellis
a.	54 inches W by 72 inches H White
H.	Raised Bed Kits: Kits include all vinyl panels, corners, ground anchors, and fasteners.
1.	2 feet by 6 feet by 8 inches D, white
2.	2 feet by 6 feet by 12 inches D, white
3.	4 feet by 6 feet by 8 inches D, white 
4.	4 feet by 6 feet by 12 inches D, white
I.	Hot Bed Kits: Kits include all vinyl panels, corners, ground anchors, and fasteners.
1.	3 feet by 6 feet by, white
2.	3 feet by 8 feet by, white
J.	Vinyl Planters: 
1.	14 inches L by 24 inches W by 12 inches H, white
2.	14 inches L by 14 inches W by 12 inches H, white
3.	14 inches L by 34 inches W by 12 inches H, white
K.	Benches: 
1.	Park Bench 5 foot:
a.	Legs 
1)	Black 
2)	Green 
b.	Rails 
1)	White 
2)	Almond
L.	Picnic Tables:
1.	Picnic Table (attached benches)
a.	6 feet Long
b.	8 feet long
c.	Color: White, Almond
2.	Picnic Table with Detached Benches
a.	6 feet Long
M.	Classic Picket Accent Corner: 
1.	1-1/2 inch picket, 6 foot section white
2.	3 inch picket, 6 foot section white
N.	Lattice: 
1.	Poly Lattice: 
a.	Size: 4 foot by 8 foot sheets.
b.	Styles: 
1)	Square 1-3/4 inch, white only.
2)	Diagonal 1 inch.
3)	Diagonal 2-3/4 inch. 
c.	Color:
1)	White
2)	Almond
3)	Clay
4)	Black
2.	Vinyl Lattice: 
a.	Size: 
1)	4 foot by 8 foot sheets.
2)	11-1/2 inch by 72 inch.
3)	11-1/2 inch by 98 inch.
b.	Styles: 
1)	Square 2 inch, white only.
2)	Diagonal 2 inch.
c.	Color:
1)	White
2)	Almond
3)	Clay
PART 3    EXECUTION
3.1	EXAMINATION
A.	Do not begin installation until conditions have been properly prepared.
B.	Verification of Conditions: Examine locations where fencing is to be installed for any conditions detrimental to the proper and timely completion of the work. 
C.	If preparation is the responsibility of another installer, notify Architect of unsatisfactory preparation before proceeding.
3.2	PREPARATION
A.	Clean surfaces thoroughly prior to installation.
B.	Prepare the grade and remove surface irregularities, if any, which may cause interference with the installation of the fence.
C.	Prepare surfaces using the methods recommended by the manufacturer for achieving the best result for the substrate under the project conditions.
3.3	INSTALLATION
A.	Install in accordance with manufacturer's instructions.
B.	Set posts and gate posts for gate openings as indicated on the Drawings.
C.	Center and align posts, place concrete around posts and vibrate or tamp for consolidation. Recheck vertical and top alignment of posts, and make necessary corrections.
D.	Install gates plumb, level, and secure for full opening without interference. For double gates, install drop rod. Adjust hardware for smooth operation.
3.4	CLEANING
A.	Touch-up, repair, or replace damaged products before Substantial Completion.
B.	Clean the work according to manufacturer's written instructions. Post hole excavations shall be scattered uniformly away from the posts. Clean fence with mild household detergent and rinse well with clean water. Remove mortar from exposed posts using a 10 percent solution of muriatic acid followed immediately by several rinses with clean water.
3.5	PROTECTION
A.	Protect installed products until completion of project.
B.	Touch-up, repair or replace damaged products before Substantial Completion.

END OF SECTION