SECTION 08 41 00 (08 41 00)

FOLDING GLAZED WALL SYSTEMS - EXTERIOR AND INTERIOR

Display hidden notes to specifier. (Don't know how? Click Here) 
 Copyright 2010 -  2021 ARCAT, Inc. - All rights reserved

PART 1    GENERAL
1.1	SECTION INCLUDES
A.	Folding Glazed Wall Systems:
1.	Aluminum-framed folding/paired system. (SL45)
2.	Thermally-broken, aluminum-framed folding systems. (SL60 and SL70)
1.2	RELATED SECTIONS
A.	Section 06 10 00 - Rough Carpentry.O. and blocking.
B.	Section 06 20 00 - Finish Carpentry.
C.	Section 07 27 00 - Air Barriers.
D.	Section 07 62 00 - Sheet Metal Flashing and Trim.
E.	Section 07 90 00 - Joint Protection.
F.	Section 08 40 00 - Entrances, Storefronts, and Curtain Walls.
G.	Section 08 41 13 - Aluminum-Framed Entrances and Storefronts.
H.	Section 08 41 26 - All-Glass Entrances and Storefronts.
I.	Section 08 43 29 - Sliding Storefronts.
J.	Section 08 43 33 - Folding Glass Wall System.
K.	Section 08 51 13 - Aluminum Windows.
L.	Section 08 70 00 - Hardware.
M.	Section 08 83 13 - Mirrored Glass Glazing.
N.	Section 09 22 16 - Non-Structural Metal Framing.O. and reinforcement.
O.	Section 10 23 26 - Operable Glass Partition*.
1.3	REFERENCES
A.	American Architectural Manufacturer's Association (AAMA):
1.	AAMA 502 - Voluntary Specification for Field Testing of Newly Installed Fenestration Products.
2.	AAMA 520 - Voluntary Specification for Rating the Severe Wind-Driven Rain Resistance of Windows, Doors and Unit Skylights.
3.	AAMA 611 - Voluntary Specification for Anodized Architectural Aluminum.
4.	AAMA 920 - Operation / Cycling Performance.
5.	AAMA 1303.5 - Voluntary Specifications for Forced-Entry Resistant Aluminum Sliding Glass Doors.
6.	AAMA 1304 - Voluntary Specification for Determining Forced Entry Resistance of Side-Hinged Door Systems.
7.	AAMA 2604 - Voluntary Specifications, Performance Requirements and Test Procedures for High Performance Organic Coatings on Aluminum Extrusions and Panels.
8.	AAMA 2605 - Voluntary Specifications, Performance Requirements and Test Procedures for Superior Performing Organic Coatings on Aluminum Extrusions and Panels.
9.	AAMA CAWM 300, Forced Entry Resistance for Sliding Glass Doors.
10.	AAMA/WDMA/CSA 101/I.S.2/A440, NAFS, North American Fenestration Standard - Specification for Windows, Doors and Skylights.
B.	American National Standards Institute: ANSI Z97.1 - For Safety Glazing Materials Used in Buildings - Safety Performance Specifications and Methods of Test.
C.	ASTM International (ASTM):
1.	ASTM C1036 - Standard Specification for Flat Glass.
2.	ASTM C1048 - Standard Specification for Heat-Strengthened and Fully Tempered Flat Glass.
3.	ASTM E90- Standard Test Method for Laboratory Measurement of Airborne Sound Transmission Loss of Building Partitions and Elements.
4.	ASTM E283 - Test Method for Rate of Air Leakage through Exterior Windows, Curtain Walls, and Doors by Uniform Static Air Pressure Difference.
5.	ASTM E330 - Test Method for Structural Performance of Exterior Windows, Curtain Walls, and Doors by Uniform Static Air Pressure Difference.
6.	ASTM E331 - Standard Test Method for Water Penetration of Exterior Windows, Skylights, Doors, and Curtain Walls by Uniform Static Air Pressure Difference.
7.	ASTM E413 - Classification for Rating Sound Insulation.
8.	ASTM E547 - Test Method for Water Penetration of Exterior Windows, Curtain Walls, and Doors by Cyclic Static Air Pressure Differential.
9.	ASTM E1332 - Standard Classification for Rating Outdoor-Indoor Sound Attenuation.
10.	ASTM E2268 - Standard Test Method for Water Penetration of Exterior Windows, Skylights, and Doors by Rapid Pulsed Air Pressure Difference.
11.	ASTM F842 - Standard Test Methods for Measuring the Forced Entry Resistance of Sliding Door Assemblies.
D.	British Standards Institution (BSI Group): PAS 24 (Publicly Available Specification), Enhanced security performance requirements for door assemblies.
E.	California Association of Window Manufacturers (CAWM): CAWM 300 - Forced Entry Resistance Tests for Sliding Glass Doors.
F.	Construction Products Directive (CPD): CE Mark.
G.	Consumer Product Safety Commission (CPSC): CPSC 16CFR-1201, Safety Standard for Architectural Glazing Materials.
H.	German Institute for Standardization (DIN):
1.	DIN EN 1191 - Windows and Pedestrian Doors - Mechanical Durability Test Method.
2.	DIN EN ISO 717-1 - Acoustics - Rating of sound insulation in buildings and building elements.
3.	DIN EN 1627 - Pedestrian door sets, windows, curtain walling, grilles and shutters - Burglar resistance - Requirements and classification.
4.	DIN EN 1630 - Pedestrian door sets, windows, curtain walling, grilles and shutters - Burglar resistance - Test method for the determination of resistance to manual burglary attempts.
5.	DIN EN ISO 10140-1, 2, 4 and 5 - Airborne sound measurement.
6.	DIN EN ISO 12400 - Windows and pedestrian doors - Mechanical durability - Requirements and classification.
7.	DIN 52210-3 - Testing of acoustics in buildings - Airborne and impact sound insulation - Laboratory measurements of sound insulation of building elements and field measurements between rooms.
8.	DIN 52210-4 - Tests in Building Acoustics - Airborne and Impact Sound.
I.	Florida Building Code: TAS 202 - Criteria for Testing Impact and Non-Impact Resistant Building Envelope Components Using Uniform Static Air Pressure.
J.	International Organization for Standardization (ISO):
1.	ISO 9001 - Quality management systems.
2.	ISO 14001 - Environmental management systems.
K.	National Fenestration Rating Council (NFRC):
1.	NFRC 100 - Procedure for Determining Fenestration Product U-factors.
2.	NFRC 200 - Procedure for Determining Fenestration Product Solar Heat Gain Coefficient and Visible Transmittance at Normal Incidence.
3.	NFRC 400 - Procedure for Determining Fenestration Product Air Leakage.
4.	NFRC 500 - Procedure for Determining Fenestration Product Condensation Resistance Rating Values.
L.	U.S. Environmental Protection Agency (EPA): Energy Star program.
1.4	SUBMITTALS
A.	Submit under provisions of Section 01 30 00 - Administrative Requirements.
B.	Product Data: Manufacturer's data sheets on each product to be used, including:
1.	Preparation instructions and recommendations.
2.	Storage and handling requirements and recommendations.
3.	Independently tested data listing performance criteria.
4.	Product literature for systems incorporated in the Work. Performance test results and details of construction relative to materials, dimensions of individual components, profiles, and colors.
5.	Manufacturers' Instructions: Submit Owner's Manual from manufacturer which includes installation instructions, operation and maintenance data.
6.	Certificates: Submit CE Mark Certificate.
C.	Product Drawings: Including but not limited to the following.
1.	Indicate system component sizes, dimensions and framing R.O., configuration, swing panels, direction of swing, stacking layout, typical head jamb, side jambs and sill details, type of glazing material, handle height and field measurements.
2.	Elevations of rough opening requirements and details for field-applied components.
D.	Contract Closeout Submittal: Owner's Manual from manufacturer. Identify Owner's Manual with project name, location and completion date, type and size of unit installed.
1.5	QUALITY ASSURANCE
A.	Regulatory Requirements: CE Mark certified.
B.	Manufacturer: Complete, precision built, engineered, pre-fitted units by a single source manufacturer with 30-year experience in providing folding and sliding door systems for large openings in the North American market.
1.	DIN EN ISO 9001: 2015 quality management system registration.
2.	DIN EN ISO 14001: 2015 environmental management system registration.
C.	Installer Qualifications:
1.	Experienced in installation of manufacturer's products or similar products.
2.	Reference list of 3 projects of similar scale and complexity successfully completed in the last 3 years.
3.	Project names, locations, completion dates, names and telephone numbers of General Contractor and Owner's contact person.
4.	Installer trained and certified by manufacturer.
D.	Single Source: Furnish system materials from one manufacturer for entire Project.
1.6	DELIVERY, STORAGE, AND HANDLING
A.	Deliver materials to job site in sealed, unopened cartons or crates.
1.	Upon receipt, inspect shipment. Ensure it is complete, in good condition and meets project requirements.
B.	Store products in manufacturer's unopened packaging until installation. Store flat in well ventilated area, no direct sunlight, in a clean and dry location. Protect units against weather and defacement or damage from construction activities, especially to panel edges.
1.7	PROJECT CONDITIONS
A.	Mark field measurements on Product Drawing submittal. Contractor shall field verify dimensions including but not limited to rough openings and inset components.
B.	Maintain environmental conditions (temperature, humidity, and ventilation) within limits recommended by manufacturer for optimum results. Do not install products under environmental conditions outside manufacturer's recommended limits.
1.8	WARRANTY
A.	Manufacturer's warranty against defects in materials and workmanship and as follows:
1.	Rollers: 10 years.
2.	Seal Failure of Insulated Glazing: 10 years.
3.	Other Components (excluding screens): Five years beginning with the earliest of 120 days from date of delivery by manufacturer or date of Substantial Completion.
4.	Other Components (excluding screens): 10 years beginning with the earliest of 120 days from date of delivery by manufacturer or Date of Substantial Completion if installed by manufacturer's specific system approved or certified trained installer.
PART 2    PRODUCTS
2.1	MANUFACTURERS
A.	Acceptable Manufacturer: Nana Wall Systems, Incorporated; 100 Meadow Creek Drive, Suite 250 Corte Madera, CA 94925; ASD Toll Free Tel: 800-873-5673; Tel: 415-383-3148; Fax: 415-383-0312; Email: info@nanawall.com; Web: http://www.nanawall.com.
B.	Substitutions: Not permitted.
C.	Requests for Substitutions: Considered in accordance with provisions of Section 01 60 00 - Product Requirements.
2.2	ALUMINUM-FRAMED FOLDING GLASS WALL SYSTEM
A.	Basis of Design: Model SL45 Aluminum Folding Glass Wall Systems manufactured by Nana Wall Systems, Incorporated. Top-hung system for straight runs, segmented angle changes, and center pivot. Manufacturer's standard frame and panel profiles, with head and floor tracks, side jambs and panels with dimensions as shown on Drawings.
1.	System Components: Aluminum frame, threshold, panels, sliding-folding and locking hardware, weather stripping, glass and glazing, and, accessories as required for a complete working installation.
a.	Insect Screen:  Fully retractable non-pleated screen. Ultra-strong, UV resistant fiberglass mesh housed in single cartridge riding on a single track.
1)	Basis-of-Design Product by Manufacturer:  The Horizon by Wizard Industries, Inc.
B.	Performance Criteria: Lab tested.
1.	Standard Sill - Inward or Outward Opening.
a.	Air Infiltration per ASTM E283: At static air pressure difference of 1.57 psf (75 Pa): 0.27 cu ft per min per sq ft (1.38 L per sec per sq m).
b.	Water Penetration per ASTM E331, ASTM E547: Weep holes by others. No uncontrolled water leakage at static test pressure of 1.56 psf (75 Pa).
2.	Low Profile Saddle Sill - Inward or Outward Opening.
a.	Air Infiltration per ASTM E283: At static air pressure difference of 1.6 psf (75 Pa): 0.25 cu ft per min per sq ft (1.28 L per sec per sq m).
b.	Water Penetration per ASTM E331, ASTM E547: Weep holes by others. No uncontrolled water leakage at static test pressure of 3.76 psf (180 Pa).
3.	Flush Sill - Inward or Outward Opening.
a.	Air Infiltration per ASTM E283: At static air pressure difference of 1.6 psf (75 Pa): 0.25 cu ft per min per sq ft (1.28 L per sec per sq m).
4.	ADA Compliant Flush Sill - Inward or Outward Opening. 
a.	Air Infiltration per ASTM E283: At static air pressure difference of 1.6 psf (75 Pa): 0.25 cu ft per min per sq ft (1.28 L per sec per sq m).
5.	Structural Load Deflection per ASTM E330:
a.	Load Structure: At 1.5 times design wind pressure with no glass breakage or permanent damage to fasteners or storefront components.
b.	Design Pressure Positive and Negative: 35 psf (1675 Pa).
6.	Forced Entry per AAMA 1303.5 and AAMA CAWM 300: Meets requirements.
7.	Swing Panel - Operation / Cycling Performance per AAMA 920: 500,000 cycles.
8.	Thermal Performance U-factor: NFRC 100 rated, certified and labeled.
9.	Solar Heat Gain Coefficient Plus Visible Light Transmission: NFRC 200 rated, certified and labeled.
10.	Florida Product Approval for Wind Loading: Units tested to AAMA 101/I.S.2/A440 and approved according to the Florida Building Code 2014, Section 1710.5, for panel sizes subject to manufacturer size charts.
a.	Product Approval Number: FL37258: Units with panel sizes up to 43 inch (1.07 m) wide x 120 inch (3.05 m) high; subject to manufacturer size chart.
11.	Acoustic Performance: STC (Rw).
a.	System STC (Rw) 35 (35) and OITC 30 with 5/16 inch (8 mm) STC 37 laminated glass.
b.	System STC (Rw) 30 (31) and OITC 27 with 1/4 inch (6 mm) STC 32 tempered glass.
c.	System STC (Rw) 34 (34) with 1/4 inch (6 mm) STC 36 enhanced laminated glass. 
d.	System STC (Rw) 33 (33) with 1/4 inch (6 mm) STC 35 laminated glass.
e.	System STC (Rw) 30 (30) with 1/4 inch (6 mm) STC 31 tempered glass.
C.	Design Criteria:
1.	Sizes and Configurations: Refer to Drawings for custom dimensions within maximum frame sizes indicated in manufacturer's literature. Refer to Drawings for number of panels and configuration.
2.	Unit Operation: Sliding and folding hardware with top and bottom tracks.
3.	Panel Configuration: Straight.
4.	Panel Configuration: Segmented curve.
5.	Panel Configuration: 90 degree angle turn.
6.	Panel Configuration: 135 degree angle turn.
7.	Panel Configuration: Window and door combination.
8.	Panel Operation: Inward opening unit. Stack Storage Configuration: Inside jamb.
9.	Panel Operation: Outward opening unit. Stack Storage Configuration: Outside jamb.
10.	Panel Operation: Center pivoted unit. Stack Storage Configuration: Center pivot.
11.	Panel Operation: Inward/outward combination opening unit. Stack Storage Configuration: Inside-outside combination.
12.	Panel Operation: Fold flat, against wall, full 180 degrees movement of door panel stack. Stack Storage Configuration: Fold flat against wall.
13.	Mounting, Top Hung: For each pair of folding panels, cardanic, independently suspended, four wheeled upper running carriage and lower guide carriage. Coated with fiberglass reinforced polyamide.
14.	Panel Type: Hinged.
15.	Panel Type: Unhinged.
16.	Primary Swing Panel of Paired Swing Panels: Swing Direction: Looking from inside.
a.	Primary Swing Panel: On the left.
b.	Primary Swing Panel: On the right.
17.	Entry and Egress Panel: Hinged to side jamb.
18.	Panel Pairing Configuration: See Drawings.
D.	Fabrication: Extruded aluminum frame and panel profiles, corner connectors, hinges, sliding and folding hardware, locking hardware, handles, glass and glazing, and weather stripping. 
1.	Factory pre-assembled. Ship with system components and installation instructions.
2.	Exposed work matched to produce continuity of line and design with all joints.
3.	No raw edges visible at joints.
E.	Materials:
1.	Panels: Single lite; standard.
2.	Panels: Horizontal mullions at specified heights from the bottom of the panel.
3.	Panels: Simulated divided lites in pattern as shown on Drawings.
4.	Panel Size (W x H): As indicated on Drawings.
5.	Rail Depth: 1-3/4 inch (45 mm).
6.	Top Rail and Stile Width: 2-1/8 inch (53 mm).
7.	Bottom Rail Width: 2-1/8 inch (53 mm)
a.	Manufacturer's standard kickplate. Height (in/mm): ______.
8.	Frame: Matching top track and side jambs.
9.	Top Track Width: 2-1/2 inch (64 mm). 
10.	Top Track and Side Jambs Depth: 1-3/4 inch (45 mm).
11.	Sill Type: Standard sill.
12.	Sill Type: Low profile saddle sill.
13.	Sill Type: Flush sill.
14.	Sill Type: ADA compliant flush sill.
15.	Sill Type: Surface mounted interior sill for interior application.
16.	Sill Finish: Aluminum with a clear anodized finish.
17.	Sill Finish: Aluminum with a dark bronze anodized finish.
18.	Sill Finish: Aluminum with finished to match panel (only with standard sill).
19.	For ADA Compliance at Swing Panel: Provide gasket to cover the channel in the sill at swing panels.
20.	Aluminum Extrusions: AIMgSi0.5 alloy, 6063-T5; F-22 - European standard.
a.	Thickness: 0.078 inch (2.0 mm) nominal.
b.	Panel and Frame Finish: One color inside and outside.
1)	Finish Type:  Anodized per AAMA 611. Clear. 
2)	Finish Type:  Anodized per AAMA 611. Dark bronze. 
3)	Finish Type:  Powder coat per AAMA 2604. 
a)	Color: Chosen from standard selection of 50 colors. Matte. 
b)	Color: Chosen from full RAL selection. High gloss. 
c)	Color: Chosen from full RAL selection. Matte. 
4)	Finish Type: PVDF Coat per AAMA 2605: Fluoropolymer Kynar with color to match custom finish.
5)	Finish Type:  Custom finish.
c.	Panel and Frame Finish: Different color inside and outside.
1)	Interior: Anodized per AAMA 611. Clear.
2)	Interior: Anodized per AAMA 611. Dark bronze.
3)	Interior: Powder coat per AAMA 2604.
a)	Color: Chosen from standard selection of 50 colors. Matte.
b)	Color: Chosen from full RAL selection. High gloss.
c)	Color: Chosen from full RAL selection. Matte.
4)	Interior: PVDF Coat per AAMA 2605: Fluoropolymer Kynar with color to match custom finish.
5)	Interior: Custom finish.
6)	Exterior: Anodized per AAMA 611. Clear. 
7)	Exterior: Anodized per AAMA 611. Dark bronze. 
8)	Exterior: Powder coat per AAMA 2604. 
a)	Color: Chosen from standard selection of 50 colors. Matte. 
b)	Color: Chosen from full RAL selection. High gloss. 
c)	Color: Chosen from full RAL selection. Matte. 
9)	Exterior: PVDF Coat per AAMA 2605: Fluoropolymer Kynar with color to match custom finish. 
10)	Exterior: Custom finish.
F.	Glass and Glazing:
1.	Safety Glazing per ASTM C1036, ASTM C1048, ANSI Z97.1 and CPSC 16CFR 1201.
2.	Manufacturer's Glass Lites: Dry glazed with glass stops on the inside.
3.	Glass Lites  Tempered.
4.	Glass Lites:  Tempered and laminated.
5.	Glass Lites:  Laminated.
6.	Glass Type:  Reduced iron; standard.
7.	Glass Lite; Single: 1/4 inch (6 mm) STC 36 enhanced laminated glass to achieve unit STC of 34. 
8.	Glass Lite; Single: 1/4 inch (6 mm) STC 35 laminated glass to achieve unit STC of 33.
9.	Glass Lite; Single: 1/4 inch (6 mm) STC 31 tempered glass to achieve unit STC of 30.
10.	Glass Lite; Double IGU: 13/16 inch (20 mm) thick.
11.	IGU Fill: Air filled 
12.	IGU Fill: Argon filled.
13.	IGU Surface: Clear.
14.	IGU Surface: Low-E coating on No. 2 surface of double IGU.
15.	IGU Surface: Low-E coating on No. 2 and No. 4 surface of double IGU.
16.	Glass Spacers: Manufacturer's standard.
17.	Glass Spacers: Gray finish with capillary tubes.
18.	Glass Spacers: Black finish with capillary tubes.
19.	Glass Spacers: Gray finish without capillary tubes.
20.	Glass Spacers: Black finish without capillary tubes.
G.	Locking Hardware and Handles:
1.	Main Entry Panel or Pair of Panels for Models with a Swing Panel or Panels:
a.	Lever Handles: On inside and outside.
b.	Lever Handles: With return on inside and outside.
c.	Standard lockset with lockable latch.
d.	Multi-point locking with concealed dead bolt and rods at top and bottom on primary panel only.
e.	Operation: After turn of key or thumb-turn, depression of handles withdraws latch. Lifting of handles engages rods and key or thumb turn engages deadbolt and operates lock.
f.	Rods to be concealed and not edge mounted.
g.	Secondary Swing Panel: Two-point locking with flat handles on inside only for secondary swing panel.
h.	Lever Handles Finish: Brushed satin stainless steel; standard.
i.	Lever Handles Finish: Titanium black stainless steel; standard.
j.	Lever Handles Finish: Copper- nickel stainless steel antiviral and antimicrobial.
k.	Lever Handles Finish: Oil rubbed bronze solid brass.
l.	Lever Handles Finish: Satin nickel solid brass.
m.	Lever Handles Finish: White solid brass.
n.	Locking: Standard profile cylinder
o.	Locking: Adapter for Small Format Interchangeable Core.
2.	Main Entry Panel for Models with a Swing Panel or a Pair of Swing Panels: Lever handles on inside and outside with single action, emergency egress, interconnected lock.
3.	Main Entry Panel or Pair of Panels for Models with a Swing Panel or Swing Panels Attached to a Side Jamb: Manufacturer's push-pull handles with separate lockset and dead bolt.
a.	Push-pull handles Finish: Brushed stainless steel.
4.	Main Entry Panel or Pair of Panels for Models with Swing or paired Swing Panels: Field installed panic devices per Section 08 71 00 - Door Hardware.
5.	Main Entry Panel or Pair of Panels for Inswing Models without Swing Panel or Panels: Manufacturer's L-shaped handle on inside, flat handle on outside and lock set with profile cylinder. Operation of lock set is by turn of key from the outside and with a thumb-turn from the inside with a two-point locking hardware operated by 180 degree turn of the handle.
a.	L-Shaped Handles: Stainless steel brushed satin finish.
b.	L-Shaped Handles: Stainless steel titanium black finish.
6.	Main Entry Panel or Pair of Panels for Outswing Models without Swing Panels: Flat handle on both sides and a lock set with a profile cylinder. Operation of lock set is by turn of key from the outside and from the inside with a two-point locking hardware operated by 180 degree turn of the handle.
7.	Main Entry Panel or Pair of Panels for Models without Swing Panels: Flat handle on inside with concealed two-point locking hardware operated by 180 degree turn of handle.
8.	Secondary Panels and Pairs of Folding Panels: Handles and concealed one or two-point locking hardware operated by 180 degree turn of handle between each pair. Face applied flush bolt locking not acceptable; except for units with paired panels.
a.	Handles: Manufacturer's flat handles.
1)	Flat Handle Finish: Brushed satin stainless steel.
2)	Flat Handle Finish: Black titanium stainless steel.
3)	Flat Handle Finish: Copper-nickel stainless steel antiviral and antimicrobial. 
4)	Flat Handle Finish: Powder coated aluminum with color finish to match frame.
b.	Handles: Removable custodial handles.
9.	Handle Height: 41-3/8 inch (105 cm) centered from bottom of panel unless otherwise indicated on Drawings.
10.	Locking Rods: End caps top and bottom;. Rod Stroke: 15/16 inch (24 mm).
11.	Additional Profile Cylinders: Keyed alike.
12.	Additional Profile Cylinders: Keyed differently.
H.	Sliding and Folding Hardware:
1.	Manufacturer's combination sliding and folding hardware with top, bottom tracks.
2.	For Each Pair of Folding Panels: Independent cardanic suspension for 4 wheeled rollers coated with fiberglass reinforced polyamide upper running carriage and lower guide carriage.
3.	Swing Panel Hinges: Zinc die cast with finish closest match to finish of frame and panels and stainless-steel security hinge pins with set-screws.
4.	Swing Panel Hinges: Stainless steel hinges and security hinge pins with set-screws.
5.	Hinge Adjustment: 1/16 inch (1.5 mm) in width per hinge. Adjustments to be made without needing to removing panels from tracks.
I.	Weather Stripping: Double layer EPDM between panels and EPDM gasket and Q-Lon gasket or brush seal between panel and frame or brush seals with a two-layer fiberglass reinforced polyamide fin attached at both inner and outer bottom edge of door panels, with a recessed sill or on frame, for sealing between panels and between panel and frame.
J.	Fasteners: Stainless steel screws for connecting frame components.
K.	Accessories: Sidelights, transoms, corner posts, or single or double doors as indicated.
2.3	THERMALLY BROKEN ALUMINUM-FRAMED FOLDING/PAIRED GLASS WALL SYSTEMS (SL60)
A.	Basis of Design: Model SL60. Thermally broken aluminum-framed folding/paired glass wall system, top hung, or floor track supported as manufactured by Nana Wall Systems, Incorporated. Manufacturer's standard frame and panel profiles, with head track, side jambs and panels with dimensions as shown on Drawings.
1.	System Components: Aluminum frame, threshold, panels, sliding-folding and locking hardware, weather stripping, glass and glazing, and, accessories as required for a complete working installation.
a.	Insect Screen:  Fully retractable non-pleated screen. Ultra-strong, UV resistant fiberglass mesh housed in single cartridge riding on a single track.
1)	Basis-of-Design Product by Manufacturer:  The Horizon by Wizard Industries, Inc.
B.	Performance Criteria: Lab tested.
1.	Standard Flush Sill - Inward and Outward Opening.
a.	Air Infiltration and Exfiltration per ASTM E283:
1)	At static air pressure difference of 1.57 psf (75 Pa):
a)	Infiltration: 0.10 cu ft per min per sq ft (0.5 L per sec per sq m).
b)	Exfiltration: 0.08 cu ft per min per sq ft (0.4 L per sec per sq m).
2)	At 6.24 psf (300 Pa):
a)	Infiltration: 0.37 cfm per sq ft (1.9 L per sec per sq m).
b)	Exfiltration: 0.17 cfm per sq ft (0.9 L per sec per sq m).
b.	Structural Loading per ASTM E330 Design Pressure:
1)	Positive Inswing or Negative Outswing: 40 psf (1920 Pa).
2)	Negative Inswing or Positive Outswing: 45 psf (2160 Pa).
c.	Swing Panel with Surface Mounted Hinges - Operation / Cycling Performance per AAMA 920: 500,000 cycles.
2.	Low Profile Saddle Sill - Inward and Outward Opening.
a.	Air Infiltration and Exfiltration per ASTM E283:
1)	At static air pressure difference of 1.57 psf (75 Pa):
a)	Infiltration: 0.10 cu ft per min per sq ft (0.5 L per sec per sq m).
b)	Exfiltration: 0.08 cu ft per min per sq ft (0.4 L per sec per sq m).
2)	At 6.24 psf (300 Pa):
a)	Infiltration: 0.37 cfm per sq ft (1.9 L per sec per sq m).
b)	Exfiltration: 0.17 cfm per sq ft (0.9 L per sec per sq m).
b.	Water Penetration per ASTM E331, ASTM E547: No uncontrolled water leakage at a static test pressure of 5.43 psf (260 Pa) with weeps by others.
c.	Structural Loading per ASTM E330 Design Pressure:
1)	Positive Inswing or Negative Outswing: 40 psf (1920 Pa).
2)	Negative Inswing or Positive Outswing: 45 psf (2160 Pa).
d.	Swing Panel with Surface Mounted Hinges - Operation / Cycling Performance per AAMA 920: 500,000 cycles.
3.	Hybrid Sill - Inward Opening.
a.	Air Infiltration per ASTM E283:
1)	At static air pressure difference of 1.57 psf (75 Pa): Infiltration: 0.05 cu ft per min per sq ft (0.09 L per sec per sq m).
2)	At 6.24 psf (300 Pa): Infiltration: 0.13 cfm per sq ft (0.67 L per sec per sq m).
b.	Water Penetration per ASTM E331, ASTM E547: No uncontrolled water leakage at a static test pressure of 7.5 psf (360 Pa). Not applicable for even-even configurations.
c.	Structural Loading per ASTM E330 Design Pressure:
1)	Positive Inswing or Negative Outswing: 45 psf (2160 Pa).
2)	Negative Inswing or Positive Outswing: 45 psf (2160 Pa).
4.	Hybrid Sill - Outward Opening.
a.	Air Infiltration per ASTM E283:
1)	At static air pressure difference of 1.57 psf (75 Pa): Infiltration: 0.02 cu ft per min per sq ft (0.07 L per sec per sq m).
2)	At 6.24 psf (300 Pa): Infiltration: 0.10 cfm per sq ft (0.51 L per sec per sq m).
b.	Water Penetration per ASTM E331, ASTM E547: No uncontrolled water leakage at a static test pressure of 7.5 psf (360 Pa). Not applicable for even-even configurations.
c.	Structural Loading per ASTM E330 Design Pressure:
1)	Positive Inswing or Negative Outswing: 45 psf (2160 Pa).
2)	Negative Inswing or Positive Outswing: 45 psf (2160 Pa).
5.	Higher Weather Performance Raised Sill; Inward Opening.
a.	Air Infiltration per ASTM E283:
1)	At static air pressure difference of 1.57 psf (75 Pa): 0.02 cfm per sq ft (0.10 L per sec per sq m) or (0.25 cu m per hour per m).
2)	At 6.24 psf (300 Pa): 0.06 cfm per sq ft (0.31 L per sec per sq m).
b.	Water Penetration per ASTM E331 and ASTM E547: No uncontrolled water entry at 7.5 psf (360 Pa). Not applicable for even-even configurations.
c.	Structural Loading per ASTM E330:
1)	Design Pressure Positive: 45 psf (2160 Pa).
2)	Design Pressure Negative: 45 psf (2160 Pa).
6.	Higher Weather Performance Raised Sill; Outward Opening.
a.	Air Infiltration per ASTM E283:
1)	At static air pressure difference of 1.57 psf (75 Pa): 0.01 cfm per sq ft (0.05 L per sec per sq m).
2)	At 6.24 psf (300 Pa): 0.01 cfm per sq ft (0.05 L per sec per sq m).
b.	Water Penetration per ASTM E331 and ASTM E547: No uncontrolled water leakage at 7.5 psf (360 Pa).
c.	Structural Loading per ASTM E330:
1)	Design Pressure Positive: 45 psf (2160 Pa).
2)	Design Pressure Negative: 40 psf (1920 Pa).
7.	Glass Acoustical Performance per DIN 52210-3,4: With 38 Db glass, unit Rw (STC) of 36
8.	System Life Cycle Performance per DIN EN 1191/12400: Pass; 20,000 cycles
9.	Forced Entry per AAMA 1304: Meets requirements
10.	Burglary Resistance: EN 1627-30, Class RC2/ RC2N; Resistance Class 2 certified.
11.	Lockset Burglary Resistance: PAS 24 certified.
12.	Florida Product Approval for Wind Loading: Units tested to AAMA/WDMA/CSA 101/I.S.2/A440 and approved according to the Florida Building Code 2014, Section 1710.5, for panel sizes subject to manufacturer size charts.
a.	Product Approval Number: FL37263. Approved for use outside hurricane zones (HVHZ) with Design Pressure plus or minus 45 psf. for tested panel size.
13.	Thermal Performance U-factor: NFRC 100 rated, certified and labeled 
14.	Solar Heat Gain Coefficient and Visible Light Transmission: NFRC 200 rated, certified and labeled.
15.	Air Leakage: NFRC 400 rated, certified and labeled.
16.	Condensation Resistance Factor (CRF): NFRC 500 rated, certified and labeled.
17.	EPA Energy Star: Meets requirements with certain, specific glass.
C.	Design Criteria:
1.	Sizes and Configurations:  As indicated by the Drawings for selected number and size of panels, location of swing panels, and stacking.
2.	Operation: Sliding and folding hardware with top and bottom tracks.
3.	Mounting Type: Top-hung.
4.	Mounting Type: Floor track supported.
5.	Panel Configuration: Straight.
6.	Panel Configuration: Window- Door Combination
7.	Panel Type: Hinged.
a.	Primary swing panel of paired swing panels, looking from inside: On the left.
b.	Primary swing panel of paired swing panels, looking from inside: On the right.
c.	Entry and Egress panel hinged to side jamb.
8.	Panel Pairing Configuration: See Drawings.
9.	Stack Storage Configuration: Inswing.
10.	Stack Storage Configuration: Outswing.
D.	Fabrication:  Extruded aluminum frame and panel profiles, corner connectors, hinges, sliding and folding hardware, locking hardware, handles, glass, glazing, and weather stripping.
1.	Factory pre-assembled. Ship with system components and installation instructions.
2.	Exposed work matched to produce continuity of line and design with joints.
3.	No raw edges visible at joints.
E.	Materials:
1.	Panels: Single lite; standard.
2.	Panels: Horizontal mullions at specified heights from the bottom of the panel.
3.	Panels: Single lite with simulated divided lites in pattern as shown on Drawings.
4.	Panel Size (W x H): As indicated on Drawings.
5.	Rail Depth: 2-5/16 inch (59 mm).
6.	Top Rail and Stile Width: 2-3/8 inch (60 mm).
7.	Bottom Rail Width: 2-3/8 inches (60 mm).
a.	Manufacturer's standard kickplate. Height (in/mm): ______.
8.	Frame: Matching top track and side jambs.
a.	Top Track Width; Top-Hung: 3-15/16 inch (100 mm).
b.	Top Track Width; Floor Supported: 2-9/16 inch (65 mm).
c.	Side Jambs Width: 2-9/16 inch (65 mm).
d.	Top Track and Side Jambs Depth: 3-1/8 inch (66 mm).
9.	Sill Type: Higher weather performance raised sill; thermally broken.
10.	Sill Type: Flush sill; thermally broken.
11.	Sill Type: Low profile saddle sill; thermally broken.
12.	Sill Type: Hybrid sill; thermally broken.
13.	Sill Type: Surface mounted interior sill; not thermally broken, only for floor supported system in interior application.
14.	Sill Aluminum Finish: Clear anodized finish.
15.	Sill Aluminum Finish: Dark bronze anodized finish.
16.	Sill Aluminum Finish: Finished to match panel only with higher weather performance sill.
17.	Aluminum Extrusions: AIMgSi0.5 alloy, 6063-T5; F-22 - European standard.
a.	Thickness: 0.078 inch (2.0 mm) nominal.
b.	Thermal Break: 7/8 inch (22 mm) wide glass fiber reinforced polyamide plastic. Narrower or poured and de-bridged type thermal breaks not acceptable.
c.	Panel and Frame Finish: One color inside and outside.
1)	Finish Type:  Anodized per AAMA 611. Clear. 
2)	Finish Type:  Anodized per AAMA 611. Dark bronze. 
3)	Finish Type:  Powder coat per AAMA 2604. 
a)	Color: Chosen from standard selection of 50 colors. Matte. 
b)	Color: Chosen from full RAL selection. High gloss. 
c)	Color: Chosen from full RAL selection. Matte. 
4)	Finish Type: PVDF Coat (AAMA 2605): Fluoropolymer Kynar with color to match custom finish.
5)	Finish Type:  Custom finish.
d.	Panel and Frame Finish: Different color inside and outside.
1)	Interior: Anodized per AAMA 611. Clear.
2)	Interior: Anodized per AAMA 611. Dark bronze.
3)	Interior: Powder coat per AAMA 2604.
a)	Color: Chosen from standard selection of 50 colors. Matte.
b)	Color: Chosen from full RAL selection. High gloss.
c)	Color: Chosen from full RAL selection. Matte.
4)	Interior: PVDF Coat (AAMA 2605): Fluoropolymer Kynar with color to match custom finish.
5)	Interior: Custom finish. 
6)	Exterior: Anodized per AAMA 611. Clear. 
7)	Exterior: Anodized per AAMA 611. Dark bronze. 
8)	Exterior: Powder coat per AAMA 2604. 
a)	Color: Chosen from standard selection of 50 colors. Matte. 
b)	Color: Chosen from full RAL selection. High gloss. 
c)	Color: Chosen from full RAL selection. Matte. 
9)	Exterior: PVDF Coat (AAMA 2605): Fluoropolymer Kynar with color to match custom finish.
10)	Exterior: Custom finish.
F.	Glass and Glazing:
1.	Safety Glazing per ASTM C1036, ASTM C1048, ANSI Z97.1 and CPSC 16CFR 1201.
2.	Glazing Units, Double Insulated: Dry glazed with glass stops on the inside.
a.	Glass Lites: Tempered.
b.	Glass Lites: Laminated.
c.	Glass Lites: Tempered and laminated.
d.	Thickness: 15/16 inch (24 mm) thick.
3.	Glazing Units, Triple Insulated: Dry glazed with glass stops on the inside.
a.	Glass Lites: Tempered.
b.	Glass Lites: Laminated.
c.	Glass Lites: Tempered and laminated.
d.	Thickness: 1-3/8 inch (35 mm) thick.
4.	Insulated Glazing Unit Fill: Air.
5.	Insulated Glazing Unit Fill: Argon.
6.	Glass Type: Standard.
7.	Glass Spacers: Gray finish with capillary tube.
8.	Glass Spacers: Black finish with capillary tubes.
9.	Glass Spacers: Gray finish without capillary tubes.
10.	Glass Spacers: Black finish without capillary tubes.
11.	Insulated Glass Unit Surfaces: Clear.
12.	Insulated Glass Unit Surfaces: Low- E coating on No. 2 surface of double IGU.
13.	Insulated Glass Unit Surfaces: Low- E coating on No. 2 surface and No. 4 surface of double IGU.
14.	Insulated Glass Unit Surfaces: Low-E coating on No. 2 surface and No. 5 surface of triple IGU.
G.	Locking Hardware and Handles:
1.	Main Entry Panels for Models with a Swing Panel or Pair of Swing Panels:
a.	Lever Handles: On inside and outside.
b.	Lever Handles: With return on inside and outside.
c.	Standard lockset with lockable latch.
d.	Multi-point locking with concealed dead bolt and rods at top and bottom on primary panel only.
e.	Operation: After turn of key or thumb-turn, depression of handles withdraws latch. Lifting of handles engages rods and key or thumb turn engages deadbolt and operates lock.
f.	Rods to be concealed and not edge mounted.
g.	Secondary Swing Panel: Dummy lever handles; both sides. Concealed flush bolts operate rods at top and bottom for secondary swing panel.
h.	Secondary Swing Panel: Two-point locking with flat handles on inside only for secondary swing panel.
i.	Lever Handles Finish: Brushed satin stainless steel; standard.
j.	Lever Handles Finish: Titanium black stainless steel; standard.
k.	Lever Handles Finish: Copper- nickel stainless steel antiviral and antimicrobial.
l.	Lever Handles Finish: Oil rubbed bronze solid brass.
m.	Lever Handles Finish: Satin nickel solid brass.
n.	Lever Handles Finish: White solid brass.
o.	Locking: Standard profile cylinder
p.	Locking: Adapter for Small Format Interchangeable Core.
2.	Main Entry Panels for Models with Swing Panels: Manufacturerï¿½s push/pull handle with separate lock set and dead bolt and one-point locking at the top and bottom consisting of locking rods operating by the 180 turn of a flat handle on the inside.
a.	Push-pull handles in a brushed stainless-steel finish
b.	Flat Handle Finish: Brushed satin stainless steel.
c.	Flat Handle Finish: Black titanium stainless steel.
d.	Flat Handle Finish:  Copper-nickel stainless steel antiviral and antimicrobial.
3.	Main Entry Panel: For models with single swing panel attached to side jamb and with surface mounted hinges. No hardware or locking provided by manufacturer; Field installed panic device per Section 08 71 00 - Door Hardware.
4.	Main Entry Panel: For models with paired swing panel attached to side jamb and with surface mounted hinges. No hardware or locking provided by manufacturer; Field installed panic device per Section 08 71 00 - Door Hardware.
5.	Main Entry Pair of Panels on Inswing Models without a Swing Panel: L-shaped handle on inside, flat handle on outside and lock set with profile cylinder.
a.	Operation of Lock Set: By turn of key from outside and with a thumb-turn from inside with a two-point locking hardware operated by 180 degree turn of handle.
b.	L-Shaped Handles: Stainless steel brushed satin finish.
c.	L-Shaped Handles: Stainless steel titanium black finish.
6.	Main Entry Panels for Outswing Models without Swing Panels: Flat handle on inside and a lock set with a profile cylinder on outside.
a.	Operation of Lock Set: By turn of key from the outside and from inside with a two-point locking hardware operated by 180 degree turn of handle.
7.	Main Entry Panels for Models without Swing Panels: Flat handle on inside only with concealed two-point locking hardware operated by 180 degree turn of handle.
8.	Secondary Panels and Pairs of Folding Panels: Handles and concealed one or two-point locking hardware operated by 180 degree turn of handle between each pair. Face applied flush bolt locking not acceptable; except for units with paired panels.
a.	Handles: Manufacturer's flat handles.
1)	Flat Handle Finish: Brushed satin stainless steel.
2)	Flat Handle Finish: Black titanium stainless steel.
3)	Flat Handle Finish: Copper-nickel stainless steel antiviral and antimicrobial. 
4)	Flat Handle Finish: Powder coated aluminum with color finish to match frame.
b.	Handles: Removable custodial handles.
9.	Handle Height: 41-3/8 inch (105 cm) centered from bottom of panel unless otherwise indicated on Drawings.
10.	Locking Rods: End caps top and bottom;. Rod Stroke: 15/16 inch (24 mm).
11.	Additional Profile Cylinders: Keyed alike.
12.	Additional Profile Cylinders: Keyed differently.
H.	Sliding-Folding Hardware: Combination with top and bottom tracks and threshold. Running carriages with sealed, self-lubrication, ball bearing multi-rollers. Surface mounted hinges and running carriages not acceptable.
1.	Each Pair of Folding Panels:
a.	Top-Hung: Independent cardanic suspension for 4 wheeled rollers coated with fiberglass reinforced polyamide upper running carriage and lower guide carriage. Running Carriage: Adjustable height, 1/4 inch (6 mm) up and down.
b.	Floor Supported: Upper guide carriage and lower running carriage, two vertical stainless-steel wheels and two horizontal wheels. Vertical wheels to ride on stainless steel guide track covers over full length of sill track. Lie above water run-off level. Lower Running Carriage Carrying Capacity: 220 lbs. (100 kg)
2.	Corner Connectors: On all four corners of panels. Thermally broken die cast zinc multi-functional corner fittings with carriage connectors and hinges.
a.	Hinge Pins: Standard.
b.	Hinge Pins: Removable.
c.	Finish: Powder coated, closest match to finish of frame and panel.
d.	Adjustment: 1/16 inch (1.5 mm) in width per hinge adjustments without removing panels from tracks and without needing to remove panels from tracks.
I.	Weather Stripping: Manufacturer's double layer EPDM between panels and EPDM gasket and Q-Lon gasket or brush seal between panel and frame or brush seals with two-layer polyamide fin attached to inner and outer edge of door panels with a recessed sill or on frame for sealing between panels and between panel and frame.
1.	UniverSILL: For outswing low profile saddle sill, UniverSILL gasket add on available for additional air and water protection. 
J.	Fasteners: Tapered pins and stainless-steel screws for connecting frame components.
K.	Accessories: Sidelights, transoms, corner posts, or single or double doors as indicated.
2.4	THERMALLY BROKEN ALUMINUM-FRAMED FOLDING GLASS WALL SYSTEMS (SL70)
A.	Basis of Design: Model SL70. Monumental thermally broken aluminum-framed folding glass wall system, floor track supported as manufactured by Nana Wall Systems, Incorporated. Manufacturer's standard or post reinforced frame and panel profiles, with top track, side jambs and panels with dimensions as shown on Drawings.
1.	System Components: Aluminum frame, threshold, panels, sliding-folding and locking hardware, weather stripping, glass and glazing, and accessories as required for a complete working installation.
a.	Insect Screen:  Fully retractable non-pleated screen. Ultra-strong, UV resistant fiberglass mesh housed in single cartridge riding on a single track.
1)	Basis-of-Design Product by Manufacturer:  The Horizon by Wizard Industries, Inc.
B.	Performance Criteria:
1.	Performance Criteria (Lab Tested): Standard Flush Sill; Inward Opening:
a.	Air Infiltration per ASTM E283 Inward Opening:
1)	At static air pressure difference of 1.57 psf (75 Pa): 0.15 cfm per sq ft (0.76 L per sec per sq m).
2)	At 6.24 psf (300 Pa): 0.29 cfm per sq ft (1.47 L per sec per sq m).
b.	Structural Loading per ASTM E330: Inward Opening.
1)	Wind load Resistance: Pass; C4.
a)	Design Pressure Positive and Negative: 70 psf (3350 Pa).
2.	Performance Criteria (Lab Tested): Standard Flush Sill; Outward Opening:
a.	Air Infiltration per ASTM E283: Outward Opening:
1)	At static air pressure difference of 1.57 psf (75 Pa): 0.14 cfm per sq ft (0.71 L per sec per sq m).
2)	At 6.24 psf (300 Pa): 0.30 cfm per sq ft (1.52 L per sec per sq m).
b.	Structural Loading per ASTM E330: Outward Opening.
1)	Wind load Resistance: Pass; C4.
a)	Design Pressure Positive and Negative: 70 psf (3350 Pa).
3.	Performance Criteria (Lab Tested): Low Profile Saddle Sill - Inward Opening.
a.	Air Infiltration per ASTM E283: Inward Opening:
1)	At static air pressure difference of 1.57 psf (75 Pa): 0.15 cfm per sq ft (0.76 L per sec per sq m).
a)	Without Weeps at 6.24 psf (300 Pa): 0.29 cfm per sq ft (1.47 L per sec per sq m).
b.	Water Penetration per ASTM E331 and ASTM E547: No uncontrolled water leakage at a static (with weeps) test pressure of 5.25 psf (250 Pa).
c.	Structural Loading per ASTM E330:
1)	Wind load Resistance: Pass; C4.
a)	Design Pressure Positive and Negative: 70 psf (3350 Pa).
4.	Performance Criteria (Lab Tested): Low Profile Saddle Sill - Outward Opening.
a.	Air Infiltration per ASTM E283: Outward Opening:
1)	At static air pressure difference of 1.57 psf (75 Pa): 0.14 cfm per sq ft (0.71 L per sec per sq m).
a)	Without Weeps at 6.24 psf (300 Pa): 0.30 cfm per sq ft (1.52 L per sec per sq m).
b.	Water Penetration per ASTM E331 and ASTM E547: No uncontrolled water leakage at a static (with weeps) test pressure of 6.00 psf (300 Pa).
c.	Structural Loading per ASTM E330:
1)	Wind load Resistance: Pass; C4.
a)	Design Pressure Positive and Negative: 70 psf (3350 Pa).
5.	Performance Criteria (Lab Tested): Higher Weather Performance Raised Sill - Inward Opening.
a.	Air Infiltration per ASTM E283:
1)	At static air pressure difference of 1.57 psf (75 Pa): 0.16 cfm per sq ft (0.81 L per sec per sq m).
2)	At 6.24 psf (300 Pa): 0.20 cfm per sq ft (1.02 L per sec per sq m).
b.	Water Penetration per ASTM E331 and ASTM E547: No uncontrolled water leakage at a static test pressure of 9 psf (440 Pa).
c.	Dynamic Water Penetration per AAMA 520 and ASTM E2268:
1)	Performance Level 2 at 6 to 18 psf (300 to 860 Pa).
d.	Structural Load Deflection per TAS 202 and ASTM E330: DP-40 and DP-45.
1)	Wind load Resistance: Pass.
a)	Design Pressure Positive: 70 psf (3350 Pa); C4.
b)	Design Pressure Negative: 100 psf (4785 Pa); C3.
6.	Performance Criteria (Lab Tested): Higher Weather Performance Raised Sill - Outward Opening.
a.	Air Infiltration per ASTM E283:
1)	At static air pressure difference of 1.57 psf (75 Pa): 0.02 cfm per sq ft (0.10 L per sec per sq m).
2)	At 6.24 psf (300 Pa): 0.08 cfm per sq ft (0.41 L per sec per sq m).
b.	Water Penetration per ASTM E331 and ASTM E547: No uncontrolled water leakage at a static test pressure of 9 psf (440 Pa).
c.	Dynamic Water Penetration per AAMA 520 and ASTM E2268: Performance Level 1 at 5 to 15 psf (250 to 715 Pa).
d.	Structural Load Deflection per TAS 202 and ASTM E330: DP-40 and DP-45.
1)	Wind load Resistance: Pass.
a)	Design Pressure Positive and Negative: 70 psf (3350 Pa); C3.
7.	Forced Entry per AAMA 1304 and ASTM F842: Meets requirements for plus F1.
8.	Swing Panel - Operation / Cycling Performance per AAMA 920: 500,000 cycles.
9.	System - Life Cycle Performance per DIN EN 1191 and 12400: 20,000 cycles.
10.	Florida Product Approval for Wind Loading: Units tested to AAMA/WDMA/CSA 101/I.S.2/A440 and approved according to the Florida Building Code 2014, Section 1710.5, for panel sizes subject to manufacturer size charts.
a.	Product Approval Number: FL35025. Standard Units with panel size up to 3 ft 2-7/8 inches (94 cm) wide x 9 ft 8-3/4 inches (292 cm) high; subject to manufacturer size chart.
11.	Acoustic Performance per DIN 52210-3,4: STC (Rw)
a.	System STC (Rw) 43 (43) and OITC 35 with 1-1/2 inch (38 mm) double IGU, 10 mm + 8 mm STC 48 laminated glass 
b.	System STC (Rw) 41 (41) and OITC 33 with 1-7/16 inch (36 mm) double IGU, 8 mm laminated and 6 mm tempered STC 43 glass
c.	System STC (Rw) 33 (33) and OITC 27 with 15/16 inch (24 mm) double IGU, 4 mm and 4 mm STC 32 tempered glass
d.	System STC (Rw) 42 (42) with 1-5/16 inch (34 mm) double IGU, 6 mm + 6 mm STC 44 enhanced laminated glass.
e.	System STC (Rw) 41 (41) with 1 inch (25 mm) double IGU, 6 mm + 6 mm STC 42 laminated glass.
f.	System STC (Rw) 38 (38) with 1/2 inch (12 mm) STC 39 enhanced laminated glass.
g.	System STC (Rw) 36 (36) with 1/4 inch (6 mm) STC 36 enhanced laminated glass.
h.	System STC (Rw) 35 (35) with 1/4 inch (6 mm) STC 35 laminated glass.
i.	System STC (Rw) 32 (32) with 1/4 inch (6 mm) STC 31 tempered glass.
12.	Thermal Performance; U-Factor: NFRC 100 rated, certified, and labeled
13.	Solar Heat Gain Coefficient Plus Visible Light Transmission: NFRC 200 rated, certified, and labeled.
14.	Air Leakage: NFRC 400 rated, certified, and labeled.
15.	Condensation Resistance Factor: NFRC 500 rated, certified, and labeled.
16.	EPA Energy Star: Meets requirements with specific glass.
C.	Design Criteria:
1.	Sizes and Configurations: As indicated by the Drawings for selected number and size of panels, location of swing panels, and location of tracks and stacking.
2.	Operation: Sliding and folding hardware with top and bottom tracks.
3.	Mounting Type: Floor track supported.
4.	Panel Configuration: Straight.
5.	Panel Configuration: Segmented curve.
6.	Panel Configuration: 90 degree angle turn.
7.	Panel Configuration: 135 degree angle turn.
8.	Panel Configuration: Window-Door combination
9.	Panel Type: Hinged.
a.	Primary swing panel of paired swing panels, looking from inside: On the left.
b.	Primary swing panel of paired swing panels, looking from inside: On the right.
c.	Entry and Egress panel hinged to side jamb.
10.	Panel Pairing Configuration: See Drawings.
11.	Stack Storage Configuration: Inswing.
12.	Stack Storage Configuration: Outswing.
D.	Fabrication: Extruded aluminum frame and panel profiles, corner connectors, hinges, sliding and folding hardware, locking hardware, handles, glass, glazing, and sound gasketing.
1.	Factory pre-assembled. Ship with system components and installation instructions.
2.	Exposed work matched to produce continuity of line and design with joints.
3.	No raw edges visible at joints.
E.	Materials:
1.	Panels: Single lite; standard.
2.	Panels: Multiple lites with horizontal mullions at specified heights from the bottom of the panel.
3.	Panels: Single lite with simulated divided lites in pattern as shown on Drawings.
4.	Panel Size (W x H): As indicated on Drawings.
5.	Rail Depth: 2-3/4 inch (70 mm).
6.	Top Rail and Stile Width: 2-1/4 inch (57 mm)
7.	Bottom Rail Width: 2-1/4 inches (57 mm)
a.	Manufacturer's standard kickplate. Height (in/mm): ______.
8.	Frame: Matching top track and side jambs.
a.	Top Track and Side Jambs Width: 2-9/16 inch (65 mm).
b.	Top Track and Side Jambs Depth: 3-1/8 inch (80 mm).
9.	Sill Type: Higher weather performance raised sill; thermally broken.
10.	Sill Type: Flush sill; thermally broken.
11.	Sill Type: Low profile saddle sill; thermally broken.
12.	Sill Type: Surface mounted interior sill; not thermally broken for interior application.
13.	Sill Aluminum Finish: Clear anodized finish.
14.	Sill Aluminum Finish: Dark bronze anodized finish.
15.	Sill Aluminum Finish: Finished to match panel only with higher weather performance sill.
16.	For ADA Compliance: Provide gasket to cover the channel in the sill at swing doors.
17.	Aluminum Extrusions: AIMgSi0.5 alloy, 6063-T5; F-22 - European standard.
a.	Thickness: 0.078 inch (2.0 mm) nominal.
b.	Thermal Break: 3/4 to 15/16 inch (20 to 24 mm)wide glass fiber reinforced polyamide plastic. Thinner or poured and de-bridged type thermal breaks not acceptable.
c.	Panel and Frame Finish: One color inside and outside.
1)	Finish Type:  Anodized per AAMA 611. Clear. 
2)	Finish Type:  Anodized per AAMA 611. Dark bronze. 
3)	Finish Type:  Powder coat per AAMA 2604. 
a)	Color: Chosen from standard selection of 50 colors. Matte.
b)	Color: Chosen from full RAL selection. High gloss.
c)	Color: Chosen from full RAL selection. Matte.
4)	Finish Type: PVDF Coat (AAMA 2605): Fluoropolymer Kynar with color to match custom finish.
5)	Finish Type: Custom finish.
d.	Panel and Frame Finish: Different color inside and outside.
1)	Interior: Anodized per AAMA 611. Clear.
2)	Interior: Anodized per AAMA 611. Dark bronze.
3)	Interior: Powder coat per AAMA 2604.
a)	Color: Chosen from standard selection of 50 colors. Matte.
b)	Color: Chosen from full RAL selection. High gloss.
c)	Color: Chosen from full RAL selection. Matte.
4)	Interior: PVDF Coat (AAMA 2605): Fluoropolymer Kynar with color to match custom finish.
5)	Interior: Custom finish.
6)	Exterior: Anodized per AAMA 611. Clear. 
7)	Exterior: Anodized per AAMA 611. Dark bronze. 
8)	Exterior: Powder coat per AAMA 2604. 
a)	Color: Chosen from standard selection of 50 colors. Matte. 
b)	Color: Chosen from full RAL selection. High gloss. 
c)	Color: Chosen from full RAL selection. Matte. 
9)	Exterior: PVDF Coat (AAMA 2605): Fluoropolymer Kynar with color to match custom finish.
10)	Exterior: Custom finish
F.	Glass and Glazing:
1.	Safety Glazing per ASTM C1036, ASTM C1048, ANSI Z97.1 and CPSC 16CFR 1201.
2.	Glazing Units, Single Insulated:  Dry glazed with glass stops on the inside.
a.	Glass Lites: Laminated.
b.	Glass Lites: Tempered.
c.	Thickness: 1/2 inch (12 mm) STC 39 enhanced laminated glass to achieve unit STC of 38
d.	Thickness: 1/4 inch (6 mm) STC 36 enhanced laminated glass to achieve unit STC of 36
e.	Thickness: 1/4 inch (6 mm) STC 35 laminated glass to achieve unit STC of 35. 
f.	Thickness: 1/4 inch (6 mm) STC 31 tempered glass to achieve unit STC of 32. 
3.	Glazing Units, Double Insulated:  Dry glazed with glass stops on the inside.
a.	Glass Lites:  Laminated.
b.	Thickness:  1-5/16 inch (34 mm), 6 mm + 6 mm STC 44 enhanced laminated glass to achieve unit STC of 42.
c.	Thickness:  1 inch (25 mm), 6 mm + 6 mm STC 42 laminated glass to achieve unit STC of 41.
4.	Glazing Units, Triple Insulated:  Dry glazed with glass stops on the inside.
a.	Glass Lites: Tempered. 
b.	Glass Lites: Laminated. 
c.	Glass Lites: Tempered and laminated. 
d.	Thickness: 1-1/2 inch (38 mm) thick.
5.	Insulated Glazing Unit Fill: Air.
6.	Insulated Glazing Unit Fill: Argon.
7.	Glass Type: Standard.
8.	Glass Spacers:  Gray finish with capillary tube.
9.	Glass Spacers: Black finish with capillary tubes. 
10.	Glass Spacers: Gray finish without capillary tubes. 
11.	Glass Spacers: Black finish without capillary tubes.
12.	Insulated Glass Unit Surfaces: Clear. 
13.	Insulated Glass Unit Surfaces: Low-E coating on No. 2 surface of double IGU. 
14.	Insulated Glass Unit Surfaces: Low-E coating on No. 2 surface and No. 4 surface of double IGU. 
15.	Insulated Glass Unit Surfaces: Low-E coating on No. 2 surface and No. 5 surface of triple IGU.
G.	Locking Hardware and Handles:
1.	Main Entry Panels for Models with a Swing Panel or Pair of Swing Panels:
a.	Lever Handles:  On inside and outside.
b.	Lever Handles:  With return on inside and outside.
c.	Standard lockset with lockable latch.
d.	Multi-point locking with concealed dead bolt and rods at top and bottom on primary panel only.
e.	Operation:  After turn of key or thumb-turn, depression of handles withdraws latch. Lifting of handles engages rods and key or thumb turn engages deadbolt and operates lock.
f.	Rods to be concealed and not edge mounted.
g.	Secondary Swing Panel:  Matching dummy lever handles on both sides and concealed flush bolts that operate the rods at the top and the bottom for the secondary swing panel.
h.	Secondary Swing Panel:  Two-point locking with U-shaped handles on inside only for the secondary swing panel.
i.	Lever Handles Finish:  Brushed satin stainless steel; standard.
j.	Lever Handles Finish:  Titanium black stainless steel; standard.
k.	Lever Handles Finish: Copper- nickel stainless steel antiviral and antimicrobial.
l.	Lever Handles Finish:  Oil rubbed bronze solid brass.
m.	Lever Handles Finish: Satin nickel solid brass. 
n.	Lever Handles Finish: White solid brass. 
o.	Locking: Standard profile cylinder. 
p.	Locking: Adapter for Small Format Interchangeable Core.
2.	Main Entry Panel for Models with Swing Panels and Pairs of Swing Panels:  Lever handles on inside and outside with single action, emergency egress, interconnected lock.
3.	Main Entry Panels for Models with a Swing Panel. Push-pull handles with separate lockset and dead bolt and one-point locking at top and bottom consisting of locking rods operated by a 180 degree turn of a flat handle on the inside.
a.	Push-pull handles in a brushed stainless-steel finish.
b.	Flat Handle Finish:  Brushed satin stainless steel.
c.	Flat Handle Finish:  Black titanium stainless steel.
4.	Main Entry Panel for Models with Swing Panels or a Pair of Swing Panels:  No hardware or locking provided by manufacturer; Field installed panic device per Section 08 71 00 - Door Hardware.
5.	Main Entry Pair of Panels Models without a Swing Panel:  L-shaped handle on inside and outside, including a lock set with profile cylinder.
a.	Operation of Lock Set:  By turn of key from outside and with a thumb-turn from inside with a two-point locking hardware operated by 180 degree turn of handle.
b.	L-Shaped Handles: Stainless steel brushed satin finish. 
c.	L-Shaped Handles: Stainless steel titanium black finish.
6.	Main Entry Panel:  U and L-shaped handle on inside only with concealed two-point locking hardware operated by 180 degree turn of handle.
7.	Secondary Panels and Pairs of Folding Panels:  Handles and concealed two-point locking hardware operated by 180 degree turn of handle between each pair. Face applied flush bolt locking not acceptable.
a.	Handles:  Manufacturer's standard.
1)	Handle Finish:  Brushed satin stainless steel.
2)	Handle Finish:  Black titanium stainless steel.
3)	Handle Finish:  Brown nylon.
4)	Handle Finish:  Gray nylon.
5)	Handle Finish:  White nylon.
b.	Handles:  Removable custodial handles.
8.	Handle Height:  41-3/8 inch (105 cm) centered from bottom of panel unless otherwise indicated on Drawings.
9.	Locking Rods:  End caps top and bottom; Rod Stroke:  15/16 inch (24 mm).
10.	Additional Profile Cylinders:  Keyed alike.
11.	Additional Profile Cylinders:  Keyed differently.
H.	Sliding-Folding Hardware:  Combination with top and bottom tracks and threshold. Running carriages with sealed, self-lubrication, ball bearing multi-rollers. Surface mounted hinges and running carriages not acceptable. Weight of panels borne by bottom of guide channel in sill is not acceptable.
1.	Lower Running Carriage Carrying Capacity:  440 lbs. (200 kgs).
2.	Upper guide carriage and lower running carriage provided with four vertical stainless-steel wheels and two horizontal polyamide wheels.
3.	Vertical wheels to ride on top of stainless-steel guide track covers over the full length of the sill track and lie above the water run-off level.
4.	Wheels riding below water run-off level and wheels riding on aluminum surfaces are not acceptable.
5.	Swing Panel Hinges:
a.	Finish:  Zinc die cast with finish closest match to finish of frame and panels and stainless-steel security hinge pins with set-screws, standard.
b.	Finish:  Stainless-steel hinges and security hinge pins with set-screws.
6.	Adjustment:  Folding-sliding hardware capable of compensation and adjustments without needing to remove panels from tracks, in width, 1/16 inch (1.5 mm) per hinge and in height, 5/64 inch (2 mm) up and down.
I.	Weather Stripping:  Manufacturerï¿½s double layer EPDM between panels and EPDM gasket and Q-Lon gasket or brush seal between panel and frame or brush seals with two-layer polyamide fin attached to inner and outer edge of door panels with a recessed sill or on frame for sealing between panels and between panel and frame.
1.	UniverSILL: For outswing low profile saddle sill, UniverSILL gasket add on available for additional air and water protection.
J.	Fasteners:  Tapered pins and stainless-steel screws for connecting frame components.
K.	Accessories:  Sidelights, transoms, corner posts, or single or double doors as indicated.
PART 3    EXECUTION
3.1	EXAMINATION AND PREPARATION
A.	Examine surfaces of openings and verify dimensions. Verify openings are level, plumb, and square, with no unevenness, bowing, or bumps on floor.
1.	Because of large dimensions involved and weight and movement of panels, verify structural integrity of header; maximum deflection with both live and dead loads to be the lesser of L/720 of span or 1/4 inches (6 mm).
2.	Structural support for lateral loads, wind load, and eccentric load when panels are stacked open.
B.	Prepare openings using methods recommended by manufacturer for achieving the best result for the substrate under the project conditions.
1.	If preparation is the responsibility of another installer, notify Architect in writing of deviations from manufacturer's recommended installation tolerances and conditions.
C.	Do not proceed with installation until substrates are prepared using methods recommended by manufacturer and deviations from manufacturer's recommended tolerances are corrected. Commencement of installation constitutes acceptance of conditions.
3.2	INSTALLATION
A.	Install per Drawings, submittals, and manufacturer's installation instructions.
1.	Properly flash, seal and waterproof around perimeter of opening.
2.	Attach anchorage devices in place, level, straight, plumb and square. Install frame in proper elevation, plane and location, and in proper alignment with other work.
3.	When lower track is designed to drain, provide connections to allow for drainage.
4.	Install panels, handles, lockset, screens and other accessories in accordance with manufacturer's recommendations and instructions.
B.	Finishing: Field finish under Division 9; seal and finish promptly after installation and prior to exposure to weather in accordance with manufacturer recommendations.
C.	Insect Screens: Install per manufacturer's recommendations and installation instructions.
3.3	FIELD QUALITY CONTROL
A.	Field Inspection: Coordinate in accordance with appropriate sections in Division 01.
B.	Verify system operates and functions properly. Adjust hardware for proper operation.
C.	Non-Conforming Work: Repair or replace non-conforming work as directed by the Architect; see General and Supplementary Conditions, and Division 01, General Requirements.
D.	Manufacturer's Services: Coordinate manufacturer's services in accordance with appropriate sections in Division 01.
3.4	CLEANING AND PROTECTION
A.	Protect installed products until completion of project. Keep units closed and protect installation against damage from construction activities.
B.	Remove protective coatings. Use manufacturer recommended methods to clean surfaces.

END OF SECTION