SECTION 08 36 13

RESIDENTIAL OVERHEAD DOORS

Display hidden notes to specifier. (Don't know how? Click Here) 
 Copyright 2010 -  2023 ARCAT, Inc. - All rights reserved

PART 1    GENERAL
1.1	SECTION INCLUDES
A.	Residential Metal Overhead Doors.
B.	Residential Glazed Aluminum Overhead Doors.
C.	Residential Wood Overhead Doors.
D.	Residential Fiberglass Overhead Doors.
E.	Residential Vinyl Overhead Doors.
F.	Electric Operators.
1.2	RELATED SECTIONS
A.	Section 03 30 00 - Cast-in-Place Concrete. Execution requirements for placement of anchors in concrete wall construction.
B.	Section 04 22 00.16 - Surface-Bonded Concrete Unit Masonry. Execution requirements for placement of anchors in masonry wall construction.
C.	Section 05 50 00 - Metal Fabrications.
D.	Section 06 10 00 - Rough Carpentry.
E.	Section 07 90 00 - Joint Protection.
F.	Section 08 71 53 - Security Door Hardware.
G.	Section 09 90 00 - Painting and Coating.
H.	Section 27 05 39 - Surface Raceways for Communications Systems.
I.	Section 26 05 00 - Common Work Results for Electrical.
1.3	REFERENCES
A.	ANSI/DASMA 108 - Standard Method for Testing Sectional Garage Doors and Rolling Doors: Determination of Structural Performance Under Uniform Static Air Pressure Difference
B.	UL: Underwriters Laboratories, Inc.
C.	ULC: Underwriters Laboratories of Canada.
1.4	DESIGN / PERFORMANCE REQUIREMENTS
A.	Wind Loads: Design and size components to withstand loads caused by pressure and suction of wind acting normal to plane of wall as calculated in accordance with applicable code.
1.	Design pressure of ________ lb/sq ft (________kPa).
B.	Wiring Connections: Requirements for electrical characteristics.
1.	115 volts, single phase, 60 Hz.
C.	Products Requiring Electrical Connection: Listed and classified by Underwriters Laboratories, Inc. acceptable to authority having jurisdiction as suitable for purpose specified.
D.	Single-Source Responsibility: Provide doors, tracks, motors, and accessories from one manufacturer for each type of door. Provide secondary components from source acceptable to manufacturer of primary components.
1.5	SUBMITTALS
A.	Submit under provisions of Section 01 30 00 - Administrative Requirements.
B.	Product Data: Manufacturer's data sheets on each product to be used, including:
1.	Preparation instructions and recommendations.
2.	Storage and handling requirements and recommendations.
3.	Installation methods.
C.	Shop Drawings: Indicate plans and elevations including opening dimensions and required tolerances, connection details, anchorage spacing, hardware locations, and installation details.
D.	Selection Samples: For each finish product specified, two complete sets of color chips representing manufacturer's full range of available colors and patterns.
E.	Verification Samples: For each finish product specified, two samples, minimum size 6 inches (150 mm) square, representing actual product, color, and patterns.
F.	Manufacturer's Certificates: Certify products meet or exceed specified requirements.
G.	Operation and Maintenance Data.
1.6	QUALITY ASSURANCE
A.	Manufacturer Qualifications: Company specializing in manufacturing products specified in this section with minimum five years documented experience.
B.	Installer Qualifications: Authorized representative of the manufacturer with minimum five years documented experience.
C.	Products Requiring Electrical Connection: Listed and classified by Underwriters Laboratories, Inc. acceptable to authority having jurisdiction as suitable for purpose specified.
1.7	DELIVERY, STORAGE, AND HANDLING
A.	Store products in manufacturer's unopened labeled packaging until ready for installation.
B.	Protect materials from exposure to moisture until ready for installation.
C.	Store materials in a dry, ventilated weathertight location.
D.	Store and dispose of solvent-based materials, and materials used with solvent-based materials, in accordance with requirements of local authorities having jurisdiction.
1.8	WARRANTY
A.	Provide manufacturers product warranty as follows:
1.	Thermacore 290 Series. Warranty: 20 year limited against splitting and cracking, 10 year against delamination of polyurethane foam from steel face and all other components for 1 year.
2.	Thermacore  5745 Series. Warranty: Limited lifetime against splitting and cracking, 10 year against delamination of polyurethane foam from steel face, 2 years against peeling or fading of finish on Product sections with Walnut or Golden Oak wood grain finish, and all other components for 1 year. 
3.	Thermacore 5765 Series. Warranty: Limited lifetime against splitting and cracking, 10 year against delamination of polyurethane foam from steel face, 2 years against peeling or fading of finish on Product sections with Walnut or Golden Oak wood grain finish, and all other components for 1 year. 
4.	Courtyard Collection 7565 Series. Warranty: Limited lifetime against splitting and cracking, 10 year against delamination of polyurethane foam from steel face, 2 years against delamination of the facial molding from the skins of the panel and all other components for 1 year. 
5.	Thermacore 190 Series. Warranty: Limited lifetime against splitting and cracking, 10 year against delamination of polyurethane foam from steel face and all other components for 1 year.
6.	Thermacore 490 Series. Warranty: Limited lifetime against splitting and cracking, 10 year against delamination of polyurethane foam from steel face and all other components for 1 year.
7.	Courtyard Collection 160 Series. Warranty: Limited lifetime against splitting and cracking, 10 year against delamination of polyurethane foam from steel face, 10 years against delamination of the facial molding from the skins of the panel and all other components for 1 year.
8.	Courtyard Collection 370 Series. Warranty: 20 year limited against splitting and cracking, 5 year against delamination of polyurethane foam from steel face and all other components for 1 year.
9.	Carriage House 300 Series. Warranty: Limited lifetime against splitting and cracking, 5 year against delamination of polyurethane foam from steel face and all other components for 1 year.
10.	Traditional Steel Collection 391/399 Series Insulated. Warranty: Limited lifetime against splitting and cracking and all other components for 1 year.
11.	Traditional Steel Collection 180/181/185 Series Insulated. Warranty: 20 year limited against splitting and cracking, 10 year on hinge and track and all other components for 1 year.
12.	Traditional Steel Collection 183/184/186 Series Insulated. Warranty: Limited lifetime against splitting and cracking, 10 year on hinge and track and all other components for 1 year.
13.	Traditional Steel Collection 170/171/175 Series Non-Insulated. Warranty: 15 year limited against splitting and cracking, 10 year on hinge and track and all other components for 1 year.
14.	Traditional Steel Collection 173/174/176 Series Non-Insulated. Warranty: Limited lifetime against splitting and cracking, 10 year on hinge and track and all other components for 1 year.
15.	Impression Collection 980 Series. Warranty: Lifetime on steel backing; 3 years on fiberglass exterior and springs for 1 year.
16.	Durafirm Collection 870 Series Insulated. Warranty: 15 year limited against flaking, chipping, cracking of vinyl skin, 5 year against color fading of the vinyl skin and all other components for 1 year.
17.	Electric Opener: Model 8060. Warranty: Lifetime motor and drive screw; 5 year limited warranty on all other parts; 1 year limited warranty on accessories
18.	Electric Opener: Model 8030. Warranty: Lifetime motor and integrated gearbox; 15 year limited warranty on belt; 5 year limited warranty on chain; 5 year limited warranty on all other parts; 1 year limited warranty on accessories.
19.	Electric Opener: Model 7060. Warranty: Lifetime motor and drive screw; 5 year limited warranty on all other parts; 1 year limited warranty on accessories.
20.	Electric Opener: Model 7030. Warranty: Lifetime motor and integrated gearbox; 15 year limited warranty on belt; 5 year limited warranty on chain; 5 year limited warranty on all other parts; 1 year limited warranty on accessories.
21.	Electric Opener: Model 2029. Warranty: 10 years on motor; 15 years on belt drive rail, 5 years on chain drive rail, 1 year warranty on all other parts.
22.	Electric Opener:  Model 1029. Warranty: 5 years on motor; 15 years on belt drive rail, 5 years on chain drive rail, 1 year warranty on all other parts.
PART 2    PRODUCTS
2.1	MANUFACTURERS
A.	Acceptable Manufacturer: Overhead Doorâ„¢ Brand, which is located at:<BR />2501 S. State Hwy. 121, Suite 200<BR />Lewisville, TX 75067<BR />Toll Free Tel: 800-275-3290<BR />Tel: 469-549-7100<BR />Fax: 972-906-1499<BR />Email: request info (info@overheaddoor.com);Web: https://www.overheaddoor.com 
B.	Substitutions: Not permitted.
C.	Requests for substitutions will be considered in accordance with provisions of Section 01 60 00 - Product Requirements.
2.2	RESIDENTIAL METAL OVERHEAD DOORS
A.	Insulated Steel Sectional Overhead Doors: Thermacore 290 Series Insulated Steel Doors by Overhead Door Corporation.
1.	Door Assembly: Rigid steel fully insulated construction with a metal foam metal sandwich panel. Fabricated with EPDM seals between sections.
a.	Size: As indicated on the Drawings.
b.	Panel Thickness: 1 inch (25 mm) nominal.
c.	Panel Style: Shiplap panels.
1)	Classic Raised Panel (short panel) 297 Series.
2)	Contemporary flush panel 298 Series.
3)	Long panel, 295 Series. 
4)	V5 panel, 296 Series. 
d.	Exterior Steel: .012 inch (.030 mm) nominal, high strength hot dipped galvanized steel with an embossed wood grain texture.
e.	Insulation: CFC-free foamed in place polyurethane.
f.	Thermal Values: R-value of 9.3.
g.	Windload Design: Provide to meet the Design/Performance requirements specified.
h.	Window Design:
1)	Window Location:
a)	Top section.
b)	Second from top section.
2)	Decorative Window Style:
a)	Full Vision (Short panel). 
b)	Full Vision (Long panel). 
c)	Ashton 1 (Short panel).
d)	Ashton 2 (Long panel). 
e)	Cascade 1 (Short panel).
f)	Cascade 2 (Long panel).
g)	Cathedral 1 (Short panel).
h)	Cathedral 2 (Long panel).
i)	Madison 1 (Short panel).
j)	Ruston 1 (Short panel).
k)	Ruston2 (Long panel).
l)	Sherwood 1 (Short panel).
m)	Sherwood 2 (Long panel).
n)	Somerton 2 (Long panel). 
o)	Stockbridge 2 - 3-lite (Long panel). 
p)	Stockford 1 (Short panel).
q)	Stockford 2 (Long panel). 
r)	Stockton 1 - 4-lite (Short panel).
s)	Stockton 2 - 4-lite (Long panel). 
t)	Stockton 2 - 6-lite (Long panel). 
u)	Stockton 2 - 12-lite (Long panel).
v)	Stockton 2 - 8-lite Arch (Long panel). 
w)	Waterton 1 (Short panel).
x)	Waterton 2 (Long panel).
y)	Winston 1 (Short panel). 
z)	Williamsburg 1 - 4 piece (Short panel). 
aa)	Williamsburg 1 - 8 piece (Short panel). 
ab)	Williamsburg 2 - 2 piece (Long panel).
ac)	Williamsburg 2 - 4 piece (Long panel).
ad)	Wynbridge 2 (Long panel).
3)	Glass Type: 
a)	Glass: Clear. 
b)	Glass: Clear Lexan.
c)	Glass: Solar Bronze.
d)	Glass: Tempered.
e)	Glass: Obscure (frosted). 
2.	Finish/Color: Two coat baked-on polyester. Color as follows:
a.	Almond.
b.	Sandstone.
c.	White.
d.	Desert Tan. 
3.	Hardware: Standard hinges.
4.	Lock: 
a.	Interior mounted slide lock.
b.	Optional keyed lock.
5.	Bottom fixture: DASMA 103 red-head fasteners.
6.	Weatherstripping: Co-extruded EPDM bulb-type strip at bottom. 
7.	Track: Provide track as recommended by manufacturer to suit loading required and clearances available.
8.	Standard rollers.
9.	Manual Operation.
10.	Electric Openers.
B.	Insulated Steel Sectional Overhead Doors: Thermacore 190 Series Insulated Steel Doors by Overhead Door Corporation.
1.	Door Assembly: Rigid steel fully insulated construction with a metal foam metal sandwich panel. Fabricated with EPDM seals between sections.
a.	Size: As indicated on the Drawings.
b.	Panel Thickness: 1-3/8 inches (34.93 mm).
c.	Panel Style: Ship lap panels.
1)	Classic Raised Panel (short panel), 194 Series.
2)	Contemporary flush panel, 195 Series.
3)	Long panel, 198 Series. 
4)	V10 panel, 192 Series.
5)	V5 panel, 199 Series. 
d.	Exterior Steel: .012 inch (.030 mm) nominal, high strength hot dipped galvanized steel with an embossed wood grain texture.
e.	Insulation: CFC-free foamed in place polyurethane.
f.	Thermal Values: R-value of 12.76. U-Factor of < 0.37 (exceeds 2015 IECC climate zone requirements for maximum U-Factor of Operable fenestrations, section C402.4).
g.	Air Infiltration: <0.40 (exceeds 2015 IECC Section C402.5.2 for Garage Doors). 
h.	Windload Design: Provide to meet the Design/Performance requirements specified.
i.	Window Design:
1)	Window Location:
a)	Top section.
b)	Second from top section.
2)	Decorative Window Style:
a)	Full Vision (Short panel). 
b)	Full Vision (Long panel). 
c)	Ashton 1 (Short panel).
d)	Ashton 2 (Long panel). 
e)	Cascade 1 (Short panel).
f)	Cascade 2 (Long panel).
g)	Cathedral 1 (Short panel).
h)	Cathedral 2 (Long panel).
i)	Madison 1 (Short panel).
j)	Ruston 1 (Short panel).
k)	Ruston2 (Long panel).
l)	Sherwood 1 (Short panel).
m)	Sherwood 2 (Long panel).
n)	Somerton 2 (Long panel). 
o)	Stockbridge 2 - 3-lite (Long panel). 
p)	Stockbridge 2 - 4-lite (Long panel). 
q)	Stockford 1 (Short panel).
r)	Stockford 2 (Long panel). 
s)	Stockton 1 - 4-lite (Short panel).
t)	Stockton 2 - 4-lite (Long panel). 
u)	Stockton 2 - 6-lite (Long panel). 
v)	Stockton 2 - 8-lite (Long panel).
w)	Stockton 2 - 12-lite (Long panel). 
x)	Stockton 2 - 8-lite Arch (Long panel). 
y)	Waterton 1 (Short panel).
z)	Waterton 2 (Long panel).
aa)	Williamsburg 1 - 4 piece (Short panel).
ab)	Williamsburg 1 - 8 piece (Short panel).
ac)	Williamsburg 2 - 2 piece (Long panel).
ad)	Williamsburg 2  - 4 piece (Long panel). 
ae)	Winston 1 (Short panel). 
af)	Wynbridge 2 (Long panel). 
ag)	Wynbridge 2 4-lite Arch (Long panel). 
3)	Glass Type: 
a)	Glass: Clear. 
b)	Glass: Clear Insulated. 
c)	Glass: Clear Lexan.
d)	Glass: Solar Bronze.
e)	Glass: Tempered.
f)	Glass: Obscure (frosted) Insulated. 
g)	Glass: High velocity impact glass. 
2.	Finish/Color: Two coat baked-on polyester. Color as follows:
a.	Almond.
b.	Brown.
c.	Hunter Green. 
d.	Sandstone.
e.	Terra Bronze.
f.	White.
g.	Desert Tan. 
h.	Walnut Bi-directional.  
i.	Golden Oak Bi-directional.  
j.	Mission Oak Bi-directional.
k.	Black. 
l.	Gray. 
3.	Hardware: Standard hinges.
4.	Lock: 
a.	Interior mounted slide lock.
b.	Optional keyed lock.
5.	Bottom fixture: DASMA 103 red-head fasteners.
6.	Weatherstripping: Co-extruded EPDM bulb-type strip at bottom. 
7.	Track: Provide track as recommended by manufacturer to suit loading required and clearances available.
8.	Standard rollers.
9.	Manual Operation.
10.	Electric Openers. 
C.	Insulated Steel Sectional Overhead Doors: Thermacore 490 Series Insulated Steel Doors by Overhead Door Corporation.
1.	Door Assembly: Rigid steel fully insulated construction with a metal foam metal sandwich panel. Fabricated with EPDM seals between sections.
a.	Size: As indicated on the Drawings.
b.	Panel Thickness: 2 inches (51 mm) nominal.
c.	Panel Style: Ship lap panels.
1)	Classic Raised Panel (short panel), 494 Series.
2)	Contemporary flush panel, 495 Series.
3)	Long panel, 496 Series. 
4)	V5 panel, 497 Series. 
d.	Exterior Steel: .012 inch (.030 mm) nominal, high strength hot dipped galvanized steel with an embossed wood grain texture.
e.	Insulation: CFC-free foamed in place polyurethane.
f.	Thermal Values: R-value of 17.5. U-Factor of < 0.37 (exceeds 2015 IECC climate zone requirements for maximum U-Factor of Operable fenestrations, section C402.4).
g.	Air Infiltration: <0.40 (exceeds 2015 IECC Section C402.5.2 for Garage Doors). 
h.	Windload Design: Provide to meet the Design/Performance requirements specified.
i.	Window Design:
1)	Window Location:
a)	Top section.
b)	Second from top section.
2)	Decorative Window Style:
a)	Full Vision (Short panel). 
b)	Full Vision (Long panel). 
c)	Ashton 1 (Short panel).
d)	Ashton 2 (Long panel). 
e)	Cascade 1 (Short panel).
f)	Cascade 2 (Long panel).
g)	Cathedral 1 (Short panel).
h)	Cathedral 2 (Long panel).
i)	Madison 1 (Short panel).
j)	Ruston 1 (Short panel).
k)	Ruston2 (Long panel).
l)	Sherwood 1 (Short panel).
m)	Sherwood 2 (Long panel).
n)	Somerton 2 (Long panel). 
o)	Stockbridge 2 - 3-lite (Long panel). 
p)	Stockford 1 (Short panel).
q)	Stockford 2 (Long panel). 
r)	Stockton 1 - 4-lite (Short panel).
s)	Stockton 2 - 4-lite (Long panel). 
t)	Stockton 2 - 6-lite (Long panel).
u)	Stockton 2 - 12-lite (Long panel).
v)	Stockton 2 - 8-lite Arch (Long panel). 
w)	Waterton 1 (Short panel).
x)	Waterton 2 (Long panel).
y)	Williamsburg 1 - 4 piece (Short panel).
z)	Williamsburg 1 - 8 piece (Short panel).
aa)	Williamsburg 2 - 2 piece (Long panel).
ab)	Williamsburg 2 - 4 piece (Long panel). 
ac)	Wynbridge 2 (Long panel). 
3)	Glass Type: 
a)	Glass: Clear. 
b)	Glass: Clear Insulated. 
c)	Glass: Clear Lexan.
d)	Glass: Solar Bronze.
e)	Glass: Tempered.
f)	Glass: Obscure (frosted) Insulated. 
2.	Finish/Color: Two coat baked-on polyester. Color as follows:
a.	Almond.
b.	Sandstone.
c.	White.
d.	Brown. 
e.	Desert Tan. 
f.	Black. 
g.	Grey.
3.	Hardware: Standard hinges.
4.	Lock: 
a.	Interior mounted slide lock.
b.	Optional keyed lock.
5.	Bottom fixture: DASMA 103 red-head fasteners.
6.	Weatherstripping: Co-extruded EPDM bulb-type strip at bottom. 
7.	Track: Provide track as recommended by manufacturer to suit loading required and clearances available.
8.	Standard rollers.
9.	Manual Operation.
10.	Electric Openers.
D.	Insulated Steel Sectional Overhead Doors: Impression Steel Collection: 5800 Series Insulated Steel Doors by Overhead Door Corporation. 
1.	Door Assembly: Rigid steel fully insulated construction with a metal foam metal sandwich panel. 
a.	Size/Design: As indicated on the Drawings. 
b.	Panel Thickness:  1-5/8 inches (41.2 mm) nominal. 
c.	Panel Style: Pinch-resistant panels. 
1)	Designs: Model 501 (VRP) 
d.	Exterior Steel: 0.016 inch (0.406 mm) exterior nominal, high strength hot-dipped galvanized with an embossed wood grain texture. 
e.	Insulation: CFC-free foamed in place polyurethane. 
f.	Thermal Values: R-value of 12. 
g.	Windload Design: Provide to meet the Design/Performance requirements specified. 
h.	Window Design: 
1)	Window Location: 
a)	Top section. 
b)	Second from top section. 
c)	Top section and second from top section (maximum of 50% of door sections can be glazed) 
2)	Decorative Window Style: 
a)	Plain Window Long 
b)	Stockbridge (3-Pane) 
c)	Stockbridge (4-Pane) 
d)	Stockton (6-Pane) 
e)	Stockton (8-Pane) 
f)	Plain Window Arched 
g)	Wyndbridge (3-Pane) 
h)	Wyndbridge (4-Pane) 
i)	Somerton (6-Pane) 
j)	Somerton (8-Pane) 
3)	Glass Type: 
a)	Glass: Clear. 
b)	Glass: Clear Insulated. 
c)	Glass: Obscure (frosted). 
d)	Glass: Obscure(frosted) Insulated 
i.	Window Section Configuration for Arched windows (Plain Window Arched, Wyndbridge (both 3 and 4-Pane), and Somerton (both 6 and 8-Pane) 
1)	Single Arch 
2)	Double Arch (available on doors 14'8" -18'2") 
2.	Finish/Color: Two coat baked-on polyester. Trim, window frame, window divides will be the same color as the door. 
a.	Painted finishes: 
1)	White. 
2)	Almond. 
3)	Sandstone. 
4)	Brown. 
3.	Premium Hardware: 
a.	Bean Design Handle. 
b.	Hammered Iron Handle. 
c.	Iron Studs. 
d.	Spade Design Hinge. 
e.	Traditional Hammertone Handle. 
f.	Traditional Hammertone Hinge 
4.	Value Hardware: 
a.	Bean Hinge 16 inch. 
b.	Large Bean Handle. 
c.	Large Spear Handle. 
d.	Small Spear Handle. 
e.	Spear Hinge 16 inch. 
f.	Spear Hinge 18 inch. 
5.	Lock: 
a.	Optional keyed lock. 
6.	Bottom fixture: DASMA 103 red-head fasteners 
7.	Weatherstripping: Co-extruded PVC bulb-type strip at bottom. 
8.	Heavy Duty Track: Provide track as recommended by manufacturer to suit loading required and clearances available. 
9.	Nylon rollers. 
10.	Manual Operation. 
11.	Electric Openers.
E.	Insulated Steel Sectional Overhead Doors: Courtyard Collection 160 Series Insulated Steel Doors by Overhead Door Corporation.
1.	Door Assembly: Rigid steel fully insulated construction with a metal foam metal sandwich panel. Fabricated with EPDM seals between sections.
a.	Size/Design: As indicated on the Drawings.
b.	Panel Thickness: 1-3/8 inches (35 mm) nominal.
c.	Panel Style: Ship lap panels.
1)	Contemporary flush panel 195 Series.
d.	Exterior Steel: .012 inch (0.30 mm) nominal, high strength hot-dipped galvanized with an embossed wood grain texture.
e.	Insulation: CFC-free foamed in place polyurethane.
f.	Thermal Values: R-value of 12.76. U-Factor of < 0.37 (exceeds 2015 IECC climate zone requirements for maximum U-Factor of Operable fenestrations, section C402.4).
g.	Air Infiltration <0.40 (exceeds 2015 IECC Section C402.5.2 for Garage Doors). 
h.	Windload Design: Provide to meet the Design/Performance requirements specified.
i.	Window Design:
1)	Window Location:
a)	Top section.
b)	Second from top section.
2)	Decorative Window Style:
a)	Full Vision (Long panel). 
b)	Stockbridge.
c)	Stockton.
d)	Stockton Arch.
e)	Somerton.
f)	Wynbridge Arch.
3)	Glass Type: 
a)	Glass: Clear. 
b)	Glass: Clear Insulated. 
c)	Glass: Obscure (frosted) Insulated. 
d)	Glass: High velocity impact glass. 
2.	Finish/Color: Two coat baked-on polyester. Color as follows:
a.	Almond.
b.	Brown.
c.	Hunter Green.
d.	Sandstone.
e.	Terra Bronze.
f.	White.
g.	Desert Tan. 
h.	Black. 
i.	Grey.
3.	Premium Hardware:
a.	Bean Design Handle.
b.	Hammered Iron Handle.
c.	Iron Studs.
d.	Spade Design Hinge.
e.	Traditional Hammertone Handle.
f.	Traditional Hammertone Hinge
4.	Value Hardware: 
a.	Bean Hinge 16 inch.
b.	Large Bean Handle.
c.	Large Spear Handle.
d.	Small Spear Handle.
e.	Spear Hinge 16 inch.
f.	Spear Hinge 18 inch.
5.	Lock: 
a.	Interior mounted slide lock.
b.	Optional keyed lock.
6.	Bottom fixture: DASMA 103 red-head fasteners.
7.	Weatherstripping: Co-extruded EPDM bulb-type strip at bottom. 
8.	Heavy Duty Track: Provide track as recommended by manufacturer to suit loading required and clearances available.
9.	Urethane ball bearing rollers.
10.	Manual Operation.
11.	Electric Openers: 
F.	Insulated Steel Sectional Overhead Doors: Thermacore 5745 Series Windstorm Wind Load-Rated Insulated Steel Doors by Overhead Door Corporation. 
1.	Door Assembly: Rigid steel fully insulated construction with a metal foam metal sandwich panel. Fabricated with EPDM seals between sections. 
a.	Size: As indicated on the Drawings. 
b.	Panel Thickness: 1-3/8 inches (34.93 mm). 
c.	Panel Style: Tongue-and-groove panels. 
1)	Classic Raised Panel (short panel), Model 901. 
2)	Contemporary flush panel, Model 905. 
3)	Long panel, Model 902. 
4)	V10 panel, Model 904. 
5)	 V5 panel, Model 903. 
d.	Exterior Steel: .012 inch (.030 mm) nominal, high strength hot dipped galvanized steel with an embossed wood grain texture. 
e.	Insulation: CFC-free foamed in place polyurethane. 
f.	Thermal Values: R-value of 12.12. U-Factor of < 0.37 (exceeds 2015 IECC climate zone requirements for maximum U-Factor of Operable fenestrations, section C402.4). 
g.	Air Infiltration: < 0.40 (meet 2015 IECC Section C402.5.2 for Garage Doors). 
h.	Windload Design: Provide to meet the Design/Performance requirements specified. 
i.	Window Design: 
1)	Window Location: 
a)	Top section. 
b)	Second from top section. 
2)	Decorative Window Style: 
a)	Full Vision (Short panel). 
b)	Full Vision (Long panel). 
c)	Arched Stockton - single design (V10 panel). 
d)	Arched Stockton - double design (V10 panel). 
e)	Arched Stockton - single design (Flush panel). 
f)	Arched Stockton - double design (Flush panel). 
g)	Arched Stockton 4 - single design (V10 panel). 
h)	Arched Stockton 4 - double design (V10 panel). 
i)	Ashton 4 (V10 panel). 
j)	Cascade 1 (Short panel). 
k)	Cascade 2 (Long panel). 
l)	Cascade 3 (V5 panel). 
m)	Cascade 3 (Flush panel). 
n)	Cascade 4 (V10 panel). 
o)	Cathedral 1 (Short panel). 
p)	Cathedral 2 (Long panel). 
q)	Cathedral 4 (V10 panel). 
r)	Prairie 1 (Short panel). 
s)	Prairie 2 (Long panel). 
t)	Ruston 4 (V10 panel). 
u)	Sherwood 1 (Short panel). 
v)	Sherwood 2 (Long panel). 
w)	Sherwood 4 (V10 panel). 
x)	Stockbridge (V5 panel). 
y)	Stockbridge (Flush panel). 
z)	Stockbridge 4 - 3 lite (V10 panel). 
aa)	Stockbridge 4 - 4 lite (V10 panel). 
ab)	Stockford 4 (V10 panel). 
ac)	Stockton 1 (Short panel). 
ad)	Stockton 2 (Long panel). 
ae)	Stockton 3 (V5 panel). 
af)	Stockton 3 (Flush panel). 
ag)	Stockton 4 - 4-lite (V10 panel). 
ah)	Stockton 4 - 6-lite (V10 panel). 
ai)	Stockton 4 - 8-lite (V10 panel). 
aj)	Stockton 4 - 8-lite Arch (V10 panel). 
ak)	Stockton 4 - 12-lite Arch (V10 panel). 
al)	Waterton 1 (Short panel). 
am)	Waterton 2 (Long panel). 
an)	Waterton 3 - (V5 panel). 
ao)	Waterton 3 - (Flush panel). 
ap)	Waterton 4 - (V10 panel). 
aq)	Williamsburg 1 - single or double design (Short panel). 
ar)	Williamsburg 2 - single or double design (Long panel). 
as)	Williamsburg 4 - (V10 panel). 
at)	Williamsburg 4 - 4 piece (V10 panel). 
au)	Wynbridge 4 - single or double design (V10 panel). 
3)	Glass Type: 
a)	Glass: Clear. 
b)	Glass: Clear Insulated. 
c)	Glass: Clear Polycarbonate Impact. 
2.	Finish/Color: Two coat baked-on polyester. Color as follows: 
a.	White. 
b.	Brown. 
c.	Almond. 
d.	Taupe. 
e.	Wood Grain Golden Oak Finish (V5 panel). 
f.	Wood Grain Golden Oak Finish (V10 panel). 
g.	Wood Grain Walnut Finish (V5 panel). 
h.	Wood Grain Walnut Finish (V10 panel). 
i.	Wood Grain Mission Oak Finish (V5 panel). 
j.	Wood Grain Mission Oak Finish (V10 panel). 
k.	Black 
3.	Hardware: Standard hinges. 
4.	Lock: 
a.	Interior mounted slide lock. 
b.	Optional keyed lock. 
5.	Bottom fixture: DASMA 103 red-head fasteners. 
6.	Weatherstripping: Co-extruded EPDM bulb-type strip at bottom. 
7.	Track: Provide track as recommended by manufacturer to suit loading required and clearances available. 
8.	Standard rollers. 
9.	Manual Operation. 
10.	Electric Openers. 
G.	Insulated Steel Sectional Overhead Doors: Thermacore 5765 Series Windstorm Wind Load-Rated Insulated Steel Doors by Overhead Door Corporation. 
1.	Door Assembly: Rigid steel fully insulated construction with a metal foam metal sandwich panel. Fabricated with EPDM seals between sections. 
a.	Size: As indicated on the Drawings. 
b.	Panel Thickness: 2 inches (51 mm) nominal. 
c.	Panel Style: Tongue-and-groove panels. 
1)	Classic Raised Panel (short panel), Model 906. 
2)	Contemporary flush panel, Model 909. 
3)	Long panel, Model 907. 
4)	V5 panel, Model 908. 
d.	Exterior Steel: .012 inch (.030 mm) nominal, high strength hot dipped galvanized steel with an embossed wood grain texture. 
e.	Insulation: CFC-free foamed in place polyurethane. 
f.	Thermal Values: R-value of 16.22. U-Factor of < 0.37 (exceeds 2015 IECC climate zone requirements for maximum U-Factor of Operable fenestrations, section C402.4). 
g.	Air Infiltration: < 0.40 (exceeds 2015 IECC Section C402.5.2 for Garage Doors). 
h.	Windload Design: Provide to meet the Design/Performance requirements specified. 
i.	Window Design: 
1)	Window Location: 
a)	Top section. 
b)	Second from top section. 
2)	Decorative Window Style: 
a)	Full Vision (Short panel). 
b)	Full Vision (Long panel). 
c)	Arched Stockton - single design (Flush panel). 
d)	Arched Stockton - double design (Flush panel). 
e)	Arched Stockton - single design (V5 panel). 
f)	Arched Stockton - double design (V5 panel). 
g)	Cascade 1 (Short panel). 
h)	Cascade 2 (Long panel). 
i)	Cascade 3 (V5 panel). 
j)	Cascade 3 (Flush panel). 
k)	Cathedral 1 (Short panel). 
l)	Cathedral 2 (Long panel). 
m)	Prairie 1 (Short panel). 
n)	Prairie 2 (Long panel). 
o)	Sherwood 1 (Short panel). 
p)	Sherwood 2 (Long panel). 
q)	Stockbridge (V5 panel). 
r)	Stockbridge (Flush panel). 
s)	Stockton 1 (Short panel). 
t)	Stockton 2 (Long panel). 
u)	Stockton 3 (V5 panel). 
v)	Stockton 3 (Flush panel). 
w)	Waterton 1 (Short panel). 
x)	Waterton 2 (Long panel). 
y)	Waterton 3 - (V5 panel). 
z)	Waterton 3 - (Flush panel). 
aa)	Williamsburg 1 - single design (Short panel). 
ab)	Williamsburg 1 - double design (Short panel). 
ac)	Williamsburg 2 - single design (Long panel). 
ad)	Williamsburg 2 - double design (Long panel). 
3)	Glass Type: 
a)	Glass: Clear. 
b)	Glass: Clear Insulated. 
c)	Glass: Clear Polycarbonate Impact. 
2.	Finish/Color: Two coat baked-on polyester. Color as follows: 
a.	White. 
b.	Brown. 
c.	Almond. 
d.	Taupe. 
e.	Wood Grain Golden Oak Finish (V5 panel). 
f.	Wood Grain Walnut Finish (V5 panel). 
g.	Wood Grain Mission Oak Finish (V5 panel). 
h.	Black 
3.	Hardware: Standard hinges. 
4.	Lock: 
a.	Interior mounted slide lock. 
b.	Optional keyed lock. 
5.	Bottom fixture: DASMA 103 red-head fasteners. 
6.	Weatherstripping: Co-extruded EPDM bulb-type strip at bottom. 
7.	Track: Provide track as recommended by manufacturer to suit loading required and clearances available. 
8.	Standard rollers. 
9.	Manual Operation. 
10.	Electric Openers. 
H.	Insulated Steel Sectional Overhead Doors: Courtyard Collection 7565 Series Windstorm Wind Load-Rated Insulated Steel Doors by Overhead Door Corporation. 
1.	Door Assembly: Rigid steel fully insulated construction with a metal foam metal sandwich panel. Fabricated with EPDM seals between sections. 
a.	Size/Design: As indicated on the Drawings. 
b.	Panel Thickness: 1-3/8 inches (35 mm) nominal. 
c.	Panel Style: Tongue-and-groove panels. 
1)	Contemporary flush panel Model 905. 
d.	Exterior Steel: .012 inch (0.30 mm) nominal, high strength hot-dipped galvanized with an embossed wood grain texture. 
e.	Insulation: CFC-free foamed in place polyurethane. 
f.	Thermal Values: R-value of 12.12. U-Factor of < 0.37 (exceeds 2015 IECC climate zone requirements for maximum U-Factor of Operable fenestrations, section C402.4). 
g.	Air Infiltration: < 0.40 (meet 2015 IECC Section C402.5.2 for Garage Doors). 
h.	Windload Design: Provide to meet the Design/Performance requirements specified. 
i.	Window Design: 
1)	Window Location: 
a)	Top section. 
b)	Second from top section. 
2)	Decorative Window Style: 
a)	Full Vision (Long panel). 
b)	Stockbridge. 
c)	Stockton. 
d)	Wyndbridge 
e)	Somerton 
f)	Stockton Arch 
g)	Stockbridge Impact 
h)	Stockton Impact 
i)	Wyndbridge Impact 
j)	Somerton Impact 
k)	Stockton Arch Impact 
3)	Glass Type: 
a)	Glass: Clear Insulated. 
b)	Glass: Clear Polycarbonate Impact. 
2.	Finish/Color: Two coat baked-on polyester. Color as follows: 
a.	White 
b.	Almond 
c.	Brown 
d.	Taupe 
e.	Black 
3.	Overlay Color: 
a.	White 
b.	Match Door Color 
4.	Overlay Material: 
a.	Smooth 
b.	Wood Grain 
5.	Premium Hardware: 
a.	Bean Design Handle. 
b.	Hammered Iron Handle. 
c.	Iron Studs. 
d.	Spade Design Hinge. 
e.	Traditional Hammertone Handle. 
f.	Traditional Hammertone Hinge 
6.	Value Hardware: 
a.	Bean Hinge 16 inch. 
b.	Large Bean Handle. 
c.	Large Spear Handle. 
d.	Small Spear Handle. 
e.	Spear Hinge 16 inch. 
f.	Spear Hinge 18 inch. 
7.	Lock: 
a.	Interior mounted slide lock. 
b.	Optional keyed lock. 
8.	Bottom fixture: DASMA 103 red-head fasteners. 
9.	Weatherstripping: Co-extruded EPDM bulb-type strip at bottom. 
10.	Heavy Duty Track: Provide track as recommended by manufacturer to suit loading required and clearances available. 
11.	Urethane ball bearing rollers. 
12.	Manual Operation. 
13.	Electric Openers:
I.	Insulated Steel Sectional Overhead Doors: Courtyard Collection 370 Series Insulated Steel Doors by Overhead Door Corporation.
1.	Door Assembly: Rigid steel fully insulated construction with a metal foam metal sandwich panel. Fabricated with EPDM seals between sections.
a.	Size/Design: As indicated on the Drawings.
b.	Panel Thickness: 1 inches (25 mm) nominal.
c.	Panel Style: Ship lap panels.
1)	Contemporary Flush Panel 298 Series.
d.	Exterior Steel: .012 inch (0.30 mm) nominal, high strength hot-dipped galvanized with an embossed wood grain texture.
e.	Insulation: CFC-free foamed in place polyurethane.
f.	Thermal Values: R-value of 9.31.
g.	Windload Design: Provide to meet the Design/Performance requirements specified.
h.	Window Design:
1)	Window Location:
a)	Top section.
b)	Second from top section.
2)	Decorative Window Style:
a)	Full Vision (Long panel). 
b)	Stockbridge.
c)	Stockton.
d)	Stockton Arch.
e)	Somerton.
f)	Wynbridge Arch.
3)	Glass Type: 
a)	Glass: Clear.
b)	Glass: Obscure (frosted).
2.	Finish/Color: Two coat baked-on polyester. Trim, window frame, window insert is available in white only.
a.	Almond.
b.	Brown.
c.	Hunter Green.
d.	Sandstone.
e.	Terra Bronze.
f.	White.
g.	Desert Tan. 
3.	Premium Hardware:
a.	Bean Design Handle.
b.	Hammered Iron Handle.
c.	Iron Studs.
d.	Spade Design Hinge.
e.	Traditional Hammertone Handle.
f.	Traditional Hammertone Hinge
4.	Value Hardware: 
a.	Bean Hinge 16 inch.
b.	Large Bean Handle.
c.	Large Spear Handle.
d.	Small Spear Handle.
e.	Spear Hinge 16 inch.
f.	Spear Hinge 18 inch.
5.	Lock: 
a.	Interior mounted slide lock.
b.	Optional keyed lock.
6.	Bottom fixture: DASMA 103 red-head fasteners.
7.	Weatherstripping: Co-extruded EPDM bulb-type strip at bottom. 
8.	Heavy Duty Track: Provide track as recommended by manufacturer to suit loading required and clearances available.
9.	Nylon rollers.
10.	Manual Operation.
11.	Electric Openers. 
J.	Insulated Steel Sectional Overhead Doors: Carriage House 300 Series Insulated Steel Doors by Overhead Door Corporation. 
1.	Door Assembly: Rigid steel fully insulated construction with a metal foam metal sandwich panel.  
a.	Size/Design: As indicated on the Drawings. 
b.	Panel Thickness:  1-1/16 inches (26.6 mm) nominal. 
c.	Panel Style: Pinch-resistant panels. 
d.	Exterior Steel: .016 inch (0.406 mm) exterior nominal, high strength hot-dipped galvanized with an embossed wood grain texture. 
e.	Insulation: CFC-free foamed in place polyurethane. 
f.	Thermal Values: R-value of 10. 
g.	Windload Design: Provide to meet the Design/Performance requirements specified. 
h.	Window Design: 
1)	Window Location: 
a)	Top section. 
b)	Second from top section. 
2)	Decorative Window Style: 
a)	Single Car Door: 
1)	Plain window arch. 
2)	Plain square panel. 
3)	6 window arch. 
4)	6 window square. 
5)	8 window square. 
6)	8 window arch. 
7)	12 window square. 
8)	12 window arch. 
9)	16 window arch. 
10)	16 window square. 
b)	Double Car Door: 
1)	Plain window single 4 panel arch. 
2)	Plain window double two 2 panel arch. 
3)	Plain square panel. 
4)	12 window single arch. 
5)	12 window double arch. 
6)	12 window square. 
7)	16 window single arch. 
8)	16 window double arch. 
9)	16 window square. 
10)	24 window single arch. 
11)	24 window double arch. 
12)	24 window square. 
13)	32 window single arch. 
14)	32 window double arch. 
15)	32 window square. 
3)	Glass Type: 
a)	Glass: Clear. 
b)	Glass: Clear Insulated. 
c)	Glass: Obscure (frosted). 
i.	Decorative Solid Top Section Arched Panels: 
1)	Solid two panel arch over single doors. 
2)	Solid four panel arch over double doors. 
3)	Two solid two panel arches over double doors. 
2.	Finish/Color: Two coat baked-on polyester. Trim, window frame, window insert is available in white only. 
a.	Painted finishes: 
1)	Clay 
2)	Green. 
3)	Gray. 
4)	White. 
5)	Clay/White 
6)	Green/White 
7)	Gray/White 
b.	Stained finishes: 
1)	Mahogany 
2)	Walnut 
3)	Oak 
4)	Green 
5)	Gray 
6)	Clay 
7)	Honduran Mahogany 
8)	Red Oak 
3.	Value Hardware:  
a.	Bean Hinge 16 inch. 
b.	Large Bean Handle. 
c.	Large Spear Handle. 
d.	Small Spear Handle. 
e.	Spear Hinge 16 inch. 
f.	Spear Hinge 18 inch. 
4.	Lock:  
a.	Optional keyed lock. 
5.	Bottom fixture: DASMA 103 tamper proof screw. 
6.	Weatherstripping: Co-extruded PVC bulb-type strip at bottom.  
7.	Heavy Duty Track: Provide track as recommended by manufacturer to suit loading required and clearances available. 
8.	Nylon rollers. 
9.	Manual Operation. 
10.	Electric Openers.
K.	Insulated Steel Sectional Overhead Doors: Traditional Steel Collection 390 Series Insulated Steel Doors by Overhead Door Corporation.
1.	Door Assembly: Rigid steel construction; fully insulated on the inside face with continuous steel backing on the inside face. Fabricated with steel end stiles and tongue and groove sections.
a.	Size: As indicated on the Drawings.
b.	Panel Thickness: 2 inches (51 mm) nominal.
c.	Panel Style: 
1)	Classic Raised Panel (short panel), 391 Series.
2)	Traditional Long Panel, 399 Series.
d.	Exterior Steel: .018 inch (.46 mm), high strength hot-dipped galvanized with an embossed simulated wood grain texture.
e.	Insulation: Polystyrene.
f.	Thermal Values: R-value of 9.83.
g.	Windload Design: Provide to meet the Design/Performance requirements specified.
h.	Window Design:
1)	Window Location:
a)	Top section.
b)	Second from top section.
2)	Decorative Window Style:
a)	Full Vision (Short panel). 
b)	Full Vision (Long panel). 
c)	Ashton 1 (Short panel).
d)	Ashton 2 (Long panel). 
e)	Cascade 1 (Short panel).
f)	Cascade 2 (Long panel).
g)	Cathedral 1 (Short panel).
h)	Cathedral 2 (Long panel).
i)	Madison 1 (Short panel).
j)	Ruston 1 (Short panel).
k)	Ruston2 (Long panel).
l)	Sherwood 1 (Short panel).
m)	Sherwood 2 (Long panel).
n)	Somerton 2 (Long panel). 
o)	Stockbridge 2 (Long panel). 
p)	Stockford 1 (Short panel).
q)	Stockford 2 (Long panel).
r)	Stockton 1 (Short panel).
s)	Stockton 2 -8 Lite Arch (Long panel). 
t)	Stockton 2 -12 Lite (Long panel).
u)	Waterton 1 (Short panel).
v)	Waterton 2 (Long panel).
w)	Williamsburg 2 (Long panel).
x)	Williamsburg 4 (Short panel).
y)	Williamsburg 8 (Short panel).
z)	Wynbridge 2 (Long panel). 
3)	Glass Type: 
a)	Glass: Clear. 
b)	Glass: Clear Insulated (Model 391 only). 
c)	Glass: Clear Lexan.
d)	Glass: Solar Bronze (Model 391 only).
e)	Glass: Tempered.
f)	Glass: Obscure (frosted). 
2.	Finish/Color: Two coat baked-on polyester. Color as follows:
a.	Almond.
b.	Brown.
c.	Sandstone.
d.	White.
3.	Hardware: Standard garage door hardware.
4.	Lock: 
a.	Interior mounted slide lock.
b.	Optional keyed lock.
5.	Bottom fixture: DASMA 103 red-head fasteners.
6.	Weatherstripping: PVC bulb-type strip at bottom. 
7.	Track: Provide track as recommended by manufacturer to suit loading required and clearances available.
8.	Nylon rollers.
9.	Manual Operation.
10.	Electric Openers: 
L.	Insulated Steel Sectional Overhead Doors: Traditional Steel Collection 180/181/185 Series Insulated Steel Doors by Overhead Door Corporation.
1.	Door Assembly: High tensile strength steel construction.
a.	Size: As indicated on the Drawings.
b.	Panel Thickness: 2 inches (51 mm) nominal.
c.	Panel Style: tongue in groove
1)	Short Panel, 180 Series.
2)	Long Panel, 181 Series.
3)	V5 Panel, 185 Series.
d.	Exterior Steel: Residential grade high strength hot-dipped galvanized steel with an embossed simulated wood grain texture. 26 gauge (.0183) nominal. 
e.	Insulation: Polystyrene.
f.	Thermal Values: R-value of 7.4.
g.	Windload Design: Provide to meet the Design/Performance requirements specified.
h.	Window Design:
1)	Window Location:
a)	Top section.
b)	Second from top section.
2)	Decorative Window Style:
a)	Full Vision (Short panel). 
b)	Full Vision (Long panel). 
c)	Ashton 1 (Short panel).
d)	Ashton 2 (Long panel).
e)	Cascade 1 (Short panel).
f)	Cascade 2 (Long panel).
g)	Cathedral 1 (Short panel).
h)	Cathedral 2 (Long panel).
i)	Madison 1 (Short panel).
j)	Madison 2 (Long panel).
k)	Prairie 1 (Short panel). 
l)	Prairie 2 (Long panel). 
m)	Ruston 1 (Short panel).
n)	Ruston 2 (Long panel).
o)	Somerton 2 (2-piece long panel).
p)	Sherwood 1 (2 piece short panel).
q)	Sherwood 2 (Long panel).
r)	Stockbridge (Short panel).
s)	Stockbridge (Long panel).
t)	Stockford 1 (Short panel).
u)	Stockford 2 (Long panel).
v)	Stockton Arch (Long panel).
w)	Stockton 1 (Short panel).
x)	Stockton 2 (4 lite long panel).
y)	Stockton 2 (10 lite long panel).
z)	Waterton 1 (Short panel).
aa)	Waterton 2 (Long panel).
ab)	Williamsburg 2 (Long panel).
ac)	Williamsburg 2 (2-piece long panel).
ad)	Williamsburg 4 (4-piece long panel).
ae)	Williamsburg 4 (4-piece short panel).
af)	Williamsburg 8 (8- piece short panel).
ag)	Winston 2 (2-piece short panel).
ah)	Wynbridge (Long panel).
3)	Glass Type: 
a)	Glass: Clear. 
b)	Glass: Clear Lexan. 
c)	Glass: Tempered. 
d)	Glass: Obscure (frosted). 
e)	Glass: High velocity impact glass. 
i.	Finish/Color: Two coat baked-on polyester. Color as follows:
1)	Almond.
2)	Brown.
3)	Desert Tan.
4)	White.
5)	Taupe.
j.	Hardware: Standard garage door hardware.
k.	Lock: 
1)	Interior mounted slide lock.
2)	Optional keyed lock.
l.	Bottom fixture: DASMA 103 tamper resistant fasteners.
m.	Weatherstripping: Extruded PVC bulb-type strip at bottom. 
n.	Track: Provide track as recommended by manufacturer to suit loading required and clearances available.
o.	Nylon rollers.
p.	Manual Operation.
q.	Electric Openers:
M.	Insulated Steel Sectional Overhead Doors: Traditional Steel Collection 183/184/186 Series Insulated Steel Doors by Overhead Door Corporation.
1.	Door Assembly: High tensile strength steel construction.
a.	Size: As indicated on the Drawings.
b.	Panel Thickness: 2 inches (51 mm) nominal.
c.	Panel Style: tongue in groove.
1)	Short Panel, 183 Series.
2)	Long Panel, 184 Series.
3)	V5 Panel, 186 Series.
d.	Exterior Steel: Residential grade high strength hot-dipped galvanized steel with an embossed simulated wood grain texture. 24 gauge (.0229) nominal. 
e.	Insulation: Polystyrene.
f.	Thermal Values: R-value of 7.4.
g.	Windload Design: Provide to meet the Design/Performance requirements specified.
h.	Window Design:
1)	Window Location:
a)	Top section.
b)	Second from top section.
2)	Decorative Window Style:
a)	Full Vision (Short panel). 
b)	Full Vision (Long panel). 
c)	Ashton 1 (Short panel).
d)	Ashton 2 (Long panel).
e)	Cascade 1 (Short panel).
f)	Cascade 2 (Long panel).
g)	Cathedral 1 (Short panel).
h)	Cathedral 2 (Long panel).
i)	Madison 1 (Short panel).
j)	Madison 2 (Long panel).
k)	Prairie 1 (Short panel). 
l)	Prairie 2 (Long panel). 
m)	Ruston 1 (Short panel).
n)	Ruston 2 (Long panel).
o)	Somerton 2 (2-piece long panel).
p)	Sherwood 1 (2 piece short panel).
q)	Sherwood 2 (Long panel).
r)	Stockbridge (Short panel).
s)	Stockbridge (Long panel).
t)	Stockford 1 (Short panel).
u)	Stockford 2 (Long panel).
v)	Stockton Arch (Long panel).
w)	Stockton 1 (Short panel).
x)	Stockton 2 (4 lite long panel).
y)	Stockton 2 (10 lite long panel).
z)	Waterton 1 (Short panel).
aa)	Waterton 2 (Long panel).
ab)	Williamsburg 2 (Long panel).
ac)	Williamsburg 2 (2-piece long panel).
ad)	Williamsburg 4 (4-piece long panel).
ae)	Williamsburg 4 (4-piece short panel).
af)	Williamsburg 8 (8- piece short panel).
ag)	Winston 2 (2-piece short panel).
ah)	Wynbridge (Long panel).
3)	Glass Type:
a)	Glass: Clear.
b)	Glass: Clear Lexan.
c)	Glass: Tempered. 
d)	Glass: Obscure (frosted). 
e)	Glass: High velocity impact glass. 
i.	Finish/Color: Two coat baked-on polyester. Color as follows:
1)	Almond.
2)	Brown.
3)	Desert Tan.
4)	White.
5)	Taupe.
j.	Hardware: Standard garage door hardware.
k.	Lock: 
1)	Interior mounted slide lock.
2)	Optional keyed lock.
l.	Bottom fixture: DASMA 103 tamper resistant fasteners.
m.	Weatherstripping: Extruded PVC bulb-type strip at bottom. 
n.	Track: Provide track as recommended by manufacturer to suit loading required and clearances available.
o.	Nylon rollers.
p.	Manual Operation.
q.	Electric Openers.
N.	Non-Insulated Steel Sectional Overhead Doors: Traditional Steel Collection 170/171/177 Series Non-Insulated Steel Doors by Overhead Door Corporation.
1.	Door Assembly: High tensile strength steel construction.
a.	Size: As indicated on the Drawings.
b.	Panel Thickness: 2 inches (51 mm) nominal.
c.	Panel Style: tongue in groove
1)	Short Panel, 170 Series.
2)	Long Panel, 171 Series.
3)	V5 Panel, 175 Series.
d.	Exterior Steel: Residential grade high strength hot-dipped galvanized steel with an embossed simulated wood grain texture. 26 gauge (.0183) nominal. 
e.	Windload Design: Provide to meet the Design/Performance requirements specified.
f.	Window Design:
1)	Window Location:
a)	Top section.
b)	Second from top section.
2)	Decorative Window Style:
a)	Full Vision (Short panel). 
b)	Full Vision (Long panel). 
c)	Ashton 1 (Short panel).
d)	Ashton 2 (Long panel).
e)	Cascade 1 (Short panel).
f)	Cascade 2 (Long panel).
g)	Cathedral 1 (Short panel).
h)	Cathedral 2 (Long panel).
i)	Madison 1 (Short panel).
j)	Madison 2 (Long panel).
k)	Prairie 1 (Short panel). 
l)	Prairie 2 (Long panel). 
m)	Ruston 1 (Short panel).
n)	Ruston 2 (Long panel).
o)	Somerton 2 (2-piece long panel).
p)	Sherwood 1 (2 piece short panel).
q)	Sherwood 2 (Long panel).
r)	Stockbridge (Short panel).
s)	Stockbridge (Long panel).
t)	Stockford 1 (Short panel).
u)	Stockford 2 (Long panel).
v)	Stockton Arch (Long panel).
w)	Stockton 1 (Short panel).
x)	Stockton 2 (4 lite long panel).
y)	Stockton 2 (10 lite long panel).
z)	Waterton 1 (Short panel).
aa)	Waterton 2 (Long panel).
ab)	Williamsburg 2 (Long panel).
ac)	Williamsburg 2 (2-piece long panel).
ad)	Williamsburg 4 (4-piece long panel).
ae)	Williamsburg 4 (4-piece short panel).
af)	Williamsburg 8 (8- piece short panel).
ag)	Winston 2 (2-piece short panel).
ah)	Wynbridge (Long panel).
3)	Glass Type:
a)	Glass: Clear.
b)	Glass: Clear Lexan.
c)	Glass: Tempered.
d)	Glass: Obscure (frosted).
e)	Glass: High velocity impact glass. 
g.	Finish/Color: Two coat baked-on polyester. Color as follows:
1)	Almond.
2)	Brown.
3)	Desert Tan.
4)	White.
5)	Taupe.
h.	Hardware: Standard garage door hardware.
i.	Lock: 
1)	Interior mounted slide lock.
2)	Optional keyed lock.
j.	Bottom fixture - DASMA 103 tamper resistant fasteners.
k.	Weatherstripping: Extruded PVC bulb-type strip at bottom. 
l.	Track: Provide track as recommended by manufacturer to suit loading required and clearances available.
m.	Nylon rollers.
n.	Manual Operation.
o.	Electric Openers.
O.	Non-Insulated Steel Sectional Overhead Doors: Traditional Steel Collection 173/174/176 Series Non-Insulated Steel Doors by Overhead Door Corporation.
1.	Door Assembly: High tensile strength steel construction.
a.	Size: As indicated on the Drawings.
b.	Panel Thickness: 2 inches (51 mm) nominal.
c.	Panel Style: tongue in groove
1)	Short Panel, 173 Series.
2)	Long Panel, 174 Series.
3)	V5 Panel, 176 Series.
d.	Exterior Steel: Residential grade high strength hot-dipped galvanized steel with an embossed simulated wood grain texture. 24 gauge (.0229) nominal.
e.	Windload Design: Provide to meet the Design/Performance requirements specified.
f.	Window Design:
1)	Window Location:
a)	Top section.
b)	Second from top section.
2)	Decorative Window Style:
a)	Full Vision (Short panel). 
b)	Full Vision (Long panel). 
c)	Ashton 1 (Short panel).
d)	Ashton 2 (Long panel).
e)	Cascade 1 (Short panel).
f)	Cascade 2 (Long panel).
g)	Cathedral 1 (Short panel).
h)	Cathedral 2 (Long panel).
i)	Madison 1 (Short panel).
j)	Madison 2 (Long panel).
k)	Prairie 1 (Short panel). 
l)	Prairie 2 (Long panel). 
m)	Ruston 1 (Short panel).
n)	Ruston 2 (Long panel).
o)	Somerton 2 (2-piece long panel).
p)	Sherwood 1 (2 piece short panel).
q)	Sherwood 2 (Long panel).
r)	Stockbridge (Short panel).
s)	Stockbridge (Long panel).
t)	Stockford 1 (Short panel).
u)	Stockford 2 (Long panel).
v)	Stockton Arch (Long panel).
w)	Stockton 1 (Short panel).
x)	Stockton 2 (4 lite long panel).
y)	Stockton 2 (10 lite long panel).
z)	Waterton 1 (Short panel).
aa)	Waterton 2 (Long panel).
ab)	Williamsburg 2 (Long panel).
ac)	Williamsburg 2 (2-piece long panel).
ad)	Williamsburg 4 (4-piece long panel).
ae)	Williamsburg 4 (4-piece short panel).
af)	Williamsburg 8 (8- piece short panel).
ag)	Winston 2 (2-piece short panel).
ah)	Wynbridge (Long panel).
3)	Glass Type:
a)	Glass: Clear.
b)	Glass: Clear Lexan.
c)	Glass: Tempered.
d)	Glass: Obscure (frosted).
e)	Glass: High velocity impact glass. 
g.	Finish/Color: Two coat baked-on polyester. Color as follows:
1)	Almond.
2)	Brown.
3)	Desert Tan.
4)	White.
5)	Taupe.
h.	Hardware: Standard garage door hardware.
i.	Lock: 
1)	Interior mounted slide lock.
2)	Optional keyed lock.
j.	Bottom fixture - DASMA 103 tamper resistant fasteners.
k.	Weatherstripping: Extruded PVC bulb-type strip at bottom. 
l.	Track: Provide track as recommended by manufacturer to suit loading required and clearances available.
m.	Nylon rollers.
2.	Manual Operation.
3.	Electric Openers.
2.3	RESIDENTIAL GLAZED ALUMINUM OVERHEAD DOORS
A.	Glazed Aluminum Overhead Doors: 511 Series Aluminum Doors by Overhead Door Corporation. Units shall have the following characteristics:
1.	Door Assembly: Stile and rail assembly secured with 1/4 inch (6 mm) diameter through rods.
a.	Size: As indicated on the Drawings.
b.	Panel Thickness: 1-3/4 inches (44 mm).
c.	Center Stile Width: 21/32 inch (17 mm).
d.	End Stile Width: 2-3/4 inches (70 mm).
e.	Intermediate Rail Pair Width: 1-3/8 inches (35 mm).
f.	Top Rail Width:
1)	2-3/8 inches (60 mm).
2)	3-3/4 inches (95 mm).
g.	Bottom Rail Width:
1)	2-3/8 inches (60 mm).
2)	3-3/4 inches (95 mm).
3)	4-1/2 inches (114 mm).
h.	Aluminum Panels: 0.050 inch (1.3 mm) thick, aluminum.
i.	Stiles and Rails: 6063 - T6 aluminum.
j.	Springs: 10,000 cycles.
k.	Glazing:
1)	1/8 inch (3 mm) Acrylic glazing.
2)	1/4 inch (6 mm) Acrylic glazing.
3)	1/8 inch (3 mm) Clear Lexan glazing.
4)	1/4 inch (6 mm) Clear Lexan glazing.
5)	1/2 inch (12.5 mm) Clear Lexan Insulated glazing. 
6)	1/8 inch (3 mm) Tempered glass.
7)	1/4 inch (6 mm) Tempered glass.
8)	1/2 inch (12.5 mm) Tempered Insulating Glass.
9)	1/4 inch (6 mm) Wire glass. 
10)	1/8 inch (3 mm) Double Strength Glass.
11)	1/2 inch (12.5 mm) Double Strength Insulating Glass. 
12)	1/8 inch (3 mm) Low E glazing. 
13)	1/4 inch (6 mm) Low E glazing. 
14)	1/2 inch (12.5 mm) Low E Insulated glazing. 
15)	1/8 inch (3 mm) Solar Bronze glazing. 
16)	1/4 inch (6 mm) Solar Bronze glazing. 
17)	1/2 inch (12.5 mm) Solar Bronze Insulated glazing. 
18)	1/8 inch (3 mm) Obscure glazing. 
19)	1/4 inch (6 mm) Obscure glazing. 
20)	1/2 inch (12.5 mm) Obscure Insulated glazing. 
21)	1/4 inch (6 mm) Twin-Wall Polycarbonate (clear, bronze, white). 
22)	3/8 inch (9.5 mm) Twin-Wall Polycarbonate (clear, bronze, white). 
23)	5/8 inch (15.87 mm) Triple-Wall Polycarbonate (clear, bronze, white).
2.	Finish/Color:
a.	Anodized Finish: Clear anodized.
b.	Anodized Finish: Bronze anodized.
c.	Powder Coating Finish: Color as selected by Architect from manufacturer's standard colors.
3.	Hardware: Galvanized steel hinges and fixtures. 
4.	Lock: Interior galvanized single unit.
5.	Weatherstripping: Flexible bulb-type strip at bottom section.
6.	Track: Provide track as recommended by manufacturer to suit loading required and clearances available. 
7.	Ball bearing rollers with hardened steel races.
8.	Manual Operation.
9.	Electric Openers:
B.	Glazed Aluminum Overhead Doors: 521 Series Aluminum Doors by Overhead Door Corporation.
1.	Door Assembly: Stile and rail assembly secured with 1/4 inch (6 mm) diameter through rods.
a.	Size: As indicated on the Drawings.
b.	Panel Thickness: 1-3/4 inches (44 mm).
c.	Windload Design: Provide to meet the Design/Performance requirements specified.
d.	Center Stile Width: 2-11/16 inches (68 mm).
e.	End Stile Width: 3-5/16 inches (84 mm).
f.	Intermediate Rail Pair Width: 3-11/16 inches (94 mm).
g.	Top Rail Width:
1)	2-3/8 inches (60 mm).
2)	3-3/4 inches (95 mm).
h.	Bottom Rail Width:
1)	3-3/4 inches (95 mm).
2)	4-1/2 inches (114 mm).
i.	Aluminum Panels: 0.050 inch (1.3 mm) thick, aluminum.
j.	Stiles and Rails: 6063 - T6 aluminum.
k.	Springs: 10,000 cycles.
l.	Glazing:
1)	1/8 inch (3 mm) Acrylic glazing.
2)	1/4 inch (6 mm) Acrylic glazing.
3)	1/8 inch (3 mm) Clear Lexan glazing.
4)	1/4 inch (6 mm) Clear Lexan glazing.
5)	1/2 inch (12.5 mm) Clear Lexan Insulated glazing. 
6)	1/8 inch (3 mm) Tempered glass.
7)	1/4 inch (6 mm) Tempered glass.
8)	1/2 inch (12.5 mm) Tempered Insulating Glass.
9)	1/4 inch (6 mm) Wire glass. 
10)	1/8 inch (3 mm) Double Strength Glass.
11)	1/2 inch (12.5 mm) Double Strength Insulating Glass.
12)	1/8 inch (3 mm) Low E glazing. 
13)	1/4 inch (6 mm) Low E glazing. 
14)	1/2 inch (12.5 mm) Low E Insulated glazing. 
15)	1/8 inch (3 mm) Solar Bronze glazing. 
16)	1/4 inch (6 mm) Solar Bronze glazing. 
17)	1/2 inch (12.5 mm) Solar Bronze Insulated glazing. 
18)	1/8 inch (3 mm) Obscure glazing. 
19)	1/4 inch (6 mm) Obscure glazing. 
20)	1/2 inch (12.5 mm) Obscure Insulated glazing. 
21)	1/4 inch (6 mm) Twin-Wall Polycarbonate (clear, bronze, white). 
22)	3/8 inch (9.5 mm) Twin-Wall Polycarbonate (clear, bronze, white). 
23)	5/8 inch (15.87 mm) Triple-Wall Polycarbonate (clear, bronze, white).
2.	Finish/Color:
a.	Anodized Finish: Clear anodized.
b.	Anodized Finish: Bronze anodized.
c.	Powder Coating Finish: Color as selected by Architect from manufacturer's standard colors.
3.	Hardware: Galvanized steel hinges and fixtures. 
4.	Lock: Interior galvanized single unit.
5.	Weatherstripping: 
a.	Flexible bulb-type strip at bottom section.
b.	Joint seal between sections available for additional weather resistance.
6.	Track: Provide track as recommended by manufacturer to suit loading required and clearances available.
7.	Ball bearing rollers with hardened steel races.
8.	Manual Operation.
9.	Electric Openers:
C.	Glazed Aluminum Overhead Doors: Envy 956 Series Aluminum Doors by Overhead Door Corporation. 
1.	Door Assembly: Stile and rail assembly of aluminum alloy 6063-T6, 1-3/8 inch thick stiles and rails, 1/4" tempered glass 
a.	Rails: Top and bottom rails with 3-1/2 inches wide, lower intermediate rail 1-3/8 inches, upper rail 1-5/8 inches, minimum wall thickness 0.062 inch, bottom and lower intermediate rails with glass ledge 
b.	Stiles: Top, bottom, and end stiles are 3-1/2 inches wide, center stile 3 inches wide, minimum wall thickness 0.062 inch. 
c.	Springs: 
1)	Standard cycle spring: 10,000 cycles. 
2)	High cycle spring: 25,000 cycles. 
3)	High cycle spring: 50,000 cycles. 
4)	High cycle spring: 75,000 cycles. 
5)	High cycle spring: 100,000 cycles. 
d.	Glazing: 
1)	1/4 inch (6 mm) White Opaque Tempered glass 
2)	1/4 inch (6 mm) Black Opaque Tempered glass 
3)	1/4 inch (6 mm) Mirrored Gray Tempered glass 
4)	1/4 inch (6 mm) Mirrored Bronze Tempered glass 
5)	1/4 inch (6 mm) Translucent Black Tempered glass 
e.	Finish and Color: 
1)	Anodized Finish: Black anodized 
2)	Anodized Finish: Bronze anodized 
3)	Powder Coating Finish: White powder coat 
4)	Powder Coating Finish: Black powder coat 
5)	Powder Coating Finish: Bronze powder coat 
f.	Hardware: Black and white powder coated steel hinges and fixtures. Ball bearing rollers with hardened steel races. 
g.	Lock: 
1)	Interior mounted slide lock. 
2)	Interior mounted slide lock with interlock switch for automatic operator. 
h.	Weatherstripping: 
1)	Flexible bulb-type strip at bottom section. 
2)	Flexible Jamb seals. 
3)	Flexible Header seal. 
i.	Track: Provide track as recommended by manufacturer to suit loading required and clearances available. 
j.	Ball bearing rollers with hardened steel races. 
k.	Manual Operation. 
l.	Electric Openers:
2.4	RESIDENTIAL WOOD OVERHEAD DOORS
A.	Insulated Wood Sectional Overhead Doors: Traditional Wood Collection Flush Series Insulated Wood Doors by Overhead Door Corporation. 
1.	Door Assembly: Two sided smooth flush wood panels with insulated core on Hemlock frame. Finger jointed rails and stiles frame construction. 
a.	Size: As indicated on the Drawings. 
b.	Panel Thickness: 1-3/8 inches (34.93 mm). 
c.	Panel Style: Shiplap flush panels. 
d.	Model 444
1)	Exterior: Smooth plywood
2)	Interior: Smooth plywood
3)	Interior: Primed smooth hardboard
e.	Insulation: Full cavity expanded polystyrene. 
f.	Thermal Value: R-value of 4.75. 
g.	Window Design: 
1)	Window Location: Top section. 
2)	Glass: 1/8 inch (3 mm) SSB clear glass. 
2.	Finish/Color:  
a.	Paint grade, factory primed white. Sanding is required prior to topcoat. 
b.	Stain grade factory sealed. Sanding is required prior to topcoat. 
3.	Hardware: 14-gauge hinges. Sections through drilled on ends. 
4.	Springs: torsion springs. 
a.	10,000 cycle. 
b.	25,000 cycle. 
c.	50,000 cycle. 
5.	Lock: Interior mounted slide lock. 
6.	Weatherstripping: Co-extruded PVC bulb-type strip at bottom.  
7.	Track: Provide track as recommended by manufacturer to suit loading required and clearances available. 
8.	Rollers:  
a.	10-ball steel. 
b.	Ball Bearing, Nylon coated. 
9.	Manual Operation. 
10.	Electric Openers.  
B.	Wood Sectional Overhead Doors: Traditional Wood Collection Rail and Stile Series Wood Doors by Overhead Door Corporation. 
1.	Door Assembly: 
a.	Size: As indicated on the Drawings. 
b.	Panel Thickness: 1-3/8 inches (34.93 mm). 
c.	Panel Style: Shiplap panels. 
1)	Model 450
a)	Framed Panel offering thin rail and stiles
b)	Rails and stiles are constructed of high quality West Coast Hemlock
c)	Paint Grade
2)	Model 453
a)	Framed Panel offering thick rail and stiles
b)	Rails and stiles are constructed of high quality West Coast Hemlock
c)	Paint Grade
3)	Model 454
a)	Raised Panel Rail and Stiles
b)	Features hemlock panels (finger-jointed), or (solid, one piece) rail and stiles options
c)	Hardboard raised panel (standard); Meranti Mahogany and Cedar panel options available
d)	Paint Grade
e)	Stain Grade
d.	Trim: V-grooved double center stile trim. 
e.	Window Design: 
1)	Window Location:  
a)	Top section. 
b)	Intermediate Section. 
2)	Glass: 1/8 inch (3 mm) SSB clear glass. 
2.	Finish/Color:  
a.	Paint grade, factory primed white. Sanding is required prior to topcoat. 
b.	Stain grade factory sealed. Sanding is required prior to topcoat. 
3.	Hardware: 14-gauge hinges. Four lift handles. 
4.	Springs: torsion springs. 
a.	10,000 cycle. 
b.	25,000 cycle. 
c.	50,000 cycle. 
5.	Lock: Interior mounted slide lock. 
6.	Weatherstripping: Co-extruded PVC bulb-type strip at bottom.  
7.	Track: Provide track as recommended by manufacturer to suit loading required and clearances available. 
8.	Rollers:  
a.	10-ball steel. 
b.	Ball Bearing, Nylon coated. 
9.	Manual Operation. 
10.	Electric Openers.
C.	Wood Sectional Overhead Doors: Signature Carriage Collection 570 Series Wood Doors by Overhead Door Corporation.
1.	Door Assembly: Wood door with panel inserts with finger jointed rail and stiles frame construction.
a.	Size: As indicated on the Drawings.
b.	Panel Thickness: 1-3/8 inches (34.93 mm).
c.	Panel Style: Ship lap panels.
d.	Panel Detail: Medium density overlay smooth plywood panels with square top section solid.
1)	Interior: 1/4 inch (6 mm) smooth Mahogany plywood
2)	Exterior:
a)	3/8 inch smooth medium density overlay plywood.
b)	3/8 inch smooth Mahogany plywood.
c)	3/8 inch grooved medium density overlay plywood, 6-3/8 inches (162 mm) on center).
e.	Trim Options:
1)	Vertical trim overlay 2 inch (specify number of panels).
2)	Single Buck (Diagonal In).
3)	Double Cross Bucks.
f.	Insulation: 
1)	Full cavity expanded polystyrene.
2)	Thermal Values: R-value of 4.75.
g.	Windload Design: Provide to meet the Design/Performance requirements specified.
h.	Window Design:
1)	Window Location: Top section.
2)	Glass: 
a)	1/8 inch (3 mm) DSB clear glass.
b)	1/8 inch (3 mm) Plexiglass.
c)	1/8 inch (3 mm) Gray tint.
d)	1/8 inch (3 mm) Bronze tint.
e)	1/8 inch (3 mm) Antique art (semi-obscure).
2.	Finish/Color: Paint grade, factory primed white. Sanding is required prior to top coat. 
3.	Rail and Stile Finish: finger jointed, 1-3/8 inches (34.93 mm) thick.
a.	Paint grade.
b.	Stain grade Hemlock or Cedar.
4.	Hardware: 14-gauge hinges.
5.	Springs: torsion springs.
a.	10,000 cycle.
b.	25,000 cycle.
c.	50,000 cycle.
6.	Lock: Interior mounted slide lock.
7.	Weatherstripping: Co-extruded PVC bulb-type strip at bottom. 
8.	Track: Provide track as recommended by manufacturer to suit loading required and clearances available.
9.	Rollers: ball bearing nylon-coated.
10.	Manual Operation.
11.	Electric Openers. 
D.	Wood Sectional Overhead Doors: Signature Carriage Collection 571 Series Wood Doors by Overhead Door Corporation.
1.	Door Assembly: Wood door with panel inserts with finger jointed Hemlock rail and stiles frame construction.
a.	Size: As indicated on the Drawings.
b.	Panel Thickness: 1-3/8 inches (34.93 mm).
c.	Panel Style: Ship lap panels.
1)	Edge glued Hemlock raised panels with 1/4 inch (6 mm) Luan Mahogany Plywood Interior (4 panel design).
2)	Edge glued cedar raised panels with 1/4 inch (6 mm) Luan Mahogany Plywood Interior (4 panel design).
3)	Prime paint over stain grade (complete door); Paint grade, factory primed white. Sanding is required prior to top coat.
d.	Insulation: 
1)	Full cavity expanded polystyrene. 
2)	Thermal Values: R-value of 4.75.
e.	Windload Design: Provide to meet the Design/Performance requirements specified.
f.	Window Design:
1)	Window Location: Top section.
2)	Glass: 
a)	1/8 inch (3 mm) DSB clear glass.
b)	1/8 inch (3 mm) Plexiglass.
c)	1/8 inch (3 mm) Gray tint.
d)	1/8 inch (3 mm) Bronze tint.
e)	1/8 inch (3 mm) Antique art (semi-obscure). 
2.	Rail and Stile Finish: finger jointed, 1-3/8 inches (34.93 mm) thick.
a.	Stain grade Hemlock.
b.	Stain grade Clear Cedar.
c.	Wire brush.
3.	Hardware: 14-gauge hinges.
4.	Springs: torsion springs.
a.	10,000 cycle.
b.	25,000 cycle.
c.	50,000 cycle.
5.	Lock: Interior mounted slide lock.
6.	Weatherstripping: Co-extruded PVC bulb-type strip at bottom. 
7.	Track: Provide track as recommended by manufacturer to suit loading required and clearances available.
8.	Rollers: ball bearing nylon-coated.
9.	Manual Operation.
10.	Electric Openers.
E.	Insulated Wood Sectional Overhead Doors: Signature Carriage Collection 580 Series Insulated Wood Doors by Overhead Door Corporation.
1.	Door Assembly: Two sided smooth flush wood panels with insulated core with 1/2 inch (12.5 mm) smooth Extira overlays. 1-1/8 inch (28.57 mm) finger jointed rail and stile frame construction.
a.	Size: As indicated on the Drawings.
b.	Panel Thickness: Overall section thickness will vary depending on the exterior face and overlay material specified.
c.	Panel Style: Ship lap panels.
d.	Panel Detail: Medium density overlay smooth plywood panels with square top section solid. 
1)	Interior: 1/4 inch (6 mm) smooth Mahogany plywood
2)	Exterior and Trim Options:
a)	3/8 inch (9.5 mm) smooth medium density overlay face material, 1/4 inch (6 mm) Mahogany plywood interior, with 1/2 inch (12.5 mm) smooth Extira overlays.
b)	T1-11 plywood (4 inch or 8 inch on center) with Western Red Cedar Clear Trim.
c)	3/8 inch (9.5 mm) textured Mahogany plywood with Western Red Cedar Clear Trim.
d)	3/8 inch (9.5 mm) smooth Mahogany plywood with Western Red Cedar Clear Trim.
e)	1/2 inch (12.5 mm) smooth Marine Mahogany with Western Red Cedar Clear Trim.
f)	Western Red Cedar Clear, Tongue and Groove)with Western Red Cedar Clear Trim.
g)	Hemlock (Tongue and Groove) Exterior with Hemlock Trim.
h)	African Mahogany, Tongue and Groove Exterior with African Mahogany Trim.
i)	Color match Exterior and Overlay Material, Tongue and Groove.
3)	Trim Design Elements:
a)	Vertical trim overlay 4 inch (101 mm) (specify number of panels, up to 5).
b)	Single buck (diagonal in).
c)	Double cross bucks.
d)	Watertable.
4)	Panel Treatments: Wire brush texturing.
2.	Insulation: Full cavity expanded polystyrene.
3.	Thermal Values: R-value of 4.75.
4.	Windload Design: Provide to meet the Design/Performance requirements specified.
5.	Window Design:
a.	Window Location: Top section.
b.	Glass: 
1)	1/8 inch (3 mm) DSB clear glass.
2)	1/8 inch (3 mm) Plexiglass.
3)	1/8 inch (3 mm) Gray tint.
4)	1/8 inch (3 mm) Bronze tint.
5)	1/8 inch (3 mm) Antique art (semi-obscure).
6)	1/2 inch (12.5 mm) Insulated divided (square top only).
7)	1/2 inch (12.5 mm) Insulated full pane.
6.	Finish/Color: 
a.	Paint grade: factory primed white - sanding is required prior to top coat; available on medium density overlay plywood panels.
b.	Stain grade: Available on Mahogany plywood panels.
7.	Hardware: 14-gauge hinges.
8.	Springs: torsion springs.
a.	10,000 cycle.
b.	25,000 cycle.
c.	50,000 cycle.
9.	Lock: Interior mounted slide lock.
10.	Weatherstripping: Co-extruded PVC bulb-type strip at bottom. 
11.	Track: Provide track as recommended by manufacturer to suit loading required and clearances available.
12.	Rollers: ball bearing nylon-coated.
13.	Manual Operation.
14.	Electric Openers. 
2.5	RESIDENTIAL FIBERGLASS OVERHEAD DOORS
A.	Insulated Fiberglass Sectional Overhead Doors: Impression Collection 980 Series Insulated Fiberglass Doors by Overhead Door Corporation.
1.	Door Assembly: Engineered with the technology of Therma-Tru Accugrain to provide molded wood-grain fiberglass surface concealing durable steel construction. 
a.	Size: As indicated on the Drawings.
b.	Panel Thickness: 1 inch (25.4 mm).
c.	Panel Style: Pinch-resistant panels available in 7 feet (2.13 m) (3 panel) or 8 feet (2.44 m) (4 panel) configurations.
1)	Vertical Raised Panel, 981 Series.
2)	Horizontal Raised Panel, 982 Series.
3)	Vertical Slat Panel, 983 Series.
4)	Horizontal V-Groove Panel, 984 Series.
d.	Exterior Skin: Fiberglass with wood grain finish.
e.	Interior Skin: Smooth surfaced, hot dipped galvanized steel, pre-painted white.
f.	Insulation: Foamed-in-place polyurethane.
g.	Thermal Values: R-value of 7.6.
h.	Windload Design: Provide to meet the Design/Performance requirements specified.
i.	Window Design:
1)	Window Location: Top section.
2)	Window Style:
a)	Full Vision (Long panel) (983 Series).
b)	6 pane lite vertical.
c)	6 pane lite horizontal (982, 984 Series).
d)	8 pane lite (983 Series).
e)	12 pane lite (983 Series).
f)	16 pane lite (983 Series).
g)	20 pane lite (983 Series).
h)	Glass: Clear.
i)	Glass: Clear Insulated.
j)	Glass: Obscure.
k)	Glass: Satin etched.
2.	Wood Grain Finish/Color
a.	Cherry.
b.	Natural Oak.
c.	Walnut.
d.	Mahogany.
e.	Green.
f.	Gray.
g.	Clay.
h.	White.
i.	Honduran Mahogany.
j.	Red Oak.
3.	Hardware: powder-coated hinges, top brackets and struts.
4.	Lock: 
a.	Interior mounted slide lock.
b.	Optional keyed lock.
5.	Weatherstripping: Co-extruded PVC bulb-type strip at bottom. 
6.	Track: Provide track as recommended by manufacturer to suit loading required and clearances available.
7.	Nylon rollers.
8.	Manual Operation.
9.	Electric Openers. 
2.6	RESIDENTIAL VINYL OVERHEAD DOORS
A.	Insulated Vinyl Sectional Overhead Doors: Durafirm Collection 870 Series Insulated Vinyl Doors by Overhead Door Corporation.
1.	Door Assembly: Exterior skin material is .052 inch (1.32 mm) thick, color-fast, precision wood grain embossed vinyl which is bonded with the structural polyurethane core to the 22 gauge galvanized steel C-Channel internal struts. Fabricated with EPDM seals between sections.
a.	Size: As indicated on the Drawings.
b.	Panel Thickness: 1-3/8 inch (34.93 mm).
c.	Panel Style: Tongue and groove.
1)	Short Panel, 870 Series. 
2)	V5 Panel, 872 Series. 
d.	Exterior Skin: .052 inch (1.32 mm), color-fast, precision wood grain embossed vinyl skin.
e.	Interior Skin: .030 inch (.76 mm) thick, white embossed vinyl interior backer skin.
f.	Insulation: Foamed-in-place polyurethane.
g.	Thermal Values: R-value of 11.7.
h.	Windload Design: Provide to meet the Design/Performance requirements specified.
i.	Window Design:
1)	Window Location: Top section.
2)	Glass Type: 1/8 inch (3 mm) double strength
a)	Clear Insulated.
b)	Clear Non-insulated.
c)	Frosted Insulated.
d)	Frosted Non-insulated.
3)	Decorative Window Style:
a)	Full Vision (Short panel). 
b)	Cathedral 1.
c)	Ruston 1.
d)	Stockton 1.
e)	Williamsburg 4 (4 piece).
f)	Williamsburg 8 (8 piece).
g)	Glass: Clear. 
h)	Glass: Clear Insulated. 
i)	Glass: Obscure. 
j)	Glass: Obscure Insulated.
2.	Glass: Insulated Satin Etched, Finish/Color: Through-and-through color PVC construction; UV-resistant resin. 
a.	Glacier White.
b.	Monterey Sand.
c.	Adobe Cream.
d.	Cape Cod Gray.
3.	Hardware: Standard hinges.
4.	Spring: Torsion spring assembly.
5.	Lock: 
a.	Interior mounted slide lock.
b.	Optional keyed lock.
6.	Weatherstripping: Co-extruded PVC bulb-type strip at bottom. 
7.	Track: Provide track as recommended by manufacturer to suit loading required and clearances available.
8.	Standard rollers.
9.	Manual Operation.
10.	Electric Openers. 
2.7	ELECTRIC DOOR OPENERS
A.	Destiny 1500 Direct Drive Screw Opener 
1.	Electric Opener: Destiny 1500, Model 8060 light-duty assembly, complete with electric motor and factory-prewired motor controls, solid state microcontroller with built-in surge suppressor, UL and ULC listed self-monitoring infrared sensing device integral to operator system and accessories required for proper operation. 
a.	Adjustments: Force -Internal Up and Down / Electronic; Limits: Internal / Electronic.
b.	Electric Motor: 140 Volt DC, 1-1/4 HPc (Horsepower Comparable):
1)	110 VAC power supply.
2)	Wall Console.
3)	Housing plastic. 
4)	Opener to work with residential sectional or one-piece door; balance within plus or minus 10 percent full travel.
5)	Door height maximum 14 foot tall for sectional, or 8 foot tall for one piece door.
2.	Drive Type / Speed: 
a.	Direct Screw Drive: Approximately 12.0 inches per second plus or minus 0.5 inch minimum for open speed, 8.5 inches per second plus or minus 0.5 inch minimum for close speed.
3.	Operator Controls: RF 315 MHz and 390 MHz Auto Seek dual frequency remote system in compliance with FCC:
a.	One transmitter (3-button remote) standard with unit.
b.	Must be compatible to Overhead Door CodeDodger system.
c.	Receiver will store up to 28 total RF devices.
d.	Open range 500 feet.
e.	HomeLink and Car2U Home Automation System compatible
4.	Lighting: 110V, designed for up to two 100W bulbs. Light is set to stay on for 4 minutes during operation of opener.
5.	Materials:
a.	Steel chassis.
b.	Solid steel C-channel rail.
1)	Standard rail must handle residential sectional or one-piece door configurations.
2)	Professional units will have solid rail available for up to 10 foot doors or two-piece rails with center support for doors over 10 feet and up to 14 feet in height.
c.	Solid steel drive screw.
6.	Optional Accessories:
a.	Wireless Keyless Entry.
b.	Additional CodeDodger remote controls.
c.	Wall console.
d.	Door Detect Remote and Network Adapter.
B.	Odyssey 1200 Direct Drive Screw Opener 
1.	Electric Opener: Odyssey 1200, Model 7060 light-duty assembly, complete with electric motor and factory-prewired motor controls, solid state microcontroller with built-in surge suppressor, UL and ULC listed self-monitoring infrared sensing device integral to operator system and accessories required for proper operation. 
a.	Adjustments: Force -Internal Up and Down / Electronic; Limits: Internal / Electronic.
b.	Electric Motor: 140 Volt DC, 1 HPc (Horsepower Comparable):
1)	110 VAC power supply.
2)	Wall Console.
3)	Housing plastic. 
4)	Opener to work with residential sectional or one-piece door; balance within plus or minus 10 percent full travel.
5)	Door height maximum 14 foot tall for sectional, or 8 foot tall for one piece door.
2.	Drive Type / Speed: 
a.	Direct Screw Drive: Approximately 10.0 inches per second plus or minus 0.5 inch minimum for open speed, 8.5 inches per second plus or minus 0.5 inch minimum for close speed.
3.	Operator Controls: RF 315 MHz and 390 MHz Auto Seek dual frequency remote system in compliance with FCC:
a.	One transmitter (3-button remote) standard with unit.
b.	Must be compatible to Overhead Door CodeDodger system.
c.	Receiver will store up to 28 total RF devices.
d.	Open range 500 feet.
e.	HomeLink and Car2U Home Automation System compatible
4.	Lighting: 110V, designed for up to two 100W bulbs. Light is set to stay on for 4 minutes during operation of opener.
5.	Materials: 
a.	Steel chassis.
b.	Solid steel C-channel rail.
1)	Standard rail must handle residential sectional or one-piece door configurations.
2)	Professional units will have solid rail available for up to 10 foot doors or two-piece rails with center support for doors over 10 feet and up to 14 feet in height.
c.	Solid steel drive screw.
6.	Optional Accessories: 
a.	Wireless Keyless Entry.
b.	Additional CodeDodger remote controls.
c.	Wall console.
d.	Door Detect Remote and Network Adapter.
C.	Destiny 1200 Belt and Chain Opener:
1.	Electric Opener: Destiny 1200, Model 8030 light-duty assembly with electric motor and factory-prewired motor controls, solid state microcontroller with built-in surge suppressor, UL listed self-monitoring infrared sensing device integral to operator system and accessories required for proper operation. 
a.	Adjustments: Force - Internal Up and Down / Electronic; Limits: Internal / Electronic.
b.	Electric Motor: 140 Volt DC, 1 HPc (Horsepower Comparable):
1)	110 VAC power supply.
2)	Wall Console with work light activation and Sure-Lock security feature.
3)	Housing plastic. 
4)	Opener to work with residential sectional or one-piece door; balance within plus or minus 10 percent full travel.
5)	Door height maximum 14 foot tall for sectional, or 8 foot tall for one piece door 
2.	Drive Type / Speed: 
a.	Belt Drive: Approximately 9.0 inches per second plus or minus 0.5 inch minimum.
b.	Chain Drive: Approximately 9.0 inches per second plus or minus 0.5 inch minimum.
3.	Operator Controls: RF 315 MHz and 390 MHz Auto Seek dual frequency remote system in compliance with FCC:
a.	One transmitter (3-button remote) standard with unit.
b.	Must be compatible to Overhead Door CodeDodger system.
c.	Receiver will store up to 28 total RF devices.
d.	Open range 500 feet.
e.	HomeLink and Car2U Home Automation System compatible
4.	Lighting: 110V, designed for up to two 100W bulbs. Light is set to stay on for 4 minutes during operation of opener.
5.	Materials: 
a.	Steel chassis
b.	Solid steel C-channel rail
1)	Standard rail must handle residential sectional or one-piece door configurations.
2)	Professional units will have solid rail available for up to 10 foot doors or two-piece rails with center support for doors over 10 feet and up to 14 feet in height.
6.	Optional Accessories: 
a.	Wireless Keyless Entry.
b.	Additional CodeDodger remote controls.
c.	Wall console.
d.	Door Detect Remote and Network Adapter.
D.	Odyssey 1000 Belt and Chain Drive Opener:
1.	Electric Opener: Odyssey 1000, Model 7030 light-duty assembly, complete with electric motor and factory-prewired motor controls, solid state microcontroller with built-in surge suppressor, UL listed self-monitoring infrared sensing device integral to operator system and accessories required for proper operation. 
a.	Adjustments: Force -Internal Up and Down / Electronic; Limits: Internal / Electronic.
b.	Electric Motor: 140 Volt DC, 3/4 HPc (Horsepower Comparable) Power Plus:
1)	110 VAC power supply.
2)	Wall Console.
3)	Housing plastic. 
4)	Opener to work with residential sectional or one-piece door; balance within plus or minus 10 percent full travel.
5)	Door height maximum 14 foot tall for sectional, or 8 foot tall for one piece door.
2.	Drive Type / Speed: 
a.	Belt Drive: Approximately 7.5 inches per second plus or minus 0.5 inch minimum.
b.	Chain Drive: Approximately 7.5 inches per second plus or minus 0.5 inch minimum.
3.	Operator Controls: RF315 MHz and 390 MHz Auto Seek dual frequency remote system in compliance with FCC:
a.	One transmitter (3-button remote) standard with unit.
b.	Must be compatible to Overhead Door CodeDodger system.
c.	Receiver will store up to 28 total RF devices.
d.	Open range 500 feet.
e.	HomeLink and Car2U Home Automation System compatible
4.	Lighting: 110V, designed for up to two 100W bulbs. Light is set to stay on for 4 minutes during operation of opener.
5.	Materials: 
a.	Steel chassis
b.	Solid steel C-channel rail
1)	Standard rail must handle residential sectional or one-piece door configurations.
2)	Professional units will have solid rail available for up to 10 foot doors or two-piece rails with center support for doors over 10 feet and up to 14 feet in height.
6.	Optional Accessories: 
a.	Wireless Keyless Entry.
b.	Additional CodeDodger remote controls.
c.	Wall console.
d.	Door Detect Remote and Network Adapter.
E.	Legacy 850 Chain and Belt Drive Operator: 
1.	Electric Operator:  Model 2029 light-duty assembly, complete with electric motor and factory-pre-wired motor controls, solid state microcontroller with built-in surge suppressor, UL listed self-monitoring infrared sensing device integral to operator system and accessories required for proper operation.
a.	Adjustments: Force -Internal Up and Down; Limits: Internal.
b.	Electric Motor: 24 Volt DC, (800 N pull force minimum).
1)	110 VAC power supply.
2)	Wall console with work-light function and vacation lock.
3)	Housing plastic.
4)	Opener door weight maximum of 500 lbs sectional door - balance within plus or minus 10 percent full travel.
5)	Door height maximum 8 foot tall sectional door only.
6)	Drawbar-pull up to 110 lbs plus or minus 9 lbs.
2.	Drive Type / Speed: 
a.	Belt Drive: Approximately 7.0 inches per second plus or minus 0.5 inch minimum.
b.	Chain Drive: Approximately 6.5 inches per second plus or minus 0.5inch minimum.
3.	Operator Controls: RF dual frequency remote system in compliance with FCC:
a.	One transmitter standard with unit.
b.	Compatible to Overhead Door CodeDodger system.
c.	Receiver will store up to 15 total RF devices.
d.	Open range 500 feet.
e.	HomeLink and Car2U Home Automation System compatible.
4.	Lighting: 110 V, designed for one 60W bulb. Light is set to stay on for 4.5 minutes during operation of opener.
5.	Self-Diagnostic Safe-T-Beam System: Automatic safety reverse on close / automatic door stop on open and self-monitoring infrared safety devices. Power Failure/Quick Release Handle is standard.
6.	Materials: 
a.	Steel chassis
b.	Solid steel C Rail
1)	Standard rail must handle 7 foot tall sectional door configurations.
2)	Professional units will have an 8 foot solid rail available.
7.	Optional Accessories: 
a.	Wireless Keyless Entry.
b.	Additional CodeDodger remote controls.
F.	Standard 650 N Chain and Belt Drive Operator:
1.	Electric Operator:  Model 1029 light-duty assembly, complete with electric motor and factory-pre-wired motor controls, solid state microcontroller with built-in surge suppressor, UL listed self-monitoring infrared sensing device integral to operator system and accessories required for proper operation.
a.	Adjustments: Force - Independent Internal Up and Down; Limit: Internal.
b.	Electric Motor: 24 Volt DC, (600 N pull force minimum).
1)	110 VAC power supply.
2)	Wall push button.
3)	Housing plastic.
4)	Opener door weight maximum of 350 lbs sectional door - balance within plus or minus 10 percent full travel.
5)	Door height maximum 8 foot tall sectional door only.
6)	Drawbar-pull up to 110 lbs plus or minus 9 lbs.
2.	Drive Type / Speed: 
a.	Belt Drive: Approximately 6.5 inches per second plus or minus 0.3 inch minimum.
b.	Chain Drive: Approximately 6 inches per second plus or minus 0.3 inch minimum.
3.	Operator Controls: RF dual frequency remote system in compliance with FCC:
a.	One transmitter standard with unit.
b.	Compatible to Overhead Door CodeDodger system.
c.	Receiver will store up to 15 total RF devices.
d.	Open range 500 feet.
e.	HomeLink and Car2U Home Automation System compatible.
4.	Lighting: 110V, designed for up to one 60W bulb. Light is set to stay on for 4.5 minutes during operation of opener.
5.	Self-Diagnostic Safe-T-Beam System: Automatic safety reverse on close / automatic door stop on open and self-monitoring infrared safety devices. Power Failure/Quick Release Handle is standard.
6.	Materials: 
a.	Steel chassis.
b.	Solid steel C Rail.
1)	Standard rail must handle 7 foot tall sectional door configurations.
2)	Professional units will have an 8 foot solid rail available.
7.	Optional Accessories: 
a.	Wireless Keyless Entry.
b.	Additional CodeDodger remote controls.
c.	Wall console.
PART 3    EXECUTION
3.1	EXAMINATION
A.	Do not begin installation until openings and substrates have been properly prepared.
B.	Verify wall openings are ready to receive work and opening dimensions and tolerances are within specified limits.
C.	Verify electric power is available and of correct characteristics.
D.	If preparation is the responsibility of another installer, notify Architect of unsatisfactory preparation before proceeding.
3.2	PREPARATION
A.	Clean surfaces thoroughly prior to installation.
B.	Prepare surfaces using the methods recommended by the manufacturer for achieving the best result for the substrate under the project conditions.
3.3	INSTALLATION
A.	Install overhead doors, track and openers in accordance with approved shop drawings and the manufacturer's printed instructions.
B.	Coordinate installation with adjacent work to ensure proper clearances and allow for maintenance.
C.	Anchor assembly to wall construction and building framing without distortion or stress.
D.	Securely brace door tracks suspended from structure. Secure tracks to structural members only.
E.	Fit and align door assembly including hardware.
F.	Coordinate installation of electrical service with Section 16150.
3.4	CLEANING AND ADJUSTING
A.	Adjust door assembly to smooth operation and in full contact with weatherstripping.
B.	Clean doors, frames and glass.
C.	Remove temporary labels and visible markings.
3.5	PROTECTION
A.	Do not permit construction traffic through overhead door openings after adjustment and cleaning.
B.	Protect installed products until completion of project.
C.	Touch-up, damaged coatings and finishes and repair minor damage before Substantial Completion.

END OF SECTION