SECTION 08 36 16

SECTIONAL OVERHEAD DOORS

Display hidden notes to specifier. (Don't know how? Click Here) 
 Copyright 2007 -  2024 ARCAT, Inc. - All rights reserved

PART 1    GENERAL
1.1	SECTION INCLUDES
A.	Insulated Steel Sectional Overhead Doors.
B.	Aluminum Sectional Overhead Doors.
C.	Hardware.
D.	Electric Operators and Controls.
1.2	RELATED SECTIONS
A.	Section 03 30 00 - Cast-in-Place Concrete.
B.	Section 04 22 00 - Surface-Bonded Concrete Unit Masonry.
C.	Section 05 50 00 - Metal Fabrications.
D.	Section 06 11 00 - Wood Framing.
E.	Section 07 90 00 - Joint Protection.
F.	Section 08 71 53 - Security Door Hardware.
G.	Section 09 90 00 - Painting and Coating.
H.	Section 11 12 26 - Parking Fee Coin Collection Equipment.
I.	Section  11 13 00 - Loading Dock Equipment
J.	Section 26 27 16 - Electrical Cabinets and Enclosures.
K.	Section 26 05 00 - Common Work Results for Electrical.
1.3	REFERENCES
A.	ANSI/DASMA 102 - American National Standard Specifications for Sectional Overhead Type Doors.
1.4	DESIGN / PERFORMANCE REQUIREMENTS
A.	Wind Loads: Design and size components to withstand loads caused by pressure and suction of wind acting normal to plane of wall as calculated in accordance with applicable code.
1.	Design pressure: Standard wind load of 60.5 mph/97 km/h (9.39 psf/0.45 kPa).
2.	Design pressure: Wind load of 75.5 mph/121 km/h (14.62 psf/0.70 kPa).
3.	Design pressure: Wind load of 90.3 mph/144.5 km/h (20.88 psf/1.0 kPa).
B.	Wiring Connections: Requirements for electrical characteristics.
1.	115 volts, single phase, 60 Hz.
2.	230 volts, single phase, 60 Hz.
3.	230 volts, three phase, 60 Hz.
4.	460 volts, three phase, 60 Hz.
5.	575 volts, three phase, 60 Hz.
C.	Single-Source Responsibility: Provide doors, tracks, motors, and accessories from one manufacturer for each type of door. Provide secondary components from source acceptable to manufacturer of primary components
1.5	SUBMITTALS
A.	Submit under provisions of Section 01 30 00.
B.	Product Data:  Manufacturer's data sheets on each product to be used, including:
1.	Preparation instructions and recommendations.
2.	Storage and handling requirements and recommendations.
3.	Installation methods.
C.	Shop Drawings: Clearly show and describe in detail, detailed door assemblies and adjacent construction, including elevations, sections and details of door, track, hardware and operating components, dimensions, gauges, finishes and relationship of door, track, hardware, and operating components to adjacent construction.
D.	Selection Samples:  For each finish product specified, two complete sets of color chips representing manufacturer's full range of available colors and patterns.
E.	Verification Samples:  For each finish product specified, two samples, minimum size 6 inches (150 mm) square representing actual product, color, and patterns.
F.	Manufacturer's Certificates: Certify products meet or exceed specified requirements.
G.	Operation and Maintenance Data.
1.6	QUALITY ASSURANCE
A.	Manufacturer Qualifications: Company specializing in manufacturing products specified in this section with minimum five years documented experience.
B.	Installer Qualifications: Authorized representative of the manufacturer with minimum five years documented experience.
C.	Products Requiring Electrical Connection: Listed and classified by Underwriters Laboratories, Inc./ULC/CSA acceptable to authority having jurisdiction as suitable for purpose specified.
1.7	DELIVERY, STORAGE, AND HANDLING
A.	Store products in manufacturer's unopened packaging until ready for installation.
B.	Protect materials from exposure to moisture. Do not deliver until after wet work is complete and dry.
C.	Store materials in a dry, warm, ventilated weathertight location.
1.8	PROJECT CONDITIONS
A.	Pre-Installation Conference: Convene a pre-installation conference just prior to commencement of field operations, to establish procedures to maintain optimum working conditions and to coordinate this work with related and adjacent work.
PART 2    PRODUCTS
2.1	MANUFACTURERS
A.	Acceptable Manufacturer: Richards-Wilcox Canada, which is located at:<BR />5100 Timberlea Blvd.<BR />Mississauga, ON, Canada L4W 2S5<BR />Tel: 905-625-0037<BR />Fax: 905-625-0057<BR />Email:  marketing@rwdoors.com;Web: https://www.rwdoors.com 
B.	Substitutions:  Not permitted.
C.	Requests for substitutions will be considered in accordance with provisions of Section 01 60 00.
2.2	INSULATED STEEL SECTIONAL OVERHEAD DOORS
A.	Richards-Wilcox Canada Thermatite Model T-150-MR / T150 1-1/2 inch.
1.	Door Assembly: Metal/foam/metal sandwich panel construction. Doors comply with:
a.	ANSI/DASMA 102 - American National Standard Specifications for Sectional Overhead Type Doors.
2.	Size: See Drawings. Door is to be 1 inch (25 mm) higher than finished door opening and extend 1 inch (25 mm) beyond jamb on either side of finished door opening width.
3.	Section Joints: 1/4 inch (6.3 mm) ship-lap with thermal break.
4.	Section Thickness: 1.50 inches (38 mm).
5.	Face Sheet Profile:
a.	T-150-MR, Multi-Rib pattern with a non-repeating random stucco surface texture. 
b.	T-150 1-1/2 inch, Ribbed pattern with a non-repeating random stucco surface texture.
6.	Exterior Steel:  Pre-painted 0.016 inches (0.41 mm), hot-dipped galvanized.
7.	Interior Surface: Rib pattern with a non-repeating random stucco surface texture.
8.	Interior Steel: Pre-painted 0.016 inches (0.41 mm), hot-dipped galvanized.
9.	End Stiles: End Caps: 16 gauge (1.6 mm) hot dipped galvanized steel.
10.	Standard Springs: 10,000 cycles.
11.	High-Usage Package: Provide with optional high-usage package.
12.	Insulation: Foamed in place CFC-free and HCFC-free polyurethane, fully encapsulated.
13.	Thermal Value: R=13.21 ft2h F/Btu.
14.	Windows:
a.	Type AA: Dual Acrylic 26 inches by 13 inches (660 mm by 330 mm).
b.	Type B: Sealed glass 24 inches by 6 inches (610 mm by 152 mm).
c.	Type CPL: Sealed glass 24 inches by 8 inches (610 mm by 203 mm).
d.	Type D: Sealed glass 34 inches by 16 inches (864 mm by 406 mm).
e.	Type E: Sealed glass 24 inches by 12 inches (610 mm by 305 mm).
15.	Full Vision Sections: Type FV full vision aluminum glazing section. 
a.	Color:  
1)	White. 
2)	Mill finish. 
b.	Glazing: 
1)	1/8 inch (3 mm) acrylic. 
2)	1/8 inch (3 mm) polycarbonate. 
3)	1/8 inch (3 mm) plain glass. 
4)	1/8 inch (3 mm) tempered glass. 
5)	1/2 inch (12.7 mm) sealed plain glass. 
6)	1/2 inch (12.7 mm) sealed tempered glass.
16.	Colors:
a.	Exterior, Manufacturer's standard White.
b.	Exterior, Manufacturer's standard Brown.
c.	Interior, Manufacturer's standard White.
17.	Colors:
a.	Exterior, Manufacturer's standard Silver.
b.	Interior, Manufacturer's standard Silver.
18.	Wind load Design: ANSI/DASMA 102 standards to meet applicable code.
19.	Hardware: Zinc coated steel hinges and fixtures. Ball bearing rollers with hardened steel races.
20.	Lock:
a.	Interior mounted slide lock.
b.	Optional keyed lock.
21.	Seals:
a.	Standard continuous, replaceable dual seals between sections.
b.	Standard bottom seal: PVC/Vinyl type.
c.	Bottom seal: 3 inch (76 mm) vinyl retained in aluminum extrusion.
d.	Bottom seal: 4 inch (102 mm) vinyl retained in aluminum extrusion.
e.	Top seal: PVC/Vinyl type. 
f.	Jamb seal: Dual fin vinyl/steel.
g.	Jamb seal: Dual fin vinyl/aluminum. 
h.	Jamb seal: ADCA mount vinyl.
22.	Track: Provide track as recommended by manufacturer to suit loading required and clearances available.
23.	Operation:
a.	Manual.
b.	Electric.
B.	Richards-Wilcox Canada Thermatite Model T-175MR / T175 1-3/4 inch.
1.	Door Assembly: Metal/foam/metal sandwich panel construction. Doors comply with:
a.	ANSI/DASMA 102 - American National Standard Specifications for Sectional Overhead Type Doors.
2.	Size: See Drawings. Door is to be 1 inch (25 mm) higher than finished door opening and extend 1 inch (25 mm) beyond jamb on either side of finished door opening width.
3.	Section Joints: 1/4 inch (6.3 mm) ship-lap, with thermal break.
4.	Section Thickness: 1.75 inches (45 mm).
5.	Face Sheet Profile: 
a.	T-175MR, Multi-Rib pattern with a non-repeating random stucco surface texture. 
b.	T175 1-3/4 inch, Ribbed pattern with a non-repeating random stucco surface texture.
6.	Exterior Steel:  Pre-painted 0.019 inches (0.48 mm), hot-dipped galvanized.
7.	Interior Surface: Rib pattern with a non-repeating random stucco surface texture.
8.	Interior Steel: Pre-painted 0.016 inches (0.41 mm), hot-dipped galvanized.
9.	End Stiles: End Caps: 16 gauge (1.6 mm) hot dipped galvanized steel.
10.	Standard Springs: 10,000 cycles.
11.	High-Usage Package: Provide with optional high-usage package.
12.	Insulation: Foamed in place CFC-free and HCFC-free polyurethane, fully encapsulated.
13.	Thermal Value: R=16.00 ft2h F/Btu.
14.	Windows:
a.	Type AA: Dual acrylic 26 inches by 13 inches (660 mm by 330 mm).
b.	Type B: Sealed glass 24 inches by 6 inches (610 mm by 152 mm).
c.	Type CPL: Sealed glass 24 inches by 8 inches (610 mm by 203 mm).
d.	Type D: Sealed glass 34 inches by 16 inches (864 mm by 406 mm).
e.	Type E: Sealed glass 24 inches by 12 inches (610 mm by 305 mm).
15.	Full Vision Sections: Type FV full vision aluminum glazing section.
a.	Color:
1)	White.
2)	Mill finish.
3)	Clear anodized. 
b.	Glazing:
1)	1/8 inch (3 mm) acrylic.
2)	1/8 inch (3 mm) polycarbonate.
3)	1/8 inch (3 mm) plain glass.
4)	1/8 inch (3 mm) tempered glass.
5)	1/4 inch (6.3 mm) acrylic. 
6)	1/4 inch (6.3 mm) polycarbonate. 
7)	1/4 inch (6.3 mm) plain glass. 
8)	1/4 inch (6.3 mm) tempered glass.
9)	1/2 inch (12.7 mm) sealed plain glass.
10)	1/2 inch (12.7 mm) sealed tempered glass
16.	Colors:
a.	Exterior, Manufacturer's standard White.
b.	Exterior, Manufacturer's standard Brown.
c.	Interior, Manufacturer's standard White.
17.	Wind load Design: ANSI/DASMA 102 standards to meet applicable code.
18.	Hardware: Zinc coated steel hinges and fixtures. Ball bearing rollers with hardened steel races.
19.	Lock:
a.	Interior mounted slide lock.
b.	Optional keyed lock.
20.	Seals:
a.	Standard continuous, replaceable dual seals between sections.
b.	Standard bottom seal: 3 inch (76 mm) vinyl retained in PVC extrusion. 
c.	Bottom seal: 3 inch (76 mm) vinyl retained in aluminum extrusion
d.	Bottom seal: 4 inch (102 mm) vinyl retained in aluminum extrusion.
e.	Top seal: PVC/Vinyl type.
f.	Jamb seal: Dual fin vinyl/steel.
g.	Jamb seal: Dual fin vinyl/aluminum.
h.	Jamb seal: ADCA mount vinyl.
21.	Track: Provide track as recommended by manufacturer to suit loading required and clearances available.
22.	Operation:
a.	Manual.
b.	Electric.
C.	Richards-Wilcox Canada Thermatite Model T200-MR / T200 2 inch.
1.	Door Assembly: Metal/foam/metal sandwich panel construction. Doors comply with:
a.	ANSI/DASMA 102 - American National Standard Specifications for Sectional Overhead Type Doors.
2.	Size: See Drawings. Door is to be 1 inch (25 mm) higher than finished door opening and extend 1 inch (25 mm) beyond jamb on either side of finished door opening width.
3.	Section Joints: 1/4 inch (6.3 mm) ship-lap.
4.	Section Thickness: 2 inches (51 mm).
5.	Face Sheet Profile:
a.	T-200-MR, Multi-Rib pattern with a non-repeating random stucco surface texture. 
b.	T-200 2 inch, Ribbed pattern with a non-repeating random stucco surface texture.
6.	Exterior Steel:  Pre-painted 0.016 inches (0.41 mm), hot-dipped galvanized.
7.	Interior Surface: Rib pattern with a non-repeating random stucco surface texture.
8.	Interior Steel: Pre-painted 0.016 inches (0.41 mm), hot-dipped galvanized.
9.	End Stiles: End Caps: 16 gauge (1.6 mm) hot dipped galvanized steel.
10.	Standard Springs: 10,000 cycles.
11.	High-Usage Package: Provide with optional high-usage package.
12.	Insulation: Foamed in place CFC-free and HCFC-free polyurethane, fully encapsulated.
13.	Thermal Value: R=18.28 ft2h F/Btu, (U=0.310 W/m2K).
14.	Windows:
a.	Type AA: Dual acrylic 26 inches by 13 inches (660 mm by 330 mm).
b.	Type CPL: Sealed glass 24 inches by 8 inches (610 mm by 203 mm).
c.	Type D: Sealed glass 34 inches by 16 inches (864 mm by 406 mm).
d.	Type E: Sealed glass 24 inches by 12 inches (610 mm by 305 mm).
15.	Full Vision Sections: Type FV full vision aluminum glazing section.
a.	Color:
1)	White.
b.	Glazing:
1)	1/8 inch (3 mm) acrylic.
2)	1/8 inch (3 mm) polycarbonate.
3)	1/8 inch (3 mm) plain glass.
4)	1/8 inch (3 mm) tempered glass.
5)	1/4 inch (6.3 mm) acrylic.
6)	1/4 inch (6.3 mm) polycarbonate.
7)	1/4 inch (6.3 mm) plain glass.
8)	1/4 inch (6.3 mm) tempered glass.
9)	1/2 inch (12.7 mm) sealed plain glass.
10)	1/2 inch (12.7 mm) sealed tempered glass.
16.	Exterior Colors:
a.	Manufacturer's standard White.
17.	Interior Colors:
a.	Manufacturer's standard White.
18.	Wind load Design: ANSI/DASMA 102 standards to meet applicable code.
19.	Hardware: Zinc coated steel hinges and fixtures. Ball bearing rollers with hardened steel races.
20.	Lock:
a.	Interior mounted slide lock.
b.	Optional keyed lock.
21.	Seals:
a.	Standard continuous, replaceable dual seals between sections.
b.	Standard bottom seal: 3 inch (76 mm) vinyl retained in aluminum extrusion.
c.	Bottom seal: 4 inch (102 mm) vinyl retained in aluminum extrusion.
d.	Top seal: PVC/Vinyl type.
e.	Jamb seal: Dual fin vinyl/steel.
f.	Jamb seal: Dual fin vinyl/aluminum.
g.	Jamb seal: ADCA mount vinyl.
22.	Track: Provide track as recommended by manufacturer to suit loading required and clearances available.
23.	Operation:
a.	Manual.
b.	Electric.
D.	Richards-Wilcox Canada Thermatite Model T200C-MR / T200C; 2 inch thick.
1.	Door Assembly: Metal/foam/metal sandwich panel construction. Doors comply with:
a.	ANSI/DASMA 102 - American National Standard Specifications for Sectional Overhead Type Doors.
2.	Size: See Drawings. Door is to be 1 inch (25 mm) higher than finished door opening and extend 1 inch (25 mm) beyond jamb on either side of finished door opening width.
3.	Section Joints: 1/4 inch (6.3 mm) tongue and groove, pvc thermal break.
4.	Section Thickness: 2 inches (51 mm).
5.	Face Sheet Profile:
a.	T200C-MR, Multi-Rib pattern with a non-repeating random stucco surface texture. 
b.	T200C, 2 inch, Ribbed pattern with a non-repeating random stucco surface texture.
6.	Exterior Steel:  Pre-painted 0.016 inches (0.41 mm), hot-dipped galvanized.
7.	Interior Surface: Rib pattern with a non-repeating random stucco surface texture.
8.	Interior Steel: Pre-painted 0.016 inches (0.41 mm), hot-dipped galvanized.
9.	End Stiles: End Caps: 16 gauge (1.6 mm) hot dipped galvanized steel.
10.	Standard Springs: 10,000 cycles.
11.	High-Usage Package: Provide with optional high-usage package.
12.	Insulation: Foamed in place CFC-free and HCFC-free polyurethane, fully encapsulated.
13.	Thermal Value: R=18.28 ft2h F/Btu.
14.	Windows:
a.	Type AA: Dual acrylic 26 inches by 13 inches (660 mm by 330 mm).
b.	Type CPL: Sealed glass 24 inches by 8 inches (610 mm by 203 mm).
c.	Type D: Sealed glass 34 inches by 16 inches (864 mm by 406 mm).
d.	Type E: Sealed glass 24 inches by 12 inches (610 mm by 305 mm).
15.	Full Vision Sections: Type FV full vision aluminum glazing section.
a.	Color:
1)	Almond.
2)	Black.
3)	Bronze.
4)	Brown. 
5)	Cafe. 
6)	Slate Grey. 
7)	Desert Tan. 
8)	Sandstone. 
b.	Glazing:
1)	1/8 inch (3 mm) acrylic.
2)	1/8 inch (3 mm) polycarbonate.
3)	1/8 inch (3 mm) plain glass.
4)	1/8 inch (3 mm) tempered glass.
5)	1/4 inch (6.3 mm) acrylic.
6)	1/4 inch (6.3 mm) polycarbonate.
7)	1/4 inch (6.3 mm) plain glass.
8)	1/4 inch (6.3 mm) tempered glass.
9)	1/2 inch (12.7 mm) sealed plain glass.
10)	1/2 inch (12.7 mm) sealed tempered glass.
16.	Exterior Colors:
a.	Manufacturer's standard Almond.
b.	Manufacturer's standard Black. 
c.	Manufacturer's standard Bronze. 
d.	Manufacturer's standard Brown. 
e.	Manufacturer's standard Cafe. 
f.	Manufacturer's standard Slate Grey. 
g.	Manufacturer's standard Desert Tan. 
h.	Manufacturer's standard Sandstone.
17.	Interior Colors:
a.	Manufacturer's standard White.
18.	Wind load Design: ANSI/DASMA 102 standards to meet applicable code.
19.	Hardware: Zinc coated steel hinges and fixtures. Ball bearing rollers with hardened steel races.
20.	Lock:
a.	Interior mounted slide lock.
b.	Optional keyed lock.
21.	Seals:
a.	Standard continuous, extruded seal between sections.
b.	Standard bottom seal: 3 inch (76 mm) vinyl retained in aluminum extrusion.
c.	Bottom seal: 4 inch (102 mm) vinyl retained in aluminum extrusion.
d.	Top seal: PVC/Vinyl type.
e.	Jamb seal: Dual fin vinyl/steel.
f.	Jamb seal: Dual fin vinyl/aluminum.
g.	Jamb seal: ADCA mount vinyl.
22.	Track: Provide track as recommended by manufacturer to suit loading required and clearances available.
23.	Operation:
a.	Manual.
b.	Electric.
E.	Richards-Wilcox Canada Thermatite Model T-200A-MR / T-200-A.
1.	Door Assembly: Metal/foam/metal sandwich panel construction. Doors comply with:
a.	ANSI/DASMA 102 - American National Standard Specifications for Sectional Overhead Type Doors.
2.	Size: See Drawings. Door is to be 1 inch (25 mm) higher than finished door opening and extend 1 inch (25 mm) beyond jamb on either side of finished door opening width.
3.	Section Joints: 1/4 inch (6.3 mm) ship-lap.
4.	Section Thickness: 2 inches (51 mm).
5.	Face Sheet Profile:
a.	T-200-MR, Multi-Rib pattern with a non-repeating random stucco surface texture. 
b.	T-200 2 inch, Ribbed pattern with a non-repeating random stucco surface texture.
6.	Exterior Aluminum:  Pre-painted 0.025 inches (0.64 mm).
7.	Interior Surface: Rib pattern with a non-repeating random stucco surface texture.
8.	Interior Aluminum: Pre-painted 0.019 inches (0.48 mm).
9.	End Stiles: End Caps: 16 gauge (1.6 mm) hot dipped galvanized steel.
10.	Standard Springs: 10,000 cycles.
11.	High-Usage Package: Provide with optional high-usage package.
12.	Insulation: Foamed in place CFC-free and HCFC-free polyurethane, fully encapsulated.
13.	Thermal Value: R=18.28 ft2h F/Btu, (U=0.310 W/m2K).
14.	Windows:
a.	Type AA: Acrylic sealed 26 inches by 13 inches (660 mm by 330 mm).
b.	Type CPL: Sealed glass 24 inches by 8 inches (610 mm by 203 mm).
c.	Type D: Sealed glass 34 inches by 16 inches (864 mm by 406 mm).
d.	Type E: Sealed glass 24 inches by 12 inches (610 mm by 305 mm).
15.	Full Vision Sections: Type FV full vision aluminum glazing section.
a.	Color:
1)	White.
b.	Glazing:
1)	1/8 inch (3 mm) acrylic.
2)	1/8 inch (3 mm) polycarbonate.
3)	1/8 inch (3 mm) plain glass.
4)	1/8 inch (3 mm) tempered glass.
5)	1/4 inch (6.3 mm) acrylic.
6)	1/4 inch (6.3 mm) polycarbonate.
7)	1/4 inch (6.3 mm) plain glass.
8)	1/4 inch (6.3 mm) tempered glass.
9)	1/2 inch (12.7 mm) sealed plain glass.
10)	1/2 inch (12.7 mm) sealed tempered glass.
16.	Exterior Colors:
a.	Manufacturer's standard White.
17.	Interior Colors:
a.	Manufacturer's standard White.
18.	Wind load Design: ANSI/DASMA 102 standards to meet applicable code.
19.	Hardware: Zinc coated steel hinges and fixtures. Ball bearing rollers with hardened steel races.
20.	Lock:
a.	Interior mounted slide lock.
b.	Optional keyed lock.
21.	Seals:
a.	Standard continuous, replaceable dual seals between sections.
b.	Standard bottom seal: 3 inch (76 mm) vinyl retained in aluminum extrusion.
c.	Bottom seal: 4 inch (102 mm) vinyl retained in aluminum extrusion.
d.	Top seal: PVC/Vinyl type.
e.	Jamb seal: Dual fin vinyl/steel.
f.	Jamb seal: Dual fin vinyl/aluminum.
g.	Jamb seal: ADCA mount vinyl.
22.	Track: Provide track as recommended by manufacturer to suit loading required and clearances available.
23.	Operation:
a.	Manual.
b.	Electric.
F.	Richards-Wilcox Canada Thermatite Model T-200-20 2 inch.
1.	Door Assembly: Metal/foam/metal sandwich panel construction. Doors comply with:
a.	ANSI/DASMA 102 - American National Standard Specifications for Sectional Overhead Type Doors.
2.	Size: See Drawings. Door is to be 1 inch (25 mm) higher than finished door opening and extend 1 inch (25 mm) beyond jamb on either side of finished door opening width.
3.	Section Joints: 1/4 inch (6.3 mm) ship-lap.
4.	Section Thickness: 2 inches (51 mm).
5.	Face Sheet Profile:
a.	T-200-20, Flush 20 gauge.
6.	Exterior Aluminum:  Pre-painted 0.025 inches (0.64 mm).
7.	Interior Surface: Rib pattern with a non-repeating random stucco surface texture.
8.	Interior Aluminum: Pre-painted 0.019 inches (0.48 mm).
9.	End Stiles: End Caps: 16 gauge (1.6 mm) hot dipped galvanized steel.
10.	Standard Springs: 10,000 cycles.
11.	High-Usage Package: Provide with optional high-usage package.
12.	Insulation: Foamed in place CFC-free and HCFC-free polyurethane, fully encapsulated.
13.	Thermal Value: R=18.28 ft2h F/Btu,
14.	Windows:
a.	Type AA: Acrylic sealed 26 inches by 13 inches (660 mm by 330 mm).
b.	Type CPL: Sealed glass 24 inches by 8 inches (610 mm by 203 mm).
c.	Type D: Sealed glass 34 inches by 16 inches (864 mm by 406 mm).
d.	Type E: Sealed glass 24 inches by 12 inches (610 mm by 305 mm).
15.	Full Vision Sections: Type FV full vision aluminum glazing section.
a.	Color:
1)	White.
b.	Glazing:
1)	1/8 inch (3 mm) acrylic.
2)	1/8 inch (3 mm) polycarbonate.
3)	1/8 inch (3 mm) plain glass.
4)	1/8 inch (3 mm) tempered glass.
5)	1/4 inch (6.3 mm) acrylic.
6)	1/4 inch (6.3 mm) polycarbonate.
7)	1/4 inch (6.3 mm) plain glass.
8)	1/4 inch (6.3 mm) tempered glass.
9)	1/2 inch (12.7 mm) sealed plain glass.
10)	1/2 inch (12.7 mm) sealed tempered glass.
16.	Exterior Colors:
a.	Manufacturer's standard White.
17.	Interior Colors:
a.	Manufacturer's standard White.
18.	Wind load Design: ANSI/DASMA 102 standards to meet applicable code.
19.	Hardware: Zinc coated steel hinges and fixtures. Ball bearing rollers with hardened steel races.
20.	Lock:
a.	Interior mounted slide lock.
b.	Optional keyed lock.
21.	Seals:
a.	Standard continuous, replaceable dual seals between sections.
b.	Standard bottom seal: 3 inch (76 mm) vinyl retained in aluminum extrusion.
c.	Bottom seal: 4 inch (102 mm) vinyl retained in aluminum extrusion.
d.	Top seal: PVC/Vinyl type.
e.	Jamb seal: Dual fin vinyl/steel.
f.	Jamb seal: Dual fin vinyl/aluminum.
g.	Jamb seal: ADCA mount vinyl.
22.	Track: Provide track as recommended by manufacturer to suit loading required and clearances available.
23.	Operation:
a.	Manual.
b.	Electric.
G.	Richards-Wilcox Canada Model Thermatite T300-MR / T300-MR T-300.
1.	Door Assembly: Metal/foam/metal sandwich panel construction. Doors comply with: 
a.	ANSI/DASMA 102 - American National Standard Specifications for Sectional Overhead Type Doors. 
2.	Size: See Drawings. Door is to be 1 inch (25 mm) higher than finished door opening and extend 1 inch (25 mm) beyond jamb on either side of finished door opening width. 
3.	Section joints: 1/4 inch (6.3 mm) tongue and groove joint. 
4.	Section Thickness: 3 inches (76.2 mm). 
5.	Face Sheet Profile:
a.	T-300-MR, Multi-Rib pattern with a non-repeating random stucco surface texture, 0.016 inch (0.41 mm). 
b.	T-300, Ribbed pattern with a non-repeating random stucco surface texture, 0.016 inch (0.41 mm). 
6.	Exterior Steel:  Pre-painted 0.016 inches (0.41 mm), hot-dipped galvanized. 
7.	Interior Surface: Rib pattern with a non-repeating random stucco surface texture. 
8.	Interior Steel: Pre-painted 0.016 inches (0.41 mm), hot-dipped galvanized. 
9.	End Stiles: End Caps: 16 gauge (1.6 mm) hot dipped galvanized steel. 
10.	Standard Springs: 10,000 cycles. 
11.	High-Usage Package: Provide with optional high-usage package. 
12.	Insulation: Foamed in place CFC-free and HCFC-free polyurethane, fully encapsulated. 
13.	Thermal Value: R=24.54 ft2h F/Btu,
14.	Windows: 
a.	Type AA: Acrylic sealed 26 inches by 13 inches (660 mm by 330 mm). 
b.	Type CPL: Sealed glass 24 inches by 8 inches (610 mm by 203 mm). 
c.	Type D: Sealed glass 34 inches by 16 inches (864 mm by 406 mm). 
d.	Type E: Sealed glass 24 inches by 12 inches (610 mm by 305 mm). 
15.	Full Vision Sections: Type FV full vision aluminum glazing section.
a.	Color:  
1)	White. 
b.	Glazing: 
1)	1/8 inch (3 mm) acrylic. 
2)	1/8 inch (3 mm) polycarbonate. 
3)	1/8 inch (3 mm) plain glass. 
4)	1/8 inch (3 mm) tempered glass. 
5)	1/4 inch (6.3 mm) acrylic. 
6)	1/4 inch (6.3 mm) polycarbonate. 
7)	1/4 inch (6.3 mm) plain glass. 
8)	1/4 inch (6.3 mm) tempered glass. 
9)	1/2 inch (12.7 mm) sealed plain glass. 
10)	1/2 inch (12.7 mm) sealed tempered glass.
16.	Exterior Colors: 
a.	Manufacturer's standard White. 
17.	Interior Colors: 
a.	Manufacturer's standard White. 
18.	Wind load Design: ANSI/DASMA 102 standards to meet applicable code. 
19.	Hardware: Zinc coated steel hinges and fixtures. Ball bearing rollers with hardened steel races. 
20.	Lock: 
a.	Interior mounted slide lock. 
b.	Optional keyed lock. 
21.	Seals: 
a.	Standard continuous, replaceable dual seals between sections. 
b.	Standard bottom seal: 3 inch (76 mm) vinyl retained in aluminum extrusion. 
c.	Bottom seal: 4 inch (102 mm) vinyl retained in aluminum extrusion. 
d.	Top seal: PVC/Vinyl type. 
e.	Jamb seal: Dual fin vinyl/steel. 
f.	Jamb seal: Dual fin vinyl/aluminum. 
g.	Jamb seal: ADCA mount vinyl.
22.	Track: Provide track as recommended by manufacturer to suit loading required and clearances available. 
23.	Operation: 
a.	Manual. 
b.	Electric.
2.3	ALUMINUM SECTIONAL OVERHEAD DOORS
A.	Richards-Wilcox Canada Alumatite Model A150.
1.	Door Assembly: Stile and rail assembly secured with 1/4 inch (6 mm) diameter bolts.
2.	Size: See Drawings. Door is to be 1 inch (25 mm) higher than finished door opening and extend 1 inch (25 mm) beyond jamb on either side of finished door opening width.
3.	Section joints: 1/4 inch (6.3 mm) ship-lap.
4.	Section Thickness: 1-1/2 inches (38.1 mm).
5.	Stiles and Rails: 6063 - T6 aluminum alloy extrusions.
6.	Center Stiles: 2 inch (51 mm) wide.
7.	End Stiles: 3-3/8 inches (86 mm) wide for single end roller brackets; 6-3/8 inches (162 mm) for double end roller brackets.
8.	Top and Bottom Rail: 3-3/8 inches (86 mm) wide.
9.	Standard Springs: 10,000 cycles.
10.	High-Usage Package: Provide with optional high-usage package.
11.	Paneled Sections:
a.	Aluminum Panels: 0.051 inch (1.3 mm) thick embossed aluminum sheets.
b.	Thermalite Insulated Kick Panels: 1/2 inch (12.7 mm) thick insulation covered on both sides with 20 gauge (1 mm) embossed steel sheets.
c.	Thermalite Insulated Kick Panels: 1/2 inch (12.7 mm) thick insulation covered on both sides with 0.032 inch (0.8 mm) embossed aluminum sheets.
d.	Thermalite Plywood Kick Panels: 3/8 inch (9.5 mm) thick plywood covered on both sides with 20 gauge (1 mm) embossed steel sheets.
e.	Thermalite Plywood Kick Panels: 3/8 inch (9.5 mm) thick plywood covered on both sides with 0.032 inch (0.8 mm) embossed aluminum sheets.
12.	Glazing Sections:
a.	1/8 inch (3 mm) Acrylic glazing.
b.	1/8 inch (3 mm) Polycarbonate glazing.
c.	1/8 inch (3 mm) Plain Glass.
d.	1/8 inch (3 mm) Tempered Glass.
e.	1/2 inch (12.7 mm) Tempered Sealed Insulating Glass.
f.	1/2 inch (12.7 mm) Plain Sealed Insulating Glass.
13.	Finish and Color:
a.	Finish: Manufacturer's standard White.
b.	Finish: Clear anodizing to AA Spec A-21. 
c.	Finish: Mill Finish.
14.	Wind load Design: ANSI/DASMA 102 standards to meet applicable code.
15.	Hardware: Zinc coated steel hinges and fixtures. Ball bearing rollers with hardened steel races.
16.	Lock:
a.	Interior mounted slide lock.
b.	Optional keyed lock.
17.	Seals:
a.	Standard continuous replaceable dual seals between sections.
b.	Standard bottom seal: Vinyl bulb shaped astragal retained in bottom rail of the bottom section.
c.	Top seal: PVC/Vinyl type.
d.	Jamb seal: Dual fin vinyl/aluminum.
e.	Jamb seal: ADCA mount vinyl.
18.	Track: Provide track as recommended by manufacturer to suit loading required and clearances available.
19.	Operation:
a.	Manual.
b.	Electric.
B.	Richards-Wilcox Canada Alumatite Model A150T.
1.	Door Assembly: Stile and rail assembly secured with 1/4 inch (6 mm) diameter bolts for the upper sections and metal/foam/metal Thermatite sandwich bottom panel construction.
2.	Size: See Drawings. Door is to be 1 inch (25 mm) higher than finished door opening and extend 1 inch (25 mm) beyond jamb on either side of finished door opening width.
3.	Section Joints: 1/4 inch (6.3 mm) ship-lap.
4.	Section Thickness: 1-1/2 inches (38.1 mm).
5.	Center Stiles: 2 inch (51 mm) wide. 
6.	End Stiles: 3-3/8 inches (86 mm) wide for single end roller brackets; 6-3/8 inches (162 mm) for double end roller brackets. 
7.	Top and Bottom  Rail: 3-3/8 inches (86 mm) wide. 
8.	Stiles and Rails: 6063 - T6 aluminum alloy extrusions. 
9.	Standard Springs: 10,000 cycles. 
10.	High-Usage Package: Provide with optional high-usage package.
11.	Bottom Section: T150MR (Multi-rib).
a.	Panel Thickness: 1-1/2 inches (38.1 mm).
b.	Exterior Surface: Multi-Rib pattern with a non-repeating random stucco surface texture.
c.	Exterior Steel:  Pre-painted 0.016 inches (0.41 mm), hot-dipped galvanized.
d.	Interior Surface: Rib pattern with a non-repeating random stucco surface texture.
e.	Interior Steel: Pre-painted 0.016 inches (0.41 mm), hot-dipped galvanized.
f.	End Stiles: End Caps: 16 gauge (1.6 mm) hot dipped galvanized steel.
g.	Insulation: Foamed in place CFC-free and HCFC-free polyurethane, fully encapsulated.
h.	Thermal Value: R=13.21 ft2h F/Btu.
i.	Seals: Continuous dual seal between sections.
12.	Paneling:
a.	Aluminum Panels: 0.051 inch (1.3 mm) thick embossed aluminum sheets.
b.	Steel Panels: Two 20 gauge (1 mm) embossed steel sheets.
13.	Glazing:
a.	1/8 inch (3 mm) Acrylic glazing.
b.	1/8 inch (3 mm) Polycarbonate glazing.
c.	1/8 inch (3 mm) Plain Glass.
d.	1/8 inch (3 mm) Tempered Glass.
e.	1/2 inch (12.7 mm) Tempered Sealed Insulating Glass.
f.	1/2 inch (12.7 mm) Plain Sealed Insulating Glass.
14.	Finish and Color:
a.	Finish: Manufacturer's standard White.
b.	Finish: Clear anodizing to AA Spec A-21. 
c.	Finish: Mill finish.
15.	Wind load Design: ANSI/DASMA 102 standards to meet applicable code.
16.	Hardware: Zinc coated steel hinges and fixtures. Ball bearing rollers with hardened steel races. 
17.	Lock:
a.	Interior mounted slide lock.
b.	Optional keyed lock.
18.	Seals:
a.	Standard continuous replaceable dual seals between sections.
b.	Standard bottom seal: Vinyl bulb shaped astragal retained in bottom rail of the bottom section.
c.	Top seal: PVC/Vinyl type.
d.	Jamb seal: Dual fin vinyl/aluminum.
e.	Jamb seal: ADCA mount vinyl.
19.	Track: Provide track as recommended by manufacturer to suit loading required and clearances available.
20.	Operation:
a.	Manual.
b.	Electric.
C.	Richards-Wilcox Canada Alumatite Model A175.
1.	Door Assembly: Stile and rail assembly secured with 1/4 inch (6 mm) diameter bolts.
2.	Size: See Drawings. Door is to be 1 inch (25 mm) higher than finished door opening and extend 1 inch (25 mm) beyond jamb on either side of finished door opening width.
3.	Section joints: 1/4 inch (6.3 mm) ship-lap.
4.	Section Thickness: 1-3/4 inches (44 mm).
5.	Center Stiles: 2 inch (51 mm) wide.
6.	End Stiles: 3-3/8 inches (86 mm) wide for single end roller brackets. Doors width 16 fee 3 inches (4953 mm) and over shall all have double 5-7/8 inches (162 mm) wide end stiles. 
7.	Top Rail:
a.	3-3/8 inches (86 mm) wide.
b.	6-3/8 inches (162 mm) wide.
8.	Bottom Rail:
a.	3-3/8 inches (86 mm) wide.
b.	6-3/8 inches (162 mm) wide.
9.	Stiles and Rails: 6063 - T6 aluminum alloy extrusions.
10.	Standard Springs: 10,000 cycles.
11.	High-Usage Package: Provide with optional high-usage package.
12.	Paneling:
a.	Aluminum Panels: 0.051 inch (1.3 mm) thick embossed aluminum sheets.
b.	Steel Panels: Two 20 gauge (1 mm) embossed steel sheets.
c.	Insulated Kick Panels: 1/2 inch (12.7 mm) thick insulation covered on both sides with 20 gauge (1 mm) embossed steel sheets.
d.	Insulated Kick Panels: 1/2 inch (12.7 mm) thick insulation covered on both sides with 0.032 inch (0.8 mm) embossed aluminum sheets.
e.	Plywood Kick Panels: 3/8 inch (9.5 mm) thick plywood covered on both sides with 20 gauge (1 mm) embossed steel sheets.
f.	Plywood Kick Panels: 3/8 inch (9.5 mm) thick plywood covered on both sides with 0.032 inch (0.8 mm) embossed aluminum sheets.
13.	Glazing:
a.	1/8 inch (3 mm) Acrylic glazing.
b.	1/4 inch (6 mm) Acrylic glazing.
c.	1/8 inch (3 mm) Polycarbonate glazing.
d.	1/4 inch (6 mm) Polycarbonate glazing.
e.	1/8 inch (3 mm) plain glass.
f.	1/4 inch (6 mm) plain glass.
g.	1/8 inch (3 mm) tempered glass.
h.	1/4 inch (6 mm) tempered Glass.
i.	1/2 inch (12.7 mm) Tempered Sealed Insulating Glass.
j.	1/2 inch (12.7 mm) Plain Sealed Insulating Glass.
14.	Finish and Color:
a.	Finish: Clear anodized.
b.	Finish: Manufacturer's standard White.
c.	Finish: Mill finish.
15.	Wind load Design: ANSI/DASMA 102 standards to meet applicable code.
16.	Hardware: Zinc coated steel hinges and fixtures. Ball bearing rollers with hardened steel races.
17.	Lock:
a.	Interior mounted slide lock.
b.	Optional keyed lock.
18.	Seals:
a.	Standard continuous, replaceable dual seals between sections.
b.	Standard bottom seal: Vinyl bulb shaped astragal retained in bottom rail of the bottom section.
c.	Top seal: PVC/Vinyl type.
d.	Jamb seal: Dual fin vinyl/aluminum.
e.	Jamb seal: ADCA mount vinyl.
19.	Track: Provide track as recommended by manufacturer to suit loading required and clearances available.
20.	Operation:
a.	Manual.
b.	Electric.
D.	Richards-Wilcox Canada Alumatite Model A175T.
1.	Door Assembly: Stile and rail assembly secured with 1/4 inch (6 mm) diameter bolts and metal/foam/metal sandwich bottom panel construction.
2.	Size: See Drawings. Door is to be 1 inch (25 mm) higher than finished door opening and extend 1 inch (25 mm) beyond jamb on either side of finished door opening width.
3.	Section Joints: 1/4 inch (6.3 mm) ship-lap.
4.	Section Thickness: 1-3/4 inches (44 mm).
5.	Center Stiles: 2 inch (51 mm) wide. 
6.	End Stiles: 3-3/8 inches (86 mm) wide for single end roller brackets; 6-3/8 inches (162 mm) for double end roller brackets. 
7.	Top and Bottom Rail: 3-3/8 inches (86 mm) wide. 
8.	Stiles and Rails: 6063 - T6 aluminum alloy extrusions.
9.	Bottom Section: T175MR (Multi-rib).
a.	Exterior Surface: Multi-Rib pattern with a non-repeating random stucco surface texture.
b.	Exterior Steel:  Pre-painted 0.0196 inches (0.481 mm), hot-dipped galvanized.
c.	Interior Surface: Rib pattern with a non-repeating random stucco surface texture.
d.	Interior Steel: Pre-painted 0.016 inches (0.41 mm), hot-dipped galvanized.
e.	End Stiles: End Caps: 16 gauge (1.6 mm) hot dipped galvanized steel.
f.	Insulation: Foamed in place CFC-free and HCFC-free polyurethane, fully encapsulated.
g.	Thermal Value: R=16.00 ft2h F/Btu.
h.	Seals: Continuous dual seal between sections.
i.	Color:
1)	Manufacturer's standard White.
2)	Manufacturer's standard Silver.
3)	Manufacturer's standard Brown.
10.	Upper Sections: A175.
11.	Center Stiles: 2 inch (51 mm) wide.
12.	End Stiles:
a.	3-3/8 inches (85.7 mm) wide.
b.	6-3/8 inches (162 mm) wide.
13.	Top Rail:
a.	3-3/8 inches (85.7 mm) wide.
b.	6-3/8 inches (162 mm) wide.
14.	Stiles and Rails: 6063 - T6 aluminum alloy extrusions.
15.	Standard Springs: 10,000 cycles.
16.	High-Usage Package: Provide with optional high-usage package.
17.	Paneling:
a.	Aluminum Panels: 0.051 inch (1.3 mm) thick embossed aluminum sheets.
b.	Steel Panels: Two 20 gauge (1 mm) embossed steel sheets.
18.	Glazing:
a.	1/8 inch (3 mm) Acrylic glazing.
b.	1/4 inch (6 mm) Acrylic glazing.
c.	1/8 inch (3 mm) Polycarbonate glazing.
d.	1/4 inch (6 mm) Polycarbonate glazing.
e.	1/8 inch (3 mm) Plain Glass.
f.	1/4 inch (6 mm) Plain Glass.
g.	1/8 inch (3 mm) Tempered Glass.
h.	1/4 inch (6 mm) Tempered Glass.
i.	1/2 inch (12.7 mm) Tempered Sealed Insulating Glass.
j.	1/2 inch (12.7 mm) Plain Sealed Insulating Glass.
19.	Finish and Color:
a.	Finish: Clear anodized.
b.	Finish: Manufacturer's standard White.
c.	Finish: Mill finish.
20.	Wind load Design: ANSI/DASMA 102 standards to meet applicable code.
21.	Hardware: Zinc coated steel hinges and fixtures. Ball bearing rollers with hardened steel races.
22.	Lock:
a.	Interior mounted slide lock.
b.	Optional keyed lock.
23.	Seals:
a.	Standard continuous, replaceable dual seals between sections.
b.	Standard bottom seal: Vinyl bulb shaped astragal retained in bottom rail of the bottom section.
c.	Top seal: PVC/Vinyl type.
d.	Jamb seal: Dual fin vinyl/aluminum.
e.	Jamb seal: ADCA mount vinyl.
24.	Track: Provide track as recommended by manufacturer to suit loading required and clearances available.
25.	Operation:
a.	Manual.
b.	Electric.
E.	Richards-Wilcox Canada Polytite Model P175.
1.	Door Assembly: Stile and rail assembly secured with 1/4 inch (6 mm) diameter bolts. 
2.	Size: See Drawings. Door is to be 1 inch (25 mm) higher than finished door opening and extend 1 inch (25 mm) beyond jamb on either side of finished door opening width. 
3.	Section Thickness: 1-3/4 inches (45 mm) deep. 
4.	Section joints: 1/4 inch (6.3 mm) ship-lap.
5.	Center Stiles: 3 inch (76 mm) wide visible inside. 
6.	End Stiles: 
a.	2-1/2 inches (64 mm) wide. 
7.	Top Rail: 
a.	2-3/16 inches (56 mm) wide. 
8.	Bottom Rail: 
a.	2-9/16 inches (65 mm) wide. 
9.	Pair of meeting rails: 
a.	4-1/2 inches (114 mm) wide. 
10.	Stiles and Rails: 6063 - T6 aluminum alloy extrusions. 
11.	Standard Springs: 10,000 cycles. 
12.	High-Usage Package: Provide with optional high-usage package. 
13.	Paneling: 
14.	Paneling 5/8 inch (16 mm) thick, triple-wall extruded polycarbonate clear panels, R= 2.5 ft2hF/Btu, light transmission 74 percent, SHGC= 75 retained with polyethylene gaskets. 
15.	UV Protection: The exterior side of the polycarbonate is protected with a coextruded layer warranting resistance to atmospheric agents and U.V. rays. 
16.	Fire Reaction: ASTM E 84 Flame spread and smoke developed: Class A. 
17.	Panel Colors:
a.	Clear. 
b.	Clear (orange peel).
c.	Dark Bronze.
d.	Dark (Orange peel)
e.	Western Bronze.
f.	Blue. 
g.	Green.
h.	White (Opal). 
18.	Stile and Rail Finish and Color: 
a.	Finish: Clear anodized. 
b.	Finish: Manufacturer's standard White. 
c.	Finish: Bronze painted finish. 
19.	Wind load Design: ANSI/DASMA 102 standards to meet applicable code. 
20.	Hardware: Zinc coated steel hinges and fixtures. Ball bearing rollers with hardened steel races. 
21.	Lock: 
a.	Interior mounted slide lock. 
22.	Seals: 
a.	Standard continuous, replaceable seals between sections. 
b.	Standard bottom seal: Vinyl bulb shaped astragal retained in bottom rail of the bottom section. 
c.	Jamb/lintel seal: Dual fin vinyl/aluminum. 
d.	Jamb seal: ADCA mount vinyl. 
23.	Track: Provide track as recommended by manufacturer to suit loading required and clearances available. 
24.	Operation: 
a.	Manual. 
b.	Electric.
F.	Richards-Wilcox Canada Alumatite Door Model: P175T. 
1.	Door Assembly: Stile and rail assembly secured with 1/4 inch (6 mm) diameter bolts and metal/foam/metal sandwich bottom panel construction. 
2.	Size: See Drawings. Door is to be 1 inch (25 mm) higher than finished door opening and extend 1 inch (25 mm) beyond jamb on either side of finished door opening width. 
3.	Section joints: 1/4 inch (6.3 mm) ship-lap. 
4.	Bottom Section: T175MR (Multi-rib). 
a.	Section Thickness: 1-3/4 inches (44.45 mm). 
b.	Exterior Surface: Multi-Rib pattern with a non-repeating random stucco surface texture. 
c.	Exterior Steel:  Pre-painted 0.019 inches (0.48 mm), hot-dipped galvanized. 
d.	Interior Surface: Rib pattern with a non-repeating random stucco surface texture. 
e.	Interior Steel: Pre-painted 0.016 inches (0.41 mm), hot-dipped galvanized. 
f.	End Stiles: End Caps: 16 gauge (1.6 mm) hot dipped galvanized steel. 
g.	Insulation: Foamed in place CFC-free and HCFC-free polyurethane, fully encapsulated. 
h.	Thermal Value: R=16.004 ft2h F/Btu,
i.	Seals: Continuous dual seal between sections. 
j.	Color: 
1)	Manufacturer's standard White. 
2)	Manufacturer's standard Silver. 
3)	Manufacturer's standard Brown. 
5.	Upper Sections: P175. 
6.	Center Stiles: 3 inch (76 mm) wide visible inside. 
7.	End Stiles: 
a.	2-1/2 inches (64 mm) wide. 
8.	Top Rail: 
a.	2-3/16 inches (56 mm) wide. 
9.	Bottom Rail: 
a.	2-9/16 inches (65 mm) wide. 
10.	Pair of meeting rails: 
a.	4-1/2 inches (114 mm) wide.
11.	Stiles and Rails: 6063 - T6 aluminum alloy extrusions. 
12.	Standard Springs: 10,000 cycles. 
13.	High-Usage Package: Provide with optional high-usage package. 
14.	Paneling: 
15.	Paneling 5/8 inch (16 mm) thick, triple-wall extruded polycarbonate clear panels, R= 2.5 ft2hF/Btu, light transmission 74 percent, SHGC= 75 retained with polyethylene gaskets. 
16.	UV Protection: The exterior side of the polycarbonate is protected with a coextruded layer warranting resistance to atmospheric agents and U.V. rays. 
17.	Fire Reaction: ASTM E 84 Flame spread and smoke developed: Class A. 
18.	Paneling: Stock colors: 
a.	Clear. 
b.	Clear (Orange peel) 
c.	Dark Bronze. 
d.	Dark Brown (Orange peel)
e.	Western Bronze. 
f.	Blue. 
g.	Green. 
h.	White. 
19.	Stiles and Rails Finish and Color: 
a.	Finish: Clear anodized. 
b.	Finish: Manufacturer's standard White. 
c.	Finish: Bronze painted finish. 
20.	Wind load Design: ANSI/DASMA 102 standards to meet applicable code. 
21.	Hardware: Zinc coated steel hinges and fixtures. Ball bearing rollers with hardened steel races. 
22.	Lock: 
a.	Interior mounted slide lock. 
23.	Seals: 
a.	Standard continuous, replaceable seals between sections. 
b.	Standard bottom seal: Vinyl bulb shaped astragal retained in bottom rail of the bottom section. 
c.	Jamb/lintel seal: Dual fin vinyl/aluminum. 
d.	Jamb seal: ADCA mount vinyl. 
24.	Track: Provide track as recommended by manufacturer to suit loading required and clearances available. 
25.	Operation: 
a.	Manual. 
b.	Electric.
2.4	HARDWARE
A.	Counter-balance System:
1.	Spring assembly: Oil tempered torsion springs:
a.	Minimum 10,000 cycles.
b.	Minimum 25,000 cycles.
c.	Minimum 50,000 cycles.
d.	Minimum 75,000 cycles.
e.	Minimum 100,000 cycles
2.	Spring: Sized to suit the cycles.
3.	Shaft:
a.	1 inch (25 mm) 14 gauge mill or galvanized tube, recommended for doors up to 450 lbs (205 kg)
b.	1 inch (25 mm) 1/8 inch (3 mm) galvanized tube with full length keyway, recommended for doors up to 675 lbs (305 kg).
c.	1 inch (25 mm) solid CRS shaft with full length keyway, recommended for doors up to 1000 lbs (450 kg).
d.	1-1/4 inch (32 mm) solid CRS shaft with full-length keyway, recommended for doors over 1000 lbs (450 kg).
4.	Wire Rope: Aircraft type 7x19 construction with a safety factor of 5:1 minimum.
B.	Hardware: Include all the required hardware and zinc plated fasteners.
1.	Hinges: Linear style 12 gauge (2.75 mm) galvanized steel.
2.	Track 2 inches (50 mm): Rolled formed from 2 inch (50 mm) 14 gauge (2.0 mm) galvanized steel.
a.	Mount:
1)	ADCA Mount: Continuous adjustable track angle ADCA. Bolted type, field adjustable to ensure weather tight seal, fabricated from 14 gauge (2.0 mm) commercially galvanized steel, designed to provide continuous track support for full opening height.
2)	Clip Angle Mount: Pre-punched angle and clips designed for field bolting, adjustable to ensure weather tight seal and serviceability, the angles are fabricated from 0.093 inch (2.4 mm) commercially galvanized steel.
3)	Bracket Mount: Track brackets. Bolted type field adjustable to ensure weather tight seal, rib reinforced, stamped from 0.123 inch (3.1 mm) thick commercially galvanized steel.
b.	Horizontal Track Curve:
1)	12 inch (305 mm).
2)	16 inch (406 mm).
c.	Rollers:
1)	2 inch (50 mm) white nylon race, with 10 ball bearings and zinc plated stem.
d.	Roller Brackets: Fabricated from 14 gauge (2.0 mm) thick commercially galvanized steel. Graduated type design to suit the slope in the vertical track to ensure weather tight seal.
3.	Track 3 inches (75 mm): Rolled formed from 3 inch (75 mm) 12 gauge (2.7 mm) galvanized steel.
a.	Mount:
1)	ADCA Mount: Continuous adjustable track angle ADCA. Bolted type, field adjustable to ensure weather tight seal, fabricated from 13 gauge (2.4 mm) commercially galvanized steel, designed to provide continuous track support for full opening height.
2)	Clip Angle Mount: Pre-punched angle and clips designed for field bolting, adjustable to ensure weather tight seal and serviceability, the angles are fabricated from 0.093 inch (2.4 mm) commercially galvanized steel.
3)	Bracket Mount: Track brackets. Bolted type field adjustable to ensure weather tight seal, rib reinforced, stamped from 0.123 inch (3.1 mm) thick commercially galvanized steel.
b.	Track Hangers: Perforated type 1-1/4 inches by 1-1/4 inches (32 mm by 32 mm) angles, roll formed from 14 gauge (2.0 mm) thick commercially galvanized steel.
c.	Horizontal Track Curve: 16 inch (406 mm) radius.
d.	Rollers: 
1)	Hardened steel outer race, 2-7/8 inch (73 mm) diameter, with ten 5/16 inch (8 mm) ball bearings, and 7/16 inch (11 mm) diameter roller axels.
2)	UHMW outer race, 2-7/8 inch (73 mm) diameter, with ten 5/16 inch (8 mm) ball bearings, and 7/16 inch (11 mm) diameter roller axels.
e.	Roller Brackets: Fabricated from commercially galvanized steel. Graduated type design to suit the slope in the vertical track to ensure weather tight seal. Thickness as follows:
1)	11 gauge (3.1 mm).
2)	13 gauge (2.3 mm).
3)	14 gauge (2.4 mm).
4.	Horizontal angle: Full length.
5.	Locking:
a.	Interior slide bolt.
b.	Optional keyed lock.
6.	Pusher springs. For all standard lift doors with manual chain hoist or jackshaft electric operators.
7.	Bumper leaf springs: For high lift and vertical lift door applications.
8.	Across-the-door bar latch: Complete with night lock with an outside cylinder and handle for manually operated doors only.
9.	Across-the-door-bar latch inside only: Complete with night lock and interior handle. Electric interlock is required on electrically operated doors.
10.	Double end roller brackets and long stem rollers.
11.	Chain hoist: Chain and sprocket type design, 3:1 reduction.
12.	Double radius low headroom track: Minimum clearance required, 5 inches (127 mm) for 2 inch (50 mm) hardware and 7-1/2 inches (190 mm) for 3 inch (hardware).
13.	Follow the roof pitch: Install the track to follow roof pitch for standard lift and high lift doors.
14.	Track guards. Formed from 3/16 inch (4.8 mm) minimum steel, 60 inches (1520 mm high).
15.	Pull chain with spring.
16.	Exhaust port:
a.	3 inch (76 mm).
b.	4 inch (102 mm).
2.5	ELECTRIC OPERATORS AND CONTROLS
A.	Dyna-Hoist DC1000 Direct Drive: DC electric motor is directly coupled to a hollow shaft (30:1 reduction) worm gear reducer designed to install over keyed door shaft.  
1.	Motor: Continuous duty 1 HP, 90 V DC, 1750 rpm motor. 
2.	Operator: Suitable for 110 to 240 V, 1 PH, and 60 Hz power supply and shall have integral absolute encoder to control the door travel.
3.	Controls: Programmable wall mountable UL325 compliant NEMA 4X control panel with LCD display and OPEN-CLOSE-STOP buttons on cover, 24V DC control voltage, containing the back-up battery pack to operate the door in case of power failure, logic circuit board. Pulse with modulation programming to provide soft-start soft-stop, dynamic brake and speed control. Cycle counter, dual upper limit for partial opening, time delay on reverse and programmable close timer, terminal blocks for external activating and reversing devices. Includes the following: 
a.	Photo Cell:  NEMA 4 photo cell for mounting across the opening wired to reverse the door closing in case it detects an obstruction. 
b.	Safety Edge:  (Optional) Wireless, Featheredge on the leading edge of the bottom section wired to reverse the door closing in case it detects an obstruction. 
c.	Remote push button station: NEMA 4, three buttons OPEN-CLOSE-STOP bush button station for remote location. 
4.	Maximum Recommended Counter balance Sectional Door size:  600 square feet. 
B.	Dyna-Hoist DC750 Direct Drive: DC electric motor directly coupled to a hollow shaft (30:1 reduction) worm gear reducer designed to install over keyed door shaft. 
1.	Motor: Continuous duty 0.75 HP, 90 V DC, 1750 rpm motor. 
2.	Operator: Suitable for 110 to 240 V, 1 PH, and 60 Hz power supply and shall have integral absolute encoder to control the door travel.
3.	Controls: Programmable wall mountable UL325 compliant NEMA 4X control panel with LCD display and OPEN-CLOSE-STOP buttons on cover, 24V DC control voltage, containing the back-up battery pack to operate the door in case of power failure, logic circuit board. Pulse with modulation programming to provide soft-start soft-stop, dynamic brake and speed control. Cycle counter, dual upper limit for partial opening, time delay on reverse and programmable close timer, terminal blocks for external activating and reversing devices. Includes the following: 
a.	Photo Cell:  NEMA 4 photo cell for mounting across the opening wired to reverse the door closing in case it detects an obstruction. 
b.	Safety Edge:  (Optional) Wireless, Featheredge on the leading edge of the bottom section wired to reverse the door closing in case it detects an obstruction. 
c.	Remote push button station: NEMA 4, three buttons OPEN-CLOSE-STOP bush button station for remote location. 
4.	Maximum Recommended Counter balance Sectional Door size: 400 square feet. 
C.	Dyna-Hoist DC500 Direct Drive: DC electric motor directly coupled to a hollow shaft (30:1 reduction) worm gear reducer designed to install over keyed door shaft. 
1.	Motor: Continuous duty 0. 5 HP, 90 V DC, 1750 rpm motor. 
2.	Operator: Suitable for 110 to 240 V, 1 PH, and 60 Hz power supply and shall have integral absolute encoder to control the door travel.
3.	Controls: Programmable wall mountable UL325 compliant NEMA 4X control panel with LCD display and OPEN-CLOSE-STOP buttons on cover, 24V DC control voltage, containing the back-up battery pack to operate the door in case of power failure, logic circuit board. Pulse with modulation programming to provide soft-start soft-stop, dynamic brake and speed control. Cycle counter, dual upper limit for partial opening, time delay on reverse and programmable close timer, terminal blocks for external activating and reversing devices. Includes the following: 
a.	Photo Cell:  NEMA 4 photo cell for mounting across the opening wired to reverse the door closing in case it detects an obstruction. 
b.	Safety Edge:  (Optional) Wireless, Featheredge on the leading edge of the bottom section wired to reverse the door closing in case it detects an obstruction. 
c.	Remote push button station: NEMA 4, three buttons OPEN-CLOSE-STOP bush button station for remote location. 
4.	Maximum Recommended Counter balance Sectional Door size:  200 square feet. 
D.	AC Jack Shaft Hoist: Provide jack shaft type electric operators, for the doors indicated on the Drawings, to operate the doors at approximate speed of 8 inch (200 mm) per second. 
1.	Standard Lift Doors: Dyna-Hoist" heavy commercial duty, logic control type operator with on board radio receiver, model "Dyna-Hoist MO-OPH" to NEMA 1, shall be equipped with an adjustable friction clutch, time delay on reverse, mechanical brake, integral enclosure containing the controls, floor level disconnect, self engaging chain hoist with electrical cut-off for manual emergency operation, continuous duty motor __ HP minimum, suitable for ___ volts, _ Ph, 60 Hz power supply. 
2.	Standard High Lift and Full Vertical Lift Doors: Dyna-Hoist" heavy industrial duty, logic control type operator with on board radio receiver, model "Dyna-Hoist MO-OSH" to NEMA 1, shall be equipped with an adjustable friction clutch, cast iron flanged bearings on input and output shafts, time delay on reverse, solenoid brake, integral enclosure containing the controls, floor level disconnect, chain hoist with electrical cut-off for manual emergency operation, continuous duty motor __ HP minimum, suitable for ___ volts, _ Ph, 60 Hz power supply 
3.	Standard Controls: 
a.	Provide one push button station "OPEN/CLOSE/STOP" to NEMA 1, for inside wall mounting near the door jamb on the operator side. 
b.	Provide and install a "Featheredge" Reversing Safety Edge along the bottom edge of door to reverse on contact with an object as supplied by Service Door Industries. Hose type pneumatic safety edges will not be accepted. Power to the safety edge shall be supplied through reelite.
2.6	FABRICATION
A.	Fabricate the doors to dimensions detailed on reviewed shop drawings, free from distortion and defects detrimental to the appearance and performance.
B.	Ensure that site dimensions are taken and confirmed prior to the fabrication of the doors, frames and other components.
C.	Accurately fit joints and intersecting members with adequate fastenings.
PART 3    EXECUTION
3.1	EXAMINATION
A.	Do not begin installation until openings have been properly prepared.
B.	Verify wall openings are ready to receive work and opening dimensions and tolerances are within specified limits.
C.	Verify electric power is available and of correct characteristics.
D.	If preparation is the responsibility of another installer, notify Architect of unsatisfactory preparation before proceeding.
3.2	PREPARATION
A.	Clean surfaces thoroughly prior to installation.
B.	Prepare surfaces using the methods recommended by the manufacturer for achieving the best result for the substrate under the project conditions.
3.3	INSTALLATION
A.	Install in accordance with manufacturer's instructions.
B.	Install doors, tracks and operating equipment complete with necessary hardware, weather-stripping, anchors, hangers, brackets and accessories, in accordance to manufacturer's printed instructions.
C.	Assemble and erect work plumb, true, square, straight, level and accurate as per Drawings and reviewed shop drawings.
D.	Isolate metals where necessary to prevent corrosion due to contact with dissimilar metals and between metals, masonry and concrete. Use bituminous paint or butyl tape or as recommended, in writing, by the door manufacturer.
3.4	ADJUSTMENT AND DEMONSTRATION
A.	Lubrication: Upon completion of erection of units and operating equipment, lubricate moving parts before operation. Grease sprockets, bearings, cables, link chains and guides. Use lubricant as recommended by the manufacturer.
B.	Demonstration: Test-operate and adjust doors to perform smoothly, free from warp, twist or distortion. Demonstrate the operation to the satisfaction of the Architect at the same time of acceptance of the completed work.
3.5	PROTECTION
A.	Do not permit construction traffic through overhead door openings after adjustment and cleaning.
B.	Protect installed products until completion of project.
C.	Touch-up damaged coatings and finishes and repair minor damage before Substantial Completion.

END OF SECTION