SECTION 05 52 10

SAFETY RAILINGS AND GATES

Display hidden notes to specifier. (Don't know how? Click Here) 
 Copyright 2015 -  2025 ARCAT, Inc. - All rights reserved

PART 1    GENERAL
1.1	SECTION INCLUDES
A.	Modular safety rails. (FabRail)
B.	Self-closing safety gates of the following types:
1.	Self-closing safety gates. (A Series)
2.	Extended coverage self-closing safety gates. (XL Series)
3.	Standard bolt-on safety gates. (R Series)
4.	Standard bolt-on extended coverage safety gates. (RX Series)
5.	Safety gates for new construction. (Z Series)
6.	Full coverage safety gates. (ZT Series)
7.	Universal hinge mount safety gates. (G Series)
8.	Mezzanine-pivot safety gates. (MZ Series)
1.2	RELATED SECTIONS
A.	Section 05 50 00 - Metal Fabrications.
1.3	REFERENCES
A.	OSHA 29 CFR 1910.23 - Guarding Floor and Wall Openings and Holes. 
1.4	SUBMITTALS
A.	Submit under provisions of Section 01 30 00 - Administrative Requirements.
B.	Product Data: Manufacturer's data sheets on each product to be used, including:
1.	Preparation instructions and recommendations.
2.	Storage and handling requirements and recommendations.
3.	Installation methods.
C.	Shop Drawings: Drawings showing plans, elevations, sections and details of components.
1.5	QUALITY ASSURANCE
A.	Provide safety gates which meet or exceed OSHA 29CFR 1910.23 standards as applicable.
1.6	PROJECT CONDITIONS
A.	Field Measurements: Where safety railings are indicated to fit to other construction, check actual dimensions of other construction by accurate field measurements before delivery.
1.7	WARRANTY
A.	Warranty: Provide manufacture's standard limited warranty.
PART 2    PRODUCTS
2.1	MANUFACTURERS
A.	Acceptable Manufacturer: Tractel Ltd., which is located at:<BR />1615 Warden Ave.<BR />Scarborough, ON, Canada M1R 2T3<BR />Tel: 416-298-8822<BR />Email: request info (steve.gallagher@alimakgroup.com);Web: http://www.tractel.com | https://www.tractel.com/us 
B.	Substitutions: Not permitted.
C.	Requests for substitutions will be considered in accordance with provisions of Section 01 60 00 - Product Requirements.
2.2	MODULAR SAFETY RAILS
A.	Product: FabRail by FabEnCo, Inc.
1.	System: Modular components of top rail, midrail, posts and fittings. Designed with 42 inches (1067 mm) toprail height and 21 inches (533 mm) midrail height with posts on 7 feet (2134 mm) centers, anchors and fittings.
2.	Compliance: OSHA-compliant barrier, and BOCA building code.
3.	Rail and Post Material: 1-1/2 inches (38 mm) Flo-Coat (1.90 O.D).
4.	Rail and Post Material: 1-1/4 inches (32 mm) Flo-Coat (1.66 O.D).
5.	Fittings: Pre-assembled to posts for installation of rails. Fittings secured by hex nut and key wrench.
6.	Finish: Factory-applied powder coated finish selected from manufacturer's standard colors. 
2.3	SELF-CLOSING SAFETY GATES
A.	Self-Closing Safety Gates: A Series by FabEnCo, Inc.
1.	Material: A36 carbon steel galvanized, Model No. A71.
2.	Material: A36 carbon steel with safety yellow powder coat, Model No. A71-PC.
3.	Material: 6061-T6 aluminum, Model No. A82.
4.	Material: 316L stainless steel, Model No. A94.
5.	Height and Width: As selected from manufacturer's standard sizes, to fit clear opening indicated on the Drawings.
6.	Hardware: Stainless steel spring and zinc-plated bolts, nuts and washers.
B.	Extended Coverage Self-Closing Safety Gates: XL Series by FabEnCo, Inc.
1.	Material: A36 carbon steel galvanized, Model No. XL71.
2.	Material: A36 carbon steel with safety yellow powder coat, Model No. XL71-PC.
3.	Material: 6061-T6 aluminum, Model No. XL82.
4.	Material: 316L stainless steel, Model No. XL94.
5.	Height and Width: As selected from manufacturer's standard sizes, to fit clear opening indicated on the Drawings.
6.	Hardware: Stainless steel spring and zinc-plated bolts, nuts and washers.
7.	Clamp-on Toe Board Kit: A36 carbon steel galvanized.
8.	Clamp-on Toe Board Kit: A36 carbon steel with safety yellow powder coat.
C.	Standard Bolt-on Safety Gates: R Series by FabEnCo, Inc.
1.	Material: A36 carbon steel galvanized, Model No. R70.
2.	Material: A36 carbon steel with safety yellow powder coat, Model No. R70-PC.
3.	Height and Width: As selected from manufacturer's standard sizes, to fit clear opening indicated on the Drawings.
4.	Hardware: Stainless steel spring and zinc-plated bolts, nuts and washers.
5.	Stop Position: Standard.
6.	Stop Position: 90 degrees.
D.	Standard Bolt-on Extended Coverage Safety Gates: RX Series by FabEnCo, Inc.
1.	Material: A36 carbon steel galvanized, Model No. RX70.
2.	Material: A36 carbon steel with safety yellow powder coat, Model No. RX70-PC.
3.	Height and Width: As selected from manufacturer's standard sizes, to fit clear opening indicated on the Drawings.
4.	Hardware: Stainless steel spring and zinc-plated bolts, nuts and washers.
5.	Stop Position: Standard.
6.	Stop Position: 90 degrees.
7.	Swing: Left-hand swing.
8.	Swing: Right-hand swing.
9.	Clamp-on Toe Board Kit: A36 carbon steel galvanized.
10.	Clamp-on Toe Board Kit: A36 carbon steel with safety yellow powder coat.
E.	Safety Gates for New Construction. Z Series by FabEnCo, Inc.
1.	Material: A36 carbon steel galvanized, Model No. Z70.
2.	Material: A36 carbon steel with safety yellow powder coat, Model No. Z70-PC.
3.	Height and Width: As selected from manufacturer's standard sizes, to fit clear opening indicated on the Drawings.
4.	Hardware: Stainless steel spring and zinc-plated bolts, nuts and washers.
5.	Stop Position: Standard.
6.	Stop Position: 90 degrees.
7.	Clamp-on Toe Board Kit: A36 carbon steel galvanized.
8.	Clamp-on Toe Board Kit: A36 carbon steel with safety yellow powder coat.
F.	Full Coverage Safety Gates: ZT Series by FabEnCo, Inc.
1.	Material: A36 carbon steel galvanized, Model No. ZT70.
2.	Material: A36 carbon steel with safety yellow powder coat, Model No. ZT70-PC.
3.	Height and Width: As selected from manufacturer's standard sizes, to fit clear opening indicated on the Drawings.
4.	Hardware: Stainless steel spring and zinc-plated bolts, nuts and washers.
5.	Stop Position: Standard.
6.	Stop Position: 90 degrees.
G.	Universal Hinge Mount Safety Gates: G Series by FabEnCo, Inc.
1.	Material: A36 carbon steel galvanized, Model No. G70.
2.	Material: A36 carbon steel with safety yellow powder coat, Model No. G70-PC.
3.	Height and Width: As selected from manufacturer's standard sizes, to fit clear opening indicated on the Drawings.
4.	Hardware: Stainless steel spring and zinc-plated bolts, nuts and washers.
5.	Lateral Adjustment: 6 inches (152 mm).
H.	Mezzanine-Pivot Safety Gates: MZ Series by FabEnCo, Inc.
1.	Material: A36 carbon steel galvanized, Model No. MZ14.
2.	Material: A36 carbon steel with safety yellow powder coat, Model No. MZ14-PC.
3.	Material: 316L stainless steel.
4.	Height and Width: As selected from manufacturer's standard sizes, to fit clear opening indicated on the Drawings.
5.	Hardware: Stainless steel spring and zinc-plated bolts, nuts and washers.
6.	Pallet Width: Single.
7.	Pallet Width: Single.
PART 3    EXECUTION
3.1	EXAMINATION
A.	Do not begin installation until substrates have been properly prepared.
B.	If substrate preparation is the responsibility of another installer, notify Architect of unsatisfactory preparation before proceeding.
3.2	PREPARATION
A.	Prepare surfaces using the methods recommended by the manufacturer for achieving the best result for the substrate under the project conditions.
3.3	INSTALLATION
A.	Install in accordance with manufacturer's instructions and in proper relationship with adjacent construction. Test for proper operation and adjust until satisfactory results are achieved.
3.4	PROTECTION
A.	Protect installed products until completion of project.
B.	Touch-up, repair or replace damaged products before Substantial Completion.

END OF SECTION